--- a/drivers/staging/octeon/cvmx-helper-board.c
+++ b/drivers/staging/octeon/cvmx-helper-board.c
@@ -90,7 +90,7 @@ int cvmx_helper_board_get_mii_address(in
 	case CVMX_BOARD_TYPE_KODAMA:
 	case CVMX_BOARD_TYPE_EBH3100:
 	case CVMX_BOARD_TYPE_HIKARI:
-	case CVMX_BOARD_TYPE_CN3010_EVB_HS5:
+	//case CVMX_BOARD_TYPE_CN3010_EVB_HS5: /* hack for the WNDAP330 */
 	case CVMX_BOARD_TYPE_CN3005_EVB_HS5:
 	case CVMX_BOARD_TYPE_CN3020_EVB_HS5:
 		/*
@@ -103,6 +103,12 @@ int cvmx_helper_board_get_mii_address(in
 			return 9;
 		else
 			return -1;
+	case CVMX_BOARD_TYPE_CN3010_EVB_HS5: /* hack for the WNDAP330 */
+		/* We have only one port, using GMII */
+		if (ipd_port == 0)
+			return 9;
+		else
+			return -1;
 	case CVMX_BOARD_TYPE_NAC38:
 		/* Board has 8 RGMII ports PHYs are 0-7 */
 		if ((ipd_port >= 0) && (ipd_port < 4))
@@ -213,7 +219,7 @@ cvmx_helper_link_info_t __cvmx_helper_bo
 		result.s.speed = 1000;
 		return result;
 	case CVMX_BOARD_TYPE_EBH3100:
-	case CVMX_BOARD_TYPE_CN3010_EVB_HS5:
+	//case CVMX_BOARD_TYPE_CN3010_EVB_HS5: /* hack for the WNDAP330 */
 	case CVMX_BOARD_TYPE_CN3005_EVB_HS5:
 	case CVMX_BOARD_TYPE_CN3020_EVB_HS5:
 		/* Port 1 on these boards is always Gigabit */
@@ -225,6 +231,9 @@ cvmx_helper_link_info_t __cvmx_helper_bo
 		}
 		/* Fall through to the generic code below */
 		break;
+	case CVMX_BOARD_TYPE_CN3010_EVB_HS5: /* hack for the WNDAP330 */
+		is_broadcom_phy = 1;
+		break;
 	case CVMX_BOARD_TYPE_CUST_NB5:
 		/* Port 1 on these boards is always Gigabit */
 		if (ipd_port == 1) {
--- a/drivers/staging/octeon/cvmx-helper-rgmii.c
+++ b/drivers/staging/octeon/cvmx-helper-rgmii.c
@@ -66,13 +66,15 @@ int __cvmx_helper_rgmii_probe(int interf
 			cvmx_dprintf("ERROR: RGMII initialize called in "
 				     "SPI interface\n");
 		} else if (OCTEON_IS_MODEL(OCTEON_CN31XX)
-			   || OCTEON_IS_MODEL(OCTEON_CN30XX)
+			   //|| OCTEON_IS_MODEL(OCTEON_CN30XX)
 			   || OCTEON_IS_MODEL(OCTEON_CN50XX)) {
 			/*
 			 * On these chips "type" says we're in
 			 * GMII/MII mode. This limits us to 2 ports
 			 */
 			num_ports = 2;
+		} else if (OCTEON_IS_MODEL(OCTEON_CN30XX)) {
+			num_ports = 1;
 		} else {
 			cvmx_dprintf("ERROR: Unsupported Octeon model in %s\n",
 				     __func__);
--- a/arch/mips/pci/pci-octeon.c
+++ b/arch/mips/pci/pci-octeon.c
@@ -210,9 +210,11 @@ const char *octeon_get_pci_interrupts(vo
 		/* This is really the NAC38 */
 		return "AAAAADABAAAAAAAAAAAAAAAAAAAAAAAA";
 	case CVMX_BOARD_TYPE_EBH3100:
-	case CVMX_BOARD_TYPE_CN3010_EVB_HS5:
+	//case CVMX_BOARD_TYPE_CN3010_EVB_HS5:
 	case CVMX_BOARD_TYPE_CN3005_EVB_HS5:
 		return "AAABAAAAAAAAAAAAAAAAAAAAAAAAAAAA";
+	case CVMX_BOARD_TYPE_CN3010_EVB_HS5:
+		return "AAAAAAAAAAAAAABAAAAAAAAAAAAAAABA";
 	case CVMX_BOARD_TYPE_BBGW_REF:
 		return "AABCD";
 	case CVMX_BOARD_TYPE_THUNDER:
