Index: linux-2.6.35.8/drivers/serial/Kconfig
===================================================================
--- linux-2.6.35.8.orig/drivers/serial/Kconfig	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/serial/Kconfig	2010-11-01 11:34:31.000000000 +0100
@@ -1397,6 +1397,14 @@
 	help
 	  Support for Console on the NWP serial ports.
 
+config SERIAL_IFXMIPS
+	bool "IFXMips serial driver"
+	depends on IFXMIPS
+	select SERIAL_CORE
+	select SERIAL_CORE_CONSOLE
+	help
+	  Driver for the ifxmipss built in ASC hardware
+
 config SERIAL_QE
 	tristate "Freescale QUICC Engine serial port support"
 	depends on QUICC_ENGINE
Index: linux-2.6.35.8/drivers/serial/Makefile
===================================================================
--- linux-2.6.35.8.orig/drivers/serial/Makefile	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/serial/Makefile	2010-11-01 11:34:55.000000000 +0100
@@ -84,3 +84,4 @@
 obj-$(CONFIG_SERIAL_GRLIB_GAISLER_APBUART) += apbuart.o
 obj-$(CONFIG_SERIAL_ALTERA_JTAGUART) += altera_jtaguart.o
 obj-$(CONFIG_SERIAL_ALTERA_UART) += altera_uart.o
+obj-$(CONFIG_SERIAL_IFXMIPS) += ifxmips.o
Index: linux-2.6.35.8/drivers/net/Kconfig
===================================================================
--- linux-2.6.35.8.orig/drivers/net/Kconfig	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/net/Kconfig	2010-11-01 11:34:31.000000000 +0100
@@ -232,6 +232,12 @@
 
 source "drivers/net/arm/Kconfig"
 
+config IFXMIPS_MII0
+	tristate "Infineon IFXMips eth0 driver"
+	depends on IFXMIPS
+	help
+	  Support for the MII0 inside the IFXMips SOC
+
 config AX88796
 	tristate "ASIX AX88796 NE2000 clone support"
 	depends on ARM || MIPS || SUPERH
Index: linux-2.6.35.8/drivers/net/Makefile
===================================================================
--- linux-2.6.35.8.orig/drivers/net/Makefile	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/net/Makefile	2010-11-01 11:35:13.000000000 +0100
@@ -252,6 +252,7 @@
 obj-$(CONFIG_ENC28J60) += enc28j60.o
 obj-$(CONFIG_ETHOC) += ethoc.o
 obj-$(CONFIG_GRETH) += greth.o
+obj-$(CONFIG_IFXMIPS_MII0) += ifxmips.o
 
 obj-$(CONFIG_XTENSA_XT2000_SONIC) += xtsonic.o
 
Index: linux-2.6.35.8/drivers/mtd/maps/Kconfig
===================================================================
--- linux-2.6.35.8.orig/drivers/mtd/maps/Kconfig	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/mtd/maps/Kconfig	2010-11-01 11:34:31.000000000 +0100
@@ -251,6 +251,12 @@
 	help
 	  Support for flash chips on NETtel/SecureEdge/SnapGear boards.
 
+config MTD_IFXMIPS
+	tristate "IFXMIPS MTD support"
+	depends on IFXMIPS
+	help
+	  Flash memory access on AMD Alchemy Pb/Db/RDK Reference Boards
+
 config MTD_DILNETPC
 	tristate "CFI Flash device mapped on DIL/Net PC"
 	depends on X86 && MTD_CONCAT && MTD_PARTITIONS && MTD_CFI_INTELEXT && BROKEN
Index: linux-2.6.35.8/drivers/mtd/maps/Makefile
===================================================================
--- linux-2.6.35.8.orig/drivers/mtd/maps/Makefile	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/mtd/maps/Makefile	2010-11-01 11:34:31.000000000 +0100
@@ -59,3 +59,4 @@
 obj-$(CONFIG_MTD_RBTX4939)	+= rbtx4939-flash.o
 obj-$(CONFIG_MTD_VMU)		+= vmu-flash.o
 obj-$(CONFIG_MTD_GPIO_ADDR)	+= gpio-addr-flash.o
+obj-$(CONFIG_MTD_IFXMIPS)  += ifxmips.o
Index: linux-2.6.35.8/drivers/watchdog/Kconfig
===================================================================
--- linux-2.6.35.8.orig/drivers/watchdog/Kconfig	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/watchdog/Kconfig	2010-11-01 11:34:31.000000000 +0100
@@ -875,6 +875,12 @@
 	help
 	  Hardware driver for the built-in watchdog timer on TXx9 MIPS SoCs.
 
+config IFXMIPS_WDT
+	bool "IFXMips watchdog"
+	depends on IFXMIPS
+	help
+	  Hardware driver for the IFXMIPS Watchdog Timer.
+
 # PARISC Architecture
 
 # POWERPC Architecture
Index: linux-2.6.35.8/drivers/watchdog/Makefile
===================================================================
--- linux-2.6.35.8.orig/drivers/watchdog/Makefile	2010-10-29 06:52:43.000000000 +0200
+++ linux-2.6.35.8/drivers/watchdog/Makefile	2010-11-01 11:34:31.000000000 +0100
@@ -114,6 +114,7 @@
 obj-$(CONFIG_SIBYTE_WDOG) += sb_wdog.o
 obj-$(CONFIG_AR7_WDT) += ar7_wdt.o
 obj-$(CONFIG_TXX9_WDT) += txx9wdt.o
+obj-$(CONFIG_IFXMIPS_WDT) += ifxmips.o
 
 # PARISC Architecture
 
Index: linux-2.6.35.8/drivers/leds/Kconfig
===================================================================
--- linux-2.6.35.8.orig/drivers/leds/Kconfig	2010-11-01 11:19:33.000000000 +0100
+++ linux-2.6.35.8/drivers/leds/Kconfig	2010-11-01 11:34:31.000000000 +0100
@@ -311,6 +311,12 @@
 
 if LEDS_TRIGGERS
 
+config LEDS_IFXMIPS
+	tristate "LED Support for IFXMIPS  LEDs"
+	depends on LEDS_CLASS && IFXMIPS
+	help
+	  This option enables support for the CM-X270 LEDs.
+
 comment "LED Triggers"
 
 config LEDS_TRIGGER_TIMER
Index: linux-2.6.35.8/drivers/leds/Makefile
===================================================================
--- linux-2.6.35.8.orig/drivers/leds/Makefile	2010-11-01 11:19:33.000000000 +0100
+++ linux-2.6.35.8/drivers/leds/Makefile	2010-11-01 11:35:43.000000000 +0100
@@ -37,6 +37,7 @@
 obj-$(CONFIG_LEDS_ADP5520)		+= leds-adp5520.o
 obj-$(CONFIG_LEDS_DELL_NETBOOKS)	+= dell-led.o
 obj-$(CONFIG_LEDS_MC13783)		+= leds-mc13783.o
+obj-$(CONFIG_LEDS_IFXMIPS)		+= leds-ifxmips.o
 
 # LED SPI Drivers
 obj-$(CONFIG_LEDS_DAC124S085)		+= leds-dac124s085.o
