---
 arch/arm/include/asm/setup.h                      |   12 
 arch/arm/plat-omap/Kconfig                        |   32 +
 arch/arm/plat-omap/Makefile                       |    5 
 arch/arm/plat-omap/bootreason.c                   |   79 ++
 arch/arm/plat-omap/common.c                       |   70 ++
 arch/arm/plat-omap/component-version.c            |   64 ++
 arch/arm/plat-omap/gpio-switch.c                  |  554 ++++++++++++++++++
 arch/arm/plat-omap/include/mach/blizzard.h        |   12 
 arch/arm/plat-omap/include/mach/board-ams-delta.h |   76 ++
 arch/arm/plat-omap/include/mach/board-sx1.h       |   52 +
 arch/arm/plat-omap/include/mach/board-voiceblue.h |   19 
 arch/arm/plat-omap/include/mach/board.h           |  169 +++++
 arch/arm/plat-omap/include/mach/cbus.h            |   31 +
 arch/arm/plat-omap/include/mach/clkdev.h          |   13 
 arch/arm/plat-omap/include/mach/clkdev_omap.h     |   41 +
 arch/arm/plat-omap/include/mach/clock.h           |  168 +++++
 arch/arm/plat-omap/include/mach/clockdomain.h     |  111 +++
 arch/arm/plat-omap/include/mach/common.h          |   83 ++
 arch/arm/plat-omap/include/mach/control.h         |  325 ++++++++++
 arch/arm/plat-omap/include/mach/cpu.h             |  516 +++++++++++++++++
 arch/arm/plat-omap/include/mach/display.h         |  575 +++++++++++++++++++
 arch/arm/plat-omap/include/mach/dma.h             |  640 +++++++++++++++++++++
 arch/arm/plat-omap/include/mach/dmtimer.h         |   84 ++
 arch/arm/plat-omap/include/mach/dsp_common.h      |   40 +
 arch/arm/plat-omap/include/mach/fpga.h            |  197 ++++++
 arch/arm/plat-omap/include/mach/gpio-switch.h     |   54 +
 arch/arm/plat-omap/include/mach/gpio.h            |  129 ++++
 arch/arm/plat-omap/include/mach/gpmc-smc91x.h     |   42 +
 arch/arm/plat-omap/include/mach/gpmc.h            |  115 +++
 arch/arm/plat-omap/include/mach/hardware.h        |  290 +++++++++
 arch/arm/plat-omap/include/mach/hwa742.h          |    8 
 arch/arm/plat-omap/include/mach/i2c.h             |   39 +
 arch/arm/plat-omap/include/mach/io.h              |  287 +++++++++
 arch/arm/plat-omap/include/mach/iommu.h           |  168 +++++
 arch/arm/plat-omap/include/mach/iommu2.h          |   96 +++
 arch/arm/plat-omap/include/mach/iovmm.h           |   94 +++
 arch/arm/plat-omap/include/mach/irda.h            |   33 +
 arch/arm/plat-omap/include/mach/irqs.h            |  506 ++++++++++++++++
 arch/arm/plat-omap/include/mach/keypad.h          |   45 +
 arch/arm/plat-omap/include/mach/lcd_mipid.h       |   29 
 arch/arm/plat-omap/include/mach/led.h             |   24 
 arch/arm/plat-omap/include/mach/mailbox.h         |  111 +++
 arch/arm/plat-omap/include/mach/mcbsp.h           |  462 +++++++++++++++
 arch/arm/plat-omap/include/mach/mcspi.h           |   15 
 arch/arm/plat-omap/include/mach/memory.h          |  103 +++
 arch/arm/plat-omap/include/mach/menelaus.h        |   49 +
 arch/arm/plat-omap/include/mach/mmc.h             |  157 +++++
 arch/arm/plat-omap/include/mach/mux.h             |  662 ++++++++++++++++++++++
 arch/arm/plat-omap/include/mach/nand.h            |   24 
 arch/arm/plat-omap/include/mach/omap-alsa.h       |  123 ++++
 arch/arm/plat-omap/include/mach/omap-pm.h         |  301 ++++++++++
 arch/arm/plat-omap/include/mach/omap1510.h        |   50 +
 arch/arm/plat-omap/include/mach/omap16xx.h        |  202 ++++++
 arch/arm/plat-omap/include/mach/omap24xx.h        |   89 ++
 arch/arm/plat-omap/include/mach/omap34xx.h        |   86 ++
 arch/arm/plat-omap/include/mach/omap44xx.h        |   48 +
 arch/arm/plat-omap/include/mach/omap730.h         |  102 +++
 arch/arm/plat-omap/include/mach/omap7xx.h         |  104 +++
 arch/arm/plat-omap/include/mach/omap850.h         |  102 +++
 arch/arm/plat-omap/include/mach/omap_device.h     |  143 ++++
 arch/arm/plat-omap/include/mach/omap_hwmod.h      |  467 +++++++++++++++
 arch/arm/plat-omap/include/mach/onenand.h         |   43 +
 arch/arm/plat-omap/include/mach/param.h           |    8 
 arch/arm/plat-omap/include/mach/powerdomain.h     |  187 ++++++
 arch/arm/plat-omap/include/mach/prcm.h            |   39 +
 arch/arm/plat-omap/include/mach/sdrc.h            |  158 +++++
 arch/arm/plat-omap/include/mach/serial.h          |   65 ++
 arch/arm/plat-omap/include/mach/smp.h             |   53 +
 arch/arm/plat-omap/include/mach/sram.h            |   78 ++
 arch/arm/plat-omap/include/mach/system.h          |   51 +
 arch/arm/plat-omap/include/mach/tc.h              |  106 +++
 arch/arm/plat-omap/include/mach/timer-gp.h        |   17 
 arch/arm/plat-omap/include/mach/timex.h           |   41 +
 arch/arm/plat-omap/include/mach/uncompress.h      |   88 ++
 arch/arm/plat-omap/include/mach/usb.h             |  162 +++++
 arch/arm/plat-omap/include/mach/vram.h            |   62 ++
 arch/arm/plat-omap/include/mach/vrfb.h            |   50 +
 arch/arm/plat-omap/include/plat/board.h           |    8 
 arch/arm/plat-omap/include/plat/cbus.h            |   31 +
 79 files changed, 10573 insertions(+), 1 deletion(-)

--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/bootreason.c
@@ -0,0 +1,79 @@
+/*
+ * linux/arch/arm/plat-omap/bootreason.c
+ *
+ * OMAP Bootreason passing
+ *
+ * Copyright (c) 2004 Nokia
+ *
+ * Written by David Weinehall <david.weinehall@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+#include <linux/proc_fs.h>
+#include <linux/errno.h>
+#include <plat/board.h>
+
+static char boot_reason[16];
+
+static int omap_bootreason_read_proc(char *page, char **start, off_t off,
+					 int count, int *eof, void *data)
+{
+	int len = 0;
+
+	len += sprintf(page + len, "%s\n", boot_reason);
+
+	*start = page + off;
+
+	if (len > off)
+		len -= off;
+	else
+		len = 0;
+
+	return len < count ? len  : count;
+}
+
+static int __init bootreason_init(void)
+{
+	const struct omap_boot_reason_config *cfg;
+	int reason_valid = 0;
+
+	cfg = omap_get_config(OMAP_TAG_BOOT_REASON, struct omap_boot_reason_config);
+	if (cfg != NULL) {
+		strncpy(boot_reason, cfg->reason_str, sizeof(cfg->reason_str));
+		boot_reason[sizeof(cfg->reason_str)] = 0;
+		reason_valid = 1;
+	} else {
+		/* Read the boot reason from the OMAP registers */
+	}
+
+	if (!reason_valid)
+		return -ENOENT;
+
+	printk(KERN_INFO "Bootup reason: %s\n", boot_reason);
+
+	if (!create_proc_read_entry("bootreason", S_IRUGO, NULL,
+					omap_bootreason_read_proc, NULL))
+		return -ENOMEM;
+
+	return 0;
+}
+
+late_initcall(bootreason_init);
--- linux-2.6.36-rc4.orig/arch/arm/plat-omap/common.c
+++ linux-2.6.36-rc4/arch/arm/plat-omap/common.c
@@ -49,11 +49,81 @@
 struct omap_board_config_kernel *omap_board_config;
 int omap_board_config_size;
 
+unsigned char omap_bootloader_tag[1024];
+int omap_bootloader_tag_len;
+
+/* used by omap-smp.c and board-4430sdp.c */
+void __iomem *gic_cpu_base_addr;
+
+#ifdef CONFIG_OMAP_BOOT_TAG
+
+static int __init parse_tag_omap(const struct tag *tag)
+{
+	u32 size = tag->hdr.size - (sizeof(tag->hdr) >> 2);
+
+        size <<= 2;
+	if (size > sizeof(omap_bootloader_tag))
+		return -1;
+
+	memcpy(omap_bootloader_tag, tag->u.omap.data, size);
+	omap_bootloader_tag_len = size;
+
+        return 0;
+}
+
+__tagtable(ATAG_BOARD, parse_tag_omap);
+
+#endif
+
 static const void *get_config(u16 tag, size_t len, int skip, size_t *len_out)
 {
 	struct omap_board_config_kernel *kinfo = NULL;
 	int i;
 
+#ifdef CONFIG_OMAP_BOOT_TAG
+	struct omap_board_config_entry *info = NULL;
+
+	if (omap_bootloader_tag_len > 4)
+		info = (struct omap_board_config_entry *) omap_bootloader_tag;
+	while (info != NULL) {
+		u8 *next;
+
+		if (info->tag == tag) {
+			if (skip == 0)
+				break;
+			skip--;
+		}
+
+		if ((info->len & 0x03) != 0) {
+			/* We bail out to avoid an alignment fault */
+			printk(KERN_ERR "OMAP peripheral config: Length (%d) not word-aligned (tag %04x)\n",
+			       info->len, info->tag);
+			return NULL;
+		}
+		next = (u8 *) info + sizeof(*info) + info->len;
+		if (next >= omap_bootloader_tag + omap_bootloader_tag_len)
+			info = NULL;
+		else
+			info = (struct omap_board_config_entry *) next;
+	}
+	if (info != NULL) {
+		/* Check the length as a lame attempt to check for
+		 * binary inconsistency. */
+		if (len != NO_LENGTH_CHECK) {
+			/* Word-align len */
+			if (len & 0x03)
+				len = (len + 3) & ~0x03;
+			if (info->len != len) {
+				printk(KERN_ERR "OMAP peripheral config: Length mismatch with tag %x (want %d, got %d)\n",
+				       tag, len, info->len);
+				return NULL;
+			}
+		}
+		if (len_out != NULL)
+			*len_out = info->len;
+		return info->data;
+	}
+#endif
 	/* Try to find the config from the board-specific structures
 	 * in the kernel. */
 	for (i = 0; i < omap_board_config_size; i++) {
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/component-version.c
@@ -0,0 +1,64 @@
+/*
+ *  linux/arch/arm/plat-omap/component-version.c
+ *
+ *  Copyright (C) 2005 Nokia Corporation
+ *  Written by Juha Yrjölä <juha.yrjola@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/err.h>
+#include <linux/proc_fs.h>
+#include <plat/board.h>
+
+static int component_version_read_proc(char *page, char **start, off_t off,
+				       int count, int *eof, void *data)
+{
+	int len, i;
+	const struct omap_version_config *ver;
+	char *p;
+
+	i = 0;
+	p = page;
+	while ((ver = omap_get_nr_config(OMAP_TAG_VERSION_STR,
+					 struct omap_version_config, i)) != NULL) {
+		p += sprintf(p, "%-12s%s\n", ver->component, ver->version);
+		i++;
+	}
+
+	len = (p - page) - off;
+	if (len < 0)
+		len = 0;
+
+	*eof = (len <= count) ? 1 : 0;
+	*start = page + off;
+
+	return len;
+}
+
+static int __init component_version_init(void)
+{
+	if (omap_get_config(OMAP_TAG_VERSION_STR, struct omap_version_config) == NULL)
+		return -ENODEV;
+	if (!create_proc_read_entry("component_version", S_IRUGO, NULL,
+				    component_version_read_proc, NULL))
+		return -ENOMEM;
+
+	return 0;
+}
+
+static void __exit component_version_exit(void)
+{
+	remove_proc_entry("component_version", NULL);
+}
+
+late_initcall(component_version_init);
+module_exit(component_version_exit);
+
+MODULE_AUTHOR("Juha Yrjölä <juha.yrjola@nokia.com>");
+MODULE_DESCRIPTION("Component version driver");
+MODULE_LICENSE("GPL");
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/blizzard.h
@@ -0,0 +1,12 @@
+#ifndef _BLIZZARD_H
+#define _BLIZZARD_H
+
+struct blizzard_platform_data {
+	void		(*power_up)(struct device *dev);
+	void		(*power_down)(struct device *dev);
+	unsigned long	(*get_clock_rate)(struct device *dev);
+
+	unsigned	te_connected : 1;
+};
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/board-ams-delta.h
@@ -0,0 +1,76 @@
+/*
+ * arch/arm/plat-omap/include/mach/board-ams-delta.h
+ *
+ * Copyright (C) 2006 Jonathan McDowell <noodles@earth.li>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+#ifndef __ASM_ARCH_OMAP_AMS_DELTA_H
+#define __ASM_ARCH_OMAP_AMS_DELTA_H
+
+#if defined (CONFIG_MACH_AMS_DELTA)
+
+#define AMS_DELTA_LATCH1_PHYS		0x01000000
+#define AMS_DELTA_LATCH1_VIRT		0xEA000000
+#define AMS_DELTA_MODEM_PHYS		0x04000000
+#define AMS_DELTA_MODEM_VIRT		0xEB000000
+#define AMS_DELTA_LATCH2_PHYS		0x08000000
+#define AMS_DELTA_LATCH2_VIRT		0xEC000000
+
+#define AMS_DELTA_LATCH1_LED_CAMERA	0x01
+#define AMS_DELTA_LATCH1_LED_ADVERT	0x02
+#define AMS_DELTA_LATCH1_LED_EMAIL	0x04
+#define AMS_DELTA_LATCH1_LED_HANDSFREE	0x08
+#define AMS_DELTA_LATCH1_LED_VOICEMAIL	0x10
+#define AMS_DELTA_LATCH1_LED_VOICE	0x20
+
+#define AMS_DELTA_LATCH2_LCD_VBLEN	0x0001
+#define AMS_DELTA_LATCH2_LCD_NDISP	0x0002
+#define AMS_DELTA_LATCH2_NAND_NCE	0x0004
+#define AMS_DELTA_LATCH2_NAND_NRE	0x0008
+#define AMS_DELTA_LATCH2_NAND_NWP	0x0010
+#define AMS_DELTA_LATCH2_NAND_NWE	0x0020
+#define AMS_DELTA_LATCH2_NAND_ALE	0x0040
+#define AMS_DELTA_LATCH2_NAND_CLE	0x0080
+#define AMD_DELTA_LATCH2_KEYBRD_PWR	0x0100
+#define AMD_DELTA_LATCH2_KEYBRD_DATA	0x0200
+#define AMD_DELTA_LATCH2_SCARD_RSTIN	0x0400
+#define AMD_DELTA_LATCH2_SCARD_CMDVCC	0x0800
+#define AMS_DELTA_LATCH2_MODEM_NRESET	0x1000
+#define AMS_DELTA_LATCH2_MODEM_CODEC	0x2000
+
+#define AMS_DELTA_GPIO_PIN_KEYBRD_DATA	0
+#define AMS_DELTA_GPIO_PIN_KEYBRD_CLK	1
+#define AMS_DELTA_GPIO_PIN_MODEM_IRQ	2
+#define AMS_DELTA_GPIO_PIN_HOOK_SWITCH	4
+#define AMS_DELTA_GPIO_PIN_SCARD_NOFF	6
+#define AMS_DELTA_GPIO_PIN_SCARD_IO	7
+#define AMS_DELTA_GPIO_PIN_CONFIG	11
+#define AMS_DELTA_GPIO_PIN_NAND_RB	12
+
+#ifndef __ASSEMBLY__
+void ams_delta_latch1_write(u8 mask, u8 value);
+void ams_delta_latch2_write(u16 mask, u16 value);
+#endif
+
+#endif /* CONFIG_MACH_AMS_DELTA */
+
+#endif /* __ASM_ARCH_OMAP_AMS_DELTA_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/board.h
@@ -0,0 +1,169 @@
+/*
+ *  arch/arm/plat-omap/include/mach/board.h
+ *
+ *  Information structures for board-specific data
+ *
+ *  Copyright (C) 2004	Nokia Corporation
+ *  Written by Juha YrjÃ¶lÃ¤ <juha.yrjola@nokia.com>
+ */
+
+#ifndef _OMAP_BOARD_H
+#define _OMAP_BOARD_H
+
+#include <linux/types.h>
+
+#include <plat/gpio-switch.h>
+
+/*
+ * OMAP35x EVM revision
+ * Run time detection of EVM revision is done by reading Ethernet
+ * PHY ID -
+ *	GEN_1	= 0x01150000
+ *	GEN_2	= 0x92200000
+ */
+enum {
+	OMAP3EVM_BOARD_GEN_1 = 0,	/* EVM Rev between  A - D */
+	OMAP3EVM_BOARD_GEN_2,		/* EVM Rev >= Rev E */
+};
+
+/* Different peripheral ids */
+#define OMAP_TAG_CLOCK		0x4f01
+#define OMAP_TAG_LCD		0x4f05
+#define OMAP_TAG_GPIO_SWITCH	0x4f06
+#define OMAP_TAG_FBMEM		0x4f08
+#define OMAP_TAG_STI_CONSOLE	0x4f09
+#define OMAP_TAG_CAMERA_SENSOR	0x4f0a
+
+#define OMAP_TAG_BOOT_REASON    0x4f80
+#define OMAP_TAG_FLASH_PART	0x4f81
+#define OMAP_TAG_VERSION_STR	0x4f82
+
+struct omap_clock_config {
+	/* 0 for 12 MHz, 1 for 13 MHz and 2 for 19.2 MHz */
+	u8 system_clock_type;
+};
+
+struct omap_serial_console_config {
+	u8 console_uart;
+	u32 console_speed;
+};
+
+struct omap_sti_console_config {
+	unsigned enable:1;
+	u8 channel;
+};
+
+struct omap_camera_sensor_config {
+	u16 reset_gpio;
+	int (*power_on)(void * data);
+	int (*power_off)(void * data);
+};
+
+struct omap_usb_config {
+	/* Configure drivers according to the connectors on your board:
+	 *  - "A" connector (rectagular)
+	 *	... for host/OHCI use, set "register_host".
+	 *  - "B" connector (squarish) or "Mini-B"
+	 *	... for device/gadget use, set "register_dev".
+	 *  - "Mini-AB" connector (very similar to Mini-B)
+	 *	... for OTG use as device OR host, initialize "otg"
+	 */
+	unsigned	register_host:1;
+	unsigned	register_dev:1;
+	u8		otg;	/* port number, 1-based:  usb1 == 2 */
+
+	u8		hmc_mode;
+
+	/* implicitly true if otg:  host supports remote wakeup? */
+	u8		rwc;
+
+	/* signaling pins used to talk to transceiver on usbN:
+	 *  0 == usbN unused
+	 *  2 == usb0-only, using internal transceiver
+	 *  3 == 3 wire bidirectional
+	 *  4 == 4 wire bidirectional
+	 *  6 == 6 wire unidirectional (or TLL)
+	 */
+	u8		pins[3];
+};
+
+struct omap_lcd_config {
+	char panel_name[16];
+	char ctrl_name[16];
+	s16  nreset_gpio;
+	u8   data_lines;
+};
+
+struct device;
+struct fb_info;
+struct omap_backlight_config {
+	int default_intensity;
+	int (*set_power)(struct device *dev, int state);
+	int (*check_fb)(struct fb_info *fb);
+};
+
+struct omap_fbmem_config {
+	u32 start;
+	u32 size;
+};
+
+struct omap_pwm_led_platform_data {
+	const char *name;
+	int intensity_timer;
+	int blink_timer;
+	void (*set_power)(struct omap_pwm_led_platform_data *self, int on_off);
+};
+
+struct omap_uart_config {
+	/* Bit field of UARTs present; bit 0 --> UART1 */
+	unsigned int enabled_uarts;
+};
+
+
+struct omap_flash_part_config {
+	char part_table[0];
+};
+
+struct omap_boot_reason_config {
+	char reason_str[12];
+};
+
+struct omap_version_config {
+	char component[12];
+	char version[12];
+};
+
+struct omap_board_config_entry {
+	u16 tag;
+	u16 len;
+	u8  data[0];
+};
+
+struct omap_board_config_kernel {
+	u16 tag;
+	const void *data;
+};
+
+extern const void *__omap_get_config(u16 tag, size_t len, int nr);
+
+#define omap_get_config(tag, type) \
+	((const type *) __omap_get_config((tag), sizeof(type), 0))
+#define omap_get_nr_config(tag, type, nr) \
+	((const type *) __omap_get_config((tag), sizeof(type), (nr)))
+
+extern const void *omap_get_var_config(u16 tag, size_t *len);
+
+extern struct omap_board_config_kernel *omap_board_config;
+extern int omap_board_config_size;
+
+
+/* for TI reference platforms sharing the same debug card */
+extern int debug_card_init(u32 addr, unsigned gpio);
+
+/* OMAP3EVM revision */
+#if defined(CONFIG_MACH_OMAP3EVM)
+u8 get_omap3_evm_rev(void);
+#else
+#define get_omap3_evm_rev() (-EINVAL)
+#endif
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/board-sx1.h
@@ -0,0 +1,52 @@
+/*
+ * Siemens SX1 board definitions
+ *
+ * Copyright: Vovan888 at gmail com
+ *
+ * This package is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * THIS PACKAGE IS PROVIDED ``AS IS'' AND WITHOUT ANY EXPRESS OR
+ * IMPLIED WARRANTIES, INCLUDING, WITHOUT LIMITATION, THE IMPLIED
+ * WARRANTIES OF MERCHANTIBILITY AND FITNESS FOR A PARTICULAR PURPOSE.
+ */
+
+#ifndef __ASM_ARCH_SX1_I2C_CHIPS_H
+#define __ASM_ARCH_SX1_I2C_CHIPS_H
+
+#define SOFIA_MAX_LIGHT_VAL	0x2B
+
+#define SOFIA_I2C_ADDR		0x32
+/* Sofia reg 3 bits masks */
+#define SOFIA_POWER1_REG	0x03
+
+#define	SOFIA_USB_POWER		0x01
+#define	SOFIA_MMC_POWER		0x04
+#define	SOFIA_BLUETOOTH_POWER	0x08
+#define	SOFIA_MMILIGHT_POWER	0x20
+
+#define SOFIA_POWER2_REG	0x04
+#define SOFIA_BACKLIGHT_REG	0x06
+#define SOFIA_KEYLIGHT_REG	0x07
+#define SOFIA_DIMMING_REG	0x09
+
+
+/* Function Prototypes for SX1 devices control on I2C bus */
+
+int sx1_setbacklight(u8 backlight);
+int sx1_getbacklight(u8 *backlight);
+int sx1_setkeylight(u8 keylight);
+int sx1_getkeylight(u8 *keylight);
+
+int sx1_setmmipower(u8 onoff);
+int sx1_setusbpower(u8 onoff);
+int sx1_i2c_read_byte(u8 devaddr, u8 regoffset, u8 *value);
+int sx1_i2c_write_byte(u8 devaddr, u8 regoffset, u8 value);
+
+/* MMC prototypes */
+
+extern void sx1_mmc_init(void);
+extern void sx1_mmc_slot_cover_handler(void *arg, int state);
+
+#endif /* __ASM_ARCH_SX1_I2C_CHIPS_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/board-voiceblue.h
@@ -0,0 +1,19 @@
+/*
+ * Copyright (C) 2004 2N Telekomunikace, Ladislav Michl <michl@2n.cz>
+ *
+ * Hardware definitions for OMAP5910 based VoiceBlue board.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __ASM_ARCH_VOICEBLUE_H
+#define __ASM_ARCH_VOICEBLUE_H
+
+extern void voiceblue_wdt_enable(void);
+extern void voiceblue_wdt_disable(void);
+extern void voiceblue_wdt_ping(void);
+
+#endif /*  __ASM_ARCH_VOICEBLUE_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/cbus.h
@@ -0,0 +1,31 @@
+/*
+ * cbus.h - CBUS platform_data definition
+ *
+ * Copyright (C) 2004 - 2009 Nokia Corporation
+ *
+ * Written by Felipe Balbi <felipe.balbi@nokia.com>
+ *
+ * This file is subject to the terms and conditions of the GNU General
+ * Public License. See the file "COPYING" in the main directory of this
+ * archive for more details.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ */
+
+#ifndef __PLAT_CBUS_H
+#define __PLAT_CBUS_H
+
+struct cbus_host_platform_data {
+	int	dat_gpio;
+	int	clk_gpio;
+	int	sel_gpio;
+};
+
+#endif /* __PLAT_CBUS_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/clkdev.h
@@ -0,0 +1,13 @@
+#ifndef __MACH_CLKDEV_H
+#define __MACH_CLKDEV_H
+
+static inline int __clk_get(struct clk *clk)
+{
+	return 1;
+}
+
+static inline void __clk_put(struct clk *clk)
+{
+}
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/clkdev_omap.h
@@ -0,0 +1,41 @@
+/*
+ * clkdev <-> OMAP integration
+ *
+ * Russell King <linux@arm.linux.org.uk>
+ *
+ */
+
+#ifndef __ARCH_ARM_PLAT_OMAP_INCLUDE_PLAT_CLKDEV_OMAP_H
+#define __ARCH_ARM_PLAT_OMAP_INCLUDE_PLAT_CLKDEV_OMAP_H
+
+#include <asm/clkdev.h>
+
+struct omap_clk {
+	u16				cpu;
+	struct clk_lookup		lk;
+};
+
+#define CLK(dev, con, ck, cp) 		\
+	{				\
+		 .cpu = cp,		\
+		.lk = {			\
+			.dev_id = dev,	\
+			.con_id = con,	\
+			.clk = ck,	\
+		},			\
+	}
+
+
+#define CK_310		(1 << 0)
+#define CK_7XX		(1 << 1)
+#define CK_1510		(1 << 2)
+#define CK_16XX		(1 << 3)
+#define CK_243X		(1 << 4)
+#define CK_242X		(1 << 5)
+#define CK_343X		(1 << 6)
+#define CK_3430ES1	(1 << 7)
+#define CK_3430ES2	(1 << 8)
+#define CK_443X		(1 << 9)
+
+#endif
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/clockdomain.h
@@ -0,0 +1,111 @@
+/*
+ * arch/arm/plat-omap/include/mach/clockdomain.h
+ *
+ * OMAP2/3 clockdomain framework functions
+ *
+ * Copyright (C) 2008 Texas Instruments, Inc.
+ * Copyright (C) 2008 Nokia Corporation
+ *
+ * Written by Paul Walmsley
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __ASM_ARM_ARCH_OMAP_CLOCKDOMAIN_H
+#define __ASM_ARM_ARCH_OMAP_CLOCKDOMAIN_H
+
+#include <plat/powerdomain.h>
+#include <plat/clock.h>
+#include <plat/cpu.h>
+
+/* Clockdomain capability flags */
+#define CLKDM_CAN_FORCE_SLEEP			(1 << 0)
+#define CLKDM_CAN_FORCE_WAKEUP			(1 << 1)
+#define CLKDM_CAN_ENABLE_AUTO			(1 << 2)
+#define CLKDM_CAN_DISABLE_AUTO			(1 << 3)
+
+#define CLKDM_CAN_HWSUP		(CLKDM_CAN_ENABLE_AUTO | CLKDM_CAN_DISABLE_AUTO)
+#define CLKDM_CAN_SWSUP		(CLKDM_CAN_FORCE_SLEEP | CLKDM_CAN_FORCE_WAKEUP)
+#define CLKDM_CAN_HWSUP_SWSUP	(CLKDM_CAN_SWSUP | CLKDM_CAN_HWSUP)
+
+/* OMAP24XX CM_CLKSTCTRL_*.AUTOSTATE_* register bit values */
+#define OMAP24XX_CLKSTCTRL_DISABLE_AUTO		0x0
+#define OMAP24XX_CLKSTCTRL_ENABLE_AUTO		0x1
+
+/* OMAP3XXX CM_CLKSTCTRL_*.CLKTRCTRL_* register bit values */
+#define OMAP34XX_CLKSTCTRL_DISABLE_AUTO		0x0
+#define OMAP34XX_CLKSTCTRL_FORCE_SLEEP		0x1
+#define OMAP34XX_CLKSTCTRL_FORCE_WAKEUP		0x2
+#define OMAP34XX_CLKSTCTRL_ENABLE_AUTO		0x3
+
+/*
+ * struct clkdm_pwrdm_autodep - a powerdomain that should have wkdeps
+ * and sleepdeps added when a powerdomain should stay active in hwsup mode;
+ * and conversely, removed when the powerdomain should be allowed to go
+ * inactive in hwsup mode.
+ */
+struct clkdm_pwrdm_autodep {
+
+	union {
+		/* Name of the powerdomain to add a wkdep/sleepdep on */
+		const char *name;
+
+		/* Powerdomain pointer (looked up at clkdm_init() time) */
+		struct powerdomain *ptr;
+	} pwrdm;
+
+	/* OMAP chip types that this clockdomain dep is valid on */
+	const struct omap_chip_id omap_chip;
+
+};
+
+struct clockdomain {
+
+	/* Clockdomain name */
+	const char *name;
+
+	union {
+		/* Powerdomain enclosing this clockdomain */
+		const char *name;
+
+		/* Powerdomain pointer assigned at clkdm_register() */
+		struct powerdomain *ptr;
+	} pwrdm;
+
+	/* CLKTRCTRL/AUTOSTATE field mask in CM_CLKSTCTRL reg */
+	const u16 clktrctrl_mask;
+
+	/* Clockdomain capability flags */
+	const u8 flags;
+
+	/* OMAP chip types that this clockdomain is valid on */
+	const struct omap_chip_id omap_chip;
+
+	/* Usecount tracking */
+	atomic_t usecount;
+
+	struct list_head node;
+
+};
+
+void clkdm_init(struct clockdomain **clkdms, struct clkdm_pwrdm_autodep *autodeps);
+int clkdm_register(struct clockdomain *clkdm);
+int clkdm_unregister(struct clockdomain *clkdm);
+struct clockdomain *clkdm_lookup(const char *name);
+
+int clkdm_for_each(int (*fn)(struct clockdomain *clkdm, void *user),
+			void *user);
+struct powerdomain *clkdm_get_pwrdm(struct clockdomain *clkdm);
+
+void omap2_clkdm_allow_idle(struct clockdomain *clkdm);
+void omap2_clkdm_deny_idle(struct clockdomain *clkdm);
+
+int omap2_clkdm_wakeup(struct clockdomain *clkdm);
+int omap2_clkdm_sleep(struct clockdomain *clkdm);
+
+int omap2_clkdm_clk_enable(struct clockdomain *clkdm, struct clk *clk);
+int omap2_clkdm_clk_disable(struct clockdomain *clkdm, struct clk *clk);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/clock.h
@@ -0,0 +1,168 @@
+/*
+ *  arch/arm/plat-omap/include/mach/clock.h
+ *
+ *  Copyright (C) 2004 - 2005 Nokia corporation
+ *  Written by Tuukka Tikkanen <tuukka.tikkanen@elektrobit.com>
+ *  Based on clocks.h by Tony Lindgren, Gordon McNutt and RidgeRun, Inc
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __ARCH_ARM_OMAP_CLOCK_H
+#define __ARCH_ARM_OMAP_CLOCK_H
+
+#include <linux/list.h>
+
+struct module;
+struct clk;
+struct clockdomain;
+
+struct clkops {
+	int			(*enable)(struct clk *);
+	void			(*disable)(struct clk *);
+	void			(*find_idlest)(struct clk *, void __iomem **, u8 *);
+	void			(*find_companion)(struct clk *, void __iomem **, u8 *);
+};
+
+#if defined(CONFIG_ARCH_OMAP2) || defined(CONFIG_ARCH_OMAP3) || \
+		defined(CONFIG_ARCH_OMAP4)
+
+struct clksel_rate {
+	u32			val;
+	u8			div;
+	u8			flags;
+};
+
+struct clksel {
+	struct clk		 *parent;
+	const struct clksel_rate *rates;
+};
+
+struct dpll_data {
+	void __iomem		*mult_div1_reg;
+	u32			mult_mask;
+	u32			div1_mask;
+	struct clk		*clk_bypass;
+	struct clk		*clk_ref;
+	void __iomem		*control_reg;
+	u32			enable_mask;
+	unsigned int		rate_tolerance;
+	unsigned long		last_rounded_rate;
+	u16			last_rounded_m;
+	u8			last_rounded_n;
+	u8			min_divider;
+	u8			max_divider;
+	u32			max_tolerance;
+	u16			max_multiplier;
+#if defined(CONFIG_ARCH_OMAP3) || defined(CONFIG_ARCH_OMAP4)
+	u8			modes;
+	void __iomem		*autoidle_reg;
+	void __iomem		*idlest_reg;
+	u32			autoidle_mask;
+	u32			freqsel_mask;
+	u32			idlest_mask;
+	u8			auto_recal_bit;
+	u8			recal_en_bit;
+	u8			recal_st_bit;
+#  endif
+};
+
+#endif
+
+struct clk {
+	struct list_head	node;
+	const struct clkops	*ops;
+	const char		*name;
+	int			id;
+	struct clk		*parent;
+	struct list_head	children;
+	struct list_head	sibling;	/* node for children */
+	unsigned long		rate;
+	__u32			flags;
+	void __iomem		*enable_reg;
+	unsigned long		(*recalc)(struct clk *);
+	int			(*set_rate)(struct clk *, unsigned long);
+	long			(*round_rate)(struct clk *, unsigned long);
+	void			(*init)(struct clk *);
+	__u8			enable_bit;
+	__s8			usecount;
+#if defined(CONFIG_ARCH_OMAP2) || defined(CONFIG_ARCH_OMAP3) || \
+		defined(CONFIG_ARCH_OMAP4)
+	u8			fixed_div;
+	void __iomem		*clksel_reg;
+	u32			clksel_mask;
+	const struct clksel	*clksel;
+	struct dpll_data	*dpll_data;
+	const char		*clkdm_name;
+	struct clockdomain	*clkdm;
+#else
+	__u8			rate_offset;
+	__u8			src_offset;
+#endif
+#if defined(CONFIG_PM_DEBUG) && defined(CONFIG_DEBUG_FS)
+	struct dentry		*dent;	/* For visible tree hierarchy */
+#endif
+};
+
+struct cpufreq_frequency_table;
+
+struct clk_functions {
+	int		(*clk_enable)(struct clk *clk);
+	void		(*clk_disable)(struct clk *clk);
+	long		(*clk_round_rate)(struct clk *clk, unsigned long rate);
+	int		(*clk_set_rate)(struct clk *clk, unsigned long rate);
+	int		(*clk_set_parent)(struct clk *clk, struct clk *parent);
+	void		(*clk_allow_idle)(struct clk *clk);
+	void		(*clk_deny_idle)(struct clk *clk);
+	void		(*clk_disable_unused)(struct clk *clk);
+#ifdef CONFIG_CPU_FREQ
+	void		(*clk_init_cpufreq_table)(struct cpufreq_frequency_table **);
+#endif
+};
+
+extern unsigned int mpurate;
+
+extern int clk_init(struct clk_functions *custom_clocks);
+extern void clk_preinit(struct clk *clk);
+extern int clk_register(struct clk *clk);
+extern void clk_reparent(struct clk *child, struct clk *parent);
+extern void clk_unregister(struct clk *clk);
+extern void propagate_rate(struct clk *clk);
+extern void recalculate_root_clocks(void);
+extern unsigned long followparent_recalc(struct clk *clk);
+extern void clk_enable_init_clocks(void);
+#ifdef CONFIG_CPU_FREQ
+extern void clk_init_cpufreq_table(struct cpufreq_frequency_table **table);
+#endif
+
+extern const struct clkops clkops_null;
+
+/* Clock flags */
+/* bit 0 is free */
+#define RATE_FIXED		(1 << 1)	/* Fixed clock rate */
+/* bits 2-4 are free */
+#define ENABLE_REG_32BIT	(1 << 5)	/* Use 32-bit access */
+#define CLOCK_IDLE_CONTROL	(1 << 7)
+#define CLOCK_NO_IDLE_PARENT	(1 << 8)
+#define DELAYED_APP		(1 << 9)	/* Delay application of clock */
+#define CONFIG_PARTICIPANT	(1 << 10)	/* Fundamental clock */
+#define ENABLE_ON_INIT		(1 << 11)	/* Enable upon framework init */
+#define INVERT_ENABLE           (1 << 12)       /* 0 enables, 1 disables */
+#define CLOCK_IN_OMAP4430	(1 << 13)
+#define ALWAYS_ENABLED		(1 << 14)
+/* bits 13-31 are currently free */
+
+/* Clksel_rate flags */
+#define DEFAULT_RATE		(1 << 0)
+#define RATE_IN_242X		(1 << 1)
+#define RATE_IN_243X		(1 << 2)
+#define RATE_IN_343X		(1 << 3)	/* rates common to all 343X */
+#define RATE_IN_3430ES2		(1 << 4)	/* 3430ES2 rates only */
+#define RATE_IN_4430            (1 << 5)
+
+#define RATE_IN_24XX		(RATE_IN_242X | RATE_IN_243X)
+
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/common.h
@@ -0,0 +1,83 @@
+/*
+ * arch/arm/plat-omap/include/mach/common.h
+ *
+ * Header for code common to all OMAP machines.
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ARCH_ARM_MACH_OMAP_COMMON_H
+#define __ARCH_ARM_MACH_OMAP_COMMON_H
+
+#include <plat/i2c.h>
+
+struct sys_timer;
+
+/* used by omap-smp.c and board-4430sdp.c */
+extern void __iomem *gic_cpu_base_addr;
+
+extern void omap_map_common_io(void);
+extern struct sys_timer omap_timer;
+
+/* IO bases for various OMAP processors */
+struct omap_globals {
+	u32		class;		/* OMAP class to detect */
+	void __iomem	*tap;		/* Control module ID code */
+	void __iomem	*sdrc;		/* SDRAM Controller */
+	void __iomem	*sms;		/* SDRAM Memory Scheduler */
+	void __iomem	*ctrl;		/* System Control Module */
+	void __iomem	*prm;		/* Power and Reset Management */
+	void __iomem	*cm;		/* Clock Management */
+	void __iomem	*cm2;
+};
+
+void omap2_set_globals_242x(void);
+void omap2_set_globals_243x(void);
+void omap2_set_globals_343x(void);
+void omap2_set_globals_443x(void);
+
+/* These get called from omap2_set_globals_xxxx(), do not call these */
+void omap2_set_globals_tap(struct omap_globals *);
+void omap2_set_globals_sdrc(struct omap_globals *);
+void omap2_set_globals_control(struct omap_globals *);
+void omap2_set_globals_prcm(struct omap_globals *);
+
+/**
+ * omap_test_timeout - busy-loop, testing a condition
+ * @cond: condition to test until it evaluates to true
+ * @timeout: maximum number of microseconds in the timeout
+ * @index: loop index (integer)
+ *
+ * Loop waiting for @cond to become true or until at least @timeout
+ * microseconds have passed.  To use, define some integer @index in the
+ * calling code.  After running, if @index == @timeout, then the loop has
+ * timed out.
+ */
+#define omap_test_timeout(cond, timeout, index)			\
+({								\
+	for (index = 0; index < timeout; index++) {		\
+		if (cond)					\
+			break;					\
+		udelay(1);					\
+	}							\
+})
+
+#endif /* __ARCH_ARM_MACH_OMAP_COMMON_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/control.h
@@ -0,0 +1,325 @@
+/*
+ * arch/arm/plat-omap/include/mach/control.h
+ *
+ * OMAP2/3/4 System Control Module definitions
+ *
+ * Copyright (C) 2007-2009 Texas Instruments, Inc.
+ * Copyright (C) 2007-2008 Nokia Corporation
+ *
+ * Written by Paul Walmsley
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation.
+ */
+
+#ifndef __ASM_ARCH_CONTROL_H
+#define __ASM_ARCH_CONTROL_H
+
+#include <mach/io.h>
+
+#ifndef __ASSEMBLY__
+#define OMAP242X_CTRL_REGADDR(reg)					\
+		OMAP2_L4_IO_ADDRESS(OMAP242X_CTRL_BASE + (reg))
+#define OMAP243X_CTRL_REGADDR(reg)					\
+		OMAP2_L4_IO_ADDRESS(OMAP243X_CTRL_BASE + (reg))
+#define OMAP343X_CTRL_REGADDR(reg)					\
+		OMAP2_L4_IO_ADDRESS(OMAP343X_CTRL_BASE + (reg))
+#else
+#define OMAP242X_CTRL_REGADDR(reg)					\
+		OMAP2_L4_IO_ADDRESS(OMAP242X_CTRL_BASE + (reg))
+#define OMAP243X_CTRL_REGADDR(reg)					\
+		OMAP2_L4_IO_ADDRESS(OMAP243X_CTRL_BASE + (reg))
+#define OMAP343X_CTRL_REGADDR(reg)					\
+		OMAP2_L4_IO_ADDRESS(OMAP343X_CTRL_BASE + (reg))
+#endif /* __ASSEMBLY__ */
+
+/*
+ * As elsewhere, the "OMAP2_" prefix indicates that the macro is valid for
+ * OMAP24XX and OMAP34XX.
+ */
+
+/* Control submodule offsets */
+
+#define OMAP2_CONTROL_INTERFACE		0x000
+#define OMAP2_CONTROL_PADCONFS		0x030
+#define OMAP2_CONTROL_GENERAL		0x270
+#define OMAP343X_CONTROL_MEM_WKUP	0x600
+#define OMAP343X_CONTROL_PADCONFS_WKUP	0xa00
+#define OMAP343X_CONTROL_GENERAL_WKUP	0xa60
+
+/* Control register offsets - read/write with omap_ctrl_{read,write}{bwl}() */
+
+#define OMAP2_CONTROL_SYSCONFIG		(OMAP2_CONTROL_INTERFACE + 0x10)
+
+/* CONTROL_GENERAL register offsets common to OMAP2 & 3 */
+#define OMAP2_CONTROL_DEVCONF0		(OMAP2_CONTROL_GENERAL + 0x0004)
+#define OMAP2_CONTROL_MSUSPENDMUX_0	(OMAP2_CONTROL_GENERAL + 0x0020)
+#define OMAP2_CONTROL_MSUSPENDMUX_1	(OMAP2_CONTROL_GENERAL + 0x0024)
+#define OMAP2_CONTROL_MSUSPENDMUX_2	(OMAP2_CONTROL_GENERAL + 0x0028)
+#define OMAP2_CONTROL_MSUSPENDMUX_3	(OMAP2_CONTROL_GENERAL + 0x002c)
+#define OMAP2_CONTROL_MSUSPENDMUX_4	(OMAP2_CONTROL_GENERAL + 0x0030)
+#define OMAP2_CONTROL_MSUSPENDMUX_5	(OMAP2_CONTROL_GENERAL + 0x0034)
+#define OMAP2_CONTROL_SEC_CTRL		(OMAP2_CONTROL_GENERAL + 0x0040)
+#define OMAP2_CONTROL_RPUB_KEY_H_0	(OMAP2_CONTROL_GENERAL + 0x0090)
+#define OMAP2_CONTROL_RPUB_KEY_H_1	(OMAP2_CONTROL_GENERAL + 0x0094)
+#define OMAP2_CONTROL_RPUB_KEY_H_2	(OMAP2_CONTROL_GENERAL + 0x0098)
+#define OMAP2_CONTROL_RPUB_KEY_H_3	(OMAP2_CONTROL_GENERAL + 0x009c)
+
+/* 242x-only CONTROL_GENERAL register offsets */
+#define OMAP242X_CONTROL_DEVCONF	OMAP2_CONTROL_DEVCONF0 /* match TRM */
+#define OMAP242X_CONTROL_OCM_RAM_PERM	(OMAP2_CONTROL_GENERAL + 0x0068)
+
+/* 243x-only CONTROL_GENERAL register offsets */
+/* CONTROL_IVA2_BOOT{ADDR,MOD} are at the same place on 343x - noted below */
+#define OMAP243X_CONTROL_DEVCONF1	(OMAP2_CONTROL_GENERAL + 0x0078)
+#define OMAP243X_CONTROL_CSIRXFE	(OMAP2_CONTROL_GENERAL + 0x007c)
+#define OMAP243X_CONTROL_IVA2_BOOTADDR	(OMAP2_CONTROL_GENERAL + 0x0190)
+#define OMAP243X_CONTROL_IVA2_BOOTMOD	(OMAP2_CONTROL_GENERAL + 0x0194)
+#define OMAP243X_CONTROL_IVA2_GEMCFG	(OMAP2_CONTROL_GENERAL + 0x0198)
+#define OMAP243X_CONTROL_PBIAS_LITE	(OMAP2_CONTROL_GENERAL + 0x0230)
+
+/* 24xx-only CONTROL_GENERAL register offsets */
+#define OMAP24XX_CONTROL_DEBOBS		(OMAP2_CONTROL_GENERAL + 0x0000)
+#define OMAP24XX_CONTROL_EMU_SUPPORT	(OMAP2_CONTROL_GENERAL + 0x0008)
+#define OMAP24XX_CONTROL_SEC_TEST	(OMAP2_CONTROL_GENERAL + 0x0044)
+#define OMAP24XX_CONTROL_PSA_CTRL	(OMAP2_CONTROL_GENERAL + 0x0048)
+#define OMAP24XX_CONTROL_PSA_CMD	(OMAP2_CONTROL_GENERAL + 0x004c)
+#define OMAP24XX_CONTROL_PSA_VALUE	(OMAP2_CONTROL_GENERAL + 0x0050)
+#define OMAP24XX_CONTROL_SEC_EMU	(OMAP2_CONTROL_GENERAL + 0x0060)
+#define OMAP24XX_CONTROL_SEC_TAP	(OMAP2_CONTROL_GENERAL + 0x0064)
+#define OMAP24XX_CONTROL_OCM_PUB_RAM_ADD	(OMAP2_CONTROL_GENERAL + 0x006c)
+#define OMAP24XX_CONTROL_EXT_SEC_RAM_START_ADD	(OMAP2_CONTROL_GENERAL + 0x0070)
+#define OMAP24XX_CONTROL_EXT_SEC_RAM_STOP_ADD	(OMAP2_CONTROL_GENERAL + 0x0074)
+#define OMAP24XX_CONTROL_SEC_STATUS		(OMAP2_CONTROL_GENERAL + 0x0080)
+#define OMAP24XX_CONTROL_SEC_ERR_STATUS		(OMAP2_CONTROL_GENERAL + 0x0084)
+#define OMAP24XX_CONTROL_STATUS			(OMAP2_CONTROL_GENERAL + 0x0088)
+#define OMAP24XX_CONTROL_GENERAL_PURPOSE_STATUS	(OMAP2_CONTROL_GENERAL + 0x008c)
+#define OMAP24XX_CONTROL_RAND_KEY_0	(OMAP2_CONTROL_GENERAL + 0x00a0)
+#define OMAP24XX_CONTROL_RAND_KEY_1	(OMAP2_CONTROL_GENERAL + 0x00a4)
+#define OMAP24XX_CONTROL_RAND_KEY_2	(OMAP2_CONTROL_GENERAL + 0x00a8)
+#define OMAP24XX_CONTROL_RAND_KEY_3	(OMAP2_CONTROL_GENERAL + 0x00ac)
+#define OMAP24XX_CONTROL_CUST_KEY_0	(OMAP2_CONTROL_GENERAL + 0x00b0)
+#define OMAP24XX_CONTROL_CUST_KEY_1	(OMAP2_CONTROL_GENERAL + 0x00b4)
+#define OMAP24XX_CONTROL_TEST_KEY_0	(OMAP2_CONTROL_GENERAL + 0x00c0)
+#define OMAP24XX_CONTROL_TEST_KEY_1	(OMAP2_CONTROL_GENERAL + 0x00c4)
+#define OMAP24XX_CONTROL_TEST_KEY_2	(OMAP2_CONTROL_GENERAL + 0x00c8)
+#define OMAP24XX_CONTROL_TEST_KEY_3	(OMAP2_CONTROL_GENERAL + 0x00cc)
+#define OMAP24XX_CONTROL_TEST_KEY_4	(OMAP2_CONTROL_GENERAL + 0x00d0)
+#define OMAP24XX_CONTROL_TEST_KEY_5	(OMAP2_CONTROL_GENERAL + 0x00d4)
+#define OMAP24XX_CONTROL_TEST_KEY_6	(OMAP2_CONTROL_GENERAL + 0x00d8)
+#define OMAP24XX_CONTROL_TEST_KEY_7	(OMAP2_CONTROL_GENERAL + 0x00dc)
+#define OMAP24XX_CONTROL_TEST_KEY_8	(OMAP2_CONTROL_GENERAL + 0x00e0)
+#define OMAP24XX_CONTROL_TEST_KEY_9	(OMAP2_CONTROL_GENERAL + 0x00e4)
+
+#define OMAP343X_CONTROL_PADCONF_SYSNIRQ (OMAP2_CONTROL_INTERFACE + 0x01b0)
+
+/* 34xx-only CONTROL_GENERAL register offsets */
+#define OMAP343X_CONTROL_PADCONF_OFF	(OMAP2_CONTROL_GENERAL + 0x0000)
+#define OMAP343X_CONTROL_MEM_DFTRW0	(OMAP2_CONTROL_GENERAL + 0x0008)
+#define OMAP343X_CONTROL_MEM_DFTRW1	(OMAP2_CONTROL_GENERAL + 0x000c)
+#define OMAP343X_CONTROL_DEVCONF1	(OMAP2_CONTROL_GENERAL + 0x0068)
+#define OMAP343X_CONTROL_CSIRXFE		(OMAP2_CONTROL_GENERAL + 0x006c)
+#define OMAP343X_CONTROL_SEC_STATUS		(OMAP2_CONTROL_GENERAL + 0x0070)
+#define OMAP343X_CONTROL_SEC_ERR_STATUS		(OMAP2_CONTROL_GENERAL + 0x0074)
+#define OMAP343X_CONTROL_SEC_ERR_STATUS_DEBUG	(OMAP2_CONTROL_GENERAL + 0x0078)
+#define OMAP343X_CONTROL_STATUS			(OMAP2_CONTROL_GENERAL + 0x0080)
+#define OMAP343X_CONTROL_GENERAL_PURPOSE_STATUS	(OMAP2_CONTROL_GENERAL + 0x0084)
+#define OMAP343X_CONTROL_RPUB_KEY_H_4	(OMAP2_CONTROL_GENERAL + 0x00a0)
+#define OMAP343X_CONTROL_RAND_KEY_0	(OMAP2_CONTROL_GENERAL + 0x00a8)
+#define OMAP343X_CONTROL_RAND_KEY_1	(OMAP2_CONTROL_GENERAL + 0x00ac)
+#define OMAP343X_CONTROL_RAND_KEY_2	(OMAP2_CONTROL_GENERAL + 0x00b0)
+#define OMAP343X_CONTROL_RAND_KEY_3	(OMAP2_CONTROL_GENERAL + 0x00b4)
+#define OMAP343X_CONTROL_TEST_KEY_0	(OMAP2_CONTROL_GENERAL + 0x00c8)
+#define OMAP343X_CONTROL_TEST_KEY_1	(OMAP2_CONTROL_GENERAL + 0x00cc)
+#define OMAP343X_CONTROL_TEST_KEY_2	(OMAP2_CONTROL_GENERAL + 0x00d0)
+#define OMAP343X_CONTROL_TEST_KEY_3	(OMAP2_CONTROL_GENERAL + 0x00d4)
+#define OMAP343X_CONTROL_TEST_KEY_4	(OMAP2_CONTROL_GENERAL + 0x00d8)
+#define OMAP343X_CONTROL_TEST_KEY_5	(OMAP2_CONTROL_GENERAL + 0x00dc)
+#define OMAP343X_CONTROL_TEST_KEY_6	(OMAP2_CONTROL_GENERAL + 0x00e0)
+#define OMAP343X_CONTROL_TEST_KEY_7	(OMAP2_CONTROL_GENERAL + 0x00e4)
+#define OMAP343X_CONTROL_TEST_KEY_8	(OMAP2_CONTROL_GENERAL + 0x00e8)
+#define OMAP343X_CONTROL_TEST_KEY_9	(OMAP2_CONTROL_GENERAL + 0x00ec)
+#define OMAP343X_CONTROL_TEST_KEY_10	(OMAP2_CONTROL_GENERAL + 0x00f0)
+#define OMAP343X_CONTROL_TEST_KEY_11	(OMAP2_CONTROL_GENERAL + 0x00f4)
+#define OMAP343X_CONTROL_TEST_KEY_12	(OMAP2_CONTROL_GENERAL + 0x00f8)
+#define OMAP343X_CONTROL_TEST_KEY_13	(OMAP2_CONTROL_GENERAL + 0x00fc)
+#define OMAP343X_CONTROL_IVA2_BOOTADDR	(OMAP2_CONTROL_GENERAL + 0x0190)
+#define OMAP343X_CONTROL_IVA2_BOOTMOD	(OMAP2_CONTROL_GENERAL + 0x0194)
+#define OMAP343X_CONTROL_DEBOBS(i)	(OMAP2_CONTROL_GENERAL + 0x01B0 \
+					+ ((i) >> 1) * 4 + (!(i) & 1) * 2)
+#define OMAP343X_CONTROL_PROG_IO0	(OMAP2_CONTROL_GENERAL + 0x01D4)
+#define OMAP343X_CONTROL_PROG_IO1	(OMAP2_CONTROL_GENERAL + 0x01D8)
+#define OMAP343X_CONTROL_DSS_DPLL_SPREADING	(OMAP2_CONTROL_GENERAL + 0x01E0)
+#define OMAP343X_CONTROL_CORE_DPLL_SPREADING	(OMAP2_CONTROL_GENERAL + 0x01E4)
+#define OMAP343X_CONTROL_PER_DPLL_SPREADING	(OMAP2_CONTROL_GENERAL + 0x01E8)
+#define OMAP343X_CONTROL_USBHOST_DPLL_SPREADING	(OMAP2_CONTROL_GENERAL + 0x01EC)
+#define OMAP343X_CONTROL_PBIAS_LITE	(OMAP2_CONTROL_GENERAL + 0x02B0)
+#define OMAP343X_CONTROL_TEMP_SENSOR	(OMAP2_CONTROL_GENERAL + 0x02B4)
+#define OMAP343X_CONTROL_SRAMLDO4	(OMAP2_CONTROL_GENERAL + 0x02B8)
+#define OMAP343X_CONTROL_SRAMLDO5	(OMAP2_CONTROL_GENERAL + 0x02C0)
+#define OMAP343X_CONTROL_CSI		(OMAP2_CONTROL_GENERAL + 0x02C4)
+
+
+/* 34xx PADCONF register offsets */
+#define OMAP343X_PADCONF_ETK(i)		(OMAP2_CONTROL_PADCONFS + 0x5a8 + \
+						(i)*2)
+#define OMAP343X_PADCONF_ETK_CLK	OMAP343X_PADCONF_ETK(0)
+#define OMAP343X_PADCONF_ETK_CTL	OMAP343X_PADCONF_ETK(1)
+#define OMAP343X_PADCONF_ETK_D0		OMAP343X_PADCONF_ETK(2)
+#define OMAP343X_PADCONF_ETK_D1		OMAP343X_PADCONF_ETK(3)
+#define OMAP343X_PADCONF_ETK_D2		OMAP343X_PADCONF_ETK(4)
+#define OMAP343X_PADCONF_ETK_D3		OMAP343X_PADCONF_ETK(5)
+#define OMAP343X_PADCONF_ETK_D4		OMAP343X_PADCONF_ETK(6)
+#define OMAP343X_PADCONF_ETK_D5		OMAP343X_PADCONF_ETK(7)
+#define OMAP343X_PADCONF_ETK_D6		OMAP343X_PADCONF_ETK(8)
+#define OMAP343X_PADCONF_ETK_D7		OMAP343X_PADCONF_ETK(9)
+#define OMAP343X_PADCONF_ETK_D8		OMAP343X_PADCONF_ETK(10)
+#define OMAP343X_PADCONF_ETK_D9		OMAP343X_PADCONF_ETK(11)
+#define OMAP343X_PADCONF_ETK_D10	OMAP343X_PADCONF_ETK(12)
+#define OMAP343X_PADCONF_ETK_D11	OMAP343X_PADCONF_ETK(13)
+#define OMAP343X_PADCONF_ETK_D12	OMAP343X_PADCONF_ETK(14)
+#define OMAP343X_PADCONF_ETK_D13	OMAP343X_PADCONF_ETK(15)
+#define OMAP343X_PADCONF_ETK_D14	OMAP343X_PADCONF_ETK(16)
+#define OMAP343X_PADCONF_ETK_D15	OMAP343X_PADCONF_ETK(17)
+
+/* 34xx GENERAL_WKUP regist offsets */
+#define OMAP343X_CONTROL_WKUP_DEBOBSMUX(i) (OMAP343X_CONTROL_GENERAL_WKUP + \
+						0x008 + (i))
+#define OMAP343X_CONTROL_WKUP_DEBOBS0 (OMAP343X_CONTROL_GENERAL_WKUP + 0x008)
+#define OMAP343X_CONTROL_WKUP_DEBOBS1 (OMAP343X_CONTROL_GENERAL_WKUP + 0x00C)
+#define OMAP343X_CONTROL_WKUP_DEBOBS2 (OMAP343X_CONTROL_GENERAL_WKUP + 0x010)
+#define OMAP343X_CONTROL_WKUP_DEBOBS3 (OMAP343X_CONTROL_GENERAL_WKUP + 0x014)
+#define OMAP343X_CONTROL_WKUP_DEBOBS4 (OMAP343X_CONTROL_GENERAL_WKUP + 0x018)
+
+/* 34xx D2D idle-related pins, handled by PM core */
+#define OMAP3_PADCONF_SAD2D_MSTANDBY   0x250
+#define OMAP3_PADCONF_SAD2D_IDLEACK    0x254
+
+/*
+ * REVISIT: This list of registers is not comprehensive - there are more
+ * that should be added.
+ */
+
+/*
+ * Control module register bit defines - these should eventually go into
+ * their own regbits file.  Some of these will be complicated, depending
+ * on the device type (general-purpose, emulator, test, secure, bad, other)
+ * and the security mode (secure, non-secure, don't care)
+ */
+/* CONTROL_DEVCONF0 bits */
+#define OMAP2_MMCSDIO1ADPCLKISEL	(1 << 24) /* MMC1 loop back clock */
+#define OMAP24XX_USBSTANDBYCTRL		(1 << 15)
+#define OMAP2_MCBSP2_CLKS_MASK		(1 << 6)
+#define OMAP2_MCBSP1_CLKS_MASK		(1 << 2)
+
+/* CONTROL_DEVCONF1 bits */
+#define OMAP243X_MMC1_ACTIVE_OVERWRITE	(1 << 31)
+#define OMAP2_MMCSDIO2ADPCLKISEL	(1 << 6) /* MMC2 loop back clock */
+#define OMAP2_MCBSP5_CLKS_MASK		(1 << 4) /* > 242x */
+#define OMAP2_MCBSP4_CLKS_MASK		(1 << 2) /* > 242x */
+#define OMAP2_MCBSP3_CLKS_MASK		(1 << 0) /* > 242x */
+
+/* CONTROL_STATUS bits */
+#define OMAP2_DEVICETYPE_MASK		(0x7 << 8)
+#define OMAP2_SYSBOOT_5_MASK		(1 << 5)
+#define OMAP2_SYSBOOT_4_MASK		(1 << 4)
+#define OMAP2_SYSBOOT_3_MASK		(1 << 3)
+#define OMAP2_SYSBOOT_2_MASK		(1 << 2)
+#define OMAP2_SYSBOOT_1_MASK		(1 << 1)
+#define OMAP2_SYSBOOT_0_MASK		(1 << 0)
+
+/* CONTROL_PBIAS_LITE bits */
+#define OMAP343X_PBIASLITESUPPLY_HIGH1	(1 << 15)
+#define OMAP343X_PBIASLITEVMODEERROR1	(1 << 11)
+#define OMAP343X_PBIASSPEEDCTRL1	(1 << 10)
+#define OMAP343X_PBIASLITEPWRDNZ1	(1 << 9)
+#define OMAP343X_PBIASLITEVMODE1	(1 << 8)
+#define OMAP343X_PBIASLITESUPPLY_HIGH0	(1 << 7)
+#define OMAP343X_PBIASLITEVMODEERROR0	(1 << 3)
+#define OMAP2_PBIASSPEEDCTRL0		(1 << 2)
+#define OMAP2_PBIASLITEPWRDNZ0		(1 << 1)
+#define OMAP2_PBIASLITEVMODE0		(1 << 0)
+
+/* CONTROL_PROG_IO1 bits */
+#define OMAP3630_PRG_SDMMC1_SPEEDCTRL	(1 << 20)
+
+/* CONTROL_IVA2_BOOTMOD bits */
+#define OMAP3_IVA2_BOOTMOD_SHIFT	0
+#define OMAP3_IVA2_BOOTMOD_MASK		(0xf << 0)
+#define OMAP3_IVA2_BOOTMOD_IDLE		(0x1 << 0)
+
+/* CONTROL_PADCONF_X bits */
+#define OMAP3_PADCONF_WAKEUPEVENT0	(1 << 15)
+#define OMAP3_PADCONF_WAKEUPENABLE0	(1 << 14)
+
+#define OMAP343X_SCRATCHPAD_ROM		(OMAP343X_CTRL_BASE + 0x860)
+#define OMAP343X_SCRATCHPAD		(OMAP343X_CTRL_BASE + 0x910)
+#define OMAP343X_SCRATCHPAD_ROM_OFFSET	0x19C
+
+/*
+ * CONTROL OMAP STATUS register to identify OMAP3 features
+ */
+#define OMAP3_CONTROL_OMAP_STATUS	0x044c
+
+#define OMAP3_SGX_SHIFT			13
+#define OMAP3_SGX_MASK			(3 << OMAP3_SGX_SHIFT)
+#define		FEAT_SGX_FULL		0
+#define		FEAT_SGX_HALF		1
+#define		FEAT_SGX_NONE		2
+
+#define OMAP3_IVA_SHIFT			12
+#define OMAP3_IVA_MASK			(1 << OMAP3_SGX_SHIFT)
+#define		FEAT_IVA		0
+#define		FEAT_IVA_NONE		1
+
+#define OMAP3_L2CACHE_SHIFT		10
+#define OMAP3_L2CACHE_MASK		(3 << OMAP3_L2CACHE_SHIFT)
+#define		FEAT_L2CACHE_NONE	0
+#define		FEAT_L2CACHE_64KB	1
+#define		FEAT_L2CACHE_128KB	2
+#define		FEAT_L2CACHE_256KB	3
+
+#define OMAP3_ISP_SHIFT			5
+#define OMAP3_ISP_MASK			(1<< OMAP3_ISP_SHIFT)
+#define		FEAT_ISP		0
+#define		FEAT_ISP_NONE		1
+
+#define OMAP3_NEON_SHIFT		4
+#define OMAP3_NEON_MASK			(1<< OMAP3_NEON_SHIFT)
+#define		FEAT_NEON		0
+#define		FEAT_NEON_NONE		1
+
+
+#ifndef __ASSEMBLY__
+#if defined(CONFIG_ARCH_OMAP2) || defined(CONFIG_ARCH_OMAP3) || \
+		defined(CONFIG_ARCH_OMAP4)
+extern void __iomem *omap_ctrl_base_get(void);
+extern u8 omap_ctrl_readb(u16 offset);
+extern u16 omap_ctrl_readw(u16 offset);
+extern u32 omap_ctrl_readl(u16 offset);
+extern void omap_ctrl_writeb(u8 val, u16 offset);
+extern void omap_ctrl_writew(u16 val, u16 offset);
+extern void omap_ctrl_writel(u32 val, u16 offset);
+
+extern void omap3_save_scratchpad_contents(void);
+extern void omap3_clear_scratchpad_contents(void);
+extern u32 *get_restore_pointer(void);
+extern u32 *get_es3_restore_pointer(void);
+extern u32 omap3_arm_context[128];
+extern void omap3_control_save_context(void);
+extern void omap3_control_restore_context(void);
+
+#else
+#define omap_ctrl_base_get()		0
+#define omap_ctrl_readb(x)		0
+#define omap_ctrl_readw(x)		0
+#define omap_ctrl_readl(x)		0
+#define omap_ctrl_writeb(x, y)		WARN_ON(1)
+#define omap_ctrl_writew(x, y)		WARN_ON(1)
+#define omap_ctrl_writel(x, y)		WARN_ON(1)
+#endif
+#endif	/* __ASSEMBLY__ */
+
+#endif /* __ASM_ARCH_CONTROL_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/cpu.h
@@ -0,0 +1,516 @@
+/*
+ * arch/arm/plat-omap/include/mach/cpu.h
+ *
+ * OMAP cpu type detection
+ *
+ * Copyright (C) 2004, 2008 Nokia Corporation
+ *
+ * Copyright (C) 2009 Texas Instruments.
+ *
+ * Written by Tony Lindgren <tony.lindgren@nokia.com>
+ *
+ * Added OMAP4 specific defines - Santosh Shilimkar<santosh.shilimkar@ti.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
+ *
+ */
+
+#ifndef __ASM_ARCH_OMAP_CPU_H
+#define __ASM_ARCH_OMAP_CPU_H
+
+#include <linux/bitops.h>
+
+/*
+ * Omap device type i.e. EMU/HS/TST/GP/BAD
+ */
+#define OMAP2_DEVICE_TYPE_TEST		0
+#define OMAP2_DEVICE_TYPE_EMU		1
+#define OMAP2_DEVICE_TYPE_SEC		2
+#define OMAP2_DEVICE_TYPE_GP		3
+#define OMAP2_DEVICE_TYPE_BAD		4
+
+int omap_type(void);
+
+struct omap_chip_id {
+	u8 oc;
+	u8 type;
+};
+
+#define OMAP_CHIP_INIT(x)	{ .oc = x }
+
+/*
+ * omap_rev bits:
+ * CPU id bits	(0730, 1510, 1710, 2422...)	[31:16]
+ * CPU revision	(See _REV_ defined in cpu.h)	[15:08]
+ * CPU class bits (15xx, 16xx, 24xx, 34xx...)	[07:00]
+ */
+unsigned int omap_rev(void);
+
+/*
+ * Define CPU revision bits
+ *
+ * Verbose meaning of the revision bits may be different for a silicon
+ * family. This difference can be handled separately.
+ */
+#define OMAP_REVBITS_00		0x00
+#define OMAP_REVBITS_10		0x10
+#define OMAP_REVBITS_20		0x20
+#define OMAP_REVBITS_30		0x30
+#define OMAP_REVBITS_40		0x40
+
+/*
+ * Get the CPU revision for OMAP devices
+ */
+#define GET_OMAP_REVISION()	((omap_rev() >> 8) & 0xff)
+
+/*
+ * Test if multicore OMAP support is needed
+ */
+#undef MULTI_OMAP1
+#undef MULTI_OMAP2
+#undef OMAP_NAME
+
+#ifdef CONFIG_ARCH_OMAP730
+# ifdef OMAP_NAME
+#  undef  MULTI_OMAP1
+#  define MULTI_OMAP1
+# else
+#  define OMAP_NAME omap730
+# endif
+#endif
+#ifdef CONFIG_ARCH_OMAP850
+# ifdef OMAP_NAME
+#  undef  MULTI_OMAP1
+#  define MULTI_OMAP1
+# else
+#  define OMAP_NAME omap850
+# endif
+#endif
+#ifdef CONFIG_ARCH_OMAP15XX
+# ifdef OMAP_NAME
+#  undef  MULTI_OMAP1
+#  define MULTI_OMAP1
+# else
+#  define OMAP_NAME omap1510
+# endif
+#endif
+#ifdef CONFIG_ARCH_OMAP16XX
+# ifdef OMAP_NAME
+#  undef  MULTI_OMAP1
+#  define MULTI_OMAP1
+# else
+#  define OMAP_NAME omap16xx
+# endif
+#endif
+#if (defined(CONFIG_ARCH_OMAP24XX) || defined(CONFIG_ARCH_OMAP34XX))
+# if (defined(OMAP_NAME) || defined(MULTI_OMAP1))
+#  error "OMAP1 and OMAP2 can't be selected at the same time"
+# endif
+#endif
+#ifdef CONFIG_ARCH_OMAP2420
+# ifdef OMAP_NAME
+#  undef  MULTI_OMAP2
+#  define MULTI_OMAP2
+# else
+#  define OMAP_NAME omap2420
+# endif
+#endif
+#ifdef CONFIG_ARCH_OMAP2430
+# ifdef OMAP_NAME
+#  undef  MULTI_OMAP2
+#  define MULTI_OMAP2
+# else
+#  define OMAP_NAME omap2430
+# endif
+#endif
+#ifdef CONFIG_ARCH_OMAP3430
+# ifdef OMAP_NAME
+#  undef  MULTI_OMAP2
+#  define MULTI_OMAP2
+# else
+#  define OMAP_NAME omap3430
+# endif
+#endif
+
+/*
+ * Macros to group OMAP into cpu classes.
+ * These can be used in most places.
+ * cpu_is_omap7xx():	True for OMAP730, OMAP850
+ * cpu_is_omap15xx():	True for OMAP1510, OMAP5910 and OMAP310
+ * cpu_is_omap16xx():	True for OMAP1610, OMAP5912 and OMAP1710
+ * cpu_is_omap24xx():	True for OMAP2420, OMAP2422, OMAP2423, OMAP2430
+ * cpu_is_omap242x():	True for OMAP2420, OMAP2422, OMAP2423
+ * cpu_is_omap243x():	True for OMAP2430
+ * cpu_is_omap343x():	True for OMAP3430
+ */
+#define GET_OMAP_CLASS	(omap_rev() & 0xff)
+
+#define IS_OMAP_CLASS(class, id)			\
+static inline int is_omap ##class (void)		\
+{							\
+	return (GET_OMAP_CLASS == (id)) ? 1 : 0;	\
+}
+
+#define GET_OMAP_SUBCLASS	((omap_rev() >> 20) & 0x0fff)
+
+#define IS_OMAP_SUBCLASS(subclass, id)			\
+static inline int is_omap ##subclass (void)		\
+{							\
+	return (GET_OMAP_SUBCLASS == (id)) ? 1 : 0;	\
+}
+
+IS_OMAP_CLASS(7xx, 0x07)
+IS_OMAP_CLASS(15xx, 0x15)
+IS_OMAP_CLASS(16xx, 0x16)
+IS_OMAP_CLASS(24xx, 0x24)
+IS_OMAP_CLASS(34xx, 0x34)
+IS_OMAP_CLASS(44xx, 0x44)
+
+IS_OMAP_SUBCLASS(242x, 0x242)
+IS_OMAP_SUBCLASS(243x, 0x243)
+IS_OMAP_SUBCLASS(343x, 0x343)
+IS_OMAP_SUBCLASS(363x, 0x363)
+IS_OMAP_SUBCLASS(443x, 0x443)
+
+#define cpu_is_omap7xx()		0
+#define cpu_is_omap15xx()		0
+#define cpu_is_omap16xx()		0
+#define cpu_is_omap24xx()		0
+#define cpu_is_omap242x()		0
+#define cpu_is_omap243x()		0
+#define cpu_is_omap34xx()		0
+#define cpu_is_omap343x()		0
+#define cpu_is_omap44xx()		0
+#define cpu_is_omap443x()		0
+
+#if defined(MULTI_OMAP1)
+# if defined(CONFIG_ARCH_OMAP730)
+#  undef  cpu_is_omap7xx
+#  define cpu_is_omap7xx()		is_omap7xx()
+# endif
+# if defined(CONFIG_ARCH_OMAP850)
+#  undef  cpu_is_omap7xx
+#  define cpu_is_omap7xx()		is_omap7xx()
+# endif
+# if defined(CONFIG_ARCH_OMAP15XX)
+#  undef  cpu_is_omap15xx
+#  define cpu_is_omap15xx()		is_omap15xx()
+# endif
+# if defined(CONFIG_ARCH_OMAP16XX)
+#  undef  cpu_is_omap16xx
+#  define cpu_is_omap16xx()		is_omap16xx()
+# endif
+#else
+# if defined(CONFIG_ARCH_OMAP730)
+#  undef  cpu_is_omap7xx
+#  define cpu_is_omap7xx()		1
+# endif
+# if defined(CONFIG_ARCH_OMAP850)
+#  undef  cpu_is_omap7xx
+#  define cpu_is_omap7xx()		1
+# endif
+# if defined(CONFIG_ARCH_OMAP15XX)
+#  undef  cpu_is_omap15xx
+#  define cpu_is_omap15xx()		1
+# endif
+# if defined(CONFIG_ARCH_OMAP16XX)
+#  undef  cpu_is_omap16xx
+#  define cpu_is_omap16xx()		1
+# endif
+#endif
+
+#if defined(MULTI_OMAP2)
+# if defined(CONFIG_ARCH_OMAP24XX)
+#  undef  cpu_is_omap24xx
+#  undef  cpu_is_omap242x
+#  undef  cpu_is_omap243x
+#  define cpu_is_omap24xx()		is_omap24xx()
+#  define cpu_is_omap242x()		is_omap242x()
+#  define cpu_is_omap243x()		is_omap243x()
+# endif
+# if defined(CONFIG_ARCH_OMAP34XX)
+#  undef  cpu_is_omap34xx
+#  undef  cpu_is_omap343x
+#  define cpu_is_omap34xx()		is_omap34xx()
+#  define cpu_is_omap343x()		is_omap343x()
+# endif
+#else
+# if defined(CONFIG_ARCH_OMAP24XX)
+#  undef  cpu_is_omap24xx
+#  define cpu_is_omap24xx()		1
+# endif
+# if defined(CONFIG_ARCH_OMAP2420)
+#  undef  cpu_is_omap242x
+#  define cpu_is_omap242x()		1
+# endif
+# if defined(CONFIG_ARCH_OMAP2430)
+#  undef  cpu_is_omap243x
+#  define cpu_is_omap243x()		1
+# endif
+# if defined(CONFIG_ARCH_OMAP34XX)
+#  undef  cpu_is_omap34xx
+#  define cpu_is_omap34xx()		1
+# endif
+# if defined(CONFIG_ARCH_OMAP3430)
+#  undef  cpu_is_omap343x
+#  define cpu_is_omap343x()		1
+# endif
+#endif
+
+/*
+ * Macros to detect individual cpu types.
+ * These are only rarely needed.
+ * cpu_is_omap330():	True for OMAP330
+ * cpu_is_omap730():	True for OMAP730
+ * cpu_is_omap850():	True for OMAP850
+ * cpu_is_omap1510():	True for OMAP1510
+ * cpu_is_omap1610():	True for OMAP1610
+ * cpu_is_omap1611():	True for OMAP1611
+ * cpu_is_omap5912():	True for OMAP5912
+ * cpu_is_omap1621():	True for OMAP1621
+ * cpu_is_omap1710():	True for OMAP1710
+ * cpu_is_omap2420():	True for OMAP2420
+ * cpu_is_omap2422():	True for OMAP2422
+ * cpu_is_omap2423():	True for OMAP2423
+ * cpu_is_omap2430():	True for OMAP2430
+ * cpu_is_omap3430():	True for OMAP3430
+ * cpu_is_omap3505():	True for OMAP3505
+ * cpu_is_omap3517():	True for OMAP3517
+ */
+#define GET_OMAP_TYPE	((omap_rev() >> 16) & 0xffff)
+
+#define IS_OMAP_TYPE(type, id)				\
+static inline int is_omap ##type (void)			\
+{							\
+	return (GET_OMAP_TYPE == (id)) ? 1 : 0;		\
+}
+
+IS_OMAP_TYPE(310, 0x0310)
+IS_OMAP_TYPE(730, 0x0730)
+IS_OMAP_TYPE(850, 0x0850)
+IS_OMAP_TYPE(1510, 0x1510)
+IS_OMAP_TYPE(1610, 0x1610)
+IS_OMAP_TYPE(1611, 0x1611)
+IS_OMAP_TYPE(5912, 0x1611)
+IS_OMAP_TYPE(1621, 0x1621)
+IS_OMAP_TYPE(1710, 0x1710)
+IS_OMAP_TYPE(2420, 0x2420)
+IS_OMAP_TYPE(2422, 0x2422)
+IS_OMAP_TYPE(2423, 0x2423)
+IS_OMAP_TYPE(2430, 0x2430)
+IS_OMAP_TYPE(3430, 0x3430)
+IS_OMAP_TYPE(3505, 0x3505)
+IS_OMAP_TYPE(3517, 0x3517)
+
+#define cpu_is_omap310()		0
+#define cpu_is_omap730()		0
+#define cpu_is_omap850()		0
+#define cpu_is_omap1510()		0
+#define cpu_is_omap1610()		0
+#define cpu_is_omap5912()		0
+#define cpu_is_omap1611()		0
+#define cpu_is_omap1621()		0
+#define cpu_is_omap1710()		0
+#define cpu_is_omap2420()		0
+#define cpu_is_omap2422()		0
+#define cpu_is_omap2423()		0
+#define cpu_is_omap2430()		0
+#define cpu_is_omap3503()		0
+#define cpu_is_omap3515()		0
+#define cpu_is_omap3525()		0
+#define cpu_is_omap3530()		0
+#define cpu_is_omap3505()		0
+#define cpu_is_omap3517()		0
+#define cpu_is_omap3430()		0
+#define cpu_is_omap3630()		0
+
+/*
+ * Whether we have MULTI_OMAP1 or not, we still need to distinguish
+ * between 730 vs 850, 330 vs. 1510 and 1611B/5912 vs. 1710.
+ */
+
+#if defined(CONFIG_ARCH_OMAP730)
+# undef  cpu_is_omap730
+# define cpu_is_omap730()		is_omap730()
+#endif
+
+#if defined(CONFIG_ARCH_OMAP850)
+# undef  cpu_is_omap850
+# define cpu_is_omap850()		is_omap850()
+#endif
+
+#if defined(CONFIG_ARCH_OMAP15XX)
+# undef  cpu_is_omap310
+# undef  cpu_is_omap1510
+# define cpu_is_omap310()		is_omap310()
+# define cpu_is_omap1510()		is_omap1510()
+#endif
+
+#if defined(CONFIG_ARCH_OMAP16XX)
+# undef  cpu_is_omap1610
+# undef  cpu_is_omap1611
+# undef  cpu_is_omap5912
+# undef  cpu_is_omap1621
+# undef  cpu_is_omap1710
+# define cpu_is_omap1610()		is_omap1610()
+# define cpu_is_omap1611()		is_omap1611()
+# define cpu_is_omap5912()		is_omap5912()
+# define cpu_is_omap1621()		is_omap1621()
+# define cpu_is_omap1710()		is_omap1710()
+#endif
+
+#if defined(CONFIG_ARCH_OMAP24XX)
+# undef  cpu_is_omap2420
+# undef  cpu_is_omap2422
+# undef  cpu_is_omap2423
+# undef  cpu_is_omap2430
+# define cpu_is_omap2420()		is_omap2420()
+# define cpu_is_omap2422()		is_omap2422()
+# define cpu_is_omap2423()		is_omap2423()
+# define cpu_is_omap2430()		is_omap2430()
+#endif
+
+#if defined(CONFIG_ARCH_OMAP34XX)
+# undef cpu_is_omap3430
+# undef cpu_is_omap3503
+# undef cpu_is_omap3515
+# undef cpu_is_omap3525
+# undef cpu_is_omap3530
+# undef cpu_is_omap3505
+# undef cpu_is_omap3517
+# define cpu_is_omap3430()		is_omap3430()
+# define cpu_is_omap3503()		(cpu_is_omap3430() &&		\
+						(!omap3_has_iva()) &&	\
+						(!omap3_has_sgx()))
+# define cpu_is_omap3515()		(cpu_is_omap3430() &&		\
+						(!omap3_has_iva()) &&	\
+						(omap3_has_sgx()))
+# define cpu_is_omap3525()		(cpu_is_omap3430() &&		\
+						(!omap3_has_sgx()) &&	\
+						(omap3_has_iva()))
+# define cpu_is_omap3530()		(cpu_is_omap3430())
+# define cpu_is_omap3505()		is_omap3505()
+# define cpu_is_omap3517()		is_omap3517()
+# undef cpu_is_omap3630
+# define cpu_is_omap3630()		is_omap363x()
+#endif
+
+# if defined(CONFIG_ARCH_OMAP4)
+# undef cpu_is_omap44xx
+# undef cpu_is_omap443x
+# define cpu_is_omap44xx()		is_omap44xx()
+# define cpu_is_omap443x()		is_omap443x()
+# endif
+
+/* Macros to detect if we have OMAP1 or OMAP2 */
+#define cpu_class_is_omap1()	(cpu_is_omap7xx() || cpu_is_omap15xx() || \
+				cpu_is_omap16xx())
+#define cpu_class_is_omap2()	(cpu_is_omap24xx() || cpu_is_omap34xx() || \
+				cpu_is_omap44xx())
+
+/* Various silicon revisions for omap2 */
+#define OMAP242X_CLASS		0x24200024
+#define OMAP2420_REV_ES1_0	0x24200024
+#define OMAP2420_REV_ES2_0	0x24201024
+
+#define OMAP243X_CLASS		0x24300024
+#define OMAP2430_REV_ES1_0	0x24300024
+
+#define OMAP343X_CLASS		0x34300034
+#define OMAP3430_REV_ES1_0	0x34300034
+#define OMAP3430_REV_ES2_0	0x34301034
+#define OMAP3430_REV_ES2_1	0x34302034
+#define OMAP3430_REV_ES3_0	0x34303034
+#define OMAP3430_REV_ES3_1	0x34304034
+
+#define OMAP3630_REV_ES1_0	0x36300034
+
+#define OMAP35XX_CLASS		0x35000034
+#define OMAP3503_REV(v)		(OMAP35XX_CLASS | (0x3503 << 16) | (v << 8))
+#define OMAP3515_REV(v)		(OMAP35XX_CLASS | (0x3515 << 16) | (v << 8))
+#define OMAP3525_REV(v)		(OMAP35XX_CLASS | (0x3525 << 16) | (v << 8))
+#define OMAP3530_REV(v)		(OMAP35XX_CLASS | (0x3530 << 16) | (v << 8))
+#define OMAP3505_REV(v)		(OMAP35XX_CLASS | (0x3505 << 16) | (v << 8))
+#define OMAP3517_REV(v)		(OMAP35XX_CLASS | (0x3517 << 16) | (v << 8))
+
+#define OMAP443X_CLASS		0x44300044
+#define OMAP4430_REV_ES1_0	0x44300044
+
+/*
+ * omap_chip bits
+ *
+ * CHIP_IS_OMAP{2420,2430,3430} indicate that a particular structure is
+ * valid on all chips of that type.  CHIP_IS_OMAP3430ES{1,2} indicates
+ * something that is only valid on that particular ES revision.
+ *
+ * These bits may be ORed together to indicate structures that are
+ * available on multiple chip types.
+ *
+ * To test whether a particular structure matches the current OMAP chip type,
+ * use omap_chip_is().
+ *
+ */
+#define CHIP_IS_OMAP2420		(1 << 0)
+#define CHIP_IS_OMAP2430		(1 << 1)
+#define CHIP_IS_OMAP3430		(1 << 2)
+#define CHIP_IS_OMAP3430ES1		(1 << 3)
+#define CHIP_IS_OMAP3430ES2		(1 << 4)
+#define CHIP_IS_OMAP3430ES3_0		(1 << 5)
+#define CHIP_IS_OMAP3430ES3_1		(1 << 6)
+#define CHIP_IS_OMAP3630ES1		(1 << 7)
+
+#define CHIP_IS_OMAP24XX		(CHIP_IS_OMAP2420 | CHIP_IS_OMAP2430)
+
+/*
+ * "GE" here represents "greater than or equal to" in terms of ES
+ * levels.  So CHIP_GE_OMAP3430ES2 is intended to match all OMAP3430
+ * chips at ES2 and beyond, but not, for example, any OMAP lines after
+ * OMAP3.
+ */
+#define CHIP_GE_OMAP3430ES2		(CHIP_IS_OMAP3430ES2 | \
+					 CHIP_IS_OMAP3430ES3_0 | \
+					 CHIP_IS_OMAP3430ES3_1 | \
+					 CHIP_IS_OMAP3630ES1)
+#define CHIP_GE_OMAP3430ES3_1		(CHIP_IS_OMAP3430ES3_1 | \
+					 CHIP_IS_OMAP3630ES1)
+
+
+int omap_chip_is(struct omap_chip_id oci);
+void omap2_check_revision(void);
+
+/*
+ * Runtime detection of OMAP3 features
+ */
+extern u32 omap3_features;
+
+#define OMAP3_HAS_L2CACHE		BIT(0)
+#define OMAP3_HAS_IVA			BIT(1)
+#define OMAP3_HAS_SGX			BIT(2)
+#define OMAP3_HAS_NEON			BIT(3)
+#define OMAP3_HAS_ISP			BIT(4)
+
+#define OMAP3_HAS_FEATURE(feat,flag)			\
+static inline unsigned int omap3_has_ ##feat(void)	\
+{							\
+	return (omap3_features & OMAP3_HAS_ ##flag);	\
+}							\
+
+OMAP3_HAS_FEATURE(l2cache, L2CACHE)
+OMAP3_HAS_FEATURE(sgx, SGX)
+OMAP3_HAS_FEATURE(iva, IVA)
+OMAP3_HAS_FEATURE(neon, NEON)
+OMAP3_HAS_FEATURE(isp, ISP)
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/display.h
@@ -0,0 +1,575 @@
+/*
+ * linux/include/asm-arm/arch-omap/display.h
+ *
+ * Copyright (C) 2008 Nokia Corporation
+ * Author: Tomi Valkeinen <tomi.valkeinen@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License version 2 as published by
+ * the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but WITHOUT
+ * ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
+ * FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License for
+ * more details.
+ *
+ * You should have received a copy of the GNU General Public License along with
+ * this program.  If not, see <http://www.gnu.org/licenses/>.
+ */
+
+#ifndef __ASM_ARCH_OMAP_DISPLAY_H
+#define __ASM_ARCH_OMAP_DISPLAY_H
+
+#include <linux/list.h>
+#include <linux/kobject.h>
+#include <linux/device.h>
+#include <asm/atomic.h>
+
+#define DISPC_IRQ_FRAMEDONE		(1 << 0)
+#define DISPC_IRQ_VSYNC			(1 << 1)
+#define DISPC_IRQ_EVSYNC_EVEN		(1 << 2)
+#define DISPC_IRQ_EVSYNC_ODD		(1 << 3)
+#define DISPC_IRQ_ACBIAS_COUNT_STAT	(1 << 4)
+#define DISPC_IRQ_PROG_LINE_NUM		(1 << 5)
+#define DISPC_IRQ_GFX_FIFO_UNDERFLOW	(1 << 6)
+#define DISPC_IRQ_GFX_END_WIN		(1 << 7)
+#define DISPC_IRQ_PAL_GAMMA_MASK	(1 << 8)
+#define DISPC_IRQ_OCP_ERR		(1 << 9)
+#define DISPC_IRQ_VID1_FIFO_UNDERFLOW	(1 << 10)
+#define DISPC_IRQ_VID1_END_WIN		(1 << 11)
+#define DISPC_IRQ_VID2_FIFO_UNDERFLOW	(1 << 12)
+#define DISPC_IRQ_VID2_END_WIN		(1 << 13)
+#define DISPC_IRQ_SYNC_LOST		(1 << 14)
+#define DISPC_IRQ_SYNC_LOST_DIGIT	(1 << 15)
+#define DISPC_IRQ_WAKEUP		(1 << 16)
+
+struct omap_dss_device;
+struct omap_overlay_manager;
+
+enum omap_display_type {
+	OMAP_DISPLAY_TYPE_NONE		= 0,
+	OMAP_DISPLAY_TYPE_DPI		= 1 << 0,
+	OMAP_DISPLAY_TYPE_DBI		= 1 << 1,
+	OMAP_DISPLAY_TYPE_SDI		= 1 << 2,
+	OMAP_DISPLAY_TYPE_DSI		= 1 << 3,
+	OMAP_DISPLAY_TYPE_VENC		= 1 << 4,
+};
+
+enum omap_plane {
+	OMAP_DSS_GFX	= 0,
+	OMAP_DSS_VIDEO1	= 1,
+	OMAP_DSS_VIDEO2	= 2
+};
+
+enum omap_channel {
+	OMAP_DSS_CHANNEL_LCD	= 0,
+	OMAP_DSS_CHANNEL_DIGIT	= 1,
+};
+
+enum omap_color_mode {
+	OMAP_DSS_COLOR_CLUT1	= 1 << 0,  /* BITMAP 1 */
+	OMAP_DSS_COLOR_CLUT2	= 1 << 1,  /* BITMAP 2 */
+	OMAP_DSS_COLOR_CLUT4	= 1 << 2,  /* BITMAP 4 */
+	OMAP_DSS_COLOR_CLUT8	= 1 << 3,  /* BITMAP 8 */
+	OMAP_DSS_COLOR_RGB12U	= 1 << 4,  /* RGB12, 16-bit container */
+	OMAP_DSS_COLOR_ARGB16	= 1 << 5,  /* ARGB16 */
+	OMAP_DSS_COLOR_RGB16	= 1 << 6,  /* RGB16 */
+	OMAP_DSS_COLOR_RGB24U	= 1 << 7,  /* RGB24, 32-bit container */
+	OMAP_DSS_COLOR_RGB24P	= 1 << 8,  /* RGB24, 24-bit container */
+	OMAP_DSS_COLOR_YUV2	= 1 << 9,  /* YUV2 4:2:2 co-sited */
+	OMAP_DSS_COLOR_UYVY	= 1 << 10, /* UYVY 4:2:2 co-sited */
+	OMAP_DSS_COLOR_ARGB32	= 1 << 11, /* ARGB32 */
+	OMAP_DSS_COLOR_RGBA32	= 1 << 12, /* RGBA32 */
+	OMAP_DSS_COLOR_RGBX32	= 1 << 13, /* RGBx32 */
+
+	OMAP_DSS_COLOR_GFX_OMAP2 =
+		OMAP_DSS_COLOR_CLUT1 | OMAP_DSS_COLOR_CLUT2 |
+		OMAP_DSS_COLOR_CLUT4 | OMAP_DSS_COLOR_CLUT8 |
+		OMAP_DSS_COLOR_RGB12U | OMAP_DSS_COLOR_RGB16 |
+		OMAP_DSS_COLOR_RGB24U | OMAP_DSS_COLOR_RGB24P,
+
+	OMAP_DSS_COLOR_VID_OMAP2 =
+		OMAP_DSS_COLOR_RGB16 | OMAP_DSS_COLOR_RGB24U |
+		OMAP_DSS_COLOR_RGB24P | OMAP_DSS_COLOR_YUV2 |
+		OMAP_DSS_COLOR_UYVY,
+
+	OMAP_DSS_COLOR_GFX_OMAP3 =
+		OMAP_DSS_COLOR_CLUT1 | OMAP_DSS_COLOR_CLUT2 |
+		OMAP_DSS_COLOR_CLUT4 | OMAP_DSS_COLOR_CLUT8 |
+		OMAP_DSS_COLOR_RGB12U | OMAP_DSS_COLOR_ARGB16 |
+		OMAP_DSS_COLOR_RGB16 | OMAP_DSS_COLOR_RGB24U |
+		OMAP_DSS_COLOR_RGB24P | OMAP_DSS_COLOR_ARGB32 |
+		OMAP_DSS_COLOR_RGBA32 | OMAP_DSS_COLOR_RGBX32,
+
+	OMAP_DSS_COLOR_VID1_OMAP3 =
+		OMAP_DSS_COLOR_RGB12U | OMAP_DSS_COLOR_RGB16 |
+		OMAP_DSS_COLOR_RGB24U | OMAP_DSS_COLOR_RGB24P |
+		OMAP_DSS_COLOR_YUV2 | OMAP_DSS_COLOR_UYVY,
+
+	OMAP_DSS_COLOR_VID2_OMAP3 =
+		OMAP_DSS_COLOR_RGB12U | OMAP_DSS_COLOR_ARGB16 |
+		OMAP_DSS_COLOR_RGB16 | OMAP_DSS_COLOR_RGB24U |
+		OMAP_DSS_COLOR_RGB24P | OMAP_DSS_COLOR_YUV2 |
+		OMAP_DSS_COLOR_UYVY | OMAP_DSS_COLOR_ARGB32 |
+		OMAP_DSS_COLOR_RGBA32 | OMAP_DSS_COLOR_RGBX32,
+};
+
+enum omap_lcd_display_type {
+	OMAP_DSS_LCD_DISPLAY_STN,
+	OMAP_DSS_LCD_DISPLAY_TFT,
+};
+
+enum omap_dss_load_mode {
+	OMAP_DSS_LOAD_CLUT_AND_FRAME	= 0,
+	OMAP_DSS_LOAD_CLUT_ONLY		= 1,
+	OMAP_DSS_LOAD_FRAME_ONLY	= 2,
+	OMAP_DSS_LOAD_CLUT_ONCE_FRAME	= 3,
+};
+
+enum omap_dss_trans_key_type {
+	OMAP_DSS_COLOR_KEY_GFX_DST = 0,
+	OMAP_DSS_COLOR_KEY_VID_SRC = 1,
+};
+
+enum omap_rfbi_te_mode {
+	OMAP_DSS_RFBI_TE_MODE_1 = 1,
+	OMAP_DSS_RFBI_TE_MODE_2 = 2,
+};
+
+enum omap_panel_config {
+	OMAP_DSS_LCD_IVS		= 1<<0,
+	OMAP_DSS_LCD_IHS		= 1<<1,
+	OMAP_DSS_LCD_IPC		= 1<<2,
+	OMAP_DSS_LCD_IEO		= 1<<3,
+	OMAP_DSS_LCD_RF			= 1<<4,
+	OMAP_DSS_LCD_ONOFF		= 1<<5,
+
+	OMAP_DSS_LCD_TFT		= 1<<20,
+};
+
+enum omap_dss_venc_type {
+	OMAP_DSS_VENC_TYPE_COMPOSITE,
+	OMAP_DSS_VENC_TYPE_SVIDEO,
+};
+
+enum omap_display_caps {
+	OMAP_DSS_DISPLAY_CAP_MANUAL_UPDATE	= 1 << 0,
+	OMAP_DSS_DISPLAY_CAP_TEAR_ELIM		= 1 << 1,
+};
+
+enum omap_dss_update_mode {
+	OMAP_DSS_UPDATE_DISABLED = 0,
+	OMAP_DSS_UPDATE_AUTO,
+	OMAP_DSS_UPDATE_MANUAL,
+};
+
+enum omap_dss_display_state {
+	OMAP_DSS_DISPLAY_DISABLED = 0,
+	OMAP_DSS_DISPLAY_ACTIVE,
+	OMAP_DSS_DISPLAY_SUSPENDED,
+};
+
+/* XXX perhaps this should be removed */
+enum omap_dss_overlay_managers {
+	OMAP_DSS_OVL_MGR_LCD,
+	OMAP_DSS_OVL_MGR_TV,
+};
+
+enum omap_dss_rotation_type {
+	OMAP_DSS_ROT_DMA = 0,
+	OMAP_DSS_ROT_VRFB = 1,
+};
+
+/* clockwise rotation angle */
+enum omap_dss_rotation_angle {
+	OMAP_DSS_ROT_0   = 0,
+	OMAP_DSS_ROT_90  = 1,
+	OMAP_DSS_ROT_180 = 2,
+	OMAP_DSS_ROT_270 = 3,
+};
+
+enum omap_overlay_caps {
+	OMAP_DSS_OVL_CAP_SCALE = 1 << 0,
+	OMAP_DSS_OVL_CAP_DISPC = 1 << 1,
+};
+
+enum omap_overlay_manager_caps {
+	OMAP_DSS_OVL_MGR_CAP_DISPC = 1 << 0,
+};
+
+/* RFBI */
+
+struct rfbi_timings {
+	int cs_on_time;
+	int cs_off_time;
+	int we_on_time;
+	int we_off_time;
+	int re_on_time;
+	int re_off_time;
+	int we_cycle_time;
+	int re_cycle_time;
+	int cs_pulse_width;
+	int access_time;
+
+	int clk_div;
+
+	u32 tim[5];             /* set by rfbi_convert_timings() */
+
+	int converted;
+};
+
+void omap_rfbi_write_command(const void *buf, u32 len);
+void omap_rfbi_read_data(void *buf, u32 len);
+void omap_rfbi_write_data(const void *buf, u32 len);
+void omap_rfbi_write_pixels(const void __iomem *buf, int scr_width,
+		u16 x, u16 y,
+		u16 w, u16 h);
+int omap_rfbi_enable_te(bool enable, unsigned line);
+int omap_rfbi_setup_te(enum omap_rfbi_te_mode mode,
+			     unsigned hs_pulse_time, unsigned vs_pulse_time,
+			     int hs_pol_inv, int vs_pol_inv, int extif_div);
+
+/* DSI */
+void dsi_bus_lock(void);
+void dsi_bus_unlock(void);
+int dsi_vc_dcs_write(int channel, u8 *data, int len);
+int dsi_vc_dcs_write_nosync(int channel, u8 *data, int len);
+int dsi_vc_dcs_read(int channel, u8 dcs_cmd, u8 *buf, int buflen);
+int dsi_vc_set_max_rx_packet_size(int channel, u16 len);
+int dsi_vc_send_null(int channel);
+int dsi_vc_send_bta_sync(int channel);
+
+/* Board specific data */
+struct omap_dss_board_info {
+	int (*get_last_off_on_transaction_id)(struct device *dev);
+	int num_devices;
+	struct omap_dss_device **devices;
+	struct omap_dss_device *default_device;
+};
+
+struct omap_video_timings {
+	/* Unit: pixels */
+	u16 x_res;
+	/* Unit: pixels */
+	u16 y_res;
+	/* Unit: KHz */
+	u32 pixel_clock;
+	/* Unit: pixel clocks */
+	u16 hsw;	/* Horizontal synchronization pulse width */
+	/* Unit: pixel clocks */
+	u16 hfp;	/* Horizontal front porch */
+	/* Unit: pixel clocks */
+	u16 hbp;	/* Horizontal back porch */
+	/* Unit: line clocks */
+	u16 vsw;	/* Vertical synchronization pulse width */
+	/* Unit: line clocks */
+	u16 vfp;	/* Vertical front porch */
+	/* Unit: line clocks */
+	u16 vbp;	/* Vertical back porch */
+};
+
+#ifdef CONFIG_OMAP2_DSS_VENC
+/* Hardcoded timings for tv modes. Venc only uses these to
+ * identify the mode, and does not actually use the configs
+ * itself. However, the configs should be something that
+ * a normal monitor can also show */
+const extern struct omap_video_timings omap_dss_pal_timings;
+const extern struct omap_video_timings omap_dss_ntsc_timings;
+#endif
+
+struct omap_overlay_info {
+	bool enabled;
+
+	u32 paddr;
+	void __iomem *vaddr;
+	u16 screen_width;
+	u16 width;
+	u16 height;
+	enum omap_color_mode color_mode;
+	u8 rotation;
+	enum omap_dss_rotation_type rotation_type;
+	bool mirror;
+
+	u16 pos_x;
+	u16 pos_y;
+	u16 out_width;	/* if 0, out_width == width */
+	u16 out_height;	/* if 0, out_height == height */
+	u8 global_alpha;
+};
+
+struct omap_overlay {
+	struct kobject kobj;
+	struct list_head list;
+
+	/* static fields */
+	const char *name;
+	int id;
+	enum omap_color_mode supported_modes;
+	enum omap_overlay_caps caps;
+
+	/* dynamic fields */
+	struct omap_overlay_manager *manager;
+	struct omap_overlay_info info;
+
+	/* if true, info has been changed, but not applied() yet */
+	bool info_dirty;
+
+	int (*set_manager)(struct omap_overlay *ovl,
+		struct omap_overlay_manager *mgr);
+	int (*unset_manager)(struct omap_overlay *ovl);
+
+	int (*set_overlay_info)(struct omap_overlay *ovl,
+			struct omap_overlay_info *info);
+	void (*get_overlay_info)(struct omap_overlay *ovl,
+			struct omap_overlay_info *info);
+
+	int (*wait_for_go)(struct omap_overlay *ovl);
+};
+
+struct omap_overlay_manager_info {
+	u32 default_color;
+
+	enum omap_dss_trans_key_type trans_key_type;
+	u32 trans_key;
+	bool trans_enabled;
+
+	bool alpha_enabled;
+};
+
+struct omap_overlay_manager {
+	struct kobject kobj;
+	struct list_head list;
+
+	/* static fields */
+	const char *name;
+	int id;
+	enum omap_overlay_manager_caps caps;
+	int num_overlays;
+	struct omap_overlay **overlays;
+	enum omap_display_type supported_displays;
+
+	/* dynamic fields */
+	struct omap_dss_device *device;
+	struct omap_overlay_manager_info info;
+
+	bool device_changed;
+	/* if true, info has been changed but not applied() yet */
+	bool info_dirty;
+
+	int (*set_device)(struct omap_overlay_manager *mgr,
+		struct omap_dss_device *dssdev);
+	int (*unset_device)(struct omap_overlay_manager *mgr);
+
+	int (*set_manager_info)(struct omap_overlay_manager *mgr,
+			struct omap_overlay_manager_info *info);
+	void (*get_manager_info)(struct omap_overlay_manager *mgr,
+			struct omap_overlay_manager_info *info);
+
+	int (*apply)(struct omap_overlay_manager *mgr);
+	int (*wait_for_go)(struct omap_overlay_manager *mgr);
+};
+
+struct omap_dss_device {
+	struct device dev;
+
+	enum omap_display_type type;
+
+	union {
+		struct {
+			u8 data_lines;
+		} dpi;
+
+		struct {
+			u8 channel;
+			u8 data_lines;
+		} rfbi;
+
+		struct {
+			u8 datapairs;
+		} sdi;
+
+		struct {
+			u8 clk_lane;
+			u8 clk_pol;
+			u8 data1_lane;
+			u8 data1_pol;
+			u8 data2_lane;
+			u8 data2_pol;
+
+			struct {
+				u16 regn;
+				u16 regm;
+				u16 regm3;
+				u16 regm4;
+
+				u16 lp_clk_div;
+
+				u16 lck_div;
+				u16 pck_div;
+			} div;
+
+			bool ext_te;
+			u8 ext_te_gpio;
+		} dsi;
+
+		struct {
+			enum omap_dss_venc_type type;
+			bool invert_polarity;
+		} venc;
+	} phy;
+
+	struct {
+		struct omap_video_timings timings;
+
+		int acbi;	/* ac-bias pin transitions per interrupt */
+		/* Unit: line clocks */
+		int acb;	/* ac-bias pin frequency */
+
+		enum omap_panel_config config;
+
+		u8 recommended_bpp;
+
+		struct omap_dss_device *ctrl;
+	} panel;
+
+	struct {
+		u8 pixel_size;
+		struct rfbi_timings rfbi_timings;
+		struct omap_dss_device *panel;
+	} ctrl;
+
+	int reset_gpio;
+
+	int max_backlight_level;
+
+	const char *name;
+
+	/* used to match device to driver */
+	const char *driver_name;
+
+	void *data;
+
+	struct omap_dss_driver *driver;
+
+	/* helper variable for driver suspend/resume */
+	bool activate_after_resume;
+
+	enum omap_display_caps caps;
+
+	struct omap_overlay_manager *manager;
+
+	enum omap_dss_display_state state;
+
+	int (*enable)(struct omap_dss_device *dssdev);
+	void (*disable)(struct omap_dss_device *dssdev);
+
+	int (*suspend)(struct omap_dss_device *dssdev);
+	int (*resume)(struct omap_dss_device *dssdev);
+
+	void (*get_resolution)(struct omap_dss_device *dssdev,
+			u16 *xres, u16 *yres);
+	int (*get_recommended_bpp)(struct omap_dss_device *dssdev);
+
+	int (*check_timings)(struct omap_dss_device *dssdev,
+			struct omap_video_timings *timings);
+	void (*set_timings)(struct omap_dss_device *dssdev,
+			struct omap_video_timings *timings);
+	void (*get_timings)(struct omap_dss_device *dssdev,
+			struct omap_video_timings *timings);
+	int (*update)(struct omap_dss_device *dssdev,
+			       u16 x, u16 y, u16 w, u16 h);
+	int (*sync)(struct omap_dss_device *dssdev);
+	int (*wait_vsync)(struct omap_dss_device *dssdev);
+
+	int (*set_update_mode)(struct omap_dss_device *dssdev,
+			enum omap_dss_update_mode);
+	enum omap_dss_update_mode (*get_update_mode)
+		(struct omap_dss_device *dssdev);
+
+	int (*enable_te)(struct omap_dss_device *dssdev, bool enable);
+	int (*get_te)(struct omap_dss_device *dssdev);
+
+	u8 (*get_rotate)(struct omap_dss_device *dssdev);
+	int (*set_rotate)(struct omap_dss_device *dssdev, u8 rotate);
+
+	bool (*get_mirror)(struct omap_dss_device *dssdev);
+	int (*set_mirror)(struct omap_dss_device *dssdev, bool enable);
+
+	int (*run_test)(struct omap_dss_device *dssdev, int test);
+	int (*memory_read)(struct omap_dss_device *dssdev,
+			void *buf, size_t size,
+			u16 x, u16 y, u16 w, u16 h);
+
+	int (*set_wss)(struct omap_dss_device *dssdev, u32 wss);
+	u32 (*get_wss)(struct omap_dss_device *dssdev);
+
+	/* platform specific  */
+	int (*platform_enable)(struct omap_dss_device *dssdev);
+	void (*platform_disable)(struct omap_dss_device *dssdev);
+	int (*set_backlight)(struct omap_dss_device *dssdev, int level);
+	int (*get_backlight)(struct omap_dss_device *dssdev);
+};
+
+struct omap_dss_driver {
+	struct device_driver driver;
+
+	int (*probe)(struct omap_dss_device *);
+	void (*remove)(struct omap_dss_device *);
+
+	int (*enable)(struct omap_dss_device *display);
+	void (*disable)(struct omap_dss_device *display);
+	int (*suspend)(struct omap_dss_device *display);
+	int (*resume)(struct omap_dss_device *display);
+	int (*run_test)(struct omap_dss_device *display, int test);
+
+	void (*setup_update)(struct omap_dss_device *dssdev,
+			u16 x, u16 y, u16 w, u16 h);
+
+	int (*enable_te)(struct omap_dss_device *dssdev, bool enable);
+	int (*wait_for_te)(struct omap_dss_device *dssdev);
+
+	u8 (*get_rotate)(struct omap_dss_device *dssdev);
+	int (*set_rotate)(struct omap_dss_device *dssdev, u8 rotate);
+
+	bool (*get_mirror)(struct omap_dss_device *dssdev);
+	int (*set_mirror)(struct omap_dss_device *dssdev, bool enable);
+
+	int (*memory_read)(struct omap_dss_device *dssdev,
+			void *buf, size_t size,
+			u16 x, u16 y, u16 w, u16 h);
+};
+
+int omap_dss_register_driver(struct omap_dss_driver *);
+void omap_dss_unregister_driver(struct omap_dss_driver *);
+
+int omap_dss_register_device(struct omap_dss_device *);
+void omap_dss_unregister_device(struct omap_dss_device *);
+
+void omap_dss_get_device(struct omap_dss_device *dssdev);
+void omap_dss_put_device(struct omap_dss_device *dssdev);
+#define for_each_dss_dev(d) while ((d = omap_dss_get_next_device(d)) != NULL)
+struct omap_dss_device *omap_dss_get_next_device(struct omap_dss_device *from);
+struct omap_dss_device *omap_dss_find_device(void *data,
+		int (*match)(struct omap_dss_device *dssdev, void *data));
+
+int omap_dss_start_device(struct omap_dss_device *dssdev);
+void omap_dss_stop_device(struct omap_dss_device *dssdev);
+
+int omap_dss_get_num_overlay_managers(void);
+struct omap_overlay_manager *omap_dss_get_overlay_manager(int num);
+
+int omap_dss_get_num_overlays(void);
+struct omap_overlay *omap_dss_get_overlay(int num);
+
+typedef void (*omap_dispc_isr_t) (void *arg, u32 mask);
+int omap_dispc_register_isr(omap_dispc_isr_t isr, void *arg, u32 mask);
+int omap_dispc_unregister_isr(omap_dispc_isr_t isr, void *arg, u32 mask);
+
+int omap_dispc_wait_for_irq_timeout(u32 irqmask, unsigned long timeout);
+int omap_dispc_wait_for_irq_interruptible_timeout(u32 irqmask,
+		unsigned long timeout);
+
+#define to_dss_driver(x) container_of((x), struct omap_dss_driver, driver)
+#define to_dss_device(x) container_of((x), struct omap_dss_device, dev)
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/dma.h
@@ -0,0 +1,640 @@
+/*
+ *  arch/arm/plat-omap/include/mach/dma.h
+ *
+ *  Copyright (C) 2003 Nokia Corporation
+ *  Author: Juha YrjÃ¶lÃ¤ <juha.yrjola@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
+ */
+#ifndef __ASM_ARCH_DMA_H
+#define __ASM_ARCH_DMA_H
+
+/* Hardware registers for omap1 */
+#define OMAP1_DMA_BASE			(0xfffed800)
+
+#define OMAP1_DMA_GCR			0x400
+#define OMAP1_DMA_GSCR			0x404
+#define OMAP1_DMA_GRST			0x408
+#define OMAP1_DMA_HW_ID			0x442
+#define OMAP1_DMA_PCH2_ID		0x444
+#define OMAP1_DMA_PCH0_ID		0x446
+#define OMAP1_DMA_PCH1_ID		0x448
+#define OMAP1_DMA_PCHG_ID		0x44a
+#define OMAP1_DMA_PCHD_ID		0x44c
+#define OMAP1_DMA_CAPS_0_U		0x44e
+#define OMAP1_DMA_CAPS_0_L		0x450
+#define OMAP1_DMA_CAPS_1_U		0x452
+#define OMAP1_DMA_CAPS_1_L		0x454
+#define OMAP1_DMA_CAPS_2		0x456
+#define OMAP1_DMA_CAPS_3		0x458
+#define OMAP1_DMA_CAPS_4		0x45a
+#define OMAP1_DMA_PCH2_SR		0x460
+#define OMAP1_DMA_PCH0_SR		0x480
+#define OMAP1_DMA_PCH1_SR		0x482
+#define OMAP1_DMA_PCHD_SR		0x4c0
+
+/* Hardware registers for omap2 and omap3 */
+#define OMAP24XX_DMA4_BASE		(L4_24XX_BASE + 0x56000)
+#define OMAP34XX_DMA4_BASE		(L4_34XX_BASE + 0x56000)
+#define OMAP44XX_DMA4_BASE		(L4_44XX_BASE + 0x56000)
+
+#define OMAP_DMA4_REVISION		0x00
+#define OMAP_DMA4_GCR			0x78
+#define OMAP_DMA4_IRQSTATUS_L0		0x08
+#define OMAP_DMA4_IRQSTATUS_L1		0x0c
+#define OMAP_DMA4_IRQSTATUS_L2		0x10
+#define OMAP_DMA4_IRQSTATUS_L3		0x14
+#define OMAP_DMA4_IRQENABLE_L0		0x18
+#define OMAP_DMA4_IRQENABLE_L1		0x1c
+#define OMAP_DMA4_IRQENABLE_L2		0x20
+#define OMAP_DMA4_IRQENABLE_L3		0x24
+#define OMAP_DMA4_SYSSTATUS		0x28
+#define OMAP_DMA4_OCP_SYSCONFIG		0x2c
+#define OMAP_DMA4_CAPS_0		0x64
+#define OMAP_DMA4_CAPS_2		0x6c
+#define OMAP_DMA4_CAPS_3		0x70
+#define OMAP_DMA4_CAPS_4		0x74
+
+#define OMAP1_LOGICAL_DMA_CH_COUNT	17
+#define OMAP_DMA4_LOGICAL_DMA_CH_COUNT	32	/* REVISIT: Is this 32 + 2? */
+
+/* Common channel specific registers for omap1 */
+#define OMAP1_DMA_CH_BASE(n)		(0x40 * (n) + 0x00)
+#define OMAP1_DMA_CSDP(n)		(0x40 * (n) + 0x00)
+#define OMAP1_DMA_CCR(n)		(0x40 * (n) + 0x02)
+#define OMAP1_DMA_CICR(n)		(0x40 * (n) + 0x04)
+#define OMAP1_DMA_CSR(n)		(0x40 * (n) + 0x06)
+#define OMAP1_DMA_CEN(n)		(0x40 * (n) + 0x10)
+#define OMAP1_DMA_CFN(n)		(0x40 * (n) + 0x12)
+#define OMAP1_DMA_CSFI(n)		(0x40 * (n) + 0x14)
+#define OMAP1_DMA_CSEI(n)		(0x40 * (n) + 0x16)
+#define OMAP1_DMA_CPC(n)		(0x40 * (n) + 0x18)	/* 15xx only */
+#define OMAP1_DMA_CSAC(n)		(0x40 * (n) + 0x18)
+#define OMAP1_DMA_CDAC(n)		(0x40 * (n) + 0x1a)
+#define OMAP1_DMA_CDEI(n)		(0x40 * (n) + 0x1c)
+#define OMAP1_DMA_CDFI(n)		(0x40 * (n) + 0x1e)
+#define OMAP1_DMA_CLNK_CTRL(n)		(0x40 * (n) + 0x28)
+
+/* Common channel specific registers for omap2 */
+#define OMAP_DMA4_CH_BASE(n)		(0x60 * (n) + 0x80)
+#define OMAP_DMA4_CCR(n)		(0x60 * (n) + 0x80)
+#define OMAP_DMA4_CLNK_CTRL(n)		(0x60 * (n) + 0x84)
+#define OMAP_DMA4_CICR(n)		(0x60 * (n) + 0x88)
+#define OMAP_DMA4_CSR(n)		(0x60 * (n) + 0x8c)
+#define OMAP_DMA4_CSDP(n)		(0x60 * (n) + 0x90)
+#define OMAP_DMA4_CEN(n)		(0x60 * (n) + 0x94)
+#define OMAP_DMA4_CFN(n)		(0x60 * (n) + 0x98)
+#define OMAP_DMA4_CSEI(n)		(0x60 * (n) + 0xa4)
+#define OMAP_DMA4_CSFI(n)		(0x60 * (n) + 0xa8)
+#define OMAP_DMA4_CDEI(n)		(0x60 * (n) + 0xac)
+#define OMAP_DMA4_CDFI(n)		(0x60 * (n) + 0xb0)
+#define OMAP_DMA4_CSAC(n)		(0x60 * (n) + 0xb4)
+#define OMAP_DMA4_CDAC(n)		(0x60 * (n) + 0xb8)
+
+/* Channel specific registers only on omap1 */
+#define OMAP1_DMA_CSSA_L(n)		(0x40 * (n) + 0x08)
+#define OMAP1_DMA_CSSA_U(n)		(0x40 * (n) + 0x0a)
+#define OMAP1_DMA_CDSA_L(n)		(0x40 * (n) + 0x0c)
+#define OMAP1_DMA_CDSA_U(n)		(0x40 * (n) + 0x0e)
+#define OMAP1_DMA_COLOR_L(n)		(0x40 * (n) + 0x20)
+#define OMAP1_DMA_COLOR_U(n)		(0x40 * (n) + 0x22)
+#define OMAP1_DMA_CCR2(n)		(0x40 * (n) + 0x24)
+#define OMAP1_DMA_LCH_CTRL(n)		(0x40 * (n) + 0x2a)	/* not on 15xx */
+#define OMAP1_DMA_CCEN(n)		0
+#define OMAP1_DMA_CCFN(n)		0
+
+/* Channel specific registers only on omap2 */
+#define OMAP_DMA4_CSSA(n)		(0x60 * (n) + 0x9c)
+#define OMAP_DMA4_CDSA(n)		(0x60 * (n) + 0xa0)
+#define OMAP_DMA4_CCEN(n)		(0x60 * (n) + 0xbc)
+#define OMAP_DMA4_CCFN(n)		(0x60 * (n) + 0xc0)
+#define OMAP_DMA4_COLOR(n)		(0x60 * (n) + 0xc4)
+
+/* Additional registers available on OMAP4 */
+#define OMAP_DMA4_CDP(n)		(0x60 * (n) + 0xd0)
+#define OMAP_DMA4_CNDP(n)		(0x60 * (n) + 0xd4)
+#define OMAP_DMA4_CCDN(n)		(0x60 * (n) + 0xd8)
+
+/* Dummy defines to keep multi-omap compiles happy */
+#define OMAP1_DMA_REVISION		0
+#define OMAP1_DMA_IRQSTATUS_L0		0
+#define OMAP1_DMA_IRQENABLE_L0		0
+#define OMAP1_DMA_OCP_SYSCONFIG		0
+#define OMAP_DMA4_HW_ID			0
+#define OMAP_DMA4_CAPS_0_L		0
+#define OMAP_DMA4_CAPS_0_U		0
+#define OMAP_DMA4_CAPS_1_L		0
+#define OMAP_DMA4_CAPS_1_U		0
+#define OMAP_DMA4_GSCR			0
+#define OMAP_DMA4_CPC(n)		0
+
+#define OMAP_DMA4_LCH_CTRL(n)		0
+#define OMAP_DMA4_COLOR_L(n)		0
+#define OMAP_DMA4_COLOR_U(n)		0
+#define OMAP_DMA4_CCR2(n)		0
+#define OMAP1_DMA_CSSA(n)		0
+#define OMAP1_DMA_CDSA(n)		0
+#define OMAP_DMA4_CSSA_L(n)		0
+#define OMAP_DMA4_CSSA_U(n)		0
+#define OMAP_DMA4_CDSA_L(n)		0
+#define OMAP_DMA4_CDSA_U(n)		0
+#define OMAP1_DMA_COLOR(n)		0
+
+/*----------------------------------------------------------------------------*/
+
+/* DMA channels for omap1 */
+#define OMAP_DMA_NO_DEVICE		0
+#define OMAP_DMA_MCSI1_TX		1
+#define OMAP_DMA_MCSI1_RX		2
+#define OMAP_DMA_I2C_RX			3
+#define OMAP_DMA_I2C_TX			4
+#define OMAP_DMA_EXT_NDMA_REQ		5
+#define OMAP_DMA_EXT_NDMA_REQ2		6
+#define OMAP_DMA_UWIRE_TX		7
+#define OMAP_DMA_MCBSP1_TX		8
+#define OMAP_DMA_MCBSP1_RX		9
+#define OMAP_DMA_MCBSP3_TX		10
+#define OMAP_DMA_MCBSP3_RX		11
+#define OMAP_DMA_UART1_TX		12
+#define OMAP_DMA_UART1_RX		13
+#define OMAP_DMA_UART2_TX		14
+#define OMAP_DMA_UART2_RX		15
+#define OMAP_DMA_MCBSP2_TX		16
+#define OMAP_DMA_MCBSP2_RX		17
+#define OMAP_DMA_UART3_TX		18
+#define OMAP_DMA_UART3_RX		19
+#define OMAP_DMA_CAMERA_IF_RX		20
+#define OMAP_DMA_MMC_TX			21
+#define OMAP_DMA_MMC_RX			22
+#define OMAP_DMA_NAND			23
+#define OMAP_DMA_IRQ_LCD_LINE		24
+#define OMAP_DMA_MEMORY_STICK		25
+#define OMAP_DMA_USB_W2FC_RX0		26
+#define OMAP_DMA_USB_W2FC_RX1		27
+#define OMAP_DMA_USB_W2FC_RX2		28
+#define OMAP_DMA_USB_W2FC_TX0		29
+#define OMAP_DMA_USB_W2FC_TX1		30
+#define OMAP_DMA_USB_W2FC_TX2		31
+
+/* These are only for 1610 */
+#define OMAP_DMA_CRYPTO_DES_IN		32
+#define OMAP_DMA_SPI_TX			33
+#define OMAP_DMA_SPI_RX			34
+#define OMAP_DMA_CRYPTO_HASH		35
+#define OMAP_DMA_CCP_ATTN		36
+#define OMAP_DMA_CCP_FIFO_NOT_EMPTY	37
+#define OMAP_DMA_CMT_APE_TX_CHAN_0	38
+#define OMAP_DMA_CMT_APE_RV_CHAN_0	39
+#define OMAP_DMA_CMT_APE_TX_CHAN_1	40
+#define OMAP_DMA_CMT_APE_RV_CHAN_1	41
+#define OMAP_DMA_CMT_APE_TX_CHAN_2	42
+#define OMAP_DMA_CMT_APE_RV_CHAN_2	43
+#define OMAP_DMA_CMT_APE_TX_CHAN_3	44
+#define OMAP_DMA_CMT_APE_RV_CHAN_3	45
+#define OMAP_DMA_CMT_APE_TX_CHAN_4	46
+#define OMAP_DMA_CMT_APE_RV_CHAN_4	47
+#define OMAP_DMA_CMT_APE_TX_CHAN_5	48
+#define OMAP_DMA_CMT_APE_RV_CHAN_5	49
+#define OMAP_DMA_CMT_APE_TX_CHAN_6	50
+#define OMAP_DMA_CMT_APE_RV_CHAN_6	51
+#define OMAP_DMA_CMT_APE_TX_CHAN_7	52
+#define OMAP_DMA_CMT_APE_RV_CHAN_7	53
+#define OMAP_DMA_MMC2_TX		54
+#define OMAP_DMA_MMC2_RX		55
+#define OMAP_DMA_CRYPTO_DES_OUT		56
+
+/* DMA channels for 24xx */
+#define OMAP24XX_DMA_NO_DEVICE		0
+#define OMAP24XX_DMA_XTI_DMA		1	/* S_DMA_0 */
+#define OMAP24XX_DMA_EXT_DMAREQ0	2	/* S_DMA_1 */
+#define OMAP24XX_DMA_EXT_DMAREQ1	3	/* S_DMA_2 */
+#define OMAP24XX_DMA_GPMC		4	/* S_DMA_3 */
+#define OMAP24XX_DMA_GFX		5	/* S_DMA_4 */
+#define OMAP24XX_DMA_DSS		6	/* S_DMA_5 */
+#define OMAP242X_DMA_VLYNQ_TX		7	/* S_DMA_6 */
+#define OMAP24XX_DMA_EXT_DMAREQ2	7	/* S_DMA_6 */
+#define OMAP24XX_DMA_CWT		8	/* S_DMA_7 */
+#define OMAP24XX_DMA_AES_TX		9	/* S_DMA_8 */
+#define OMAP24XX_DMA_AES_RX		10	/* S_DMA_9 */
+#define OMAP24XX_DMA_DES_TX		11	/* S_DMA_10 */
+#define OMAP24XX_DMA_DES_RX		12	/* S_DMA_11 */
+#define OMAP24XX_DMA_SHA1MD5_RX		13	/* S_DMA_12 */
+#define OMAP34XX_DMA_SHA2MD5_RX		13	/* S_DMA_12 */
+#define OMAP242X_DMA_EXT_DMAREQ2	14	/* S_DMA_13 */
+#define OMAP242X_DMA_EXT_DMAREQ3	15	/* S_DMA_14 */
+#define OMAP242X_DMA_EXT_DMAREQ4	16	/* S_DMA_15 */
+#define OMAP242X_DMA_EAC_AC_RD		17	/* S_DMA_16 */
+#define OMAP242X_DMA_EAC_AC_WR		18	/* S_DMA_17 */
+#define OMAP242X_DMA_EAC_MD_UL_RD	19	/* S_DMA_18 */
+#define OMAP242X_DMA_EAC_MD_UL_WR	20	/* S_DMA_19 */
+#define OMAP242X_DMA_EAC_MD_DL_RD	21	/* S_DMA_20 */
+#define OMAP242X_DMA_EAC_MD_DL_WR	22	/* S_DMA_21 */
+#define OMAP242X_DMA_EAC_BT_UL_RD	23	/* S_DMA_22 */
+#define OMAP242X_DMA_EAC_BT_UL_WR	24	/* S_DMA_23 */
+#define OMAP242X_DMA_EAC_BT_DL_RD	25	/* S_DMA_24 */
+#define OMAP242X_DMA_EAC_BT_DL_WR	26	/* S_DMA_25 */
+#define OMAP243X_DMA_EXT_DMAREQ3	14	/* S_DMA_13 */
+#define OMAP24XX_DMA_SPI3_TX0		15	/* S_DMA_14 */
+#define OMAP24XX_DMA_SPI3_RX0		16	/* S_DMA_15 */
+#define OMAP24XX_DMA_MCBSP3_TX		17	/* S_DMA_16 */
+#define OMAP24XX_DMA_MCBSP3_RX		18	/* S_DMA_17 */
+#define OMAP24XX_DMA_MCBSP4_TX		19	/* S_DMA_18 */
+#define OMAP24XX_DMA_MCBSP4_RX		20	/* S_DMA_19 */
+#define OMAP24XX_DMA_MCBSP5_TX		21	/* S_DMA_20 */
+#define OMAP24XX_DMA_MCBSP5_RX		22	/* S_DMA_21 */
+#define OMAP24XX_DMA_SPI3_TX1		23	/* S_DMA_22 */
+#define OMAP24XX_DMA_SPI3_RX1		24	/* S_DMA_23 */
+#define OMAP243X_DMA_EXT_DMAREQ4	25	/* S_DMA_24 */
+#define OMAP243X_DMA_EXT_DMAREQ5	26	/* S_DMA_25 */
+#define OMAP34XX_DMA_I2C3_TX		25	/* S_DMA_24 */
+#define OMAP34XX_DMA_I2C3_RX		26	/* S_DMA_25 */
+#define OMAP24XX_DMA_I2C1_TX		27	/* S_DMA_26 */
+#define OMAP24XX_DMA_I2C1_RX		28	/* S_DMA_27 */
+#define OMAP24XX_DMA_I2C2_TX		29	/* S_DMA_28 */
+#define OMAP24XX_DMA_I2C2_RX		30	/* S_DMA_29 */
+#define OMAP24XX_DMA_MCBSP1_TX		31	/* S_DMA_30 */
+#define OMAP24XX_DMA_MCBSP1_RX		32	/* S_DMA_31 */
+#define OMAP24XX_DMA_MCBSP2_TX		33	/* S_DMA_32 */
+#define OMAP24XX_DMA_MCBSP2_RX		34	/* S_DMA_33 */
+#define OMAP24XX_DMA_SPI1_TX0		35	/* S_DMA_34 */
+#define OMAP24XX_DMA_SPI1_RX0		36	/* S_DMA_35 */
+#define OMAP24XX_DMA_SPI1_TX1		37	/* S_DMA_36 */
+#define OMAP24XX_DMA_SPI1_RX1		38	/* S_DMA_37 */
+#define OMAP24XX_DMA_SPI1_TX2		39	/* S_DMA_38 */
+#define OMAP24XX_DMA_SPI1_RX2		40	/* S_DMA_39 */
+#define OMAP24XX_DMA_SPI1_TX3		41	/* S_DMA_40 */
+#define OMAP24XX_DMA_SPI1_RX3		42	/* S_DMA_41 */
+#define OMAP24XX_DMA_SPI2_TX0		43	/* S_DMA_42 */
+#define OMAP24XX_DMA_SPI2_RX0		44	/* S_DMA_43 */
+#define OMAP24XX_DMA_SPI2_TX1		45	/* S_DMA_44 */
+#define OMAP24XX_DMA_SPI2_RX1		46	/* S_DMA_45 */
+#define OMAP24XX_DMA_MMC2_TX		47	/* S_DMA_46 */
+#define OMAP24XX_DMA_MMC2_RX		48	/* S_DMA_47 */
+#define OMAP24XX_DMA_UART1_TX		49	/* S_DMA_48 */
+#define OMAP24XX_DMA_UART1_RX		50	/* S_DMA_49 */
+#define OMAP24XX_DMA_UART2_TX		51	/* S_DMA_50 */
+#define OMAP24XX_DMA_UART2_RX		52	/* S_DMA_51 */
+#define OMAP24XX_DMA_UART3_TX		53	/* S_DMA_52 */
+#define OMAP24XX_DMA_UART3_RX		54	/* S_DMA_53 */
+#define OMAP24XX_DMA_USB_W2FC_TX0	55	/* S_DMA_54 */
+#define OMAP24XX_DMA_USB_W2FC_RX0	56	/* S_DMA_55 */
+#define OMAP24XX_DMA_USB_W2FC_TX1	57	/* S_DMA_56 */
+#define OMAP24XX_DMA_USB_W2FC_RX1	58	/* S_DMA_57 */
+#define OMAP24XX_DMA_USB_W2FC_TX2	59	/* S_DMA_58 */
+#define OMAP24XX_DMA_USB_W2FC_RX2	60	/* S_DMA_59 */
+#define OMAP24XX_DMA_MMC1_TX		61	/* S_DMA_60 */
+#define OMAP24XX_DMA_MMC1_RX		62	/* S_DMA_61 */
+#define OMAP24XX_DMA_MS			63	/* S_DMA_62 */
+#define OMAP242X_DMA_EXT_DMAREQ5	64	/* S_DMA_63 */
+#define OMAP243X_DMA_EXT_DMAREQ6	64	/* S_DMA_63 */
+#define OMAP34XX_DMA_EXT_DMAREQ3	64	/* S_DMA_63 */
+#define OMAP34XX_DMA_AES2_TX		65	/* S_DMA_64 */
+#define OMAP34XX_DMA_AES2_RX		66	/* S_DMA_65 */
+#define OMAP34XX_DMA_DES2_TX		67	/* S_DMA_66 */
+#define OMAP34XX_DMA_DES2_RX		68	/* S_DMA_67 */
+#define OMAP34XX_DMA_SHA1MD5_RX		69	/* S_DMA_68 */
+#define OMAP34XX_DMA_SPI4_TX0		70	/* S_DMA_69 */
+#define OMAP34XX_DMA_SPI4_RX0		71	/* S_DMA_70 */
+#define OMAP34XX_DSS_DMA0		72	/* S_DMA_71 */
+#define OMAP34XX_DSS_DMA1		73	/* S_DMA_72 */
+#define OMAP34XX_DSS_DMA2		74	/* S_DMA_73 */
+#define OMAP34XX_DSS_DMA3		75	/* S_DMA_74 */
+#define OMAP34XX_DMA_MMC3_TX		77	/* S_DMA_76 */
+#define OMAP34XX_DMA_MMC3_RX		78	/* S_DMA_77 */
+#define OMAP34XX_DMA_USIM_TX		79	/* S_DMA_78 */
+#define OMAP34XX_DMA_USIM_RX		80	/* S_DMA_79 */
+
+/* DMA request lines for 44xx */
+#define OMAP44XX_DMA_DSS_DISPC_REQ	6	/* S_DMA_5 */
+#define OMAP44XX_DMA_SYS_REQ2		7	/* S_DMA_6 */
+#define OMAP44XX_DMA_ISS_REQ1		9	/* S_DMA_8 */
+#define OMAP44XX_DMA_ISS_REQ2		10	/* S_DMA_9 */
+#define OMAP44XX_DMA_ISS_REQ3		12	/* S_DMA_11 */
+#define OMAP44XX_DMA_ISS_REQ4		13	/* S_DMA_12 */
+#define OMAP44XX_DMA_DSS_RFBI_REQ	14	/* S_DMA_13 */
+#define OMAP44XX_DMA_SPI3_TX0		15	/* S_DMA_14 */
+#define OMAP44XX_DMA_SPI3_RX0		16	/* S_DMA_15 */
+#define OMAP44XX_DMA_MCBSP2_TX		17	/* S_DMA_16 */
+#define OMAP44XX_DMA_MCBSP2_RX		18	/* S_DMA_17 */
+#define OMAP44XX_DMA_MCBSP3_TX		19	/* S_DMA_18 */
+#define OMAP44XX_DMA_MCBSP3_RX		20	/* S_DMA_19 */
+#define OMAP44XX_DMA_SPI3_TX1		23	/* S_DMA_22 */
+#define OMAP44XX_DMA_SPI3_RX1		24	/* S_DMA_23 */
+#define OMAP44XX_DMA_I2C3_TX		25	/* S_DMA_24 */
+#define OMAP44XX_DMA_I2C3_RX		26	/* S_DMA_25 */
+#define OMAP44XX_DMA_I2C1_TX		27	/* S_DMA_26 */
+#define OMAP44XX_DMA_I2C1_RX		28	/* S_DMA_27 */
+#define OMAP44XX_DMA_I2C2_TX		29	/* S_DMA_28 */
+#define OMAP44XX_DMA_I2C2_RX		30	/* S_DMA_29 */
+#define OMAP44XX_DMA_MCBSP4_TX		31	/* S_DMA_30 */
+#define OMAP44XX_DMA_MCBSP4_RX		32	/* S_DMA_31 */
+#define OMAP44XX_DMA_MCBSP1_TX		33	/* S_DMA_32 */
+#define OMAP44XX_DMA_MCBSP1_RX		34	/* S_DMA_33 */
+#define OMAP44XX_DMA_SPI1_TX0		35	/* S_DMA_34 */
+#define OMAP44XX_DMA_SPI1_RX0		36	/* S_DMA_35 */
+#define OMAP44XX_DMA_SPI1_TX1		37	/* S_DMA_36 */
+#define OMAP44XX_DMA_SPI1_RX1		38	/* S_DMA_37 */
+#define OMAP44XX_DMA_SPI1_TX2		39	/* S_DMA_38 */
+#define OMAP44XX_DMA_SPI1_RX2		40	/* S_DMA_39 */
+#define OMAP44XX_DMA_SPI1_TX3		41	/* S_DMA_40 */
+#define OMAP44XX_DMA_SPI1_RX3		42	/* S_DMA_41 */
+#define OMAP44XX_DMA_SPI2_TX0		43	/* S_DMA_42 */
+#define OMAP44XX_DMA_SPI2_RX0		44	/* S_DMA_43 */
+#define OMAP44XX_DMA_SPI2_TX1		45	/* S_DMA_44 */
+#define OMAP44XX_DMA_SPI2_RX1		46	/* S_DMA_45 */
+#define OMAP44XX_DMA_MMC2_TX		47	/* S_DMA_46 */
+#define OMAP44XX_DMA_MMC2_RX		48	/* S_DMA_47 */
+#define OMAP44XX_DMA_UART1_TX		49	/* S_DMA_48 */
+#define OMAP44XX_DMA_UART1_RX		50	/* S_DMA_49 */
+#define OMAP44XX_DMA_UART2_TX		51	/* S_DMA_50 */
+#define OMAP44XX_DMA_UART2_RX		52	/* S_DMA_51 */
+#define OMAP44XX_DMA_UART3_TX		53	/* S_DMA_52 */
+#define OMAP44XX_DMA_UART3_RX		54	/* S_DMA_53 */
+#define OMAP44XX_DMA_UART4_TX		55	/* S_DMA_54 */
+#define OMAP44XX_DMA_UART4_RX		56	/* S_DMA_55 */
+#define OMAP44XX_DMA_MMC4_TX		57	/* S_DMA_56 */
+#define OMAP44XX_DMA_MMC4_RX		58	/* S_DMA_57 */
+#define OMAP44XX_DMA_MMC5_TX		59	/* S_DMA_58 */
+#define OMAP44XX_DMA_MMC5_RX		60	/* S_DMA_59 */
+#define OMAP44XX_DMA_MMC1_TX		61	/* S_DMA_60 */
+#define OMAP44XX_DMA_MMC1_RX		62	/* S_DMA_61 */
+#define OMAP44XX_DMA_SYS_REQ3		64	/* S_DMA_63 */
+#define OMAP44XX_DMA_MCPDM_UP		65	/* S_DMA_64 */
+#define OMAP44XX_DMA_MCPDM_DL		66	/* S_DMA_65 */
+#define OMAP44XX_DMA_SPI4_TX0		70	/* S_DMA_69 */
+#define OMAP44XX_DMA_SPI4_RX0		71	/* S_DMA_70 */
+#define OMAP44XX_DMA_DSS_DSI1_REQ0	72	/* S_DMA_71 */
+#define OMAP44XX_DMA_DSS_DSI1_REQ1	73	/* S_DMA_72 */
+#define OMAP44XX_DMA_DSS_DSI1_REQ2	74	/* S_DMA_73 */
+#define OMAP44XX_DMA_DSS_DSI1_REQ3	75	/* S_DMA_74 */
+#define OMAP44XX_DMA_DSS_HDMI_REQ	76	/* S_DMA_75 */
+#define OMAP44XX_DMA_MMC3_TX		77	/* S_DMA_76 */
+#define OMAP44XX_DMA_MMC3_RX		78	/* S_DMA_77 */
+#define OMAP44XX_DMA_USIM_TX		79	/* S_DMA_78 */
+#define OMAP44XX_DMA_USIM_RX		80	/* S_DMA_79 */
+#define OMAP44XX_DMA_DSS_DSI2_REQ0	81	/* S_DMA_80 */
+#define OMAP44XX_DMA_DSS_DSI2_REQ1	82	/* S_DMA_81 */
+#define OMAP44XX_DMA_DSS_DSI2_REQ2	83	/* S_DMA_82 */
+#define OMAP44XX_DMA_DSS_DSI2_REQ3	84	/* S_DMA_83 */
+#define OMAP44XX_DMA_ABE_REQ0		101	/* S_DMA_100 */
+#define OMAP44XX_DMA_ABE_REQ1		102	/* S_DMA_101 */
+#define OMAP44XX_DMA_ABE_REQ2		103	/* S_DMA_102 */
+#define OMAP44XX_DMA_ABE_REQ3		104	/* S_DMA_103 */
+#define OMAP44XX_DMA_ABE_REQ4		105	/* S_DMA_104 */
+#define OMAP44XX_DMA_ABE_REQ5		106	/* S_DMA_105 */
+#define OMAP44XX_DMA_ABE_REQ6		107	/* S_DMA_106 */
+#define OMAP44XX_DMA_ABE_REQ7		108	/* S_DMA_107 */
+#define OMAP44XX_DMA_I2C4_TX		124	/* S_DMA_123 */
+#define OMAP44XX_DMA_I2C4_RX		125	/* S_DMA_124 */
+
+/*----------------------------------------------------------------------------*/
+
+#define OMAP1_DMA_TOUT_IRQ		(1 << 0)
+#define OMAP_DMA_DROP_IRQ		(1 << 1)
+#define OMAP_DMA_HALF_IRQ		(1 << 2)
+#define OMAP_DMA_FRAME_IRQ		(1 << 3)
+#define OMAP_DMA_LAST_IRQ		(1 << 4)
+#define OMAP_DMA_BLOCK_IRQ		(1 << 5)
+#define OMAP1_DMA_SYNC_IRQ		(1 << 6)
+#define OMAP2_DMA_PKT_IRQ		(1 << 7)
+#define OMAP2_DMA_TRANS_ERR_IRQ		(1 << 8)
+#define OMAP2_DMA_SECURE_ERR_IRQ	(1 << 9)
+#define OMAP2_DMA_SUPERVISOR_ERR_IRQ	(1 << 10)
+#define OMAP2_DMA_MISALIGNED_ERR_IRQ	(1 << 11)
+
+#define OMAP_DMA_CCR_EN			(1 << 7)
+
+#define OMAP_DMA_DATA_TYPE_S8		0x00
+#define OMAP_DMA_DATA_TYPE_S16		0x01
+#define OMAP_DMA_DATA_TYPE_S32		0x02
+
+#define OMAP_DMA_SYNC_ELEMENT		0x00
+#define OMAP_DMA_SYNC_FRAME		0x01
+#define OMAP_DMA_SYNC_BLOCK		0x02
+#define OMAP_DMA_SYNC_PACKET		0x03
+
+#define OMAP_DMA_SRC_SYNC		0x01
+#define OMAP_DMA_DST_SYNC		0x00
+
+#define OMAP_DMA_PORT_EMIFF		0x00
+#define OMAP_DMA_PORT_EMIFS		0x01
+#define OMAP_DMA_PORT_OCP_T1		0x02
+#define OMAP_DMA_PORT_TIPB		0x03
+#define OMAP_DMA_PORT_OCP_T2		0x04
+#define OMAP_DMA_PORT_MPUI		0x05
+
+#define OMAP_DMA_AMODE_CONSTANT		0x00
+#define OMAP_DMA_AMODE_POST_INC		0x01
+#define OMAP_DMA_AMODE_SINGLE_IDX	0x02
+#define OMAP_DMA_AMODE_DOUBLE_IDX	0x03
+
+#define DMA_DEFAULT_FIFO_DEPTH		0x10
+#define DMA_DEFAULT_ARB_RATE		0x01
+/* Pass THREAD_RESERVE ORed with THREAD_FIFO for tparams */
+#define DMA_THREAD_RESERVE_NORM		(0x00 << 12) /* Def */
+#define DMA_THREAD_RESERVE_ONET		(0x01 << 12)
+#define DMA_THREAD_RESERVE_TWOT		(0x02 << 12)
+#define DMA_THREAD_RESERVE_THREET	(0x03 << 12)
+#define DMA_THREAD_FIFO_NONE		(0x00 << 14) /* Def */
+#define DMA_THREAD_FIFO_75		(0x01 << 14)
+#define DMA_THREAD_FIFO_25		(0x02 << 14)
+#define DMA_THREAD_FIFO_50		(0x03 << 14)
+
+/* DMA4_OCP_SYSCONFIG bits */
+#define DMA_SYSCONFIG_MIDLEMODE_MASK		(3 << 12)
+#define DMA_SYSCONFIG_CLOCKACTIVITY_MASK	(3 << 8)
+#define DMA_SYSCONFIG_EMUFREE			(1 << 5)
+#define DMA_SYSCONFIG_SIDLEMODE_MASK		(3 << 3)
+#define DMA_SYSCONFIG_SOFTRESET			(1 << 2)
+#define DMA_SYSCONFIG_AUTOIDLE			(1 << 0)
+
+#define DMA_SYSCONFIG_MIDLEMODE(n)		((n) << 12)
+#define DMA_SYSCONFIG_SIDLEMODE(n)		((n) << 3)
+
+#define DMA_IDLEMODE_SMARTIDLE			0x2
+#define DMA_IDLEMODE_NO_IDLE			0x1
+#define DMA_IDLEMODE_FORCE_IDLE			0x0
+
+/* Chaining modes*/
+#ifndef CONFIG_ARCH_OMAP1
+#define OMAP_DMA_STATIC_CHAIN		0x1
+#define OMAP_DMA_DYNAMIC_CHAIN		0x2
+#define OMAP_DMA_CHAIN_ACTIVE		0x1
+#define OMAP_DMA_CHAIN_INACTIVE		0x0
+#endif
+
+#define DMA_CH_PRIO_HIGH		0x1
+#define DMA_CH_PRIO_LOW			0x0 /* Def */
+
+enum omap_dma_burst_mode {
+	OMAP_DMA_DATA_BURST_DIS = 0,
+	OMAP_DMA_DATA_BURST_4,
+	OMAP_DMA_DATA_BURST_8,
+	OMAP_DMA_DATA_BURST_16,
+};
+
+enum end_type {
+	OMAP_DMA_LITTLE_ENDIAN = 0,
+	OMAP_DMA_BIG_ENDIAN
+};
+
+enum omap_dma_color_mode {
+	OMAP_DMA_COLOR_DIS = 0,
+	OMAP_DMA_CONSTANT_FILL,
+	OMAP_DMA_TRANSPARENT_COPY
+};
+
+enum omap_dma_write_mode {
+	OMAP_DMA_WRITE_NON_POSTED = 0,
+	OMAP_DMA_WRITE_POSTED,
+	OMAP_DMA_WRITE_LAST_NON_POSTED
+};
+
+enum omap_dma_channel_mode {
+	OMAP_DMA_LCH_2D = 0,
+	OMAP_DMA_LCH_G,
+	OMAP_DMA_LCH_P,
+	OMAP_DMA_LCH_PD
+};
+
+struct omap_dma_channel_params {
+	int data_type;		/* data type 8,16,32 */
+	int elem_count;		/* number of elements in a frame */
+	int frame_count;	/* number of frames in a element */
+
+	int src_port;		/* Only on OMAP1 REVISIT: Is this needed? */
+	int src_amode;		/* constant, post increment, indexed,
+					double indexed */
+	unsigned long src_start;	/* source address : physical */
+	int src_ei;		/* source element index */
+	int src_fi;		/* source frame index */
+
+	int dst_port;		/* Only on OMAP1 REVISIT: Is this needed? */
+	int dst_amode;		/* constant, post increment, indexed,
+					double indexed */
+	unsigned long dst_start;	/* source address : physical */
+	int dst_ei;		/* source element index */
+	int dst_fi;		/* source frame index */
+
+	int trigger;		/* trigger attached if the channel is
+					synchronized */
+	int sync_mode;		/* sycn on element, frame , block or packet */
+	int src_or_dst_synch;	/* source synch(1) or destination synch(0) */
+
+	int ie;			/* interrupt enabled */
+
+	unsigned char read_prio;/* read priority */
+	unsigned char write_prio;/* write priority */
+
+#ifndef CONFIG_ARCH_OMAP1
+	enum omap_dma_burst_mode burst_mode; /* Burst mode 4/8/16 words */
+#endif
+};
+
+
+extern void omap_set_dma_priority(int lch, int dst_port, int priority);
+extern int omap_request_dma(int dev_id, const char *dev_name,
+			void (*callback)(int lch, u16 ch_status, void *data),
+			void *data, int *dma_ch);
+extern void omap_enable_dma_irq(int ch, u16 irq_bits);
+extern void omap_disable_dma_irq(int ch, u16 irq_bits);
+extern void omap_free_dma(int ch);
+extern void omap_start_dma(int lch);
+extern void omap_stop_dma(int lch);
+extern void omap_set_dma_transfer_params(int lch, int data_type,
+					 int elem_count, int frame_count,
+					 int sync_mode,
+					 int dma_trigger, int src_or_dst_synch);
+extern void omap_set_dma_color_mode(int lch, enum omap_dma_color_mode mode,
+				    u32 color);
+extern void omap_set_dma_write_mode(int lch, enum omap_dma_write_mode mode);
+extern void omap_set_dma_channel_mode(int lch, enum omap_dma_channel_mode mode);
+
+extern void omap_set_dma_src_params(int lch, int src_port, int src_amode,
+				    unsigned long src_start,
+				    int src_ei, int src_fi);
+extern void omap_set_dma_src_index(int lch, int eidx, int fidx);
+extern void omap_set_dma_src_data_pack(int lch, int enable);
+extern void omap_set_dma_src_burst_mode(int lch,
+					enum omap_dma_burst_mode burst_mode);
+
+extern void omap_set_dma_dest_params(int lch, int dest_port, int dest_amode,
+				     unsigned long dest_start,
+				     int dst_ei, int dst_fi);
+extern void omap_set_dma_dest_index(int lch, int eidx, int fidx);
+extern void omap_set_dma_dest_data_pack(int lch, int enable);
+extern void omap_set_dma_dest_burst_mode(int lch,
+					 enum omap_dma_burst_mode burst_mode);
+
+extern void omap_set_dma_params(int lch,
+				struct omap_dma_channel_params *params);
+
+extern void omap_dma_link_lch(int lch_head, int lch_queue);
+extern void omap_dma_unlink_lch(int lch_head, int lch_queue);
+
+extern int omap_set_dma_callback(int lch,
+			void (*callback)(int lch, u16 ch_status, void *data),
+			void *data);
+extern dma_addr_t omap_get_dma_src_pos(int lch);
+extern dma_addr_t omap_get_dma_dst_pos(int lch);
+extern void omap_clear_dma(int lch);
+extern int omap_get_dma_active_status(int lch);
+extern int omap_dma_running(void);
+extern void omap_dma_set_global_params(int arb_rate, int max_fifo_depth,
+				       int tparams);
+extern int omap_dma_set_prio_lch(int lch, unsigned char read_prio,
+				 unsigned char write_prio);
+extern void omap_set_dma_dst_endian_type(int lch, enum end_type etype);
+extern void omap_set_dma_src_endian_type(int lch, enum end_type etype);
+extern int omap_get_dma_index(int lch, int *ei, int *fi);
+
+void omap_dma_global_context_save(void);
+void omap_dma_global_context_restore(void);
+
+extern void omap_dma_disable_irq(int lch);
+
+/* Chaining APIs */
+#ifndef CONFIG_ARCH_OMAP1
+extern int omap_request_dma_chain(int dev_id, const char *dev_name,
+				  void (*callback) (int lch, u16 ch_status,
+						    void *data),
+				  int *chain_id, int no_of_chans,
+				  int chain_mode,
+				  struct omap_dma_channel_params params);
+extern int omap_free_dma_chain(int chain_id);
+extern int omap_dma_chain_a_transfer(int chain_id, int src_start,
+				     int dest_start, int elem_count,
+				     int frame_count, void *callbk_data);
+extern int omap_start_dma_chain_transfers(int chain_id);
+extern int omap_stop_dma_chain_transfers(int chain_id);
+extern int omap_get_dma_chain_index(int chain_id, int *ei, int *fi);
+extern int omap_get_dma_chain_dst_pos(int chain_id);
+extern int omap_get_dma_chain_src_pos(int chain_id);
+
+extern int omap_modify_dma_chain_params(int chain_id,
+					struct omap_dma_channel_params params);
+extern int omap_dma_chain_status(int chain_id);
+#endif
+
+#if defined(CONFIG_ARCH_OMAP1) && defined(CONFIG_FB_OMAP)
+#include <mach/lcd_dma.h>
+#else
+static inline int omap_lcd_dma_running(void)
+{
+	return 0;
+}
+#endif
+
+#endif /* __ASM_ARCH_DMA_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/dmtimer.h
@@ -0,0 +1,84 @@
+/*
+ * arch/arm/plat-omap/include/mach/dmtimer.h
+ *
+ * OMAP Dual-Mode Timers
+ *
+ * Copyright (C) 2005 Nokia Corporation
+ * Author: Lauri Leukkunen <lauri.leukkunen@nokia.com>
+ * PWM and clock framwork support by Timo Teras.
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_DMTIMER_H
+#define __ASM_ARCH_DMTIMER_H
+
+/* clock sources */
+#define OMAP_TIMER_SRC_SYS_CLK			0x00
+#define OMAP_TIMER_SRC_32_KHZ			0x01
+#define OMAP_TIMER_SRC_EXT_CLK			0x02
+
+/* timer interrupt enable bits */
+#define OMAP_TIMER_INT_CAPTURE			(1 << 2)
+#define OMAP_TIMER_INT_OVERFLOW			(1 << 1)
+#define OMAP_TIMER_INT_MATCH			(1 << 0)
+
+/* trigger types */
+#define OMAP_TIMER_TRIGGER_NONE			0x00
+#define OMAP_TIMER_TRIGGER_OVERFLOW		0x01
+#define OMAP_TIMER_TRIGGER_OVERFLOW_AND_COMPARE	0x02
+
+struct omap_dm_timer;
+struct clk;
+
+int omap_dm_timer_init(void);
+
+struct omap_dm_timer *omap_dm_timer_request(void);
+struct omap_dm_timer *omap_dm_timer_request_specific(int timer_id);
+void omap_dm_timer_free(struct omap_dm_timer *timer);
+void omap_dm_timer_enable(struct omap_dm_timer *timer);
+void omap_dm_timer_disable(struct omap_dm_timer *timer);
+
+int omap_dm_timer_get_irq(struct omap_dm_timer *timer);
+
+u32 omap_dm_timer_modify_idlect_mask(u32 inputmask);
+struct clk *omap_dm_timer_get_fclk(struct omap_dm_timer *timer);
+
+void omap_dm_timer_trigger(struct omap_dm_timer *timer);
+void omap_dm_timer_start(struct omap_dm_timer *timer);
+void omap_dm_timer_stop(struct omap_dm_timer *timer);
+
+int omap_dm_timer_set_source(struct omap_dm_timer *timer, int source);
+void omap_dm_timer_set_load(struct omap_dm_timer *timer, int autoreload, unsigned int value);
+void omap_dm_timer_set_load_start(struct omap_dm_timer *timer, int autoreload, unsigned int value);
+void omap_dm_timer_set_match(struct omap_dm_timer *timer, int enable, unsigned int match);
+void omap_dm_timer_set_pwm(struct omap_dm_timer *timer, int def_on, int toggle, int trigger);
+void omap_dm_timer_set_prescaler(struct omap_dm_timer *timer, int prescaler);
+
+void omap_dm_timer_set_int_enable(struct omap_dm_timer *timer, unsigned int value);
+
+unsigned int omap_dm_timer_read_status(struct omap_dm_timer *timer);
+void omap_dm_timer_write_status(struct omap_dm_timer *timer, unsigned int value);
+unsigned int omap_dm_timer_read_counter(struct omap_dm_timer *timer);
+void omap_dm_timer_write_counter(struct omap_dm_timer *timer, unsigned int value);
+
+int omap_dm_timers_active(void);
+
+
+#endif /* __ASM_ARCH_DMTIMER_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/dsp_common.h
@@ -0,0 +1,40 @@
+/*
+ * This file is part of OMAP DSP driver (DSP Gateway version 3.3.1)
+ *
+ * Copyright (C) 2004-2006 Nokia Corporation. All rights reserved.
+ *
+ * Contact: Toshihiro Kobayashi <toshihiro.kobayashi@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA
+ * 02110-1301 USA
+ *
+ */
+
+#ifndef ASM_ARCH_DSP_COMMON_H
+#define ASM_ARCH_DSP_COMMON_H
+
+#if defined(CONFIG_ARCH_OMAP1) && defined(CONFIG_OMAP_MMU_FWK)
+extern void omap_dsp_request_mpui(void);
+extern void omap_dsp_release_mpui(void);
+extern int omap_dsp_request_mem(void);
+extern int omap_dsp_release_mem(void);
+#else
+static inline int omap_dsp_request_mem(void)
+{
+	return 0;
+}
+#define omap_dsp_release_mem()	do {} while (0)
+#endif
+
+#endif /* ASM_ARCH_DSP_COMMON_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/fpga.h
@@ -0,0 +1,197 @@
+/*
+ * arch/arm/plat-omap/include/mach/fpga.h
+ *
+ * Interrupt handler for OMAP-1510 FPGA
+ *
+ * Copyright (C) 2001 RidgeRun, Inc.
+ * Author: Greg Lonnon <glonnon@ridgerun.com>
+ *
+ * Copyright (C) 2002 MontaVista Software, Inc.
+ *
+ * Separated FPGA interrupts from innovator1510.c and cleaned up for 2.6
+ * Copyright (C) 2004 Nokia Corporation by Tony Lindrgen <tony@atomide.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __ASM_ARCH_OMAP_FPGA_H
+#define __ASM_ARCH_OMAP_FPGA_H
+
+#if defined(CONFIG_MACH_OMAP_INNOVATOR) && defined(CONFIG_ARCH_OMAP15XX)
+extern void omap1510_fpga_init_irq(void);
+#else
+#define omap1510_fpga_init_irq()	(0)
+#endif
+
+#define fpga_read(reg)			__raw_readb(reg)
+#define fpga_write(val, reg)		__raw_writeb(val, reg)
+
+/*
+ * ---------------------------------------------------------------------------
+ *  H2/P2 Debug board FPGA
+ * ---------------------------------------------------------------------------
+ */
+/* maps in the FPGA registers and the ETHR registers */
+#define H2P2_DBG_FPGA_BASE		IOMEM(0xE8000000)	/* VA */
+#define H2P2_DBG_FPGA_SIZE		SZ_4K			/* SIZE */
+#define H2P2_DBG_FPGA_START		0x04000000		/* PA */
+
+#define H2P2_DBG_FPGA_ETHR_START	(H2P2_DBG_FPGA_START + 0x300)
+#define H2P2_DBG_FPGA_FPGA_REV		(H2P2_DBG_FPGA_BASE + 0x10)	/* FPGA Revision */
+#define H2P2_DBG_FPGA_BOARD_REV		(H2P2_DBG_FPGA_BASE + 0x12)	/* Board Revision */
+#define H2P2_DBG_FPGA_GPIO		(H2P2_DBG_FPGA_BASE + 0x14)	/* GPIO outputs */
+#define H2P2_DBG_FPGA_LEDS		(H2P2_DBG_FPGA_BASE + 0x16)	/* LEDs outputs */
+#define H2P2_DBG_FPGA_MISC_INPUTS	(H2P2_DBG_FPGA_BASE + 0x18)	/* Misc inputs */
+#define H2P2_DBG_FPGA_LAN_STATUS	(H2P2_DBG_FPGA_BASE + 0x1A)	/* LAN Status line */
+#define H2P2_DBG_FPGA_LAN_RESET		(H2P2_DBG_FPGA_BASE + 0x1C)	/* LAN Reset line */
+
+/* NOTE:  most boards don't have a static mapping for the FPGA ... */
+struct h2p2_dbg_fpga {
+	/* offset 0x00 */
+	u16		smc91x[8];
+	/* offset 0x10 */
+	u16		fpga_rev;
+	u16		board_rev;
+	u16		gpio_outputs;
+	u16		leds;
+	/* offset 0x18 */
+	u16		misc_inputs;
+	u16		lan_status;
+	u16		lan_reset;
+	u16		reserved0;
+	/* offset 0x20 */
+	u16		ps2_data;
+	u16		ps2_ctrl;
+	/* plus also 4 rs232 ports ... */
+};
+
+/* LEDs definition on debug board (16 LEDs, all physically green) */
+#define H2P2_DBG_FPGA_LED_GREEN		(1 << 15)
+#define H2P2_DBG_FPGA_LED_AMBER		(1 << 14)
+#define H2P2_DBG_FPGA_LED_RED		(1 << 13)
+#define H2P2_DBG_FPGA_LED_BLUE		(1 << 12)
+/*  cpu0 load-meter LEDs */
+#define H2P2_DBG_FPGA_LOAD_METER	(1 << 0)	// A bit of fun on our board ...
+#define H2P2_DBG_FPGA_LOAD_METER_SIZE	11
+#define H2P2_DBG_FPGA_LOAD_METER_MASK	((1 << H2P2_DBG_FPGA_LOAD_METER_SIZE) - 1)
+
+#define H2P2_DBG_FPGA_P2_LED_TIMER		(1 << 0)
+#define H2P2_DBG_FPGA_P2_LED_IDLE		(1 << 1)
+
+/*
+ * ---------------------------------------------------------------------------
+ *  OMAP-1510 FPGA
+ * ---------------------------------------------------------------------------
+ */
+#define OMAP1510_FPGA_BASE		IOMEM(0xE8000000)	/* VA */
+#define OMAP1510_FPGA_SIZE		SZ_4K
+#define OMAP1510_FPGA_START		0x08000000		/* PA */
+
+/* Revision */
+#define OMAP1510_FPGA_REV_LOW			(OMAP1510_FPGA_BASE + 0x0)
+#define OMAP1510_FPGA_REV_HIGH			(OMAP1510_FPGA_BASE + 0x1)
+
+#define OMAP1510_FPGA_LCD_PANEL_CONTROL		(OMAP1510_FPGA_BASE + 0x2)
+#define OMAP1510_FPGA_LED_DIGIT			(OMAP1510_FPGA_BASE + 0x3)
+#define INNOVATOR_FPGA_HID_SPI			(OMAP1510_FPGA_BASE + 0x4)
+#define OMAP1510_FPGA_POWER			(OMAP1510_FPGA_BASE + 0x5)
+
+/* Interrupt status */
+#define OMAP1510_FPGA_ISR_LO			(OMAP1510_FPGA_BASE + 0x6)
+#define OMAP1510_FPGA_ISR_HI			(OMAP1510_FPGA_BASE + 0x7)
+
+/* Interrupt mask */
+#define OMAP1510_FPGA_IMR_LO			(OMAP1510_FPGA_BASE + 0x8)
+#define OMAP1510_FPGA_IMR_HI			(OMAP1510_FPGA_BASE + 0x9)
+
+/* Reset registers */
+#define OMAP1510_FPGA_HOST_RESET		(OMAP1510_FPGA_BASE + 0xa)
+#define OMAP1510_FPGA_RST			(OMAP1510_FPGA_BASE + 0xb)
+
+#define OMAP1510_FPGA_AUDIO			(OMAP1510_FPGA_BASE + 0xc)
+#define OMAP1510_FPGA_DIP			(OMAP1510_FPGA_BASE + 0xe)
+#define OMAP1510_FPGA_FPGA_IO			(OMAP1510_FPGA_BASE + 0xf)
+#define OMAP1510_FPGA_UART1			(OMAP1510_FPGA_BASE + 0x14)
+#define OMAP1510_FPGA_UART2			(OMAP1510_FPGA_BASE + 0x15)
+#define OMAP1510_FPGA_OMAP1510_STATUS		(OMAP1510_FPGA_BASE + 0x16)
+#define OMAP1510_FPGA_BOARD_REV			(OMAP1510_FPGA_BASE + 0x18)
+#define OMAP1510P1_PPT_DATA			(OMAP1510_FPGA_BASE + 0x100)
+#define OMAP1510P1_PPT_STATUS			(OMAP1510_FPGA_BASE + 0x101)
+#define OMAP1510P1_PPT_CONTROL			(OMAP1510_FPGA_BASE + 0x102)
+
+#define OMAP1510_FPGA_TOUCHSCREEN		(OMAP1510_FPGA_BASE + 0x204)
+
+#define INNOVATOR_FPGA_INFO			(OMAP1510_FPGA_BASE + 0x205)
+#define INNOVATOR_FPGA_LCD_BRIGHT_LO		(OMAP1510_FPGA_BASE + 0x206)
+#define INNOVATOR_FPGA_LCD_BRIGHT_HI		(OMAP1510_FPGA_BASE + 0x207)
+#define INNOVATOR_FPGA_LED_GRN_LO		(OMAP1510_FPGA_BASE + 0x208)
+#define INNOVATOR_FPGA_LED_GRN_HI		(OMAP1510_FPGA_BASE + 0x209)
+#define INNOVATOR_FPGA_LED_RED_LO		(OMAP1510_FPGA_BASE + 0x20a)
+#define INNOVATOR_FPGA_LED_RED_HI		(OMAP1510_FPGA_BASE + 0x20b)
+#define INNOVATOR_FPGA_CAM_USB_CONTROL		(OMAP1510_FPGA_BASE + 0x20c)
+#define INNOVATOR_FPGA_EXP_CONTROL		(OMAP1510_FPGA_BASE + 0x20d)
+#define INNOVATOR_FPGA_ISR2			(OMAP1510_FPGA_BASE + 0x20e)
+#define INNOVATOR_FPGA_IMR2			(OMAP1510_FPGA_BASE + 0x210)
+
+#define OMAP1510_FPGA_ETHR_START		(OMAP1510_FPGA_START + 0x300)
+
+/*
+ * Power up Giga UART driver, turn on HID clock.
+ * Turn off BT power, since we're not using it and it
+ * draws power.
+ */
+#define OMAP1510_FPGA_RESET_VALUE		0x42
+
+#define OMAP1510_FPGA_PCR_IF_PD0		(1 << 7)
+#define OMAP1510_FPGA_PCR_COM2_EN		(1 << 6)
+#define OMAP1510_FPGA_PCR_COM1_EN		(1 << 5)
+#define OMAP1510_FPGA_PCR_EXP_PD0		(1 << 4)
+#define OMAP1510_FPGA_PCR_EXP_PD1		(1 << 3)
+#define OMAP1510_FPGA_PCR_48MHZ_CLK		(1 << 2)
+#define OMAP1510_FPGA_PCR_4MHZ_CLK		(1 << 1)
+#define OMAP1510_FPGA_PCR_RSRVD_BIT0		(1 << 0)
+
+/*
+ * Innovator/OMAP1510 FPGA HID register bit definitions
+ */
+#define OMAP1510_FPGA_HID_SCLK	(1<<0)	/* output */
+#define OMAP1510_FPGA_HID_MOSI	(1<<1)	/* output */
+#define OMAP1510_FPGA_HID_nSS	(1<<2)	/* output 0/1 chip idle/select */
+#define OMAP1510_FPGA_HID_nHSUS	(1<<3)	/* output 0/1 host active/suspended */
+#define OMAP1510_FPGA_HID_MISO	(1<<4)	/* input */
+#define OMAP1510_FPGA_HID_ATN	(1<<5)	/* input  0/1 chip idle/ATN */
+#define OMAP1510_FPGA_HID_rsrvd	(1<<6)
+#define OMAP1510_FPGA_HID_RESETn (1<<7)	/* output - 0/1 USAR reset/run */
+
+/* The FPGA IRQ is cascaded through GPIO_13 */
+#define OMAP1510_INT_FPGA		(IH_GPIO_BASE + 13)
+
+/* IRQ Numbers for interrupts muxed through the FPGA */
+#define OMAP1510_INT_FPGA_ATN		(OMAP_FPGA_IRQ_BASE + 0)
+#define OMAP1510_INT_FPGA_ACK		(OMAP_FPGA_IRQ_BASE + 1)
+#define OMAP1510_INT_FPGA2		(OMAP_FPGA_IRQ_BASE + 2)
+#define OMAP1510_INT_FPGA3		(OMAP_FPGA_IRQ_BASE + 3)
+#define OMAP1510_INT_FPGA4		(OMAP_FPGA_IRQ_BASE + 4)
+#define OMAP1510_INT_FPGA5		(OMAP_FPGA_IRQ_BASE + 5)
+#define OMAP1510_INT_FPGA6		(OMAP_FPGA_IRQ_BASE + 6)
+#define OMAP1510_INT_FPGA7		(OMAP_FPGA_IRQ_BASE + 7)
+#define OMAP1510_INT_FPGA8		(OMAP_FPGA_IRQ_BASE + 8)
+#define OMAP1510_INT_FPGA9		(OMAP_FPGA_IRQ_BASE + 9)
+#define OMAP1510_INT_FPGA10		(OMAP_FPGA_IRQ_BASE + 10)
+#define OMAP1510_INT_FPGA11		(OMAP_FPGA_IRQ_BASE + 11)
+#define OMAP1510_INT_FPGA12		(OMAP_FPGA_IRQ_BASE + 12)
+#define OMAP1510_INT_ETHER		(OMAP_FPGA_IRQ_BASE + 13)
+#define OMAP1510_INT_FPGAUART1		(OMAP_FPGA_IRQ_BASE + 14)
+#define OMAP1510_INT_FPGAUART2		(OMAP_FPGA_IRQ_BASE + 15)
+#define OMAP1510_INT_FPGA_TS		(OMAP_FPGA_IRQ_BASE + 16)
+#define OMAP1510_INT_FPGA17		(OMAP_FPGA_IRQ_BASE + 17)
+#define OMAP1510_INT_FPGA_CAM		(OMAP_FPGA_IRQ_BASE + 18)
+#define OMAP1510_INT_FPGA_RTC_A		(OMAP_FPGA_IRQ_BASE + 19)
+#define OMAP1510_INT_FPGA_RTC_B		(OMAP_FPGA_IRQ_BASE + 20)
+#define OMAP1510_INT_FPGA_CD		(OMAP_FPGA_IRQ_BASE + 21)
+#define OMAP1510_INT_FPGA22		(OMAP_FPGA_IRQ_BASE + 22)
+#define OMAP1510_INT_FPGA23		(OMAP_FPGA_IRQ_BASE + 23)
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/gpio.h
@@ -0,0 +1,129 @@
+/*
+ * arch/arm/plat-omap/include/mach/gpio.h
+ *
+ * OMAP GPIO handling defines and functions
+ *
+ * Copyright (C) 2003-2005 Nokia Corporation
+ *
+ * Written by Juha YrjÃ¶lÃ¤ <juha.yrjola@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
+ *
+ */
+
+#ifndef __ASM_ARCH_OMAP_GPIO_H
+#define __ASM_ARCH_OMAP_GPIO_H
+
+#include <linux/io.h>
+#include <mach/irqs.h>
+
+#define OMAP1_MPUIO_BASE			0xfffb5000
+
+#if (defined(CONFIG_ARCH_OMAP730) || defined(CONFIG_ARCH_OMAP850))
+
+#define OMAP_MPUIO_INPUT_LATCH		0x00
+#define OMAP_MPUIO_OUTPUT		0x02
+#define OMAP_MPUIO_IO_CNTL		0x04
+#define OMAP_MPUIO_KBR_LATCH		0x08
+#define OMAP_MPUIO_KBC			0x0a
+#define OMAP_MPUIO_GPIO_EVENT_MODE	0x0c
+#define OMAP_MPUIO_GPIO_INT_EDGE	0x0e
+#define OMAP_MPUIO_KBD_INT		0x10
+#define OMAP_MPUIO_GPIO_INT		0x12
+#define OMAP_MPUIO_KBD_MASKIT		0x14
+#define OMAP_MPUIO_GPIO_MASKIT		0x16
+#define OMAP_MPUIO_GPIO_DEBOUNCING	0x18
+#define OMAP_MPUIO_LATCH		0x1a
+#else
+#define OMAP_MPUIO_INPUT_LATCH		0x00
+#define OMAP_MPUIO_OUTPUT		0x04
+#define OMAP_MPUIO_IO_CNTL		0x08
+#define OMAP_MPUIO_KBR_LATCH		0x10
+#define OMAP_MPUIO_KBC			0x14
+#define OMAP_MPUIO_GPIO_EVENT_MODE	0x18
+#define OMAP_MPUIO_GPIO_INT_EDGE	0x1c
+#define OMAP_MPUIO_KBD_INT		0x20
+#define OMAP_MPUIO_GPIO_INT		0x24
+#define OMAP_MPUIO_KBD_MASKIT		0x28
+#define OMAP_MPUIO_GPIO_MASKIT		0x2c
+#define OMAP_MPUIO_GPIO_DEBOUNCING	0x30
+#define OMAP_MPUIO_LATCH		0x34
+#endif
+
+#define OMAP34XX_NR_GPIOS		6
+
+#define OMAP_MPUIO(nr)		(OMAP_MAX_GPIO_LINES + (nr))
+#define OMAP_GPIO_IS_MPUIO(nr)	((nr) >= OMAP_MAX_GPIO_LINES)
+
+#define OMAP_GPIO_IRQ(nr)	(OMAP_GPIO_IS_MPUIO(nr) ? \
+				 IH_MPUIO_BASE + ((nr) & 0x0f) : \
+				 IH_GPIO_BASE + (nr))
+
+extern int omap_gpio_init(void);	/* Call from board init only */
+extern void omap2_gpio_prepare_for_retention(void);
+extern void omap2_gpio_resume_after_retention(void);
+extern void omap_set_gpio_debounce(int gpio, int enable);
+extern void omap_set_gpio_debounce_time(int gpio, int enable);
+extern void omap_gpio_save_context(void);
+extern void omap_gpio_restore_context(void);
+/*-------------------------------------------------------------------------*/
+
+/* Wrappers for "new style" GPIO calls, using the new infrastructure
+ * which lets us plug in FPGA, I2C, and other implementations.
+ * *
+ * The original OMAP-specfic calls should eventually be removed.
+ */
+
+#include <linux/errno.h>
+#include <asm-generic/gpio.h>
+
+static inline int gpio_get_value(unsigned gpio)
+{
+	return __gpio_get_value(gpio);
+}
+
+static inline void gpio_set_value(unsigned gpio, int value)
+{
+	__gpio_set_value(gpio, value);
+}
+
+static inline int gpio_cansleep(unsigned gpio)
+{
+	return __gpio_cansleep(gpio);
+}
+
+static inline int gpio_to_irq(unsigned gpio)
+{
+	return __gpio_to_irq(gpio);
+}
+
+static inline int irq_to_gpio(unsigned irq)
+{
+	int tmp;
+
+	/* omap1 SOC mpuio */
+	if (cpu_class_is_omap1() && (irq < (IH_MPUIO_BASE + 16)))
+		return (irq - IH_MPUIO_BASE) + OMAP_MAX_GPIO_LINES;
+
+	/* SOC gpio */
+	tmp = irq - IH_GPIO_BASE;
+	if (tmp < OMAP_MAX_GPIO_LINES)
+		return tmp;
+
+	/* we don't supply reverse mappings for non-SOC gpios */
+	return -EIO;
+}
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/gpio-switch.h
@@ -0,0 +1,54 @@
+/*
+ * GPIO switch definitions
+ *
+ * Copyright (C) 2006 Nokia Corporation
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __ASM_ARCH_OMAP_GPIO_SWITCH_H
+#define __ASM_ARCH_OMAP_GPIO_SWITCH_H
+
+#include <linux/types.h>
+
+/* Cover:
+ *	high -> closed
+ *	low  -> open
+ * Connection:
+ *	high -> connected
+ *	low  -> disconnected
+ * Activity:
+ *	high -> active
+ *	low  -> inactive
+ *
+ */
+#define OMAP_GPIO_SWITCH_TYPE_COVER		0x0000
+#define OMAP_GPIO_SWITCH_TYPE_CONNECTION	0x0001
+#define OMAP_GPIO_SWITCH_TYPE_ACTIVITY		0x0002
+#define OMAP_GPIO_SWITCH_FLAG_INVERTED		0x0001
+#define OMAP_GPIO_SWITCH_FLAG_OUTPUT		0x0002
+
+struct omap_gpio_switch {
+	const char *name;
+	s16 gpio;
+	unsigned flags:4;
+	unsigned type:4;
+
+	/* Time in ms to debounce when transitioning from
+	 * inactive state to active state. */
+	u16 debounce_rising;
+	/* Same for transition from active to inactive state. */
+	u16 debounce_falling;
+
+	/* notify board-specific code about state changes */
+	void (* notify)(void *data, int state);
+	void *notify_data;
+};
+
+/* Call at init time only */
+extern void omap_register_gpio_switches(const struct omap_gpio_switch *tbl,
+					int count);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/gpmc.h
@@ -0,0 +1,115 @@
+/*
+ * General-Purpose Memory Controller for OMAP2
+ *
+ * Copyright (C) 2005-2006 Nokia Corporation
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __OMAP2_GPMC_H
+#define __OMAP2_GPMC_H
+
+/* Maximum Number of Chip Selects */
+#define GPMC_CS_NUM		8
+
+#define GPMC_CS_CONFIG1		0x00
+#define GPMC_CS_CONFIG2		0x04
+#define GPMC_CS_CONFIG3		0x08
+#define GPMC_CS_CONFIG4		0x0c
+#define GPMC_CS_CONFIG5		0x10
+#define GPMC_CS_CONFIG6		0x14
+#define GPMC_CS_CONFIG7		0x18
+#define GPMC_CS_NAND_COMMAND	0x1c
+#define GPMC_CS_NAND_ADDRESS	0x20
+#define GPMC_CS_NAND_DATA	0x24
+
+#define GPMC_CONFIG		0x50
+#define GPMC_STATUS		0x54
+
+#define GPMC_CONFIG1_WRAPBURST_SUPP     (1 << 31)
+#define GPMC_CONFIG1_READMULTIPLE_SUPP  (1 << 30)
+#define GPMC_CONFIG1_READTYPE_ASYNC     (0 << 29)
+#define GPMC_CONFIG1_READTYPE_SYNC      (1 << 29)
+#define GPMC_CONFIG1_WRITEMULTIPLE_SUPP (1 << 28)
+#define GPMC_CONFIG1_WRITETYPE_ASYNC    (0 << 27)
+#define GPMC_CONFIG1_WRITETYPE_SYNC     (1 << 27)
+#define GPMC_CONFIG1_CLKACTIVATIONTIME(val) ((val & 3) << 25)
+#define GPMC_CONFIG1_PAGE_LEN(val)      ((val & 3) << 23)
+#define GPMC_CONFIG1_WAIT_READ_MON      (1 << 22)
+#define GPMC_CONFIG1_WAIT_WRITE_MON     (1 << 21)
+#define GPMC_CONFIG1_WAIT_MON_IIME(val) ((val & 3) << 18)
+#define GPMC_CONFIG1_WAIT_PIN_SEL(val)  ((val & 3) << 16)
+#define GPMC_CONFIG1_DEVICESIZE(val)    ((val & 3) << 12)
+#define GPMC_CONFIG1_DEVICESIZE_16      GPMC_CONFIG1_DEVICESIZE(1)
+#define GPMC_CONFIG1_DEVICETYPE(val)    ((val & 3) << 10)
+#define GPMC_CONFIG1_DEVICETYPE_NOR     GPMC_CONFIG1_DEVICETYPE(0)
+#define GPMC_CONFIG1_DEVICETYPE_NAND    GPMC_CONFIG1_DEVICETYPE(2)
+#define GPMC_CONFIG1_MUXADDDATA         (1 << 9)
+#define GPMC_CONFIG1_TIME_PARA_GRAN     (1 << 4)
+#define GPMC_CONFIG1_FCLK_DIV(val)      (val & 3)
+#define GPMC_CONFIG1_FCLK_DIV2          (GPMC_CONFIG1_FCLK_DIV(1))
+#define GPMC_CONFIG1_FCLK_DIV3          (GPMC_CONFIG1_FCLK_DIV(2))
+#define GPMC_CONFIG1_FCLK_DIV4          (GPMC_CONFIG1_FCLK_DIV(3))
+#define GPMC_CONFIG7_CSVALID		(1 << 6)
+
+/*
+ * Note that all values in this struct are in nanoseconds, while
+ * the register values are in gpmc_fck cycles.
+ */
+struct gpmc_timings {
+	/* Minimum clock period for synchronous mode */
+	u16 sync_clk;
+
+	/* Chip-select signal timings corresponding to GPMC_CS_CONFIG2 */
+	u16 cs_on;		/* Assertion time */
+	u16 cs_rd_off;		/* Read deassertion time */
+	u16 cs_wr_off;		/* Write deassertion time */
+
+	/* ADV signal timings corresponding to GPMC_CONFIG3 */
+	u16 adv_on;		/* Assertion time */
+	u16 adv_rd_off;		/* Read deassertion time */
+	u16 adv_wr_off;		/* Write deassertion time */
+
+	/* WE signals timings corresponding to GPMC_CONFIG4 */
+	u16 we_on;		/* WE assertion time */
+	u16 we_off;		/* WE deassertion time */
+
+	/* OE signals timings corresponding to GPMC_CONFIG4 */
+	u16 oe_on;		/* OE assertion time */
+	u16 oe_off;		/* OE deassertion time */
+
+	/* Access time and cycle time timings corresponding to GPMC_CONFIG5 */
+	u16 page_burst_access;	/* Multiple access word delay */
+	u16 access;		/* Start-cycle to first data valid delay */
+	u16 rd_cycle;		/* Total read cycle time */
+	u16 wr_cycle;		/* Total write cycle time */
+
+	/* The following are only on OMAP3430 */
+	u16 wr_access;		/* WRACCESSTIME */
+	u16 wr_data_mux_bus;	/* WRDATAONADMUXBUS */
+};
+
+extern unsigned int gpmc_ns_to_ticks(unsigned int time_ns);
+extern unsigned int gpmc_ticks_to_ns(unsigned int ticks);
+extern unsigned int gpmc_round_ns_to_ticks(unsigned int time_ns);
+extern unsigned long gpmc_get_fclk_period(void);
+
+extern void gpmc_cs_write_reg(int cs, int idx, u32 val);
+extern u32 gpmc_cs_read_reg(int cs, int idx);
+extern int gpmc_cs_calc_divider(int cs, unsigned int sync_clk);
+extern int gpmc_cs_set_timings(int cs, const struct gpmc_timings *t);
+extern int gpmc_cs_request(int cs, unsigned long size, unsigned long *base);
+extern void gpmc_cs_free(int cs);
+extern int gpmc_cs_set_reserved(int cs, int reserved);
+extern int gpmc_cs_reserved(int cs);
+extern int gpmc_prefetch_enable(int cs, int dma_mode,
+					unsigned int u32_count, int is_write);
+extern void gpmc_prefetch_reset(void);
+extern int gpmc_prefetch_status(void);
+extern void omap3_gpmc_save_context(void);
+extern void omap3_gpmc_restore_context(void);
+extern void __init gpmc_init(void);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/gpmc-smc91x.h
@@ -0,0 +1,42 @@
+/*
+ * arch/arm/plat-omap/include/mach/gpmc-smc91x.h
+ *
+ * Copyright (C) 2009 Nokia Corporation
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __ASM_ARCH_OMAP_GPMC_SMC91X_H__
+
+#define GPMC_TIMINGS_SMC91C96	(1 << 4)
+#define GPMC_MUX_ADD_DATA	(1 << 5) /* GPMC_CONFIG1_MUXADDDATA */
+#define GPMC_READ_MON		(1 << 6) /* GPMC_CONFIG1_WAIT_READ_MON */
+#define GPMC_WRITE_MON		(1 << 7) /* GPMC_CONFIG1_WAIT_WRITE_MON */
+
+struct omap_smc91x_platform_data {
+	int	cs;
+	int	gpio_irq;
+	int	gpio_pwrdwn;
+	int	gpio_reset;
+	int	wait_pin;	/* Optional GPMC_CONFIG1_WAITPINSELECT */
+	u32	flags;
+	int	(*retime)(void);
+};
+
+#if defined(CONFIG_SMC91X) || \
+	defined(CONFIG_SMC91X_MODULE)
+
+extern void gpmc_smc91x_init(struct omap_smc91x_platform_data *d);
+
+#else
+
+#define board_smc91x_data	NULL
+
+static inline void gpmc_smc91x_init(struct omap_smc91x_platform_data *d)
+{
+}
+
+#endif
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/hardware.h
@@ -0,0 +1,290 @@
+/*
+ * arch/arm/plat-omap/include/mach/hardware.h
+ *
+ * Hardware definitions for TI OMAP processors and boards
+ *
+ * NOTE: Please put device driver specific defines into a separate header
+ *	 file for each driver.
+ *
+ * Copyright (C) 2001 RidgeRun, Inc.
+ * Author: RidgeRun, Inc. Greg Lonnon <glonnon@ridgerun.com>
+ *
+ * Reorganized for Linux-2.6 by Tony Lindgren <tony@atomide.com>
+ *                          and Dirk Behme <dirk.behme@de.bosch.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_OMAP_HARDWARE_H
+#define __ASM_ARCH_OMAP_HARDWARE_H
+
+#include <asm/sizes.h>
+#ifndef __ASSEMBLER__
+#include <asm/types.h>
+#include <plat/cpu.h>
+#endif
+#include <plat/serial.h>
+
+/*
+ * ---------------------------------------------------------------------------
+ * Common definitions for all OMAP processors
+ * NOTE: Put all processor or board specific parts to the special header
+ *	 files.
+ * ---------------------------------------------------------------------------
+ */
+
+/*
+ * ----------------------------------------------------------------------------
+ * Timers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP_MPU_TIMER1_BASE	(0xfffec500)
+#define OMAP_MPU_TIMER2_BASE	(0xfffec600)
+#define OMAP_MPU_TIMER3_BASE	(0xfffec700)
+#define MPU_TIMER_FREE		(1 << 6)
+#define MPU_TIMER_CLOCK_ENABLE	(1 << 5)
+#define MPU_TIMER_AR		(1 << 1)
+#define MPU_TIMER_ST		(1 << 0)
+
+/*
+ * ----------------------------------------------------------------------------
+ * Clocks
+ * ----------------------------------------------------------------------------
+ */
+#define CLKGEN_REG_BASE		(0xfffece00)
+#define ARM_CKCTL		(CLKGEN_REG_BASE + 0x0)
+#define ARM_IDLECT1		(CLKGEN_REG_BASE + 0x4)
+#define ARM_IDLECT2		(CLKGEN_REG_BASE + 0x8)
+#define ARM_EWUPCT		(CLKGEN_REG_BASE + 0xC)
+#define ARM_RSTCT1		(CLKGEN_REG_BASE + 0x10)
+#define ARM_RSTCT2		(CLKGEN_REG_BASE + 0x14)
+#define ARM_SYSST		(CLKGEN_REG_BASE + 0x18)
+#define ARM_IDLECT3		(CLKGEN_REG_BASE + 0x24)
+
+#define CK_RATEF		1
+#define CK_IDLEF		2
+#define CK_ENABLEF		4
+#define CK_SELECTF		8
+#define SETARM_IDLE_SHIFT
+
+/* DPLL control registers */
+#define DPLL_CTL		(0xfffecf00)
+
+/* DSP clock control. Must use __raw_readw() and __raw_writew() with these */
+#define DSP_CONFIG_REG_BASE     IOMEM(0xe1008000)
+#define DSP_CKCTL		(DSP_CONFIG_REG_BASE + 0x0)
+#define DSP_IDLECT1		(DSP_CONFIG_REG_BASE + 0x4)
+#define DSP_IDLECT2		(DSP_CONFIG_REG_BASE + 0x8)
+#define DSP_RSTCT2		(DSP_CONFIG_REG_BASE + 0x14)
+
+/*
+ * ---------------------------------------------------------------------------
+ * UPLD
+ * ---------------------------------------------------------------------------
+ */
+#define ULPD_REG_BASE		(0xfffe0800)
+#define ULPD_IT_STATUS		(ULPD_REG_BASE + 0x14)
+#define ULPD_SETUP_ANALOG_CELL_3	(ULPD_REG_BASE + 0x24)
+#define ULPD_CLOCK_CTRL		(ULPD_REG_BASE + 0x30)
+#	define DIS_USB_PVCI_CLK		(1 << 5)	/* no USB/FAC synch */
+#	define USB_MCLK_EN		(1 << 4)	/* enable W4_USB_CLKO */
+#define ULPD_SOFT_REQ		(ULPD_REG_BASE + 0x34)
+#	define SOFT_UDC_REQ		(1 << 4)
+#	define SOFT_USB_CLK_REQ		(1 << 3)
+#	define SOFT_DPLL_REQ		(1 << 0)
+#define ULPD_DPLL_CTRL		(ULPD_REG_BASE + 0x3c)
+#define ULPD_STATUS_REQ		(ULPD_REG_BASE + 0x40)
+#define ULPD_APLL_CTRL		(ULPD_REG_BASE + 0x4c)
+#define ULPD_POWER_CTRL		(ULPD_REG_BASE + 0x50)
+#define ULPD_SOFT_DISABLE_REQ_REG	(ULPD_REG_BASE + 0x68)
+#	define DIS_MMC2_DPLL_REQ	(1 << 11)
+#	define DIS_MMC1_DPLL_REQ	(1 << 10)
+#	define DIS_UART3_DPLL_REQ	(1 << 9)
+#	define DIS_UART2_DPLL_REQ	(1 << 8)
+#	define DIS_UART1_DPLL_REQ	(1 << 7)
+#	define DIS_USB_HOST_DPLL_REQ	(1 << 6)
+#define ULPD_SDW_CLK_DIV_CTRL_SEL	(ULPD_REG_BASE + 0x74)
+#define ULPD_CAM_CLK_CTRL	(ULPD_REG_BASE + 0x7c)
+
+/*
+ * ---------------------------------------------------------------------------
+ * Watchdog timer
+ * ---------------------------------------------------------------------------
+ */
+
+/* Watchdog timer within the OMAP3.2 gigacell */
+#define OMAP_MPU_WATCHDOG_BASE	(0xfffec800)
+#define OMAP_WDT_TIMER		(OMAP_MPU_WATCHDOG_BASE + 0x0)
+#define OMAP_WDT_LOAD_TIM	(OMAP_MPU_WATCHDOG_BASE + 0x4)
+#define OMAP_WDT_READ_TIM	(OMAP_MPU_WATCHDOG_BASE + 0x4)
+#define OMAP_WDT_TIMER_MODE	(OMAP_MPU_WATCHDOG_BASE + 0x8)
+
+/*
+ * ---------------------------------------------------------------------------
+ * Interrupts
+ * ---------------------------------------------------------------------------
+ */
+#ifdef CONFIG_ARCH_OMAP1
+
+/*
+ * XXX: These probably want to be moved to arch/arm/mach-omap/omap1/irq.c
+ * or something similar.. -- PFM.
+ */
+
+#define OMAP_IH1_BASE		0xfffecb00
+#define OMAP_IH2_BASE		0xfffe0000
+
+#define OMAP_IH1_ITR		(OMAP_IH1_BASE + 0x00)
+#define OMAP_IH1_MIR		(OMAP_IH1_BASE + 0x04)
+#define OMAP_IH1_SIR_IRQ	(OMAP_IH1_BASE + 0x10)
+#define OMAP_IH1_SIR_FIQ	(OMAP_IH1_BASE + 0x14)
+#define OMAP_IH1_CONTROL	(OMAP_IH1_BASE + 0x18)
+#define OMAP_IH1_ILR0		(OMAP_IH1_BASE + 0x1c)
+#define OMAP_IH1_ISR		(OMAP_IH1_BASE + 0x9c)
+
+#define OMAP_IH2_ITR		(OMAP_IH2_BASE + 0x00)
+#define OMAP_IH2_MIR		(OMAP_IH2_BASE + 0x04)
+#define OMAP_IH2_SIR_IRQ	(OMAP_IH2_BASE + 0x10)
+#define OMAP_IH2_SIR_FIQ	(OMAP_IH2_BASE + 0x14)
+#define OMAP_IH2_CONTROL	(OMAP_IH2_BASE + 0x18)
+#define OMAP_IH2_ILR0		(OMAP_IH2_BASE + 0x1c)
+#define OMAP_IH2_ISR		(OMAP_IH2_BASE + 0x9c)
+
+#define IRQ_ITR_REG_OFFSET	0x00
+#define IRQ_MIR_REG_OFFSET	0x04
+#define IRQ_SIR_IRQ_REG_OFFSET	0x10
+#define IRQ_SIR_FIQ_REG_OFFSET	0x14
+#define IRQ_CONTROL_REG_OFFSET	0x18
+#define IRQ_ISR_REG_OFFSET	0x9c
+#define IRQ_ILR0_REG_OFFSET	0x1c
+#define IRQ_GMR_REG_OFFSET	0xa0
+
+#endif
+
+/*
+ * ----------------------------------------------------------------------------
+ * System control registers
+ * ----------------------------------------------------------------------------
+ */
+#define MOD_CONF_CTRL_0		0xfffe1080
+#define MOD_CONF_CTRL_1		0xfffe1110
+
+/*
+ * ----------------------------------------------------------------------------
+ * Pin multiplexing registers
+ * ----------------------------------------------------------------------------
+ */
+#define FUNC_MUX_CTRL_0		0xfffe1000
+#define FUNC_MUX_CTRL_1		0xfffe1004
+#define FUNC_MUX_CTRL_2		0xfffe1008
+#define COMP_MODE_CTRL_0	0xfffe100c
+#define FUNC_MUX_CTRL_3		0xfffe1010
+#define FUNC_MUX_CTRL_4		0xfffe1014
+#define FUNC_MUX_CTRL_5		0xfffe1018
+#define FUNC_MUX_CTRL_6		0xfffe101C
+#define FUNC_MUX_CTRL_7		0xfffe1020
+#define FUNC_MUX_CTRL_8		0xfffe1024
+#define FUNC_MUX_CTRL_9		0xfffe1028
+#define FUNC_MUX_CTRL_A		0xfffe102C
+#define FUNC_MUX_CTRL_B		0xfffe1030
+#define FUNC_MUX_CTRL_C		0xfffe1034
+#define FUNC_MUX_CTRL_D		0xfffe1038
+#define PULL_DWN_CTRL_0		0xfffe1040
+#define PULL_DWN_CTRL_1		0xfffe1044
+#define PULL_DWN_CTRL_2		0xfffe1048
+#define PULL_DWN_CTRL_3		0xfffe104c
+#define PULL_DWN_CTRL_4		0xfffe10ac
+
+/* OMAP-1610 specific multiplexing registers */
+#define FUNC_MUX_CTRL_E		0xfffe1090
+#define FUNC_MUX_CTRL_F		0xfffe1094
+#define FUNC_MUX_CTRL_10	0xfffe1098
+#define FUNC_MUX_CTRL_11	0xfffe109c
+#define FUNC_MUX_CTRL_12	0xfffe10a0
+#define PU_PD_SEL_0		0xfffe10b4
+#define PU_PD_SEL_1		0xfffe10b8
+#define PU_PD_SEL_2		0xfffe10bc
+#define PU_PD_SEL_3		0xfffe10c0
+#define PU_PD_SEL_4		0xfffe10c4
+
+/* Timer32K for 1610 and 1710*/
+#define OMAP_TIMER32K_BASE	0xFFFBC400
+
+/*
+ * ---------------------------------------------------------------------------
+ * TIPB bus interface
+ * ---------------------------------------------------------------------------
+ */
+#define TIPB_PUBLIC_CNTL_BASE		0xfffed300
+#define MPU_PUBLIC_TIPB_CNTL		(TIPB_PUBLIC_CNTL_BASE + 0x8)
+#define TIPB_PRIVATE_CNTL_BASE		0xfffeca00
+#define MPU_PRIVATE_TIPB_CNTL		(TIPB_PRIVATE_CNTL_BASE + 0x8)
+
+/*
+ * ----------------------------------------------------------------------------
+ * MPUI interface
+ * ----------------------------------------------------------------------------
+ */
+#define MPUI_BASE			(0xfffec900)
+#define MPUI_CTRL			(MPUI_BASE + 0x0)
+#define MPUI_DEBUG_ADDR			(MPUI_BASE + 0x4)
+#define MPUI_DEBUG_DATA			(MPUI_BASE + 0x8)
+#define MPUI_DEBUG_FLAG			(MPUI_BASE + 0xc)
+#define MPUI_STATUS_REG			(MPUI_BASE + 0x10)
+#define MPUI_DSP_STATUS			(MPUI_BASE + 0x14)
+#define MPUI_DSP_BOOT_CONFIG		(MPUI_BASE + 0x18)
+#define MPUI_DSP_API_CONFIG		(MPUI_BASE + 0x1c)
+
+/*
+ * ----------------------------------------------------------------------------
+ * LED Pulse Generator
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP_LPG1_BASE			0xfffbd000
+#define OMAP_LPG2_BASE			0xfffbd800
+#define OMAP_LPG1_LCR			(OMAP_LPG1_BASE + 0x00)
+#define OMAP_LPG1_PMR			(OMAP_LPG1_BASE + 0x04)
+#define OMAP_LPG2_LCR			(OMAP_LPG2_BASE + 0x00)
+#define OMAP_LPG2_PMR			(OMAP_LPG2_BASE + 0x04)
+
+/*
+ * ----------------------------------------------------------------------------
+ * Pulse-Width Light
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP_PWL_BASE			0xfffb5800
+#define OMAP_PWL_ENABLE			(OMAP_PWL_BASE + 0x00)
+#define OMAP_PWL_CLK_ENABLE		(OMAP_PWL_BASE + 0x04)
+
+/*
+ * ---------------------------------------------------------------------------
+ * Processor specific defines
+ * ---------------------------------------------------------------------------
+ */
+
+#include <plat/omap7xx.h>
+#include <plat/omap1510.h>
+#include <plat/omap16xx.h>
+#include <plat/omap24xx.h>
+#include <plat/omap34xx.h>
+#include <plat/omap44xx.h>
+
+#endif	/* __ASM_ARCH_OMAP_HARDWARE_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/hwa742.h
@@ -0,0 +1,8 @@
+#ifndef _HWA742_H
+#define _HWA742_H
+
+struct hwa742_platform_data {
+	unsigned	te_connected:1;
+};
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/i2c.h
@@ -0,0 +1,39 @@
+/*
+ * Helper module for board specific I2C bus registration
+ *
+ * Copyright (C) 2009 Nokia Corporation.
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA
+ * 02110-1301 USA
+ *
+ */
+
+#include <linux/i2c.h>
+
+#if defined(CONFIG_I2C_OMAP) || defined(CONFIG_I2C_OMAP_MODULE)
+extern int omap_register_i2c_bus(int bus_id, u32 clkrate,
+				 struct i2c_board_info const *info,
+				 unsigned len);
+#else
+static inline int omap_register_i2c_bus(int bus_id, u32 clkrate,
+				 struct i2c_board_info const *info,
+				 unsigned len)
+{
+	return 0;
+}
+#endif
+
+int omap_plat_register_i2c_bus(int bus_id, u32 clkrate,
+				 struct i2c_board_info const *info,
+				 unsigned len);
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/io.h
@@ -0,0 +1,287 @@
+/*
+ * arch/arm/plat-omap/include/mach/io.h
+ *
+ * IO definitions for TI OMAP processors and boards
+ *
+ * Copied from arch/arm/mach-sa1100/include/mach/io.h
+ * Copyright (C) 1997-1999 Russell King
+ *
+ * Copyright (C) 2009 Texas Instruments
+ * Added OMAP4 support - Santosh Shilimkar <santosh.shilimkar@ti.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ * Modifications:
+ *  06-12-1997	RMK	Created.
+ *  07-04-1999	RMK	Major cleanup
+ */
+
+#ifndef __ASM_ARM_ARCH_IO_H
+#define __ASM_ARM_ARCH_IO_H
+
+#include <mach/hardware.h>
+
+#define IO_SPACE_LIMIT 0xffffffff
+
+/*
+ * We don't actually have real ISA nor PCI buses, but there is so many
+ * drivers out there that might just work if we fake them...
+ */
+#define __io(a)		__typesafe_io(a)
+#define __mem_pci(a)	(a)
+
+/*
+ * ----------------------------------------------------------------------------
+ * I/O mapping
+ * ----------------------------------------------------------------------------
+ */
+
+#ifdef __ASSEMBLER__
+#define IOMEM(x)		(x)
+#else
+#define IOMEM(x)		((void __force __iomem *)(x))
+#endif
+
+#define OMAP1_IO_OFFSET		0x01000000	/* Virtual IO = 0xfefb0000 */
+#define OMAP1_IO_ADDRESS(pa)	IOMEM((pa) - OMAP1_IO_OFFSET)
+
+#define OMAP2_L3_IO_OFFSET	0x90000000
+#define OMAP2_L3_IO_ADDRESS(pa)	IOMEM((pa) + OMAP2_L3_IO_OFFSET) /* L3 */
+
+
+#define OMAP2_L4_IO_OFFSET	0xb2000000
+#define OMAP2_L4_IO_ADDRESS(pa)	IOMEM((pa) + OMAP2_L4_IO_OFFSET) /* L4 */
+
+#define OMAP4_L3_IO_OFFSET	0xb4000000
+#define OMAP4_L3_IO_ADDRESS(pa)	IOMEM((pa) + OMAP4_L3_IO_OFFSET) /* L3 */
+
+#define OMAP4_L3_PER_IO_OFFSET	0xb1100000
+#define OMAP4_L3_PER_IO_ADDRESS(pa)	IOMEM((pa) + OMAP4_L3_PER_IO_OFFSET)
+
+#define OMAP4_GPMC_IO_OFFSET		0xa9000000
+#define OMAP4_GPMC_IO_ADDRESS(pa)	IOMEM((pa) + OMAP4_GPMC_IO_OFFSET)
+
+#define OMAP2_EMU_IO_OFFSET		0xaa800000	/* Emulation */
+#define OMAP2_EMU_IO_ADDRESS(pa)	IOMEM((pa) + OMAP2_EMU_IO_OFFSET)
+
+/*
+ * ----------------------------------------------------------------------------
+ * Omap1 specific IO mapping
+ * ----------------------------------------------------------------------------
+ */
+
+#define OMAP1_IO_PHYS		0xFFFB0000
+#define OMAP1_IO_SIZE		0x40000
+#define OMAP1_IO_VIRT		(OMAP1_IO_PHYS - OMAP1_IO_OFFSET)
+
+/*
+ * ----------------------------------------------------------------------------
+ * Omap2 specific IO mapping
+ * ----------------------------------------------------------------------------
+ */
+
+/* We map both L3 and L4 on OMAP2 */
+#define L3_24XX_PHYS	L3_24XX_BASE	/* 0x68000000 --> 0xf8000000*/
+#define L3_24XX_VIRT	(L3_24XX_PHYS + OMAP2_L3_IO_OFFSET)
+#define L3_24XX_SIZE	SZ_1M		/* 44kB of 128MB used, want 1MB sect */
+#define L4_24XX_PHYS	L4_24XX_BASE	/* 0x48000000 --> 0xfa000000 */
+#define L4_24XX_VIRT	(L4_24XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_24XX_SIZE	SZ_1M		/* 1MB of 128MB used, want 1MB sect */
+
+#define L4_WK_243X_PHYS		L4_WK_243X_BASE	/* 0x49000000 --> 0xfb000000 */
+#define L4_WK_243X_VIRT		(L4_WK_243X_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_WK_243X_SIZE		SZ_1M
+#define OMAP243X_GPMC_PHYS	OMAP243X_GPMC_BASE
+#define OMAP243X_GPMC_VIRT	(OMAP243X_GPMC_PHYS + OMAP2_L3_IO_OFFSET)
+						/* 0x6e000000 --> 0xfe000000 */
+#define OMAP243X_GPMC_SIZE	SZ_1M
+#define OMAP243X_SDRC_PHYS	OMAP243X_SDRC_BASE
+						/* 0x6D000000 --> 0xfd000000 */
+#define OMAP243X_SDRC_VIRT	(OMAP243X_SDRC_PHYS + OMAP2_L3_IO_OFFSET)
+#define OMAP243X_SDRC_SIZE	SZ_1M
+#define OMAP243X_SMS_PHYS	OMAP243X_SMS_BASE
+						/* 0x6c000000 --> 0xfc000000 */
+#define OMAP243X_SMS_VIRT	(OMAP243X_SMS_PHYS + OMAP2_L3_IO_OFFSET)
+#define OMAP243X_SMS_SIZE	SZ_1M
+
+/* DSP */
+#define DSP_MEM_24XX_PHYS	OMAP2420_DSP_MEM_BASE	/* 0x58000000 */
+#define DSP_MEM_24XX_VIRT	0xe0000000
+#define DSP_MEM_24XX_SIZE	0x28000
+#define DSP_IPI_24XX_PHYS	OMAP2420_DSP_IPI_BASE	/* 0x59000000 */
+#define DSP_IPI_24XX_VIRT	0xe1000000
+#define DSP_IPI_24XX_SIZE	SZ_4K
+#define DSP_MMU_24XX_PHYS	OMAP2420_DSP_MMU_BASE	/* 0x5a000000 */
+#define DSP_MMU_24XX_VIRT	0xe2000000
+#define DSP_MMU_24XX_SIZE	SZ_4K
+
+/*
+ * ----------------------------------------------------------------------------
+ * Omap3 specific IO mapping
+ * ----------------------------------------------------------------------------
+ */
+
+/* We map both L3 and L4 on OMAP3 */
+#define L3_34XX_PHYS		L3_34XX_BASE	/* 0x68000000 --> 0xf8000000 */
+#define L3_34XX_VIRT		(L3_34XX_PHYS + OMAP2_L3_IO_OFFSET)
+#define L3_34XX_SIZE		SZ_1M   /* 44kB of 128MB used, want 1MB sect */
+
+#define L4_34XX_PHYS		L4_34XX_BASE	/* 0x48000000 --> 0xfa000000 */
+#define L4_34XX_VIRT		(L4_34XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_34XX_SIZE		SZ_4M   /* 1MB of 128MB used, want 1MB sect */
+
+/*
+ * Need to look at the Size 4M for L4.
+ * VPOM3430 was not working for Int controller
+ */
+
+#define L4_WK_34XX_PHYS		L4_WK_34XX_BASE	/* 0x48300000 --> 0xfa300000 */
+#define L4_WK_34XX_VIRT		(L4_WK_34XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_WK_34XX_SIZE		SZ_1M
+
+#define L4_PER_34XX_PHYS	L4_PER_34XX_BASE
+						/* 0x49000000 --> 0xfb000000 */
+#define L4_PER_34XX_VIRT	(L4_PER_34XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_PER_34XX_SIZE	SZ_1M
+
+#define L4_EMU_34XX_PHYS	L4_EMU_34XX_BASE
+						/* 0x54000000 --> 0xfe800000 */
+#define L4_EMU_34XX_VIRT	(L4_EMU_34XX_PHYS + OMAP2_EMU_IO_OFFSET)
+#define L4_EMU_34XX_SIZE	SZ_8M
+
+#define OMAP34XX_GPMC_PHYS	OMAP34XX_GPMC_BASE
+						/* 0x6e000000 --> 0xfe000000 */
+#define OMAP34XX_GPMC_VIRT	(OMAP34XX_GPMC_PHYS + OMAP2_L3_IO_OFFSET)
+#define OMAP34XX_GPMC_SIZE	SZ_1M
+
+#define OMAP343X_SMS_PHYS	OMAP343X_SMS_BASE
+						/* 0x6c000000 --> 0xfc000000 */
+#define OMAP343X_SMS_VIRT	(OMAP343X_SMS_PHYS + OMAP2_L3_IO_OFFSET)
+#define OMAP343X_SMS_SIZE	SZ_1M
+
+#define OMAP343X_SDRC_PHYS	OMAP343X_SDRC_BASE
+						/* 0x6D000000 --> 0xfd000000 */
+#define OMAP343X_SDRC_VIRT	(OMAP343X_SDRC_PHYS + OMAP2_L3_IO_OFFSET)
+#define OMAP343X_SDRC_SIZE	SZ_1M
+
+/* DSP */
+#define DSP_MEM_34XX_PHYS	OMAP34XX_DSP_MEM_BASE	/* 0x58000000 */
+#define DSP_MEM_34XX_VIRT	0xe0000000
+#define DSP_MEM_34XX_SIZE	0x28000
+#define DSP_IPI_34XX_PHYS	OMAP34XX_DSP_IPI_BASE	/* 0x59000000 */
+#define DSP_IPI_34XX_VIRT	0xe1000000
+#define DSP_IPI_34XX_SIZE	SZ_4K
+#define DSP_MMU_34XX_PHYS	OMAP34XX_DSP_MMU_BASE	/* 0x5a000000 */
+#define DSP_MMU_34XX_VIRT	0xe2000000
+#define DSP_MMU_34XX_SIZE	SZ_4K
+
+/*
+ * ----------------------------------------------------------------------------
+ * Omap4 specific IO mapping
+ * ----------------------------------------------------------------------------
+ */
+
+/* We map both L3 and L4 on OMAP4 */
+#define L3_44XX_PHYS		L3_44XX_BASE	/* 0x44000000 --> 0xf8000000 */
+#define L3_44XX_VIRT		(L3_44XX_PHYS + OMAP4_L3_IO_OFFSET)
+#define L3_44XX_SIZE		SZ_1M
+
+#define L4_44XX_PHYS		L4_44XX_BASE	/* 0x4a000000 --> 0xfc000000 */
+#define L4_44XX_VIRT		(L4_44XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_44XX_SIZE		SZ_4M
+
+
+#define L4_WK_44XX_PHYS		L4_WK_44XX_BASE	/* 0x4a300000 --> 0xfc300000 */
+#define L4_WK_44XX_VIRT		(L4_WK_44XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_WK_44XX_SIZE		SZ_1M
+
+#define L4_PER_44XX_PHYS	L4_PER_44XX_BASE
+						/* 0x48000000 --> 0xfa000000 */
+#define L4_PER_44XX_VIRT	(L4_PER_44XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_PER_44XX_SIZE	SZ_4M
+
+#define L4_ABE_44XX_PHYS	L4_ABE_44XX_BASE
+						/* 0x49000000 --> 0xfb000000 */
+#define L4_ABE_44XX_VIRT	(L4_ABE_44XX_PHYS + OMAP2_L4_IO_OFFSET)
+#define L4_ABE_44XX_SIZE	SZ_1M
+
+#define L4_EMU_44XX_PHYS	L4_EMU_44XX_BASE
+						/* 0x54000000 --> 0xfe800000 */
+#define L4_EMU_44XX_VIRT	(L4_EMU_44XX_PHYS + OMAP2_EMU_IO_OFFSET)
+#define L4_EMU_44XX_SIZE	SZ_8M
+
+#define OMAP44XX_GPMC_PHYS	OMAP44XX_GPMC_BASE
+						/* 0x50000000 --> 0xf9000000 */
+#define OMAP44XX_GPMC_VIRT	(OMAP44XX_GPMC_PHYS + OMAP4_GPMC_IO_OFFSET)
+#define OMAP44XX_GPMC_SIZE	SZ_1M
+
+
+#define OMAP44XX_EMIF1_PHYS	OMAP44XX_EMIF1_BASE
+						/* 0x4c000000 --> 0xfd100000 */
+#define OMAP44XX_EMIF1_VIRT	(OMAP44XX_EMIF1_PHYS + OMAP4_L3_PER_IO_OFFSET)
+#define OMAP44XX_EMIF1_SIZE	SZ_1M
+
+#define OMAP44XX_EMIF2_PHYS	OMAP44XX_EMIF2_BASE
+						/* 0x4d000000 --> 0xfd200000 */
+#define OMAP44XX_EMIF2_VIRT	(OMAP44XX_EMIF2_PHYS + OMAP4_L3_PER_IO_OFFSET)
+#define OMAP44XX_EMIF2_SIZE	SZ_1M
+
+#define OMAP44XX_DMM_PHYS	OMAP44XX_DMM_BASE
+						/* 0x4e000000 --> 0xfd300000 */
+#define OMAP44XX_DMM_VIRT	(OMAP44XX_DMM_PHYS + OMAP4_L3_PER_IO_OFFSET)
+#define OMAP44XX_DMM_SIZE	SZ_1M
+/*
+ * ----------------------------------------------------------------------------
+ * Omap specific register access
+ * ----------------------------------------------------------------------------
+ */
+
+#ifndef __ASSEMBLER__
+
+/*
+ * NOTE: Please use ioremap + __raw_read/write where possible instead of these
+ */
+
+extern u8 omap_readb(u32 pa);
+extern u16 omap_readw(u32 pa);
+extern u32 omap_readl(u32 pa);
+extern void omap_writeb(u8 v, u32 pa);
+extern void omap_writew(u16 v, u32 pa);
+extern void omap_writel(u32 v, u32 pa);
+
+struct omap_sdrc_params;
+
+extern void omap1_map_common_io(void);
+extern void omap1_init_common_hw(void);
+
+extern void omap2_map_common_io(void);
+extern void omap2_init_common_hw(struct omap_sdrc_params *sdrc_cs0,
+				 struct omap_sdrc_params *sdrc_cs1);
+
+#define __arch_ioremap(p,s,t)	omap_ioremap(p,s,t)
+#define __arch_iounmap(v)	omap_iounmap(v)
+
+void __iomem *omap_ioremap(unsigned long phys, size_t size, unsigned int type);
+void omap_iounmap(volatile void __iomem *addr);
+
+#endif
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/iommu2.h
@@ -0,0 +1,96 @@
+/*
+ * omap iommu: omap2 architecture specific definitions
+ *
+ * Copyright (C) 2008-2009 Nokia Corporation
+ *
+ * Written by Hiroshi DOYU <Hiroshi.DOYU@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __MACH_IOMMU2_H
+#define __MACH_IOMMU2_H
+
+#include <linux/io.h>
+
+/*
+ * MMU Register offsets
+ */
+#define MMU_REVISION		0x00
+#define MMU_SYSCONFIG		0x10
+#define MMU_SYSSTATUS		0x14
+#define MMU_IRQSTATUS		0x18
+#define MMU_IRQENABLE		0x1c
+#define MMU_WALKING_ST		0x40
+#define MMU_CNTL		0x44
+#define MMU_FAULT_AD		0x48
+#define MMU_TTB			0x4c
+#define MMU_LOCK		0x50
+#define MMU_LD_TLB		0x54
+#define MMU_CAM			0x58
+#define MMU_RAM			0x5c
+#define MMU_GFLUSH		0x60
+#define MMU_FLUSH_ENTRY		0x64
+#define MMU_READ_CAM		0x68
+#define MMU_READ_RAM		0x6c
+#define MMU_EMU_FAULT_AD	0x70
+
+#define MMU_REG_SIZE		256
+
+/*
+ * MMU Register bit definitions
+ */
+#define MMU_LOCK_BASE_SHIFT	10
+#define MMU_LOCK_BASE_MASK	(0x1f << MMU_LOCK_BASE_SHIFT)
+#define MMU_LOCK_BASE(x)	\
+	((x & MMU_LOCK_BASE_MASK) >> MMU_LOCK_BASE_SHIFT)
+
+#define MMU_LOCK_VICT_SHIFT	4
+#define MMU_LOCK_VICT_MASK	(0x1f << MMU_LOCK_VICT_SHIFT)
+#define MMU_LOCK_VICT(x)	\
+	((x & MMU_LOCK_VICT_MASK) >> MMU_LOCK_VICT_SHIFT)
+
+#define MMU_CAM_VATAG_SHIFT	12
+#define MMU_CAM_VATAG_MASK \
+	((~0UL >> MMU_CAM_VATAG_SHIFT) << MMU_CAM_VATAG_SHIFT)
+#define MMU_CAM_P		(1 << 3)
+#define MMU_CAM_V		(1 << 2)
+#define MMU_CAM_PGSZ_MASK	3
+#define MMU_CAM_PGSZ_1M		(0 << 0)
+#define MMU_CAM_PGSZ_64K	(1 << 0)
+#define MMU_CAM_PGSZ_4K		(2 << 0)
+#define MMU_CAM_PGSZ_16M	(3 << 0)
+
+#define MMU_RAM_PADDR_SHIFT	12
+#define MMU_RAM_PADDR_MASK \
+	((~0UL >> MMU_RAM_PADDR_SHIFT) << MMU_RAM_PADDR_SHIFT)
+#define MMU_RAM_ENDIAN_SHIFT	9
+#define MMU_RAM_ENDIAN_MASK	(1 << MMU_RAM_ENDIAN_SHIFT)
+#define MMU_RAM_ENDIAN_BIG	(1 << MMU_RAM_ENDIAN_SHIFT)
+#define MMU_RAM_ENDIAN_LITTLE	(0 << MMU_RAM_ENDIAN_SHIFT)
+#define MMU_RAM_ELSZ_SHIFT	7
+#define MMU_RAM_ELSZ_MASK	(3 << MMU_RAM_ELSZ_SHIFT)
+#define MMU_RAM_ELSZ_8		(0 << MMU_RAM_ELSZ_SHIFT)
+#define MMU_RAM_ELSZ_16		(1 << MMU_RAM_ELSZ_SHIFT)
+#define MMU_RAM_ELSZ_32		(2 << MMU_RAM_ELSZ_SHIFT)
+#define MMU_RAM_ELSZ_NONE	(3 << MMU_RAM_ELSZ_SHIFT)
+#define MMU_RAM_MIXED_SHIFT	6
+#define MMU_RAM_MIXED_MASK	(1 << MMU_RAM_MIXED_SHIFT)
+#define MMU_RAM_MIXED		MMU_RAM_MIXED_MASK
+
+/*
+ * register accessors
+ */
+static inline u32 iommu_read_reg(struct iommu *obj, size_t offs)
+{
+	return __raw_readl(obj->regbase + offs);
+}
+
+static inline void iommu_write_reg(struct iommu *obj, u32 val, size_t offs)
+{
+	__raw_writel(val, obj->regbase + offs);
+}
+
+#endif /* __MACH_IOMMU2_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/iommu.h
@@ -0,0 +1,168 @@
+/*
+ * omap iommu: main structures
+ *
+ * Copyright (C) 2008-2009 Nokia Corporation
+ *
+ * Written by Hiroshi DOYU <Hiroshi.DOYU@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __MACH_IOMMU_H
+#define __MACH_IOMMU_H
+
+struct iotlb_entry {
+	u32 da;
+	u32 pa;
+	u32 pgsz, prsvd, valid;
+	union {
+		u16 ap;
+		struct {
+			u32 endian, elsz, mixed;
+		};
+	};
+};
+
+struct iommu {
+	const char	*name;
+	struct module	*owner;
+	struct clk	*clk;
+	void __iomem	*regbase;
+	struct device	*dev;
+
+	unsigned int	refcount;
+	struct mutex	iommu_lock;	/* global for this whole object */
+
+	/*
+	 * We don't change iopgd for a situation like pgd for a task,
+	 * but share it globally for each iommu.
+	 */
+	u32		*iopgd;
+	spinlock_t	page_table_lock; /* protect iopgd */
+
+	int		nr_tlb_entries;
+
+	struct list_head	mmap;
+	struct mutex		mmap_lock; /* protect mmap */
+
+	int (*isr)(struct iommu *obj);
+
+	void *ctx; /* iommu context: registres saved area */
+};
+
+struct cr_regs {
+	union {
+		struct {
+			u16 cam_l;
+			u16 cam_h;
+		};
+		u32 cam;
+	};
+	union {
+		struct {
+			u16 ram_l;
+			u16 ram_h;
+		};
+		u32 ram;
+	};
+};
+
+struct iotlb_lock {
+	short base;
+	short vict;
+};
+
+/* architecture specific functions */
+struct iommu_functions {
+	unsigned long	version;
+
+	int (*enable)(struct iommu *obj);
+	void (*disable)(struct iommu *obj);
+	u32 (*fault_isr)(struct iommu *obj, u32 *ra);
+
+	void (*tlb_read_cr)(struct iommu *obj, struct cr_regs *cr);
+	void (*tlb_load_cr)(struct iommu *obj, struct cr_regs *cr);
+
+	struct cr_regs *(*alloc_cr)(struct iommu *obj, struct iotlb_entry *e);
+	int (*cr_valid)(struct cr_regs *cr);
+	u32 (*cr_to_virt)(struct cr_regs *cr);
+	void (*cr_to_e)(struct cr_regs *cr, struct iotlb_entry *e);
+	ssize_t (*dump_cr)(struct iommu *obj, struct cr_regs *cr, char *buf);
+
+	u32 (*get_pte_attr)(struct iotlb_entry *e);
+
+	void (*save_ctx)(struct iommu *obj);
+	void (*restore_ctx)(struct iommu *obj);
+	ssize_t (*dump_ctx)(struct iommu *obj, char *buf, ssize_t len);
+};
+
+struct iommu_platform_data {
+	const char *name;
+	const char *clk_name;
+	const int nr_tlb_entries;
+};
+
+#if defined(CONFIG_ARCH_OMAP1)
+#error "iommu for this processor not implemented yet"
+#else
+#include <plat/iommu2.h>
+#endif
+
+/*
+ * utilities for super page(16MB, 1MB, 64KB and 4KB)
+ */
+
+#define iopgsz_max(bytes)			\
+	(((bytes) >= SZ_16M) ? SZ_16M :		\
+	 ((bytes) >= SZ_1M)  ? SZ_1M  :		\
+	 ((bytes) >= SZ_64K) ? SZ_64K :		\
+	 ((bytes) >= SZ_4K)  ? SZ_4K  :	0)
+
+#define bytes_to_iopgsz(bytes)				\
+	(((bytes) == SZ_16M) ? MMU_CAM_PGSZ_16M :	\
+	 ((bytes) == SZ_1M)  ? MMU_CAM_PGSZ_1M  :	\
+	 ((bytes) == SZ_64K) ? MMU_CAM_PGSZ_64K :	\
+	 ((bytes) == SZ_4K)  ? MMU_CAM_PGSZ_4K  : -1)
+
+#define iopgsz_to_bytes(iopgsz)				\
+	(((iopgsz) == MMU_CAM_PGSZ_16M)	? SZ_16M :	\
+	 ((iopgsz) == MMU_CAM_PGSZ_1M)	? SZ_1M  :	\
+	 ((iopgsz) == MMU_CAM_PGSZ_64K)	? SZ_64K :	\
+	 ((iopgsz) == MMU_CAM_PGSZ_4K)	? SZ_4K  : 0)
+
+#define iopgsz_ok(bytes) (bytes_to_iopgsz(bytes) >= 0)
+
+/*
+ * global functions
+ */
+extern u32 iommu_arch_version(void);
+
+extern void iotlb_cr_to_e(struct cr_regs *cr, struct iotlb_entry *e);
+extern u32 iotlb_cr_to_virt(struct cr_regs *cr);
+
+extern int load_iotlb_entry(struct iommu *obj, struct iotlb_entry *e);
+extern void flush_iotlb_page(struct iommu *obj, u32 da);
+extern void flush_iotlb_range(struct iommu *obj, u32 start, u32 end);
+extern void flush_iotlb_all(struct iommu *obj);
+
+extern int iopgtable_store_entry(struct iommu *obj, struct iotlb_entry *e);
+extern size_t iopgtable_clear_entry(struct iommu *obj, u32 iova);
+
+extern struct iommu *iommu_get(const char *name);
+extern void iommu_put(struct iommu *obj);
+
+extern void iommu_save_ctx(struct iommu *obj);
+extern void iommu_restore_ctx(struct iommu *obj);
+
+extern int install_iommu_arch(const struct iommu_functions *ops);
+extern void uninstall_iommu_arch(const struct iommu_functions *ops);
+
+extern int foreach_iommu_device(void *data,
+				int (*fn)(struct device *, void *));
+
+extern ssize_t iommu_dump_ctx(struct iommu *obj, char *buf, ssize_t len);
+extern size_t dump_tlb_entries(struct iommu *obj, char *buf, ssize_t len);
+
+#endif /* __MACH_IOMMU_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/iovmm.h
@@ -0,0 +1,94 @@
+/*
+ * omap iommu: simple virtual address space management
+ *
+ * Copyright (C) 2008-2009 Nokia Corporation
+ *
+ * Written by Hiroshi DOYU <Hiroshi.DOYU@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __IOMMU_MMAP_H
+#define __IOMMU_MMAP_H
+
+struct iovm_struct {
+	struct iommu		*iommu;	/* iommu object which this belongs to */
+	u32			da_start; /* area definition */
+	u32			da_end;
+	u32			flags; /* IOVMF_: see below */
+	struct list_head	list; /* linked in ascending order */
+	const struct sg_table	*sgt; /* keep 'page' <-> 'da' mapping */
+	void			*va; /* mpu side mapped address */
+};
+
+/*
+ * IOVMF_FLAGS: attribute for iommu virtual memory area(iovma)
+ *
+ * lower 16 bit is used for h/w and upper 16 bit is for s/w.
+ */
+#define IOVMF_SW_SHIFT		16
+#define IOVMF_HW_SIZE		(1 << IOVMF_SW_SHIFT)
+#define IOVMF_HW_MASK		(IOVMF_HW_SIZE - 1)
+#define IOVMF_SW_MASK		(~IOVMF_HW_MASK)UL
+
+/*
+ * iovma: h/w flags derived from cam and ram attribute
+ */
+#define IOVMF_CAM_MASK		(~((1 << 10) - 1))
+#define IOVMF_RAM_MASK		(~IOVMF_CAM_MASK)
+
+#define IOVMF_PGSZ_MASK		(3 << 0)
+#define IOVMF_PGSZ_1M		MMU_CAM_PGSZ_1M
+#define IOVMF_PGSZ_64K		MMU_CAM_PGSZ_64K
+#define IOVMF_PGSZ_4K		MMU_CAM_PGSZ_4K
+#define IOVMF_PGSZ_16M		MMU_CAM_PGSZ_16M
+
+#define IOVMF_ENDIAN_MASK	(1 << 9)
+#define IOVMF_ENDIAN_BIG	MMU_RAM_ENDIAN_BIG
+#define IOVMF_ENDIAN_LITTLE	MMU_RAM_ENDIAN_LITTLE
+
+#define IOVMF_ELSZ_MASK		(3 << 7)
+#define IOVMF_ELSZ_8		MMU_RAM_ELSZ_8
+#define IOVMF_ELSZ_16		MMU_RAM_ELSZ_16
+#define IOVMF_ELSZ_32		MMU_RAM_ELSZ_32
+#define IOVMF_ELSZ_NONE		MMU_RAM_ELSZ_NONE
+
+#define IOVMF_MIXED_MASK	(1 << 6)
+#define IOVMF_MIXED		MMU_RAM_MIXED
+
+/*
+ * iovma: s/w flags, used for mapping and umapping internally.
+ */
+#define IOVMF_MMIO		(1 << IOVMF_SW_SHIFT)
+#define IOVMF_ALLOC		(2 << IOVMF_SW_SHIFT)
+#define IOVMF_ALLOC_MASK	(3 << IOVMF_SW_SHIFT)
+
+/* "superpages" is supported just with physically linear pages */
+#define IOVMF_DISCONT		(1 << (2 + IOVMF_SW_SHIFT))
+#define IOVMF_LINEAR		(2 << (2 + IOVMF_SW_SHIFT))
+#define IOVMF_LINEAR_MASK	(3 << (2 + IOVMF_SW_SHIFT))
+
+#define IOVMF_DA_FIXED		(1 << (4 + IOVMF_SW_SHIFT))
+#define IOVMF_DA_ANON		(2 << (4 + IOVMF_SW_SHIFT))
+#define IOVMF_DA_MASK		(3 << (4 + IOVMF_SW_SHIFT))
+
+
+extern struct iovm_struct *find_iovm_area(struct iommu *obj, u32 da);
+extern u32 iommu_vmap(struct iommu *obj, u32 da,
+			const struct sg_table *sgt, u32 flags);
+extern struct sg_table *iommu_vunmap(struct iommu *obj, u32 da);
+extern u32 iommu_vmalloc(struct iommu *obj, u32 da, size_t bytes,
+			   u32 flags);
+extern void iommu_vfree(struct iommu *obj, const u32 da);
+extern u32 iommu_kmap(struct iommu *obj, u32 da, u32 pa, size_t bytes,
+			u32 flags);
+extern void iommu_kunmap(struct iommu *obj, u32 da);
+extern u32 iommu_kmalloc(struct iommu *obj, u32 da, size_t bytes,
+			   u32 flags);
+extern void iommu_kfree(struct iommu *obj, u32 da);
+
+extern void *da_to_va(struct iommu *obj, u32 da);
+
+#endif /* __IOMMU_MMAP_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/irda.h
@@ -0,0 +1,33 @@
+/*
+ *  arch/arm/plat-omap/include/mach/irda.h
+ *
+ *  Copyright (C) 2005-2006 Komal Shah <komal_shah802003@yahoo.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+#ifndef ASMARM_ARCH_IRDA_H
+#define ASMARM_ARCH_IRDA_H
+
+/* board specific transceiver capabilities */
+
+#define IR_SEL		1	/* Selects IrDA */
+#define IR_SIRMODE	2
+#define IR_FIRMODE	4
+#define IR_MIRMODE	8
+
+struct omap_irda_config {
+	int transceiver_cap;
+	int (*transceiver_mode)(struct device *dev, int mode);
+	int (*select_irda)(struct device *dev, int state);
+	int rx_channel;
+	int tx_channel;
+	unsigned long dest_start;
+	unsigned long src_start;
+	int tx_trigger;
+	int rx_trigger;
+	int mode;
+};
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/irqs.h
@@ -0,0 +1,506 @@
+/*
+ *  arch/arm/plat-omap/include/mach/irqs.h
+ *
+ *  Copyright (C) Greg Lonnon 2001
+ *  Updated for OMAP-1610 by Tony Lindgren <tony@atomide.com>
+ *
+ * Copyright (C) 2009 Texas Instruments
+ * Added OMAP4 support - Santosh Shilimkar <santosh.shilimkar@ti.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
+ *
+ * NOTE: The interrupt vectors for the OMAP-1509, OMAP-1510, and OMAP-1610
+ *	 are different.
+ */
+
+#ifndef __ASM_ARCH_OMAP15XX_IRQS_H
+#define __ASM_ARCH_OMAP15XX_IRQS_H
+
+/*
+ * IRQ numbers for interrupt handler 1
+ *
+ * NOTE: See also the OMAP-1510 and 1610 specific IRQ numbers below
+ *
+ */
+#define INT_CAMERA		1
+#define INT_FIQ			3
+#define INT_RTDX		6
+#define INT_DSP_MMU_ABORT	7
+#define INT_HOST		8
+#define INT_ABORT		9
+#define INT_BRIDGE_PRIV		13
+#define INT_GPIO_BANK1		14
+#define INT_UART3		15
+#define INT_TIMER3		16
+#define INT_DMA_CH0_6		19
+#define INT_DMA_CH1_7		20
+#define INT_DMA_CH2_8		21
+#define INT_DMA_CH3		22
+#define INT_DMA_CH4		23
+#define INT_DMA_CH5		24
+#define INT_DMA_LCD		25
+#define INT_TIMER1		26
+#define INT_WD_TIMER		27
+#define INT_BRIDGE_PUB		28
+#define INT_TIMER2		30
+#define INT_LCD_CTRL		31
+
+/*
+ * OMAP-1510 specific IRQ numbers for interrupt handler 1
+ */
+#define INT_1510_IH2_IRQ	0
+#define INT_1510_RES2		2
+#define INT_1510_SPI_TX		4
+#define INT_1510_SPI_RX		5
+#define INT_1510_DSP_MAILBOX1	10
+#define INT_1510_DSP_MAILBOX2	11
+#define INT_1510_RES12		12
+#define INT_1510_LB_MMU		17
+#define INT_1510_RES18		18
+#define INT_1510_LOCAL_BUS	29
+
+/*
+ * OMAP-1610 specific IRQ numbers for interrupt handler 1
+ */
+#define INT_1610_IH2_IRQ	0
+#define INT_1610_IH2_FIQ	2
+#define INT_1610_McBSP2_TX	4
+#define INT_1610_McBSP2_RX	5
+#define INT_1610_DSP_MAILBOX1	10
+#define INT_1610_DSP_MAILBOX2	11
+#define INT_1610_LCD_LINE	12
+#define INT_1610_GPTIMER1	17
+#define INT_1610_GPTIMER2	18
+#define INT_1610_SSR_FIFO_0	29
+
+/*
+ * OMAP-7xx specific IRQ numbers for interrupt handler 1
+ */
+#define INT_7XX_IH2_FIQ		0
+#define INT_7XX_IH2_IRQ		1
+#define INT_7XX_USB_NON_ISO	2
+#define INT_7XX_USB_ISO		3
+#define INT_7XX_ICR		4
+#define INT_7XX_EAC		5
+#define INT_7XX_GPIO_BANK1	6
+#define INT_7XX_GPIO_BANK2	7
+#define INT_7XX_GPIO_BANK3	8
+#define INT_7XX_McBSP2TX	10
+#define INT_7XX_McBSP2RX	11
+#define INT_7XX_McBSP2RX_OVF	12
+#define INT_7XX_LCD_LINE	14
+#define INT_7XX_GSM_PROTECT	15
+#define INT_7XX_TIMER3		16
+#define INT_7XX_GPIO_BANK5	17
+#define INT_7XX_GPIO_BANK6	18
+#define INT_7XX_SPGIO_WR	29
+
+/*
+ * IRQ numbers for interrupt handler 2
+ *
+ * NOTE: See also the OMAP-1510 and 1610 specific IRQ numbers below
+ */
+#define IH2_BASE		32
+
+#define INT_KEYBOARD		(1 + IH2_BASE)
+#define INT_uWireTX		(2 + IH2_BASE)
+#define INT_uWireRX		(3 + IH2_BASE)
+#define INT_I2C			(4 + IH2_BASE)
+#define INT_MPUIO		(5 + IH2_BASE)
+#define INT_USB_HHC_1		(6 + IH2_BASE)
+#define INT_McBSP3TX		(10 + IH2_BASE)
+#define INT_McBSP3RX		(11 + IH2_BASE)
+#define INT_McBSP1TX		(12 + IH2_BASE)
+#define INT_McBSP1RX		(13 + IH2_BASE)
+#define INT_UART1		(14 + IH2_BASE)
+#define INT_UART2		(15 + IH2_BASE)
+#define INT_BT_MCSI1TX		(16 + IH2_BASE)
+#define INT_BT_MCSI1RX		(17 + IH2_BASE)
+#define INT_SOSSI_MATCH		(19 + IH2_BASE)
+#define INT_USB_W2FC		(20 + IH2_BASE)
+#define INT_1WIRE		(21 + IH2_BASE)
+#define INT_OS_TIMER		(22 + IH2_BASE)
+#define INT_MMC			(23 + IH2_BASE)
+#define INT_GAUGE_32K		(24 + IH2_BASE)
+#define INT_RTC_TIMER		(25 + IH2_BASE)
+#define INT_RTC_ALARM		(26 + IH2_BASE)
+#define INT_MEM_STICK		(27 + IH2_BASE)
+
+/*
+ * OMAP-1510 specific IRQ numbers for interrupt handler 2
+ */
+#define INT_1510_DSP_MMU	(28 + IH2_BASE)
+#define INT_1510_COM_SPI_RO	(31 + IH2_BASE)
+
+/*
+ * OMAP-1610 specific IRQ numbers for interrupt handler 2
+ */
+#define INT_1610_FAC		(0 + IH2_BASE)
+#define INT_1610_USB_HHC_2	(7 + IH2_BASE)
+#define INT_1610_USB_OTG	(8 + IH2_BASE)
+#define INT_1610_SoSSI		(9 + IH2_BASE)
+#define INT_1610_SoSSI_MATCH	(19 + IH2_BASE)
+#define INT_1610_DSP_MMU	(28 + IH2_BASE)
+#define INT_1610_McBSP2RX_OF	(31 + IH2_BASE)
+#define INT_1610_STI		(32 + IH2_BASE)
+#define INT_1610_STI_WAKEUP	(33 + IH2_BASE)
+#define INT_1610_GPTIMER3	(34 + IH2_BASE)
+#define INT_1610_GPTIMER4	(35 + IH2_BASE)
+#define INT_1610_GPTIMER5	(36 + IH2_BASE)
+#define INT_1610_GPTIMER6	(37 + IH2_BASE)
+#define INT_1610_GPTIMER7	(38 + IH2_BASE)
+#define INT_1610_GPTIMER8	(39 + IH2_BASE)
+#define INT_1610_GPIO_BANK2	(40 + IH2_BASE)
+#define INT_1610_GPIO_BANK3	(41 + IH2_BASE)
+#define INT_1610_MMC2		(42 + IH2_BASE)
+#define INT_1610_CF		(43 + IH2_BASE)
+#define INT_1610_WAKE_UP_REQ	(46 + IH2_BASE)
+#define INT_1610_GPIO_BANK4	(48 + IH2_BASE)
+#define INT_1610_SPI		(49 + IH2_BASE)
+#define INT_1610_DMA_CH6	(53 + IH2_BASE)
+#define INT_1610_DMA_CH7	(54 + IH2_BASE)
+#define INT_1610_DMA_CH8	(55 + IH2_BASE)
+#define INT_1610_DMA_CH9	(56 + IH2_BASE)
+#define INT_1610_DMA_CH10	(57 + IH2_BASE)
+#define INT_1610_DMA_CH11	(58 + IH2_BASE)
+#define INT_1610_DMA_CH12	(59 + IH2_BASE)
+#define INT_1610_DMA_CH13	(60 + IH2_BASE)
+#define INT_1610_DMA_CH14	(61 + IH2_BASE)
+#define INT_1610_DMA_CH15	(62 + IH2_BASE)
+#define INT_1610_NAND		(63 + IH2_BASE)
+#define INT_1610_SHA1MD5	(91 + IH2_BASE)
+
+/*
+ * OMAP-7xx specific IRQ numbers for interrupt handler 2
+ */
+#define INT_7XX_HW_ERRORS	(0 + IH2_BASE)
+#define INT_7XX_NFIQ_PWR_FAIL	(1 + IH2_BASE)
+#define INT_7XX_CFCD		(2 + IH2_BASE)
+#define INT_7XX_CFIREQ		(3 + IH2_BASE)
+#define INT_7XX_I2C		(4 + IH2_BASE)
+#define INT_7XX_PCC		(5 + IH2_BASE)
+#define INT_7XX_MPU_EXT_NIRQ	(6 + IH2_BASE)
+#define INT_7XX_SPI_100K_1	(7 + IH2_BASE)
+#define INT_7XX_SYREN_SPI	(8 + IH2_BASE)
+#define INT_7XX_VLYNQ		(9 + IH2_BASE)
+#define INT_7XX_GPIO_BANK4	(10 + IH2_BASE)
+#define INT_7XX_McBSP1TX	(11 + IH2_BASE)
+#define INT_7XX_McBSP1RX	(12 + IH2_BASE)
+#define INT_7XX_McBSP1RX_OF	(13 + IH2_BASE)
+#define INT_7XX_UART_MODEM_IRDA_2 (14 + IH2_BASE)
+#define INT_7XX_UART_MODEM_1	(15 + IH2_BASE)
+#define INT_7XX_MCSI		(16 + IH2_BASE)
+#define INT_7XX_uWireTX		(17 + IH2_BASE)
+#define INT_7XX_uWireRX		(18 + IH2_BASE)
+#define INT_7XX_SMC_CD		(19 + IH2_BASE)
+#define INT_7XX_SMC_IREQ	(20 + IH2_BASE)
+#define INT_7XX_HDQ_1WIRE	(21 + IH2_BASE)
+#define INT_7XX_TIMER32K	(22 + IH2_BASE)
+#define INT_7XX_MMC_SDIO	(23 + IH2_BASE)
+#define INT_7XX_UPLD		(24 + IH2_BASE)
+#define INT_7XX_USB_HHC_1	(27 + IH2_BASE)
+#define INT_7XX_USB_HHC_2	(28 + IH2_BASE)
+#define INT_7XX_USB_GENI	(29 + IH2_BASE)
+#define INT_7XX_USB_OTG		(30 + IH2_BASE)
+#define INT_7XX_CAMERA_IF	(31 + IH2_BASE)
+#define INT_7XX_RNG		(32 + IH2_BASE)
+#define INT_7XX_DUAL_MODE_TIMER (33 + IH2_BASE)
+#define INT_7XX_DBB_RF_EN	(34 + IH2_BASE)
+#define INT_7XX_MPUIO_KEYPAD	(35 + IH2_BASE)
+#define INT_7XX_SHA1_MD5	(36 + IH2_BASE)
+#define INT_7XX_SPI_100K_2	(37 + IH2_BASE)
+#define INT_7XX_RNG_IDLE	(38 + IH2_BASE)
+#define INT_7XX_MPUIO		(39 + IH2_BASE)
+#define INT_7XX_LLPC_LCD_CTRL_CAN_BE_OFF	(40 + IH2_BASE)
+#define INT_7XX_LLPC_OE_FALLING (41 + IH2_BASE)
+#define INT_7XX_LLPC_OE_RISING	(42 + IH2_BASE)
+#define INT_7XX_LLPC_VSYNC	(43 + IH2_BASE)
+#define INT_7XX_WAKE_UP_REQ	(46 + IH2_BASE)
+#define INT_7XX_DMA_CH6		(53 + IH2_BASE)
+#define INT_7XX_DMA_CH7		(54 + IH2_BASE)
+#define INT_7XX_DMA_CH8		(55 + IH2_BASE)
+#define INT_7XX_DMA_CH9		(56 + IH2_BASE)
+#define INT_7XX_DMA_CH10	(57 + IH2_BASE)
+#define INT_7XX_DMA_CH11	(58 + IH2_BASE)
+#define INT_7XX_DMA_CH12	(59 + IH2_BASE)
+#define INT_7XX_DMA_CH13	(60 + IH2_BASE)
+#define INT_7XX_DMA_CH14	(61 + IH2_BASE)
+#define INT_7XX_DMA_CH15	(62 + IH2_BASE)
+#define INT_7XX_NAND		(63 + IH2_BASE)
+
+#define INT_24XX_SYS_NIRQ	7
+#define INT_24XX_SDMA_IRQ0	12
+#define INT_24XX_SDMA_IRQ1	13
+#define INT_24XX_SDMA_IRQ2	14
+#define INT_24XX_SDMA_IRQ3	15
+#define INT_24XX_CAM_IRQ	24
+#define INT_24XX_DSS_IRQ	25
+#define INT_24XX_MAIL_U0_MPU	26
+#define INT_24XX_DSP_UMA	27
+#define INT_24XX_DSP_MMU	28
+#define INT_24XX_GPIO_BANK1	29
+#define INT_24XX_GPIO_BANK2	30
+#define INT_24XX_GPIO_BANK3	31
+#define INT_24XX_GPIO_BANK4	32
+#define INT_24XX_GPIO_BANK5	33
+#define INT_24XX_MAIL_U3_MPU	34
+#define INT_24XX_GPTIMER1	37
+#define INT_24XX_GPTIMER2	38
+#define INT_24XX_GPTIMER3	39
+#define INT_24XX_GPTIMER4	40
+#define INT_24XX_GPTIMER5	41
+#define INT_24XX_GPTIMER6	42
+#define INT_24XX_GPTIMER7	43
+#define INT_24XX_GPTIMER8	44
+#define INT_24XX_GPTIMER9	45
+#define INT_24XX_GPTIMER10	46
+#define INT_24XX_GPTIMER11	47
+#define INT_24XX_GPTIMER12	48
+#define INT_24XX_SHA1MD5	51
+#define INT_24XX_MCBSP4_IRQ_TX	54
+#define INT_24XX_MCBSP4_IRQ_RX	55
+#define INT_24XX_I2C1_IRQ	56
+#define INT_24XX_I2C2_IRQ	57
+#define INT_24XX_HDQ_IRQ	58
+#define INT_24XX_MCBSP1_IRQ_TX	59
+#define INT_24XX_MCBSP1_IRQ_RX	60
+#define INT_24XX_MCBSP2_IRQ_TX	62
+#define INT_24XX_MCBSP2_IRQ_RX	63
+#define INT_24XX_SPI1_IRQ	65
+#define INT_24XX_SPI2_IRQ	66
+#define INT_24XX_UART1_IRQ	72
+#define INT_24XX_UART2_IRQ	73
+#define INT_24XX_UART3_IRQ	74
+#define INT_24XX_USB_IRQ_GEN	75
+#define INT_24XX_USB_IRQ_NISO	76
+#define INT_24XX_USB_IRQ_ISO	77
+#define INT_24XX_USB_IRQ_HGEN	78
+#define INT_24XX_USB_IRQ_HSOF	79
+#define INT_24XX_USB_IRQ_OTG	80
+#define INT_24XX_MCBSP5_IRQ_TX	81
+#define INT_24XX_MCBSP5_IRQ_RX	82
+#define INT_24XX_MMC_IRQ	83
+#define INT_24XX_MMC2_IRQ	86
+#define INT_24XX_MCBSP3_IRQ_TX	89
+#define INT_24XX_MCBSP3_IRQ_RX	90
+#define INT_24XX_SPI3_IRQ	91
+
+#define INT_243X_MCBSP2_IRQ	16
+#define INT_243X_MCBSP3_IRQ	17
+#define INT_243X_MCBSP4_IRQ	18
+#define INT_243X_MCBSP5_IRQ	19
+#define INT_243X_MCBSP1_IRQ	64
+#define INT_243X_HS_USB_MC	92
+#define INT_243X_HS_USB_DMA	93
+#define INT_243X_CARKIT_IRQ	94
+
+#define INT_34XX_BENCH_MPU_EMUL	3
+#define INT_34XX_ST_MCBSP2_IRQ	4
+#define INT_34XX_ST_MCBSP3_IRQ	5
+#define INT_34XX_SSM_ABORT_IRQ	6
+#define INT_34XX_SYS_NIRQ	7
+#define INT_34XX_D2D_FW_IRQ	8
+#define INT_34XX_PRCM_MPU_IRQ	11
+#define INT_34XX_MCBSP1_IRQ	16
+#define INT_34XX_MCBSP2_IRQ	17
+#define INT_34XX_MCBSP3_IRQ	22
+#define INT_34XX_MCBSP4_IRQ	23
+#define INT_34XX_CAM_IRQ	24
+#define INT_34XX_MCBSP5_IRQ	27
+#define INT_34XX_GPIO_BANK1	29
+#define INT_34XX_GPIO_BANK2	30
+#define INT_34XX_GPIO_BANK3	31
+#define INT_34XX_GPIO_BANK4	32
+#define INT_34XX_GPIO_BANK5	33
+#define INT_34XX_GPIO_BANK6	34
+#define INT_34XX_USIM_IRQ	35
+#define INT_34XX_WDT3_IRQ	36
+#define INT_34XX_SPI4_IRQ	48
+#define INT_34XX_SHA1MD52_IRQ	49
+#define INT_34XX_FPKA_READY_IRQ	50
+#define INT_34XX_SHA1MD51_IRQ	51
+#define INT_34XX_RNG_IRQ	52
+#define INT_34XX_I2C3_IRQ	61
+#define INT_34XX_FPKA_ERROR_IRQ	64
+#define INT_34XX_PBIAS_IRQ	75
+#define INT_34XX_OHCI_IRQ	76
+#define INT_34XX_EHCI_IRQ	77
+#define INT_34XX_TLL_IRQ	78
+#define INT_34XX_PARTHASH_IRQ	79
+#define INT_34XX_MMC3_IRQ	94
+#define INT_34XX_GPT12_IRQ	95
+
+#define	INT_34XX_BENCH_MPU_EMUL	3
+
+
+#define IRQ_GIC_START		32
+#define INT_44XX_LOCALTIMER_IRQ	29
+#define INT_44XX_LOCALWDT_IRQ	30
+
+#define INT_44XX_BENCH_MPU_EMUL	(3 + IRQ_GIC_START)
+#define INT_44XX_SSM_ABORT_IRQ	(6 + IRQ_GIC_START)
+#define INT_44XX_SYS_NIRQ	(7 + IRQ_GIC_START)
+#define INT_44XX_D2D_FW_IRQ	(8 + IRQ_GIC_START)
+#define INT_44XX_PRCM_MPU_IRQ	(11 + IRQ_GIC_START)
+#define INT_44XX_SDMA_IRQ0	(12 + IRQ_GIC_START)
+#define INT_44XX_SDMA_IRQ1	(13 + IRQ_GIC_START)
+#define INT_44XX_SDMA_IRQ2	(14 + IRQ_GIC_START)
+#define INT_44XX_SDMA_IRQ3	(15 + IRQ_GIC_START)
+#define INT_44XX_ISS_IRQ	(24 + IRQ_GIC_START)
+#define INT_44XX_DSS_IRQ	(25 + IRQ_GIC_START)
+#define INT_44XX_MAIL_U0_MPU	(26 + IRQ_GIC_START)
+#define INT_44XX_DSP_MMU	(28 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER1	(37 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER2	(38 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER3	(39 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER4	(40 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER5	(41 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER6	(42 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER7	(43 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER8	(44 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER9	(45 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER10	(46 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER11	(47 + IRQ_GIC_START)
+#define INT_44XX_GPTIMER12	(95 + IRQ_GIC_START)
+#define INT_44XX_SHA1MD5	(51 + IRQ_GIC_START)
+#define INT_44XX_I2C1_IRQ	(56 + IRQ_GIC_START)
+#define INT_44XX_I2C2_IRQ	(57 + IRQ_GIC_START)
+#define INT_44XX_HDQ_IRQ	(58 + IRQ_GIC_START)
+#define INT_44XX_SPI1_IRQ	(65 + IRQ_GIC_START)
+#define INT_44XX_SPI2_IRQ	(66 + IRQ_GIC_START)
+#define INT_44XX_HSI_1_IRQ0	(67 + IRQ_GIC_START)
+#define INT_44XX_HSI_2_IRQ1	(68 + IRQ_GIC_START)
+#define INT_44XX_HSI_1_DMAIRQ	(71 + IRQ_GIC_START)
+#define INT_44XX_UART1_IRQ	(72 + IRQ_GIC_START)
+#define INT_44XX_UART2_IRQ	(73 + IRQ_GIC_START)
+#define INT_44XX_UART3_IRQ	(74 + IRQ_GIC_START)
+#define INT_44XX_UART4_IRQ	(70 + IRQ_GIC_START)
+#define INT_44XX_USB_IRQ_NISO	(76 + IRQ_GIC_START)
+#define INT_44XX_USB_IRQ_ISO	(77 + IRQ_GIC_START)
+#define INT_44XX_USB_IRQ_HGEN	(78 + IRQ_GIC_START)
+#define INT_44XX_USB_IRQ_HSOF	(79 + IRQ_GIC_START)
+#define INT_44XX_USB_IRQ_OTG	(80 + IRQ_GIC_START)
+#define INT_44XX_MCBSP4_IRQ_TX	(81 + IRQ_GIC_START)
+#define INT_44XX_MCBSP4_IRQ_RX	(82 + IRQ_GIC_START)
+#define INT_44XX_MMC_IRQ	(83 + IRQ_GIC_START)
+#define INT_44XX_MMC2_IRQ	(86 + IRQ_GIC_START)
+#define INT_44XX_MCBSP2_IRQ_TX	(89 + IRQ_GIC_START)
+#define INT_44XX_MCBSP2_IRQ_RX	(90 + IRQ_GIC_START)
+#define INT_44XX_SPI3_IRQ	(91 + IRQ_GIC_START)
+#define INT_44XX_SPI5_IRQ	(69 + IRQ_GIC_START)
+
+#define INT_44XX_MCBSP5_IRQ	(16 + IRQ_GIC_START)
+#define INT_44xX_MCBSP1_IRQ	(17 + IRQ_GIC_START)
+#define INT_44XX_MCBSP2_IRQ	(22 + IRQ_GIC_START)
+#define INT_44XX_MCBSP3_IRQ	(23 + IRQ_GIC_START)
+#define INT_44XX_MCBSP4_IRQ	(27 + IRQ_GIC_START)
+#define INT_44XX_HS_USB_MC	(92 + IRQ_GIC_START)
+#define INT_44XX_HS_USB_DMA	(93 + IRQ_GIC_START)
+
+#define INT_44XX_GPIO_BANK1	(29 + IRQ_GIC_START)
+#define INT_44XX_GPIO_BANK2	(30 + IRQ_GIC_START)
+#define INT_44XX_GPIO_BANK3	(31 + IRQ_GIC_START)
+#define INT_44XX_GPIO_BANK4	(32 + IRQ_GIC_START)
+#define INT_44XX_GPIO_BANK5	(33 + IRQ_GIC_START)
+#define INT_44XX_GPIO_BANK6	(34 + IRQ_GIC_START)
+#define INT_44XX_USIM_IRQ	(35 + IRQ_GIC_START)
+#define INT_44XX_WDT3_IRQ	(36 + IRQ_GIC_START)
+#define INT_44XX_SPI4_IRQ	(48 + IRQ_GIC_START)
+#define INT_44XX_SHA1MD52_IRQ	(49 + IRQ_GIC_START)
+#define INT_44XX_FPKA_READY_IRQ	(50 + IRQ_GIC_START)
+#define INT_44XX_SHA1MD51_IRQ	(51 + IRQ_GIC_START)
+#define INT_44XX_RNG_IRQ	(52 + IRQ_GIC_START)
+#define INT_44XX_MMC5_IRQ	(59 + IRQ_GIC_START)
+#define INT_44XX_I2C3_IRQ	(61 + IRQ_GIC_START)
+#define INT_44XX_FPKA_ERROR_IRQ	(64 + IRQ_GIC_START)
+#define INT_44XX_PBIAS_IRQ	(75 + IRQ_GIC_START)
+#define INT_44XX_OHCI_IRQ	(76 + IRQ_GIC_START)
+#define INT_44XX_EHCI_IRQ	(77 + IRQ_GIC_START)
+#define INT_44XX_TLL_IRQ	(78 + IRQ_GIC_START)
+#define INT_44XX_PARTHASH_IRQ	(79 + IRQ_GIC_START)
+#define INT_44XX_MMC3_IRQ	(94 + IRQ_GIC_START)
+#define INT_44XX_MMC4_IRQ	(96 + IRQ_GIC_START)
+
+
+/* Max. 128 level 2 IRQs (OMAP1610), 192 GPIOs (OMAP730/850) and
+ * 16 MPUIO lines */
+#define OMAP_MAX_GPIO_LINES	192
+#define IH_GPIO_BASE		(128 + IH2_BASE)
+#define IH_MPUIO_BASE		(OMAP_MAX_GPIO_LINES + IH_GPIO_BASE)
+#define OMAP_IRQ_END		(IH_MPUIO_BASE + 16)
+
+/* External FPGA handles interrupts on Innovator boards */
+#define	OMAP_FPGA_IRQ_BASE	(OMAP_IRQ_END)
+#ifdef	CONFIG_MACH_OMAP_INNOVATOR
+#define OMAP_FPGA_NR_IRQS	24
+#else
+#define OMAP_FPGA_NR_IRQS	0
+#endif
+#define OMAP_FPGA_IRQ_END	(OMAP_FPGA_IRQ_BASE + OMAP_FPGA_NR_IRQS)
+
+/* External TWL4030 can handle interrupts on 2430 and 34xx boards */
+#define	TWL4030_IRQ_BASE	(OMAP_FPGA_IRQ_END)
+#ifdef	CONFIG_TWL4030_CORE
+#define	TWL4030_BASE_NR_IRQS	8
+#define	TWL4030_PWR_NR_IRQS	8
+#else
+#define	TWL4030_BASE_NR_IRQS	0
+#define	TWL4030_PWR_NR_IRQS	0
+#endif
+#define TWL4030_IRQ_END		(TWL4030_IRQ_BASE + TWL4030_BASE_NR_IRQS)
+#define TWL4030_PWR_IRQ_BASE	TWL4030_IRQ_END
+#define	TWL4030_PWR_IRQ_END	(TWL4030_PWR_IRQ_BASE + TWL4030_PWR_NR_IRQS)
+
+/* External TWL4030 gpio interrupts are optional */
+#define TWL4030_GPIO_IRQ_BASE	TWL4030_PWR_IRQ_END
+#ifdef	CONFIG_GPIO_TWL4030
+#define TWL4030_GPIO_NR_IRQS	18
+#else
+#define	TWL4030_GPIO_NR_IRQS	0
+#endif
+#define TWL4030_GPIO_IRQ_END	(TWL4030_GPIO_IRQ_BASE + TWL4030_GPIO_NR_IRQS)
+
+#define	TWL6030_IRQ_BASE	(OMAP_FPGA_IRQ_END)
+#ifdef CONFIG_TWL4030_CORE
+#define	TWL6030_BASE_NR_IRQS	20
+#else
+#define	TWL6030_BASE_NR_IRQS	0
+#endif
+#define TWL6030_IRQ_END		(TWL6030_IRQ_BASE + TWL6030_BASE_NR_IRQS)
+
+/* Total number of interrupts depends on the enabled blocks above */
+#if (TWL4030_GPIO_IRQ_END > TWL6030_IRQ_END)
+#define TWL_IRQ_END 		TWL4030_GPIO_IRQ_END
+#else
+#define TWL_IRQ_END		TWL6030_IRQ_END
+#endif
+
+#define NR_IRQS			TWL_IRQ_END
+
+#define OMAP_IRQ_BIT(irq)	(1 << ((irq) % 32))
+
+#define INTCPS_NR_MIR_REGS	3
+#define INTCPS_NR_IRQS		96
+
+#ifndef __ASSEMBLY__
+extern void omap_init_irq(void);
+extern int omap_irq_pending(void);
+void omap_intc_save_context(void);
+void omap_intc_restore_context(void);
+#endif
+
+#include <mach/hardware.h>
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/keypad.h
@@ -0,0 +1,45 @@
+/*
+ *  arch/arm/plat-omap/include/mach/keypad.h
+ *
+ *  Copyright (C) 2006 Komal Shah <komal_shah802003@yahoo.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+#ifndef ASMARM_ARCH_KEYPAD_H
+#define ASMARM_ARCH_KEYPAD_H
+
+#warning: Please update the board to use matrix_keypad.h instead
+
+struct omap_kp_platform_data {
+	int rows;
+	int cols;
+	int *keymap;
+	unsigned int keymapsize;
+	unsigned int rep:1;
+	unsigned long delay;
+	unsigned int dbounce:1;
+	/* specific to OMAP242x*/
+	unsigned int *row_gpios;
+	unsigned int *col_gpios;
+};
+
+/* Group (0..3) -- when multiple keys are pressed, only the
+ * keys pressed in the same group are considered as pressed. This is
+ * in order to workaround certain crappy HW designs that produce ghost
+ * keypresses. */
+#define GROUP_0		(0 << 16)
+#define GROUP_1		(1 << 16)
+#define GROUP_2		(2 << 16)
+#define GROUP_3		(3 << 16)
+#define GROUP_MASK	GROUP_3
+
+#define KEY_PERSISTENT		0x00800000
+#define KEYNUM_MASK		0x00EFFFFF
+#define KEY(col, row, val) (((col) << 28) | ((row) << 24) | (val))
+#define PERSISTENT_KEY(col, row) (((col) << 28) | ((row) << 24) | \
+						KEY_PERSISTENT)
+
+#endif
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/lcd_mipid.h
@@ -0,0 +1,29 @@
+#ifndef __LCD_MIPID_H
+#define __LCD_MIPID_H
+
+enum mipid_test_num {
+	MIPID_TEST_RGB_LINES,
+};
+
+enum mipid_test_result {
+	MIPID_TEST_SUCCESS,
+	MIPID_TEST_INVALID,
+	MIPID_TEST_FAILED,
+};
+
+#ifdef __KERNEL__
+
+struct mipid_platform_data {
+	int	nreset_gpio;
+	int	data_lines;
+
+	void	(*shutdown)(struct mipid_platform_data *pdata);
+	void	(*set_bklight_level)(struct mipid_platform_data *pdata,
+				     int level);
+	int	(*get_bklight_level)(struct mipid_platform_data *pdata);
+	int	(*get_bklight_max)(struct mipid_platform_data *pdata);
+};
+
+#endif
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/led.h
@@ -0,0 +1,24 @@
+/*
+ *  arch/arm/plat-omap/include/mach/led.h
+ *
+ *  Copyright (C) 2006 Samsung Electronics
+ *  Kyungmin Park <kyungmin.park@samsung.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+#ifndef ASMARM_ARCH_LED_H
+#define ASMARM_ARCH_LED_H
+
+struct omap_led_config {
+	struct led_classdev	cdev;
+	s16			gpio;
+};
+
+struct omap_led_platform_data {
+	s16			nr_leds;
+	struct omap_led_config	*leds;
+};
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/mailbox.h
@@ -0,0 +1,111 @@
+/* mailbox.h */
+
+#ifndef MAILBOX_H
+#define MAILBOX_H
+
+#include <linux/wait.h>
+#include <linux/workqueue.h>
+#include <linux/blkdev.h>
+#include <linux/interrupt.h>
+
+typedef u32 mbox_msg_t;
+struct omap_mbox;
+
+typedef int __bitwise omap_mbox_irq_t;
+#define IRQ_TX ((__force omap_mbox_irq_t) 1)
+#define IRQ_RX ((__force omap_mbox_irq_t) 2)
+
+typedef int __bitwise omap_mbox_type_t;
+#define OMAP_MBOX_TYPE1 ((__force omap_mbox_type_t) 1)
+#define OMAP_MBOX_TYPE2 ((__force omap_mbox_type_t) 2)
+
+struct omap_mbox_ops {
+	omap_mbox_type_t	type;
+	int		(*startup)(struct omap_mbox *mbox);
+	void		(*shutdown)(struct omap_mbox *mbox);
+	/* fifo */
+	mbox_msg_t	(*fifo_read)(struct omap_mbox *mbox);
+	void		(*fifo_write)(struct omap_mbox *mbox, mbox_msg_t msg);
+	int		(*fifo_empty)(struct omap_mbox *mbox);
+	int		(*fifo_full)(struct omap_mbox *mbox);
+	/* irq */
+	void		(*enable_irq)(struct omap_mbox *mbox,
+						omap_mbox_irq_t irq);
+	void		(*disable_irq)(struct omap_mbox *mbox,
+						omap_mbox_irq_t irq);
+	void		(*ack_irq)(struct omap_mbox *mbox, omap_mbox_irq_t irq);
+	int		(*is_irq)(struct omap_mbox *mbox, omap_mbox_irq_t irq);
+	/* ctx */
+	void		(*save_ctx)(struct omap_mbox *mbox);
+	void		(*restore_ctx)(struct omap_mbox *mbox);
+};
+
+struct omap_mbox_queue {
+	spinlock_t		lock;
+	struct request_queue	*queue;
+	struct work_struct	work;
+	struct tasklet_struct	tasklet;
+	int	(*callback)(void *);
+	struct omap_mbox	*mbox;
+};
+
+struct omap_mbox {
+	char			*name;
+	unsigned int		irq;
+
+	struct omap_mbox_queue	*txq, *rxq;
+
+	struct omap_mbox_ops	*ops;
+
+	mbox_msg_t		seq_snd, seq_rcv;
+
+	struct device		*dev;
+
+	struct omap_mbox	*next;
+	void			*priv;
+
+	void			(*err_notify)(void);
+};
+
+int omap_mbox_msg_send(struct omap_mbox *, mbox_msg_t msg);
+void omap_mbox_init_seq(struct omap_mbox *);
+
+struct omap_mbox *omap_mbox_get(const char *);
+void omap_mbox_put(struct omap_mbox *);
+
+int omap_mbox_register(struct device *parent, struct omap_mbox *);
+int omap_mbox_unregister(struct omap_mbox *);
+
+static inline void omap_mbox_save_ctx(struct omap_mbox *mbox)
+{
+	if (!mbox->ops->save_ctx) {
+		dev_err(mbox->dev, "%s:\tno save\n", __func__);
+		return;
+	}
+
+	mbox->ops->save_ctx(mbox);
+}
+
+static inline void omap_mbox_restore_ctx(struct omap_mbox *mbox)
+{
+	if (!mbox->ops->restore_ctx) {
+		dev_err(mbox->dev, "%s:\tno restore\n", __func__);
+		return;
+	}
+
+	mbox->ops->restore_ctx(mbox);
+}
+
+static inline void omap_mbox_enable_irq(struct omap_mbox *mbox,
+					omap_mbox_irq_t irq)
+{
+	mbox->ops->enable_irq(mbox, irq);
+}
+
+static inline void omap_mbox_disable_irq(struct omap_mbox *mbox,
+					 omap_mbox_irq_t irq)
+{
+	mbox->ops->disable_irq(mbox, irq);
+}
+
+#endif /* MAILBOX_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/mcbsp.h
@@ -0,0 +1,462 @@
+/*
+ * arch/arm/plat-omap/include/mach/mcbsp.h
+ *
+ * Defines for Multi-Channel Buffered Serial Port
+ *
+ * Copyright (C) 2002 RidgeRun, Inc.
+ * Author: Steve Johnson
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
+ *
+ */
+#ifndef __ASM_ARCH_OMAP_MCBSP_H
+#define __ASM_ARCH_OMAP_MCBSP_H
+
+#include <linux/completion.h>
+#include <linux/spinlock.h>
+
+#include <mach/hardware.h>
+#include <plat/clock.h>
+
+#define OMAP7XX_MCBSP1_BASE	0xfffb1000
+#define OMAP7XX_MCBSP2_BASE	0xfffb1800
+
+#define OMAP1510_MCBSP1_BASE	0xe1011800
+#define OMAP1510_MCBSP2_BASE	0xfffb1000
+#define OMAP1510_MCBSP3_BASE	0xe1017000
+
+#define OMAP1610_MCBSP1_BASE	0xe1011800
+#define OMAP1610_MCBSP2_BASE	0xfffb1000
+#define OMAP1610_MCBSP3_BASE	0xe1017000
+
+#define OMAP24XX_MCBSP1_BASE	0x48074000
+#define OMAP24XX_MCBSP2_BASE	0x48076000
+#define OMAP2430_MCBSP3_BASE	0x4808c000
+#define OMAP2430_MCBSP4_BASE	0x4808e000
+#define OMAP2430_MCBSP5_BASE	0x48096000
+
+#define OMAP34XX_MCBSP1_BASE	0x48074000
+#define OMAP34XX_MCBSP2_BASE	0x49022000
+#define OMAP34XX_MCBSP3_BASE	0x49024000
+#define OMAP34XX_MCBSP4_BASE	0x49026000
+#define OMAP34XX_MCBSP5_BASE	0x48096000
+
+#define OMAP44XX_MCBSP1_BASE	0x49022000
+#define OMAP44XX_MCBSP2_BASE	0x49024000
+#define OMAP44XX_MCBSP3_BASE	0x49026000
+#define OMAP44XX_MCBSP4_BASE	0x48074000
+
+#if defined(CONFIG_ARCH_OMAP15XX) || defined(CONFIG_ARCH_OMAP16XX) || defined(CONFIG_ARCH_OMAP730) || defined(CONFIG_ARCH_OMAP850)
+
+#define OMAP_MCBSP_REG_DRR2	0x00
+#define OMAP_MCBSP_REG_DRR1	0x02
+#define OMAP_MCBSP_REG_DXR2	0x04
+#define OMAP_MCBSP_REG_DXR1	0x06
+#define OMAP_MCBSP_REG_SPCR2	0x08
+#define OMAP_MCBSP_REG_SPCR1	0x0a
+#define OMAP_MCBSP_REG_RCR2	0x0c
+#define OMAP_MCBSP_REG_RCR1	0x0e
+#define OMAP_MCBSP_REG_XCR2	0x10
+#define OMAP_MCBSP_REG_XCR1	0x12
+#define OMAP_MCBSP_REG_SRGR2	0x14
+#define OMAP_MCBSP_REG_SRGR1	0x16
+#define OMAP_MCBSP_REG_MCR2	0x18
+#define OMAP_MCBSP_REG_MCR1	0x1a
+#define OMAP_MCBSP_REG_RCERA	0x1c
+#define OMAP_MCBSP_REG_RCERB	0x1e
+#define OMAP_MCBSP_REG_XCERA	0x20
+#define OMAP_MCBSP_REG_XCERB	0x22
+#define OMAP_MCBSP_REG_PCR0	0x24
+#define OMAP_MCBSP_REG_RCERC	0x26
+#define OMAP_MCBSP_REG_RCERD	0x28
+#define OMAP_MCBSP_REG_XCERC	0x2A
+#define OMAP_MCBSP_REG_XCERD	0x2C
+#define OMAP_MCBSP_REG_RCERE	0x2E
+#define OMAP_MCBSP_REG_RCERF	0x30
+#define OMAP_MCBSP_REG_XCERE	0x32
+#define OMAP_MCBSP_REG_XCERF	0x34
+#define OMAP_MCBSP_REG_RCERG	0x36
+#define OMAP_MCBSP_REG_RCERH	0x38
+#define OMAP_MCBSP_REG_XCERG	0x3A
+#define OMAP_MCBSP_REG_XCERH	0x3C
+
+/* Dummy defines, these are not available on omap1 */
+#define OMAP_MCBSP_REG_XCCR	0x00
+#define OMAP_MCBSP_REG_RCCR	0x00
+
+#define AUDIO_MCBSP_DATAWRITE	(OMAP1510_MCBSP1_BASE + OMAP_MCBSP_REG_DXR1)
+#define AUDIO_MCBSP_DATAREAD	(OMAP1510_MCBSP1_BASE + OMAP_MCBSP_REG_DRR1)
+
+#define AUDIO_MCBSP		OMAP_MCBSP1
+#define AUDIO_DMA_TX		OMAP_DMA_MCBSP1_TX
+#define AUDIO_DMA_RX		OMAP_DMA_MCBSP1_RX
+
+#elif defined(CONFIG_ARCH_OMAP24XX) || defined(CONFIG_ARCH_OMAP34XX) || \
+	defined(CONFIG_ARCH_OMAP4)
+
+#define OMAP_MCBSP_REG_DRR2	0x00
+#define OMAP_MCBSP_REG_DRR1	0x04
+#define OMAP_MCBSP_REG_DXR2	0x08
+#define OMAP_MCBSP_REG_DXR1	0x0C
+#define OMAP_MCBSP_REG_DRR	0x00
+#define OMAP_MCBSP_REG_DXR	0x08
+#define OMAP_MCBSP_REG_SPCR2	0x10
+#define OMAP_MCBSP_REG_SPCR1	0x14
+#define OMAP_MCBSP_REG_RCR2	0x18
+#define OMAP_MCBSP_REG_RCR1	0x1C
+#define OMAP_MCBSP_REG_XCR2	0x20
+#define OMAP_MCBSP_REG_XCR1	0x24
+#define OMAP_MCBSP_REG_SRGR2	0x28
+#define OMAP_MCBSP_REG_SRGR1	0x2C
+#define OMAP_MCBSP_REG_MCR2	0x30
+#define OMAP_MCBSP_REG_MCR1	0x34
+#define OMAP_MCBSP_REG_RCERA	0x38
+#define OMAP_MCBSP_REG_RCERB	0x3C
+#define OMAP_MCBSP_REG_XCERA	0x40
+#define OMAP_MCBSP_REG_XCERB	0x44
+#define OMAP_MCBSP_REG_PCR0	0x48
+#define OMAP_MCBSP_REG_RCERC	0x4C
+#define OMAP_MCBSP_REG_RCERD	0x50
+#define OMAP_MCBSP_REG_XCERC	0x54
+#define OMAP_MCBSP_REG_XCERD	0x58
+#define OMAP_MCBSP_REG_RCERE	0x5C
+#define OMAP_MCBSP_REG_RCERF	0x60
+#define OMAP_MCBSP_REG_XCERE	0x64
+#define OMAP_MCBSP_REG_XCERF	0x68
+#define OMAP_MCBSP_REG_RCERG	0x6C
+#define OMAP_MCBSP_REG_RCERH	0x70
+#define OMAP_MCBSP_REG_XCERG	0x74
+#define OMAP_MCBSP_REG_XCERH	0x78
+#define OMAP_MCBSP_REG_SYSCON	0x8C
+#define OMAP_MCBSP_REG_THRSH2	0x90
+#define OMAP_MCBSP_REG_THRSH1	0x94
+#define OMAP_MCBSP_REG_IRQST	0xA0
+#define OMAP_MCBSP_REG_IRQEN	0xA4
+#define OMAP_MCBSP_REG_WAKEUPEN	0xA8
+#define OMAP_MCBSP_REG_XCCR	0xAC
+#define OMAP_MCBSP_REG_RCCR	0xB0
+
+#define AUDIO_MCBSP_DATAWRITE	(OMAP24XX_MCBSP2_BASE + OMAP_MCBSP_REG_DXR1)
+#define AUDIO_MCBSP_DATAREAD	(OMAP24XX_MCBSP2_BASE + OMAP_MCBSP_REG_DRR1)
+
+#define AUDIO_MCBSP		OMAP_MCBSP2
+#define AUDIO_DMA_TX		OMAP24XX_DMA_MCBSP2_TX
+#define AUDIO_DMA_RX		OMAP24XX_DMA_MCBSP2_RX
+
+#endif
+
+/************************** McBSP SPCR1 bit definitions ***********************/
+#define RRST			0x0001
+#define RRDY			0x0002
+#define RFULL			0x0004
+#define RSYNC_ERR		0x0008
+#define RINTM(value)		((value)<<4)	/* bits 4:5 */
+#define ABIS			0x0040
+#define DXENA			0x0080
+#define CLKSTP(value)		((value)<<11)	/* bits 11:12 */
+#define RJUST(value)		((value)<<13)	/* bits 13:14 */
+#define ALB			0x8000
+#define DLB			0x8000
+
+/************************** McBSP SPCR2 bit definitions ***********************/
+#define XRST		0x0001
+#define XRDY		0x0002
+#define XEMPTY		0x0004
+#define XSYNC_ERR	0x0008
+#define XINTM(value)	((value)<<4)		/* bits 4:5 */
+#define GRST		0x0040
+#define FRST		0x0080
+#define SOFT		0x0100
+#define FREE		0x0200
+
+/************************** McBSP PCR bit definitions *************************/
+#define CLKRP		0x0001
+#define CLKXP		0x0002
+#define FSRP		0x0004
+#define FSXP		0x0008
+#define DR_STAT		0x0010
+#define DX_STAT		0x0020
+#define CLKS_STAT	0x0040
+#define SCLKME		0x0080
+#define CLKRM		0x0100
+#define CLKXM		0x0200
+#define FSRM		0x0400
+#define FSXM		0x0800
+#define RIOEN		0x1000
+#define XIOEN		0x2000
+#define IDLE_EN		0x4000
+
+/************************** McBSP RCR1 bit definitions ************************/
+#define RWDLEN1(value)		((value)<<5)	/* Bits 5:7 */
+#define RFRLEN1(value)		((value)<<8)	/* Bits 8:14 */
+
+/************************** McBSP XCR1 bit definitions ************************/
+#define XWDLEN1(value)		((value)<<5)	/* Bits 5:7 */
+#define XFRLEN1(value)		((value)<<8)	/* Bits 8:14 */
+
+/*************************** McBSP RCR2 bit definitions ***********************/
+#define RDATDLY(value)		(value)		/* Bits 0:1 */
+#define RFIG			0x0004
+#define RCOMPAND(value)		((value)<<3)	/* Bits 3:4 */
+#define RWDLEN2(value)		((value)<<5)	/* Bits 5:7 */
+#define RFRLEN2(value)		((value)<<8)	/* Bits 8:14 */
+#define RPHASE			0x8000
+
+/*************************** McBSP XCR2 bit definitions ***********************/
+#define XDATDLY(value)		(value)		/* Bits 0:1 */
+#define XFIG			0x0004
+#define XCOMPAND(value)		((value)<<3)	/* Bits 3:4 */
+#define XWDLEN2(value)		((value)<<5)	/* Bits 5:7 */
+#define XFRLEN2(value)		((value)<<8)	/* Bits 8:14 */
+#define XPHASE			0x8000
+
+/************************* McBSP SRGR1 bit definitions ************************/
+#define CLKGDV(value)		(value)		/* Bits 0:7 */
+#define FWID(value)		((value)<<8)	/* Bits 8:15 */
+
+/************************* McBSP SRGR2 bit definitions ************************/
+#define FPER(value)		(value)		/* Bits 0:11 */
+#define FSGM			0x1000
+#define CLKSM			0x2000
+#define CLKSP			0x4000
+#define GSYNC			0x8000
+
+/************************* McBSP MCR1 bit definitions *************************/
+#define RMCM			0x0001
+#define RCBLK(value)		((value)<<2)	/* Bits 2:4 */
+#define RPABLK(value)		((value)<<5)	/* Bits 5:6 */
+#define RPBBLK(value)		((value)<<7)	/* Bits 7:8 */
+
+/************************* McBSP MCR2 bit definitions *************************/
+#define XMCM(value)		(value)		/* Bits 0:1 */
+#define XCBLK(value)		((value)<<2)	/* Bits 2:4 */
+#define XPABLK(value)		((value)<<5)	/* Bits 5:6 */
+#define XPBBLK(value)		((value)<<7)	/* Bits 7:8 */
+
+/*********************** McBSP XCCR bit definitions *************************/
+#define EXTCLKGATE		0x8000
+#define PPCONNECT		0x4000
+#define DXENDLY(value)		((value)<<12)	/* Bits 12:13 */
+#define XFULL_CYCLE		0x0800
+#define DILB			0x0020
+#define XDMAEN			0x0008
+#define XDISABLE		0x0001
+
+/********************** McBSP RCCR bit definitions *************************/
+#define RFULL_CYCLE		0x0800
+#define RDMAEN			0x0008
+#define RDISABLE		0x0001
+
+/********************** McBSP SYSCONFIG bit definitions ********************/
+#define CLOCKACTIVITY(value)	((value)<<8)
+#define SIDLEMODE(value)	((value)<<3)
+#define ENAWAKEUP		0x0004
+#define SOFTRST			0x0002
+
+/********************** McBSP DMA operating modes **************************/
+#define MCBSP_DMA_MODE_ELEMENT		0
+#define MCBSP_DMA_MODE_THRESHOLD	1
+#define MCBSP_DMA_MODE_FRAME		2
+
+/********************** McBSP WAKEUPEN bit definitions *********************/
+#define XEMPTYEOFEN		0x4000
+#define XRDYEN			0x0400
+#define XEOFEN			0x0200
+#define XFSXEN			0x0100
+#define XSYNCERREN		0x0080
+#define RRDYEN			0x0008
+#define REOFEN			0x0004
+#define RFSREN			0x0002
+#define RSYNCERREN		0x0001
+
+/* we don't do multichannel for now */
+struct omap_mcbsp_reg_cfg {
+	u16 spcr2;
+	u16 spcr1;
+	u16 rcr2;
+	u16 rcr1;
+	u16 xcr2;
+	u16 xcr1;
+	u16 srgr2;
+	u16 srgr1;
+	u16 mcr2;
+	u16 mcr1;
+	u16 pcr0;
+	u16 rcerc;
+	u16 rcerd;
+	u16 xcerc;
+	u16 xcerd;
+	u16 rcere;
+	u16 rcerf;
+	u16 xcere;
+	u16 xcerf;
+	u16 rcerg;
+	u16 rcerh;
+	u16 xcerg;
+	u16 xcerh;
+	u16 xccr;
+	u16 rccr;
+};
+
+typedef enum {
+	OMAP_MCBSP1 = 0,
+	OMAP_MCBSP2,
+	OMAP_MCBSP3,
+	OMAP_MCBSP4,
+	OMAP_MCBSP5
+} omap_mcbsp_id;
+
+typedef int __bitwise omap_mcbsp_io_type_t;
+#define OMAP_MCBSP_IRQ_IO ((__force omap_mcbsp_io_type_t) 1)
+#define OMAP_MCBSP_POLL_IO ((__force omap_mcbsp_io_type_t) 2)
+
+typedef enum {
+	OMAP_MCBSP_WORD_8 = 0,
+	OMAP_MCBSP_WORD_12,
+	OMAP_MCBSP_WORD_16,
+	OMAP_MCBSP_WORD_20,
+	OMAP_MCBSP_WORD_24,
+	OMAP_MCBSP_WORD_32,
+} omap_mcbsp_word_length;
+
+typedef enum {
+	OMAP_MCBSP_CLK_RISING = 0,
+	OMAP_MCBSP_CLK_FALLING,
+} omap_mcbsp_clk_polarity;
+
+typedef enum {
+	OMAP_MCBSP_FS_ACTIVE_HIGH = 0,
+	OMAP_MCBSP_FS_ACTIVE_LOW,
+} omap_mcbsp_fs_polarity;
+
+typedef enum {
+	OMAP_MCBSP_CLK_STP_MODE_NO_DELAY = 0,
+	OMAP_MCBSP_CLK_STP_MODE_DELAY,
+} omap_mcbsp_clk_stp_mode;
+
+
+/******* SPI specific mode **********/
+typedef enum {
+	OMAP_MCBSP_SPI_MASTER = 0,
+	OMAP_MCBSP_SPI_SLAVE,
+} omap_mcbsp_spi_mode;
+
+struct omap_mcbsp_spi_cfg {
+	omap_mcbsp_spi_mode		spi_mode;
+	omap_mcbsp_clk_polarity		rx_clock_polarity;
+	omap_mcbsp_clk_polarity		tx_clock_polarity;
+	omap_mcbsp_fs_polarity		fsx_polarity;
+	u8				clk_div;
+	omap_mcbsp_clk_stp_mode		clk_stp_mode;
+	omap_mcbsp_word_length		word_length;
+};
+
+/* Platform specific configuration */
+struct omap_mcbsp_ops {
+	void (*request)(unsigned int);
+	void (*free)(unsigned int);
+};
+
+struct omap_mcbsp_platform_data {
+	unsigned long phys_base;
+	u8 dma_rx_sync, dma_tx_sync;
+	u16 rx_irq, tx_irq;
+	struct omap_mcbsp_ops *ops;
+#ifdef CONFIG_ARCH_OMAP34XX
+	u16 buffer_size;
+#endif
+};
+
+struct omap_mcbsp {
+	struct device *dev;
+	unsigned long phys_base;
+	void __iomem *io_base;
+	u8 id;
+	u8 free;
+	omap_mcbsp_word_length rx_word_length;
+	omap_mcbsp_word_length tx_word_length;
+
+	omap_mcbsp_io_type_t io_type; /* IRQ or poll */
+	/* IRQ based TX/RX */
+	int rx_irq;
+	int tx_irq;
+
+	/* DMA stuff */
+	u8 dma_rx_sync;
+	short dma_rx_lch;
+	u8 dma_tx_sync;
+	short dma_tx_lch;
+
+	/* Completion queues */
+	struct completion tx_irq_completion;
+	struct completion rx_irq_completion;
+	struct completion tx_dma_completion;
+	struct completion rx_dma_completion;
+
+	/* Protect the field .free, while checking if the mcbsp is in use */
+	spinlock_t lock;
+	struct omap_mcbsp_platform_data *pdata;
+	struct clk *iclk;
+	struct clk *fclk;
+#ifdef CONFIG_ARCH_OMAP34XX
+	int dma_op_mode;
+	u16 max_tx_thres;
+	u16 max_rx_thres;
+#endif
+};
+extern struct omap_mcbsp **mcbsp_ptr;
+extern int omap_mcbsp_count;
+
+int omap_mcbsp_init(void);
+void omap_mcbsp_register_board_cfg(struct omap_mcbsp_platform_data *config,
+					int size);
+void omap_mcbsp_config(unsigned int id, const struct omap_mcbsp_reg_cfg * config);
+#ifdef CONFIG_ARCH_OMAP34XX
+void omap_mcbsp_set_tx_threshold(unsigned int id, u16 threshold);
+void omap_mcbsp_set_rx_threshold(unsigned int id, u16 threshold);
+u16 omap_mcbsp_get_max_tx_threshold(unsigned int id);
+u16 omap_mcbsp_get_max_rx_threshold(unsigned int id);
+int omap_mcbsp_get_dma_op_mode(unsigned int id);
+#else
+static inline void omap_mcbsp_set_tx_threshold(unsigned int id, u16 threshold)
+{ }
+static inline void omap_mcbsp_set_rx_threshold(unsigned int id, u16 threshold)
+{ }
+static inline u16 omap_mcbsp_get_max_tx_threshold(unsigned int id) { return 0; }
+static inline u16 omap_mcbsp_get_max_rx_threshold(unsigned int id) { return 0; }
+static inline int omap_mcbsp_get_dma_op_mode(unsigned int id) { return 0; }
+#endif
+int omap_mcbsp_request(unsigned int id);
+void omap_mcbsp_free(unsigned int id);
+void omap_mcbsp_start(unsigned int id, int tx, int rx);
+void omap_mcbsp_stop(unsigned int id, int tx, int rx);
+void omap_mcbsp_xmit_word(unsigned int id, u32 word);
+u32 omap_mcbsp_recv_word(unsigned int id);
+
+int omap_mcbsp_xmit_buffer(unsigned int id, dma_addr_t buffer, unsigned int length);
+int omap_mcbsp_recv_buffer(unsigned int id, dma_addr_t buffer, unsigned int length);
+int omap_mcbsp_spi_master_xmit_word_poll(unsigned int id, u32 word);
+int omap_mcbsp_spi_master_recv_word_poll(unsigned int id, u32 * word);
+
+
+/* SPI specific API */
+void omap_mcbsp_set_spi_mode(unsigned int id, const struct omap_mcbsp_spi_cfg * spi_cfg);
+
+/* Polled read/write functions */
+int omap_mcbsp_pollread(unsigned int id, u16 * buf);
+int omap_mcbsp_pollwrite(unsigned int id, u16 buf);
+int omap_mcbsp_set_io_type(unsigned int id, omap_mcbsp_io_type_t io_type);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/mcspi.h
@@ -0,0 +1,15 @@
+#ifndef _OMAP2_MCSPI_H
+#define _OMAP2_MCSPI_H
+
+struct omap2_mcspi_platform_config {
+	unsigned short	num_cs;
+};
+
+struct omap2_mcspi_device_config {
+	unsigned turbo_mode:1;
+
+	/* Do we want one channel enabled at the same time? */
+	unsigned single_channel:1;
+};
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/memory.h
@@ -0,0 +1,103 @@
+/*
+ * arch/arm/plat-omap/include/mach/memory.h
+ *
+ * Memory map for OMAP-1510 and 1610
+ *
+ * Copyright (C) 2000 RidgeRun, Inc.
+ * Author: Greg Lonnon <glonnon@ridgerun.com>
+ *
+ * This file was derived from arch/arm/mach-intergrator/include/mach/memory.h
+ * Copyright (C) 1999 ARM Limited
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_MEMORY_H
+#define __ASM_ARCH_MEMORY_H
+
+/*
+ * Physical DRAM offset.
+ */
+#if defined(CONFIG_ARCH_OMAP1)
+#define PHYS_OFFSET		UL(0x10000000)
+#elif defined(CONFIG_ARCH_OMAP2) || defined(CONFIG_ARCH_OMAP3) || \
+			defined(CONFIG_ARCH_OMAP4)
+#define PHYS_OFFSET		UL(0x80000000)
+#endif
+
+/*
+ * Bus address is physical address, except for OMAP-1510 Local Bus.
+ * OMAP-1510 bus address is translated into a Local Bus address if the
+ * OMAP bus type is lbus. We do the address translation based on the
+ * device overriding the defaults used in the dma-mapping API.
+ * Note that the is_lbus_device() test is not very efficient on 1510
+ * because of the strncmp().
+ */
+#ifdef CONFIG_ARCH_OMAP15XX
+
+/*
+ * OMAP-1510 Local Bus address offset
+ */
+#define OMAP1510_LB_OFFSET	UL(0x30000000)
+
+#define virt_to_lbus(x)		((x) - PAGE_OFFSET + OMAP1510_LB_OFFSET)
+#define lbus_to_virt(x)		((x) - OMAP1510_LB_OFFSET + PAGE_OFFSET)
+#define is_lbus_device(dev)	(cpu_is_omap15xx() && dev && (strncmp(dev_name(dev), "ohci", 4) == 0))
+
+#define __arch_page_to_dma(dev, page)	\
+	({ dma_addr_t __dma = page_to_phys(page); \
+	   if (is_lbus_device(dev)) \
+		__dma = __dma - PHYS_OFFSET + OMAP1510_LB_OFFSET; \
+	   __dma; })
+
+#define __arch_dma_to_page(dev, addr)	\
+	({ dma_addr_t __dma = addr;				\
+	   if (is_lbus_device(dev))				\
+		__dma += PHYS_OFFSET - OMAP1510_LB_OFFSET;	\
+	   phys_to_page(__dma);					\
+	})
+
+#define __arch_dma_to_virt(dev, addr)	({ (void *) (is_lbus_device(dev) ? \
+						lbus_to_virt(addr) : \
+						__phys_to_virt(addr)); })
+
+#define __arch_virt_to_dma(dev, addr)	({ unsigned long __addr = (unsigned long)(addr); \
+					   (dma_addr_t) (is_lbus_device(dev) ? \
+						virt_to_lbus(__addr) : \
+						__virt_to_phys(__addr)); })
+
+#endif	/* CONFIG_ARCH_OMAP15XX */
+
+/* Override the ARM default */
+#ifdef CONFIG_FB_OMAP_CONSISTENT_DMA_SIZE
+
+#if (CONFIG_FB_OMAP_CONSISTENT_DMA_SIZE == 0)
+#undef CONFIG_FB_OMAP_CONSISTENT_DMA_SIZE
+#define CONFIG_FB_OMAP_CONSISTENT_DMA_SIZE 2
+#endif
+
+#define CONSISTENT_DMA_SIZE \
+	(((CONFIG_FB_OMAP_CONSISTENT_DMA_SIZE + 1) & ~1) * 1024 * 1024)
+
+#endif
+
+#endif
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/menelaus.h
@@ -0,0 +1,49 @@
+/*
+ * arch/arm/plat-omap/include/mach/menelaus.h
+ *
+ * Functions to access Menelaus power management chip
+ */
+
+#ifndef __ASM_ARCH_MENELAUS_H
+#define __ASM_ARCH_MENELAUS_H
+
+struct device;
+
+struct menelaus_platform_data {
+	int (* late_init)(struct device *dev);
+};
+
+extern int menelaus_register_mmc_callback(void (*callback)(void *data, u8 card_mask),
+					  void *data);
+extern void menelaus_unregister_mmc_callback(void);
+extern int menelaus_set_mmc_opendrain(int slot, int enable);
+extern int menelaus_set_mmc_slot(int slot, int enable, int power, int cd_on);
+
+extern int menelaus_set_vmem(unsigned int mV);
+extern int menelaus_set_vio(unsigned int mV);
+extern int menelaus_set_vmmc(unsigned int mV);
+extern int menelaus_set_vaux(unsigned int mV);
+extern int menelaus_set_vdcdc(int dcdc, unsigned int mV);
+extern int menelaus_set_slot_sel(int enable);
+extern int menelaus_get_slot_pin_states(void);
+extern int menelaus_set_vcore_sw(unsigned int mV);
+extern int menelaus_set_vcore_hw(unsigned int roof_mV, unsigned int floor_mV);
+
+#define EN_VPLL_SLEEP	(1 << 7)
+#define EN_VMMC_SLEEP	(1 << 6)
+#define EN_VAUX_SLEEP	(1 << 5)
+#define EN_VIO_SLEEP	(1 << 4)
+#define EN_VMEM_SLEEP	(1 << 3)
+#define EN_DC3_SLEEP	(1 << 2)
+#define EN_DC2_SLEEP	(1 << 1)
+#define EN_VC_SLEEP	(1 << 0)
+
+extern int menelaus_set_regulator_sleep(int enable, u32 val);
+
+#if defined(CONFIG_ARCH_OMAP24XX) && defined(CONFIG_MENELAUS)
+#define omap_has_menelaus()	1
+#else
+#define omap_has_menelaus()	0
+#endif
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/mmc.h
@@ -0,0 +1,157 @@
+/*
+ * MMC definitions for OMAP2
+ *
+ * Copyright (C) 2006 Nokia Corporation
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __OMAP2_MMC_H
+#define __OMAP2_MMC_H
+
+#include <linux/types.h>
+#include <linux/device.h>
+#include <linux/mmc/host.h>
+
+#include <plat/board.h>
+
+#define OMAP15XX_NR_MMC		1
+#define OMAP16XX_NR_MMC		2
+#define OMAP1_MMC_SIZE		0x080
+#define OMAP1_MMC1_BASE		0xfffb7800
+#define OMAP1_MMC2_BASE		0xfffb7c00	/* omap16xx only */
+
+#define OMAP24XX_NR_MMC		2
+#define OMAP34XX_NR_MMC		3
+#define OMAP44XX_NR_MMC		5
+#define OMAP2420_MMC_SIZE	OMAP1_MMC_SIZE
+#define OMAP3_HSMMC_SIZE	0x200
+#define OMAP4_HSMMC_SIZE	0x1000
+#define OMAP2_MMC1_BASE		0x4809c000
+#define OMAP2_MMC2_BASE		0x480b4000
+#define OMAP3_MMC3_BASE		0x480ad000
+#define OMAP4_MMC4_BASE		0x480d1000
+#define OMAP4_MMC5_BASE		0x480d5000
+#define OMAP4_MMC_REG_OFFSET	0x100
+#define HSMMC5			(1 << 4)
+#define HSMMC4			(1 << 3)
+#define HSMMC3			(1 << 2)
+#define HSMMC2			(1 << 1)
+#define HSMMC1			(1 << 0)
+
+#define OMAP_MMC_MAX_SLOTS	2
+
+struct omap_mmc_platform_data {
+	/* back-link to device */
+	struct device *dev;
+
+	/* number of slots per controller */
+	unsigned nr_slots:2;
+
+	/* set if your board has components or wiring that limits the
+	 * maximum frequency on the MMC bus */
+	unsigned int max_freq;
+
+	/* switch the bus to a new slot */
+	int (* switch_slot)(struct device *dev, int slot);
+	/* initialize board-specific MMC functionality, can be NULL if
+	 * not supported */
+	int (* init)(struct device *dev);
+	void (* cleanup)(struct device *dev);
+	void (* shutdown)(struct device *dev);
+
+	/* To handle board related suspend/resume functionality for MMC */
+	int (*suspend)(struct device *dev, int slot);
+	int (*resume)(struct device *dev, int slot);
+
+	/* Return context loss count due to PM states changing */
+	int (*get_context_loss_count)(struct device *dev);
+
+	u64 dma_mask;
+
+	struct omap_mmc_slot_data {
+
+		/* 4 wire signaling is optional, and is used for SD/SDIO/HSMMC;
+		 * 8 wire signaling is also optional, and is used with HSMMC
+		 */
+		u8 wires;
+
+		/*
+		 * nomux means "standard" muxing is wrong on this board, and
+		 * that board-specific code handled it before common init logic.
+		 */
+		unsigned nomux:1;
+
+		/* switch pin can be for card detect (default) or card cover */
+		unsigned cover:1;
+
+		/* use the internal clock */
+		unsigned internal_clock:1;
+
+		/* nonremovable e.g. eMMC */
+		unsigned nonremovable:1;
+
+		/* Try to sleep or power off when possible */
+		unsigned power_saving:1;
+
+		int switch_pin;			/* gpio (card detect) */
+		int gpio_wp;			/* gpio (write protect) */
+
+		int (* set_bus_mode)(struct device *dev, int slot, int bus_mode);
+		int (* set_power)(struct device *dev, int slot, int power_on, int vdd);
+		int (* get_ro)(struct device *dev, int slot);
+		int (*set_sleep)(struct device *dev, int slot, int sleep,
+				 int vdd, int cardsleep);
+
+		/* return MMC cover switch state, can be NULL if not supported.
+		 *
+		 * possible return values:
+		 *   0 - closed
+		 *   1 - open
+		 */
+		int (* get_cover_state)(struct device *dev, int slot);
+
+		const char *name;
+		u32 ocr_mask;
+
+		/* Card detection IRQs */
+		int card_detect_irq;
+		int (* card_detect)(int irq);
+
+		unsigned int ban_openended:1;
+
+	} slots[OMAP_MMC_MAX_SLOTS];
+};
+
+/* called from board-specific card detection service routine */
+extern void omap_mmc_notify_cover_event(struct device *dev, int slot, int is_closed);
+
+#if	defined(CONFIG_MMC_OMAP) || defined(CONFIG_MMC_OMAP_MODULE) || \
+	defined(CONFIG_MMC_OMAP_HS) || defined(CONFIG_MMC_OMAP_HS_MODULE)
+void omap1_init_mmc(struct omap_mmc_platform_data **mmc_data,
+				int nr_controllers);
+void omap2_init_mmc(struct omap_mmc_platform_data **mmc_data,
+				int nr_controllers);
+int omap_mmc_add(const char *name, int id, unsigned long base,
+				unsigned long size, unsigned int irq,
+				struct omap_mmc_platform_data *data);
+#else
+static inline void omap1_init_mmc(struct omap_mmc_platform_data **mmc_data,
+				int nr_controllers)
+{
+}
+static inline void omap2_init_mmc(struct omap_mmc_platform_data **mmc_data,
+				int nr_controllers)
+{
+}
+static inline int omap_mmc_add(const char *name, int id, unsigned long base,
+				unsigned long size, unsigned int irq,
+				struct omap_mmc_platform_data *data)
+{
+	return 0;
+}
+
+#endif
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/mux.h
@@ -0,0 +1,662 @@
+/*
+ * arch/arm/plat-omap/include/mach/mux.h
+ *
+ * Table of the Omap register configurations for the FUNC_MUX and
+ * PULL_DWN combinations.
+ *
+ * Copyright (C) 2004 - 2008 Texas Instruments Inc.
+ * Copyright (C) 2003 - 2008 Nokia Corporation
+ *
+ * Written by Tony Lindgren
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
+ *
+ * NOTE: Please use the following naming style for new pin entries.
+ *	 For example, W8_1610_MMC2_DAT0, where:
+ *	 - W8	     = ball
+ *	 - 1610	     = 1510 or 1610, none if common for both 1510 and 1610
+ *	 - MMC2_DAT0 = function
+ */
+
+#ifndef __ASM_ARCH_MUX_H
+#define __ASM_ARCH_MUX_H
+
+#define PU_PD_SEL_NA		0	/* No pu_pd reg available */
+#define PULL_DWN_CTRL_NA	0	/* No pull-down control needed */
+
+#ifdef	CONFIG_OMAP_MUX_DEBUG
+#define MUX_REG(reg, mode_offset, mode) .mux_reg_name = "FUNC_MUX_CTRL_"#reg, \
+					.mux_reg = FUNC_MUX_CTRL_##reg, \
+					.mask_offset = mode_offset, \
+					.mask = mode,
+
+#define PULL_REG(reg, bit, status)	.pull_name = "PULL_DWN_CTRL_"#reg, \
+					.pull_reg = PULL_DWN_CTRL_##reg, \
+					.pull_bit = bit, \
+					.pull_val = status,
+
+#define PU_PD_REG(reg, status)		.pu_pd_name = "PU_PD_SEL_"#reg, \
+					.pu_pd_reg = PU_PD_SEL_##reg, \
+					.pu_pd_val = status,
+
+#define MUX_REG_7XX(reg, mode_offset, mode) .mux_reg_name = "OMAP7XX_IO_CONF_"#reg, \
+					.mux_reg = OMAP7XX_IO_CONF_##reg, \
+					.mask_offset = mode_offset, \
+					.mask = mode,
+
+#define PULL_REG_7XX(reg, bit, status)	.pull_name = "OMAP7XX_IO_CONF_"#reg, \
+					.pull_reg = OMAP7XX_IO_CONF_##reg, \
+					.pull_bit = bit, \
+					.pull_val = status,
+
+#else
+
+#define MUX_REG(reg, mode_offset, mode) .mux_reg = FUNC_MUX_CTRL_##reg, \
+					.mask_offset = mode_offset, \
+					.mask = mode,
+
+#define PULL_REG(reg, bit, status)	.pull_reg = PULL_DWN_CTRL_##reg, \
+					.pull_bit = bit, \
+					.pull_val = status,
+
+#define PU_PD_REG(reg, status)		.pu_pd_reg = PU_PD_SEL_##reg, \
+					.pu_pd_val = status,
+
+#define MUX_REG_7XX(reg, mode_offset, mode) \
+					.mux_reg = OMAP7XX_IO_CONF_##reg, \
+					.mask_offset = mode_offset, \
+					.mask = mode,
+
+#define PULL_REG_7XX(reg, bit, status)	.pull_reg = OMAP7XX_IO_CONF_##reg, \
+					.pull_bit = bit, \
+					.pull_val = status,
+
+#endif /* CONFIG_OMAP_MUX_DEBUG */
+
+#define MUX_CFG(desc, mux_reg, mode_offset, mode,	\
+		pull_reg, pull_bit, pull_status,	\
+		pu_pd_reg, pu_pd_status, debug_status)	\
+{							\
+	.name =	 desc,					\
+	.debug = debug_status,				\
+	MUX_REG(mux_reg, mode_offset, mode)		\
+	PULL_REG(pull_reg, pull_bit, pull_status)	\
+	PU_PD_REG(pu_pd_reg, pu_pd_status)		\
+},
+
+
+/*
+ * OMAP730/850 has a slightly different config for the pin mux.
+ * - config regs are the OMAP7XX_IO_CONF_x regs (see omap730.h) regs and
+ *   not the FUNC_MUX_CTRL_x regs from hardware.h
+ * - for pull-up/down, only has one enable bit which is is in the same register
+ *   as mux config
+ */
+#define MUX_CFG_7XX(desc, mux_reg, mode_offset, mode,	\
+		   pull_bit, pull_status, debug_status)\
+{							\
+	.name =	 desc,					\
+	.debug = debug_status,				\
+	MUX_REG_7XX(mux_reg, mode_offset, mode)		\
+	PULL_REG_7XX(mux_reg, pull_bit, pull_status)	\
+	PU_PD_REG(NA, 0)		\
+},
+
+#define MUX_CFG_24XX(desc, reg_offset, mode,			\
+				pull_en, pull_mode, dbg)	\
+{								\
+	.name		= desc,					\
+	.debug		= dbg,					\
+	.mux_reg	= reg_offset,				\
+	.mask		= mode,					\
+	.pull_val	= pull_en,				\
+	.pu_pd_val	= pull_mode,				\
+},
+
+/* 24xx/34xx mux bit defines */
+#define OMAP2_PULL_ENA		(1 << 3)
+#define OMAP2_PULL_UP		(1 << 4)
+#define OMAP2_ALTELECTRICALSEL	(1 << 5)
+
+struct pin_config {
+	char 			*name;
+	const unsigned int 	mux_reg;
+	unsigned char		debug;
+
+#if	defined(CONFIG_ARCH_OMAP1) || defined(CONFIG_ARCH_OMAP24XX)
+	const unsigned char mask_offset;
+	const unsigned char mask;
+
+	const char *pull_name;
+	const unsigned int pull_reg;
+	const unsigned char pull_val;
+	const unsigned char pull_bit;
+
+	const char *pu_pd_name;
+	const unsigned int pu_pd_reg;
+	const unsigned char pu_pd_val;
+#endif
+
+#if	defined(CONFIG_OMAP_MUX_DEBUG) || defined(CONFIG_OMAP_MUX_WARNINGS)
+	const char *mux_reg_name;
+#endif
+
+};
+
+enum omap7xx_index {
+	/* OMAP 730 keyboard */
+	E2_7XX_KBR0,
+	J7_7XX_KBR1,
+	E1_7XX_KBR2,
+	F3_7XX_KBR3,
+	D2_7XX_KBR4,
+	C2_7XX_KBC0,
+	D3_7XX_KBC1,
+	E4_7XX_KBC2,
+	F4_7XX_KBC3,
+	E3_7XX_KBC4,
+
+	/* USB */
+	AA17_7XX_USB_DM,
+	W16_7XX_USB_PU_EN,
+	W17_7XX_USB_VBUSI,
+	W18_7XX_USB_DMCK_OUT,
+	W19_7XX_USB_DCRST,
+
+	/* MMC */
+	MMC_7XX_CMD,
+	MMC_7XX_CLK,
+	MMC_7XX_DAT0,
+
+	/* I2C */
+	I2C_7XX_SCL,
+	I2C_7XX_SDA,
+};
+
+enum omap1xxx_index {
+	/* UART1 (BT_UART_GATING)*/
+	UART1_TX = 0,
+	UART1_RTS,
+
+	/* UART2 (COM_UART_GATING)*/
+	UART2_TX,
+	UART2_RX,
+	UART2_CTS,
+	UART2_RTS,
+
+	/* UART3 (GIGA_UART_GATING) */
+	UART3_TX,
+	UART3_RX,
+	UART3_CTS,
+	UART3_RTS,
+	UART3_CLKREQ,
+	UART3_BCLK,	/* 12MHz clock out */
+	Y15_1610_UART3_RTS,
+
+	/* PWT & PWL */
+	PWT,
+	PWL,
+
+	/* USB master generic */
+	R18_USB_VBUS,
+	R18_1510_USB_GPIO0,
+	W4_USB_PUEN,
+	W4_USB_CLKO,
+	W4_USB_HIGHZ,
+	W4_GPIO58,
+
+	/* USB1 master */
+	USB1_SUSP,
+	USB1_SEO,
+	W13_1610_USB1_SE0,
+	USB1_TXEN,
+	USB1_TXD,
+	USB1_VP,
+	USB1_VM,
+	USB1_RCV,
+	USB1_SPEED,
+	R13_1610_USB1_SPEED,
+	R13_1710_USB1_SE0,
+
+	/* USB2 master */
+	USB2_SUSP,
+	USB2_VP,
+	USB2_TXEN,
+	USB2_VM,
+	USB2_RCV,
+	USB2_SEO,
+	USB2_TXD,
+
+	/* OMAP-1510 GPIO */
+	R18_1510_GPIO0,
+	R19_1510_GPIO1,
+	M14_1510_GPIO2,
+
+	/* OMAP1610 GPIO */
+	P18_1610_GPIO3,
+	Y15_1610_GPIO17,
+
+	/* OMAP-1710 GPIO */
+	R18_1710_GPIO0,
+	V2_1710_GPIO10,
+	N21_1710_GPIO14,
+	W15_1710_GPIO40,
+
+	/* MPUIO */
+	MPUIO2,
+	N15_1610_MPUIO2,
+	MPUIO4,
+	MPUIO5,
+	T20_1610_MPUIO5,
+	W11_1610_MPUIO6,
+	V10_1610_MPUIO7,
+	W11_1610_MPUIO9,
+	V10_1610_MPUIO10,
+	W10_1610_MPUIO11,
+	E20_1610_MPUIO13,
+	U20_1610_MPUIO14,
+	E19_1610_MPUIO15,
+
+	/* MCBSP2 */
+	MCBSP2_CLKR,
+	MCBSP2_CLKX,
+	MCBSP2_DR,
+	MCBSP2_DX,
+	MCBSP2_FSR,
+	MCBSP2_FSX,
+
+	/* MCBSP3 */
+	MCBSP3_CLKX,
+
+	/* Misc ballouts */
+	BALLOUT_V8_ARMIO3,
+	N20_HDQ,
+
+	/* OMAP-1610 MMC2 */
+	W8_1610_MMC2_DAT0,
+	V8_1610_MMC2_DAT1,
+	W15_1610_MMC2_DAT2,
+	R10_1610_MMC2_DAT3,
+	Y10_1610_MMC2_CLK,
+	Y8_1610_MMC2_CMD,
+	V9_1610_MMC2_CMDDIR,
+	V5_1610_MMC2_DATDIR0,
+	W19_1610_MMC2_DATDIR1,
+	R18_1610_MMC2_CLKIN,
+
+	/* OMAP-1610 External Trace Interface */
+	M19_1610_ETM_PSTAT0,
+	L15_1610_ETM_PSTAT1,
+	L18_1610_ETM_PSTAT2,
+	L19_1610_ETM_D0,
+	J19_1610_ETM_D6,
+	J18_1610_ETM_D7,
+
+	/* OMAP16XX GPIO */
+	P20_1610_GPIO4,
+	V9_1610_GPIO7,
+	W8_1610_GPIO9,
+	N20_1610_GPIO11,
+	N19_1610_GPIO13,
+	P10_1610_GPIO22,
+	V5_1610_GPIO24,
+	AA20_1610_GPIO_41,
+	W19_1610_GPIO48,
+	M7_1610_GPIO62,
+	V14_16XX_GPIO37,
+	R9_16XX_GPIO18,
+	L14_16XX_GPIO49,
+
+	/* OMAP-1610 uWire */
+	V19_1610_UWIRE_SCLK,
+	U18_1610_UWIRE_SDI,
+	W21_1610_UWIRE_SDO,
+	N14_1610_UWIRE_CS0,
+	P15_1610_UWIRE_CS3,
+	N15_1610_UWIRE_CS1,
+
+	/* OMAP-1610 SPI */
+	U19_1610_SPIF_SCK,
+	U18_1610_SPIF_DIN,
+	P20_1610_SPIF_DIN,
+	W21_1610_SPIF_DOUT,
+	R18_1610_SPIF_DOUT,
+	N14_1610_SPIF_CS0,
+	N15_1610_SPIF_CS1,
+	T19_1610_SPIF_CS2,
+	P15_1610_SPIF_CS3,
+
+	/* OMAP-1610 Flash */
+	L3_1610_FLASH_CS2B_OE,
+	M8_1610_FLASH_CS2B_WE,
+
+	/* First MMC */
+	MMC_CMD,
+	MMC_DAT1,
+	MMC_DAT2,
+	MMC_DAT0,
+	MMC_CLK,
+	MMC_DAT3,
+
+	/* OMAP-1710 MMC CMDDIR and DATDIR0 */
+	M15_1710_MMC_CLKI,
+	P19_1710_MMC_CMDDIR,
+	P20_1710_MMC_DATDIR0,
+
+	/* OMAP-1610 USB0 alternate pin configuration */
+	W9_USB0_TXEN,
+	AA9_USB0_VP,
+	Y5_USB0_RCV,
+	R9_USB0_VM,
+	V6_USB0_TXD,
+	W5_USB0_SE0,
+	V9_USB0_SPEED,
+	V9_USB0_SUSP,
+
+	/* USB2 */
+	W9_USB2_TXEN,
+	AA9_USB2_VP,
+	Y5_USB2_RCV,
+	R9_USB2_VM,
+	V6_USB2_TXD,
+	W5_USB2_SE0,
+
+	/* 16XX UART */
+	R13_1610_UART1_TX,
+	V14_16XX_UART1_RX,
+	R14_1610_UART1_CTS,
+	AA15_1610_UART1_RTS,
+	R9_16XX_UART2_RX,
+	L14_16XX_UART3_RX,
+
+	/* I2C OMAP-1610 */
+	I2C_SCL,
+	I2C_SDA,
+
+	/* Keypad */
+	F18_1610_KBC0,
+	D20_1610_KBC1,
+	D19_1610_KBC2,
+	E18_1610_KBC3,
+	C21_1610_KBC4,
+	G18_1610_KBR0,
+	F19_1610_KBR1,
+	H14_1610_KBR2,
+	E20_1610_KBR3,
+	E19_1610_KBR4,
+	N19_1610_KBR5,
+
+	/* Power management */
+	T20_1610_LOW_PWR,
+
+	/* MCLK Settings */
+	V5_1710_MCLK_ON,
+	V5_1710_MCLK_OFF,
+	R10_1610_MCLK_ON,
+	R10_1610_MCLK_OFF,
+
+	/* CompactFlash controller */
+	P11_1610_CF_CD2,
+	R11_1610_CF_IOIS16,
+	V10_1610_CF_IREQ,
+	W10_1610_CF_RESET,
+	W11_1610_CF_CD1,
+
+	/* parallel camera */
+	J15_1610_CAM_LCLK,
+	J18_1610_CAM_D7,
+	J19_1610_CAM_D6,
+	J14_1610_CAM_D5,
+	K18_1610_CAM_D4,
+	K19_1610_CAM_D3,
+	K15_1610_CAM_D2,
+	K14_1610_CAM_D1,
+	L19_1610_CAM_D0,
+	L18_1610_CAM_VS,
+	L15_1610_CAM_HS,
+	M19_1610_CAM_RSTZ,
+	Y15_1610_CAM_OUTCLK,
+
+	/* serial camera */
+	H19_1610_CAM_EXCLK,
+	Y12_1610_CCP_CLKP,
+	W13_1610_CCP_CLKM,
+	W14_1610_CCP_DATAP,
+	Y14_1610_CCP_DATAM,
+
+};
+
+enum omap24xx_index {
+	/* 24xx I2C */
+	M19_24XX_I2C1_SCL,
+	L15_24XX_I2C1_SDA,
+	J15_24XX_I2C2_SCL,
+	H19_24XX_I2C2_SDA,
+
+	/* 24xx Menelaus interrupt */
+	W19_24XX_SYS_NIRQ,
+
+	/* 24xx clock */
+	W14_24XX_SYS_CLKOUT,
+
+	/* 24xx GPMC chipselects, wait pin monitoring */
+	E2_GPMC_NCS2,
+	L2_GPMC_NCS7,
+	L3_GPMC_WAIT0,
+	N7_GPMC_WAIT1,
+	M1_GPMC_WAIT2,
+	P1_GPMC_WAIT3,
+
+	/* 242X McBSP */
+	Y15_24XX_MCBSP2_CLKX,
+	R14_24XX_MCBSP2_FSX,
+	W15_24XX_MCBSP2_DR,
+	V15_24XX_MCBSP2_DX,
+
+	/* 24xx GPIO */
+	M21_242X_GPIO11,
+	P21_242X_GPIO12,
+	AA10_242X_GPIO13,
+	AA6_242X_GPIO14,
+	AA4_242X_GPIO15,
+	Y11_242X_GPIO16,
+	AA12_242X_GPIO17,
+	AA8_242X_GPIO58,
+	Y20_24XX_GPIO60,
+	W4__24XX_GPIO74,
+	N15_24XX_GPIO85,
+	M15_24XX_GPIO92,
+	P20_24XX_GPIO93,
+	P18_24XX_GPIO95,
+	M18_24XX_GPIO96,
+	L14_24XX_GPIO97,
+	J15_24XX_GPIO99,
+	V14_24XX_GPIO117,
+	P14_24XX_GPIO125,
+
+	/* 242x DBG GPIO */
+	V4_242X_GPIO49,
+	W2_242X_GPIO50,
+	U4_242X_GPIO51,
+	V3_242X_GPIO52,
+	V2_242X_GPIO53,
+	V6_242X_GPIO53,
+	T4_242X_GPIO54,
+	Y4_242X_GPIO54,
+	T3_242X_GPIO55,
+	U2_242X_GPIO56,
+
+	/* 24xx external DMA requests */
+	AA10_242X_DMAREQ0,
+	AA6_242X_DMAREQ1,
+	E4_242X_DMAREQ2,
+	G4_242X_DMAREQ3,
+	D3_242X_DMAREQ4,
+	E3_242X_DMAREQ5,
+
+	/* UART3 */
+	K15_24XX_UART3_TX,
+	K14_24XX_UART3_RX,
+
+	/* MMC/SDIO */
+	G19_24XX_MMC_CLKO,
+	H18_24XX_MMC_CMD,
+	F20_24XX_MMC_DAT0,
+	H14_24XX_MMC_DAT1,
+	E19_24XX_MMC_DAT2,
+	D19_24XX_MMC_DAT3,
+	F19_24XX_MMC_DAT_DIR0,
+	E20_24XX_MMC_DAT_DIR1,
+	F18_24XX_MMC_DAT_DIR2,
+	E18_24XX_MMC_DAT_DIR3,
+	G18_24XX_MMC_CMD_DIR,
+	H15_24XX_MMC_CLKI,
+
+	/* Full speed USB */
+	J20_24XX_USB0_PUEN,
+	J19_24XX_USB0_VP,
+	K20_24XX_USB0_VM,
+	J18_24XX_USB0_RCV,
+	K19_24XX_USB0_TXEN,
+	J14_24XX_USB0_SE0,
+	K18_24XX_USB0_DAT,
+
+	N14_24XX_USB1_SE0,
+	W12_24XX_USB1_SE0,
+	P15_24XX_USB1_DAT,
+	R13_24XX_USB1_DAT,
+	W20_24XX_USB1_TXEN,
+	P13_24XX_USB1_TXEN,
+	V19_24XX_USB1_RCV,
+	V12_24XX_USB1_RCV,
+
+	AA10_24XX_USB2_SE0,
+	Y11_24XX_USB2_DAT,
+	AA12_24XX_USB2_TXEN,
+	AA6_24XX_USB2_RCV,
+	AA4_24XX_USB2_TLLSE0,
+
+	/* Keypad GPIO*/
+	T19_24XX_KBR0,
+	R19_24XX_KBR1,
+	V18_24XX_KBR2,
+	M21_24XX_KBR3,
+	E5__24XX_KBR4,
+	M18_24XX_KBR5,
+	R20_24XX_KBC0,
+	M14_24XX_KBC1,
+	H19_24XX_KBC2,
+	V17_24XX_KBC3,
+	P21_24XX_KBC4,
+	L14_24XX_KBC5,
+	N19_24XX_KBC6,
+
+	/* 24xx Menelaus Keypad GPIO */
+	B3__24XX_KBR5,
+	AA4_24XX_KBC2,
+	B13_24XX_KBC6,
+
+	/* 2430 USB */
+	AD9_2430_USB0_PUEN,
+	Y11_2430_USB0_VP,
+	AD7_2430_USB0_VM,
+	AE7_2430_USB0_RCV,
+	AD4_2430_USB0_TXEN,
+	AF9_2430_USB0_SE0,
+	AE6_2430_USB0_DAT,
+	AD24_2430_USB1_SE0,
+	AB24_2430_USB1_RCV,
+	Y25_2430_USB1_TXEN,
+	AA26_2430_USB1_DAT,
+
+	/* 2430 HS-USB */
+	AD9_2430_USB0HS_DATA3,
+	Y11_2430_USB0HS_DATA4,
+	AD7_2430_USB0HS_DATA5,
+	AE7_2430_USB0HS_DATA6,
+	AD4_2430_USB0HS_DATA2,
+	AF9_2430_USB0HS_DATA0,
+	AE6_2430_USB0HS_DATA1,
+	AE8_2430_USB0HS_CLK,
+	AD8_2430_USB0HS_DIR,
+	AE5_2430_USB0HS_STP,
+	AE9_2430_USB0HS_NXT,
+	AC7_2430_USB0HS_DATA7,
+
+	/* 2430 McBSP */
+	AD6_2430_MCBSP_CLKS,
+
+	AB2_2430_MCBSP1_CLKR,
+	AD5_2430_MCBSP1_FSR,
+	AA1_2430_MCBSP1_DX,
+	AF3_2430_MCBSP1_DR,
+	AB3_2430_MCBSP1_FSX,
+	Y9_2430_MCBSP1_CLKX,
+
+	AC10_2430_MCBSP2_FSX,
+	AD16_2430_MCBSP2_CLX,
+	AE13_2430_MCBSP2_DX,
+	AD13_2430_MCBSP2_DR,
+	AC10_2430_MCBSP2_FSX_OFF,
+	AD16_2430_MCBSP2_CLX_OFF,
+	AE13_2430_MCBSP2_DX_OFF,
+	AD13_2430_MCBSP2_DR_OFF,
+
+	AC9_2430_MCBSP3_CLKX,
+	AE4_2430_MCBSP3_FSX,
+	AE2_2430_MCBSP3_DR,
+	AF4_2430_MCBSP3_DX,
+
+	N3_2430_MCBSP4_CLKX,
+	AD23_2430_MCBSP4_DR,
+	AB25_2430_MCBSP4_DX,
+	AC25_2430_MCBSP4_FSX,
+
+	AE16_2430_MCBSP5_CLKX,
+	AF12_2430_MCBSP5_FSX,
+	K7_2430_MCBSP5_DX,
+	M1_2430_MCBSP5_DR,
+
+	/* 2430 McSPI*/
+	Y18_2430_MCSPI1_CLK,
+	AD15_2430_MCSPI1_SIMO,
+	AE17_2430_MCSPI1_SOMI,
+	U1_2430_MCSPI1_CS0,
+
+	/* Touchscreen GPIO */
+	AF19_2430_GPIO_85,
+
+};
+
+struct omap_mux_cfg {
+	struct pin_config	*pins;
+	unsigned long		size;
+	int			(*cfg_reg)(const struct pin_config *cfg);
+};
+
+#ifdef	CONFIG_OMAP_MUX
+/* setup pin muxing in Linux */
+extern int omap1_mux_init(void);
+extern int omap_mux_register(struct omap_mux_cfg *);
+extern int omap_cfg_reg(unsigned long reg_cfg);
+#else
+/* boot loader does it all (no warnings from CONFIG_OMAP_MUX_WARNINGS) */
+static inline int omap1_mux_init(void) { return 0; }
+static inline int omap_cfg_reg(unsigned long reg_cfg) { return 0; }
+#endif
+
+extern int omap2_mux_init(void);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/nand.h
@@ -0,0 +1,24 @@
+/*
+ * arch/arm/plat-omap/include/mach/nand.h
+ *
+ * Copyright (C) 2006 Micron Technology Inc.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/mtd/partitions.h>
+
+struct omap_nand_platform_data {
+	unsigned int		options;
+	int			cs;
+	int			gpio_irq;
+	struct mtd_partition	*parts;
+	int			nr_parts;
+	int			(*nand_setup)(void __iomem *);
+	int			(*dev_ready)(struct omap_nand_platform_data *);
+	int			dma_channel;
+	void __iomem		*gpmc_cs_baseaddr;
+	void __iomem		*gpmc_baseaddr;
+};
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap1510.h
@@ -0,0 +1,50 @@
+/* arch/arm/plat-omap/include/mach/omap1510.h
+ *
+ * Hardware definitions for TI OMAP1510 processor.
+ *
+ * Cleanup for Linux-2.6 by Dirk Behme <dirk.behme@de.bosch.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_OMAP15XX_H
+#define __ASM_ARCH_OMAP15XX_H
+
+/*
+ * ----------------------------------------------------------------------------
+ * Base addresses
+ * ----------------------------------------------------------------------------
+ */
+
+/* Syntax: XX_BASE = Virtual base address, XX_START = Physical base address */
+
+#define OMAP1510_DSP_BASE	0xE0000000
+#define OMAP1510_DSP_SIZE	0x28000
+#define OMAP1510_DSP_START	0xE0000000
+
+#define OMAP1510_DSPREG_BASE	0xE1000000
+#define OMAP1510_DSPREG_SIZE	SZ_128K
+#define OMAP1510_DSPREG_START	0xE1000000
+
+#define OMAP1510_DSP_MMU_BASE	(0xfffed200)
+
+#endif /*  __ASM_ARCH_OMAP15XX_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap16xx.h
@@ -0,0 +1,202 @@
+/* arch/arm/plat-omap/include/mach/omap16xx.h
+ *
+ * Hardware definitions for TI OMAP1610/5912/1710 processors.
+ *
+ * Cleanup for Linux-2.6 by Dirk Behme <dirk.behme@de.bosch.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_OMAP16XX_H
+#define __ASM_ARCH_OMAP16XX_H
+
+/*
+ * ----------------------------------------------------------------------------
+ * Base addresses
+ * ----------------------------------------------------------------------------
+ */
+
+/* Syntax: XX_BASE = Virtual base address, XX_START = Physical base address */
+
+#define OMAP16XX_DSP_BASE	0xE0000000
+#define OMAP16XX_DSP_SIZE	0x28000
+#define OMAP16XX_DSP_START	0xE0000000
+
+#define OMAP16XX_DSPREG_BASE	0xE1000000
+#define OMAP16XX_DSPREG_SIZE	SZ_128K
+#define OMAP16XX_DSPREG_START	0xE1000000
+
+#define OMAP16XX_SEC_BASE	0xFFFE4000
+#define OMAP16XX_SEC_DES	(OMAP16XX_SEC_BASE + 0x0000)
+#define OMAP16XX_SEC_SHA1MD5	(OMAP16XX_SEC_BASE + 0x0800)
+#define OMAP16XX_SEC_RNG	(OMAP16XX_SEC_BASE + 0x1000)
+
+/*
+ * ---------------------------------------------------------------------------
+ * Interrupts
+ * ---------------------------------------------------------------------------
+ */
+#define OMAP_IH2_0_BASE		(0xfffe0000)
+#define OMAP_IH2_1_BASE		(0xfffe0100)
+#define OMAP_IH2_2_BASE		(0xfffe0200)
+#define OMAP_IH2_3_BASE		(0xfffe0300)
+
+#define OMAP_IH2_0_ITR		(OMAP_IH2_0_BASE + 0x00)
+#define OMAP_IH2_0_MIR		(OMAP_IH2_0_BASE + 0x04)
+#define OMAP_IH2_0_SIR_IRQ	(OMAP_IH2_0_BASE + 0x10)
+#define OMAP_IH2_0_SIR_FIQ	(OMAP_IH2_0_BASE + 0x14)
+#define OMAP_IH2_0_CONTROL	(OMAP_IH2_0_BASE + 0x18)
+#define OMAP_IH2_0_ILR0		(OMAP_IH2_0_BASE + 0x1c)
+#define OMAP_IH2_0_ISR		(OMAP_IH2_0_BASE + 0x9c)
+
+#define OMAP_IH2_1_ITR		(OMAP_IH2_1_BASE + 0x00)
+#define OMAP_IH2_1_MIR		(OMAP_IH2_1_BASE + 0x04)
+#define OMAP_IH2_1_SIR_IRQ	(OMAP_IH2_1_BASE + 0x10)
+#define OMAP_IH2_1_SIR_FIQ	(OMAP_IH2_1_BASE + 0x14)
+#define OMAP_IH2_1_CONTROL	(OMAP_IH2_1_BASE + 0x18)
+#define OMAP_IH2_1_ILR1		(OMAP_IH2_1_BASE + 0x1c)
+#define OMAP_IH2_1_ISR		(OMAP_IH2_1_BASE + 0x9c)
+
+#define OMAP_IH2_2_ITR		(OMAP_IH2_2_BASE + 0x00)
+#define OMAP_IH2_2_MIR		(OMAP_IH2_2_BASE + 0x04)
+#define OMAP_IH2_2_SIR_IRQ	(OMAP_IH2_2_BASE + 0x10)
+#define OMAP_IH2_2_SIR_FIQ	(OMAP_IH2_2_BASE + 0x14)
+#define OMAP_IH2_2_CONTROL	(OMAP_IH2_2_BASE + 0x18)
+#define OMAP_IH2_2_ILR2		(OMAP_IH2_2_BASE + 0x1c)
+#define OMAP_IH2_2_ISR		(OMAP_IH2_2_BASE + 0x9c)
+
+#define OMAP_IH2_3_ITR		(OMAP_IH2_3_BASE + 0x00)
+#define OMAP_IH2_3_MIR		(OMAP_IH2_3_BASE + 0x04)
+#define OMAP_IH2_3_SIR_IRQ	(OMAP_IH2_3_BASE + 0x10)
+#define OMAP_IH2_3_SIR_FIQ	(OMAP_IH2_3_BASE + 0x14)
+#define OMAP_IH2_3_CONTROL	(OMAP_IH2_3_BASE + 0x18)
+#define OMAP_IH2_3_ILR3		(OMAP_IH2_3_BASE + 0x1c)
+#define OMAP_IH2_3_ISR		(OMAP_IH2_3_BASE + 0x9c)
+
+/*
+ * ----------------------------------------------------------------------------
+ * Clocks
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP16XX_ARM_IDLECT3	(CLKGEN_REG_BASE + 0x24)
+
+/*
+ * ----------------------------------------------------------------------------
+ * Pin configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP16XX_CONF_VOLTAGE_VDDSHV6	(1 << 8)
+#define OMAP16XX_CONF_VOLTAGE_VDDSHV7	(1 << 9)
+#define OMAP16XX_CONF_VOLTAGE_VDDSHV8	(1 << 10)
+#define OMAP16XX_CONF_VOLTAGE_VDDSHV9	(1 << 11)
+#define OMAP16XX_SUBLVDS_CONF_VALID	(1 << 13)
+
+/*
+ * ----------------------------------------------------------------------------
+ * System control registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP1610_RESET_CONTROL  0xfffe1140
+
+/*
+ * ---------------------------------------------------------------------------
+ * TIPB bus interface
+ * ---------------------------------------------------------------------------
+ */
+#define TIPB_SWITCH_BASE		 (0xfffbc800)
+#define OMAP16XX_MMCSD2_SSW_MPU_CONF	(TIPB_SWITCH_BASE + 0x160)
+
+/* UART3 Registers Mapping through MPU bus */
+#define UART3_RHR               (OMAP_UART3_BASE + 0)
+#define UART3_THR               (OMAP_UART3_BASE + 0)
+#define UART3_DLL               (OMAP_UART3_BASE + 0)
+#define UART3_IER               (OMAP_UART3_BASE + 4)
+#define UART3_DLH               (OMAP_UART3_BASE + 4)
+#define UART3_IIR               (OMAP_UART3_BASE + 8)
+#define UART3_FCR               (OMAP_UART3_BASE + 8)
+#define UART3_EFR               (OMAP_UART3_BASE + 8)
+#define UART3_LCR               (OMAP_UART3_BASE + 0x0C)
+#define UART3_MCR               (OMAP_UART3_BASE + 0x10)
+#define UART3_XON1_ADDR1        (OMAP_UART3_BASE + 0x10)
+#define UART3_XON2_ADDR2        (OMAP_UART3_BASE + 0x14)
+#define UART3_LSR               (OMAP_UART3_BASE + 0x14)
+#define UART3_TCR               (OMAP_UART3_BASE + 0x18)
+#define UART3_MSR               (OMAP_UART3_BASE + 0x18)
+#define UART3_XOFF1             (OMAP_UART3_BASE + 0x18)
+#define UART3_XOFF2             (OMAP_UART3_BASE + 0x1C)
+#define UART3_SPR               (OMAP_UART3_BASE + 0x1C)
+#define UART3_TLR               (OMAP_UART3_BASE + 0x1C)
+#define UART3_MDR1              (OMAP_UART3_BASE + 0x20)
+#define UART3_MDR2              (OMAP_UART3_BASE + 0x24)
+#define UART3_SFLSR             (OMAP_UART3_BASE + 0x28)
+#define UART3_TXFLL             (OMAP_UART3_BASE + 0x28)
+#define UART3_RESUME            (OMAP_UART3_BASE + 0x2C)
+#define UART3_TXFLH             (OMAP_UART3_BASE + 0x2C)
+#define UART3_SFREGL            (OMAP_UART3_BASE + 0x30)
+#define UART3_RXFLL             (OMAP_UART3_BASE + 0x30)
+#define UART3_SFREGH            (OMAP_UART3_BASE + 0x34)
+#define UART3_RXFLH             (OMAP_UART3_BASE + 0x34)
+#define UART3_BLR               (OMAP_UART3_BASE + 0x38)
+#define UART3_ACREG             (OMAP_UART3_BASE + 0x3C)
+#define UART3_DIV16             (OMAP_UART3_BASE + 0x3C)
+#define UART3_SCR               (OMAP_UART3_BASE + 0x40)
+#define UART3_SSR               (OMAP_UART3_BASE + 0x44)
+#define UART3_EBLR              (OMAP_UART3_BASE + 0x48)
+#define UART3_OSC_12M_SEL       (OMAP_UART3_BASE + 0x4C)
+#define UART3_MVR               (OMAP_UART3_BASE + 0x50)
+
+/*
+ * ---------------------------------------------------------------------------
+ * Watchdog timer
+ * ---------------------------------------------------------------------------
+ */
+
+/* 32-bit Watchdog timer in OMAP 16XX */
+#define OMAP_16XX_WATCHDOG_BASE        (0xfffeb000)
+#define OMAP_16XX_WIDR         (OMAP_16XX_WATCHDOG_BASE + 0x00)
+#define OMAP_16XX_WD_SYSCONFIG (OMAP_16XX_WATCHDOG_BASE + 0x10)
+#define OMAP_16XX_WD_SYSSTATUS (OMAP_16XX_WATCHDOG_BASE + 0x14)
+#define OMAP_16XX_WCLR         (OMAP_16XX_WATCHDOG_BASE + 0x24)
+#define OMAP_16XX_WCRR         (OMAP_16XX_WATCHDOG_BASE + 0x28)
+#define OMAP_16XX_WLDR         (OMAP_16XX_WATCHDOG_BASE + 0x2c)
+#define OMAP_16XX_WTGR         (OMAP_16XX_WATCHDOG_BASE + 0x30)
+#define OMAP_16XX_WWPS         (OMAP_16XX_WATCHDOG_BASE + 0x34)
+#define OMAP_16XX_WSPR         (OMAP_16XX_WATCHDOG_BASE + 0x48)
+
+#define WCLR_PRE_SHIFT         5
+#define WCLR_PTV_SHIFT         2
+
+#define WWPS_W_PEND_WSPR       (1 << 4)
+#define WWPS_W_PEND_WTGR       (1 << 3)
+#define WWPS_W_PEND_WLDR       (1 << 2)
+#define WWPS_W_PEND_WCRR       (1 << 1)
+#define WWPS_W_PEND_WCLR       (1 << 0)
+
+#define WSPR_ENABLE_0          (0x0000bbbb)
+#define WSPR_ENABLE_1          (0x00004444)
+#define WSPR_DISABLE_0         (0x0000aaaa)
+#define WSPR_DISABLE_1         (0x00005555)
+
+#define OMAP16XX_DSP_MMU_BASE	(0xfffed200)
+#define OMAP16XX_MAILBOX_BASE	(0xfffcf000)
+
+#endif /*  __ASM_ARCH_OMAP16XX_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap24xx.h
@@ -0,0 +1,89 @@
+/*
+ * arch/arm/plat-omap/include/mach/omap24xx.h
+ *
+ * This file contains the processor specific definitions
+ * of the TI OMAP24XX.
+ *
+ * Copyright (C) 2007 Texas Instruments.
+ * Copyright (C) 2007 Nokia Corporation.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ *
+ */
+
+#ifndef __ASM_ARCH_OMAP24XX_H
+#define __ASM_ARCH_OMAP24XX_H
+
+/*
+ * Please place only base defines here and put the rest in device
+ * specific headers. Note also that some of these defines are needed
+ * for omap1 to compile without adding ifdefs.
+ */
+
+#define L4_24XX_BASE		0x48000000
+#define L4_WK_243X_BASE		0x49000000
+#define L3_24XX_BASE		0x68000000
+
+/* interrupt controller */
+#define OMAP24XX_IC_BASE	(L4_24XX_BASE + 0xfe000)
+#define OMAP24XX_IVA_INTC_BASE	0x40000000
+
+#define OMAP2420_CTRL_BASE	L4_24XX_BASE
+#define OMAP2420_32KSYNCT_BASE	(L4_24XX_BASE + 0x4000)
+#define OMAP2420_PRCM_BASE	(L4_24XX_BASE + 0x8000)
+#define OMAP2420_CM_BASE	(L4_24XX_BASE + 0x8000)
+#define OMAP2420_PRM_BASE	OMAP2420_CM_BASE
+#define OMAP2420_SDRC_BASE	(L3_24XX_BASE + 0x9000)
+#define OMAP2420_SMS_BASE	0x68008000
+#define OMAP2420_GPMC_BASE	0x6800a000
+
+#define OMAP2430_32KSYNCT_BASE	(L4_WK_243X_BASE + 0x20000)
+#define OMAP2430_PRCM_BASE	(L4_WK_243X_BASE + 0x6000)
+#define OMAP2430_CM_BASE	(L4_WK_243X_BASE + 0x6000)
+#define OMAP2430_PRM_BASE	OMAP2430_CM_BASE
+
+#define OMAP243X_SMS_BASE	0x6C000000
+#define OMAP243X_SDRC_BASE	0x6D000000
+#define OMAP243X_GPMC_BASE	0x6E000000
+#define OMAP243X_SCM_BASE	(L4_WK_243X_BASE + 0x2000)
+#define OMAP243X_CTRL_BASE	OMAP243X_SCM_BASE
+#define OMAP243X_HS_BASE	(L4_24XX_BASE + 0x000ac000)
+
+/* DSP SS */
+#define OMAP2420_DSP_BASE	0x58000000
+#define OMAP2420_DSP_MEM_BASE	(OMAP2420_DSP_BASE + 0x0)
+#define OMAP2420_DSP_IPI_BASE	(OMAP2420_DSP_BASE + 0x1000000)
+#define OMAP2420_DSP_MMU_BASE	(OMAP2420_DSP_BASE + 0x2000000)
+
+#define OMAP243X_DSP_BASE	0x5C000000
+#define OMAP243X_DSP_MEM_BASE	(OMAP243X_DSP_BASE + 0x0)
+#define OMAP243X_DSP_MMU_BASE	(OMAP243X_DSP_BASE + 0x1000000)
+
+/* Mailbox */
+#define OMAP24XX_MAILBOX_BASE	(L4_24XX_BASE + 0x94000)
+
+/* Camera */
+#define OMAP24XX_CAMERA_BASE	(L4_24XX_BASE + 0x52000)
+
+/* Security */
+#define OMAP24XX_SEC_BASE	(L4_24XX_BASE + 0xA0000)
+#define OMAP24XX_SEC_RNG_BASE	(OMAP24XX_SEC_BASE + 0x0000)
+#define OMAP24XX_SEC_DES_BASE	(OMAP24XX_SEC_BASE + 0x2000)
+#define OMAP24XX_SEC_SHA1MD5_BASE (OMAP24XX_SEC_BASE + 0x4000)
+#define OMAP24XX_SEC_AES_BASE	(OMAP24XX_SEC_BASE + 0x6000)
+#define OMAP24XX_SEC_PKA_BASE	(OMAP24XX_SEC_BASE + 0x8000)
+
+#endif /* __ASM_ARCH_OMAP24XX_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap34xx.h
@@ -0,0 +1,86 @@
+/*
+ * arch/arm/plat-omap/include/mach/omap34xx.h
+ *
+ * This file contains the processor specific definitions of the TI OMAP34XX.
+ *
+ * Copyright (C) 2007 Texas Instruments.
+ * Copyright (C) 2007 Nokia Corporation.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ */
+
+#ifndef __ASM_ARCH_OMAP34XX_H
+#define __ASM_ARCH_OMAP34XX_H
+
+/*
+ * Please place only base defines here and put the rest in device
+ * specific headers.
+ */
+
+#define L4_34XX_BASE		0x48000000
+#define L4_WK_34XX_BASE		0x48300000
+#define L4_PER_34XX_BASE	0x49000000
+#define L4_EMU_34XX_BASE	0x54000000
+#define L3_34XX_BASE		0x68000000
+
+#define OMAP3430_32KSYNCT_BASE	0x48320000
+#define OMAP3430_CM_BASE	0x48004800
+#define OMAP3430_PRM_BASE	0x48306800
+#define OMAP343X_SMS_BASE	0x6C000000
+#define OMAP343X_SDRC_BASE	0x6D000000
+#define OMAP34XX_GPMC_BASE	0x6E000000
+#define OMAP343X_SCM_BASE	0x48002000
+#define OMAP343X_CTRL_BASE	OMAP343X_SCM_BASE
+
+#define OMAP34XX_IC_BASE	0x48200000
+
+#define OMAP3430_ISP_BASE		(L4_34XX_BASE + 0xBC000)
+#define OMAP3430_ISP_CBUFF_BASE		(OMAP3430_ISP_BASE + 0x0100)
+#define OMAP3430_ISP_CCP2_BASE		(OMAP3430_ISP_BASE + 0x0400)
+#define OMAP3430_ISP_CCDC_BASE		(OMAP3430_ISP_BASE + 0x0600)
+#define OMAP3430_ISP_HIST_BASE		(OMAP3430_ISP_BASE + 0x0A00)
+#define OMAP3430_ISP_H3A_BASE		(OMAP3430_ISP_BASE + 0x0C00)
+#define OMAP3430_ISP_PREV_BASE		(OMAP3430_ISP_BASE + 0x0E00)
+#define OMAP3430_ISP_RESZ_BASE		(OMAP3430_ISP_BASE + 0x1000)
+#define OMAP3430_ISP_SBL_BASE		(OMAP3430_ISP_BASE + 0x1200)
+#define OMAP3430_ISP_MMU_BASE		(OMAP3430_ISP_BASE + 0x1400)
+#define OMAP3430_ISP_CSI2A_BASE		(OMAP3430_ISP_BASE + 0x1800)
+#define OMAP3430_ISP_CSI2PHY_BASE	(OMAP3430_ISP_BASE + 0x1970)
+
+#define OMAP3430_ISP_END		(OMAP3430_ISP_BASE         + 0x06F)
+#define OMAP3430_ISP_CBUFF_END		(OMAP3430_ISP_CBUFF_BASE   + 0x077)
+#define OMAP3430_ISP_CCP2_END		(OMAP3430_ISP_CCP2_BASE    + 0x1EF)
+#define OMAP3430_ISP_CCDC_END		(OMAP3430_ISP_CCDC_BASE    + 0x0A7)
+#define OMAP3430_ISP_HIST_END		(OMAP3430_ISP_HIST_BASE    + 0x047)
+#define OMAP3430_ISP_H3A_END		(OMAP3430_ISP_H3A_BASE     + 0x05F)
+#define OMAP3430_ISP_PREV_END		(OMAP3430_ISP_PREV_BASE    + 0x09F)
+#define OMAP3430_ISP_RESZ_END		(OMAP3430_ISP_RESZ_BASE    + 0x0AB)
+#define OMAP3430_ISP_SBL_END		(OMAP3430_ISP_SBL_BASE     + 0x0FB)
+#define OMAP3430_ISP_MMU_END		(OMAP3430_ISP_MMU_BASE     + 0x06F)
+#define OMAP3430_ISP_CSI2A_END		(OMAP3430_ISP_CSI2A_BASE   + 0x16F)
+#define OMAP3430_ISP_CSI2PHY_END	(OMAP3430_ISP_CSI2PHY_BASE + 0x007)
+
+#define OMAP34XX_HSUSB_OTG_BASE	(L4_34XX_BASE + 0xAB000)
+#define OMAP34XX_USBTLL_BASE	(L4_34XX_BASE + 0x62000)
+#define OMAP34XX_UHH_CONFIG_BASE	(L4_34XX_BASE + 0x64000)
+#define OMAP34XX_OHCI_BASE	(L4_34XX_BASE + 0x64400)
+#define OMAP34XX_EHCI_BASE	(L4_34XX_BASE + 0x64800)
+#define OMAP34XX_SR1_BASE	0x480C9000
+#define OMAP34XX_SR2_BASE	0x480CB000
+
+#define OMAP34XX_MAILBOX_BASE		(L4_34XX_BASE + 0x94000)
+
+#endif /* __ASM_ARCH_OMAP34XX_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap44xx.h
@@ -0,0 +1,48 @@
+/*:
+ * Address mappings and base address for OMAP4 interconnects
+ * and peripherals.
+ *
+ * Copyright (C) 2009 Texas Instruments
+ *
+ * Author: Santosh Shilimkar <santosh.shilimkar@ti.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+#ifndef __ASM_ARCH_OMAP44XX_H
+#define __ASM_ARCH_OMAP44XX_H
+
+/*
+ * Please place only base defines here and put the rest in device
+ * specific headers.
+ */
+#define L4_44XX_BASE			0x4a000000
+#define L4_WK_44XX_BASE			0x4a300000
+#define L4_PER_44XX_BASE		0x48000000
+#define L4_EMU_44XX_BASE		0x54000000
+#define L3_44XX_BASE			0x44000000
+#define OMAP44XX_EMIF1_BASE		0x4c000000
+#define OMAP44XX_EMIF2_BASE		0x4d000000
+#define OMAP44XX_DMM_BASE		0x4e000000
+#define OMAP4430_32KSYNCT_BASE		0x4a304000
+#define OMAP4430_CM1_BASE		0x4a004000
+#define OMAP4430_CM_BASE		OMAP4430_CM1_BASE
+#define OMAP4430_CM2_BASE		0x4a008000
+#define OMAP4430_PRM_BASE		0x4a306000
+#define OMAP44XX_GPMC_BASE		0x50000000
+#define OMAP443X_SCM_BASE		0x4a002000
+#define OMAP443X_CTRL_BASE		OMAP443X_SCM_BASE
+#define OMAP44XX_IC_BASE		0x48200000
+#define OMAP44XX_IVA_INTC_BASE		0x40000000
+#define IRQ_SIR_IRQ			0x0040
+#define OMAP44XX_GIC_DIST_BASE		0x48241000
+#define OMAP44XX_GIC_CPU_BASE		0x48240100
+#define OMAP44XX_SCU_BASE		0x48240000
+#define OMAP44XX_LOCAL_TWD_BASE		0x48240600
+#define OMAP44XX_WKUPGEN_BASE		0x48281000
+
+#define OMAP44XX_MAILBOX_BASE		(L4_44XX_BASE + 0xF4000)
+
+#endif /* __ASM_ARCH_OMAP44XX_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap730.h
@@ -0,0 +1,102 @@
+/* arch/arm/plat-omap/include/mach/omap730.h
+ *
+ * Hardware definitions for TI OMAP730 processor.
+ *
+ * Cleanup for Linux-2.6 by Dirk Behme <dirk.behme@de.bosch.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_OMAP730_H
+#define __ASM_ARCH_OMAP730_H
+
+/*
+ * ----------------------------------------------------------------------------
+ * Base addresses
+ * ----------------------------------------------------------------------------
+ */
+
+/* Syntax: XX_BASE = Virtual base address, XX_START = Physical base address */
+
+#define OMAP730_DSP_BASE	0xE0000000
+#define OMAP730_DSP_SIZE	0x50000
+#define OMAP730_DSP_START	0xE0000000
+
+#define OMAP730_DSPREG_BASE	0xE1000000
+#define OMAP730_DSPREG_SIZE	SZ_128K
+#define OMAP730_DSPREG_START	0xE1000000
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP730 specific configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP730_CONFIG_BASE	0xfffe1000
+#define OMAP730_IO_CONF_0	0xfffe1070
+#define OMAP730_IO_CONF_1	0xfffe1074
+#define OMAP730_IO_CONF_2	0xfffe1078
+#define OMAP730_IO_CONF_3	0xfffe107c
+#define OMAP730_IO_CONF_4	0xfffe1080
+#define OMAP730_IO_CONF_5	0xfffe1084
+#define OMAP730_IO_CONF_6	0xfffe1088
+#define OMAP730_IO_CONF_7	0xfffe108c
+#define OMAP730_IO_CONF_8	0xfffe1090
+#define OMAP730_IO_CONF_9	0xfffe1094
+#define OMAP730_IO_CONF_10	0xfffe1098
+#define OMAP730_IO_CONF_11	0xfffe109c
+#define OMAP730_IO_CONF_12	0xfffe10a0
+#define OMAP730_IO_CONF_13	0xfffe10a4
+
+#define OMAP730_MODE_1		0xfffe1010
+#define OMAP730_MODE_2		0xfffe1014
+
+/* CSMI specials: in terms of base + offset */
+#define OMAP730_MODE2_OFFSET	0x14
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP730 traffic controller configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP730_FLASH_CFG_0	0xfffecc10
+#define OMAP730_FLASH_ACFG_0	0xfffecc50
+#define OMAP730_FLASH_CFG_1	0xfffecc14
+#define OMAP730_FLASH_ACFG_1	0xfffecc54
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP730 DSP control registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP730_ICR_BASE	0xfffbb800
+#define OMAP730_DSP_M_CTL	0xfffbb804
+#define OMAP730_DSP_MMU_BASE	0xfffed200
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP730 PCC_UPLD configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP730_PCC_UPLD_CTRL_BASE	(0xfffe0900)
+#define OMAP730_PCC_UPLD_CTRL		(OMAP730_PCC_UPLD_CTRL_BASE + 0x00)
+
+#endif /*  __ASM_ARCH_OMAP730_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap7xx.h
@@ -0,0 +1,104 @@
+/* arch/arm/plat-omap/include/mach/omap7xx.h
+ *
+ * Hardware definitions for TI OMAP7XX processor.
+ *
+ * Cleanup for Linux-2.6 by Dirk Behme <dirk.behme@de.bosch.com>
+ * Adapted for omap850 by Zebediah C. McClure <zmc@lurian.net>
+ * Adapted for omap7xx by Alistair Buxton <a.j.buxton@gmail.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_OMAP7XX_H
+#define __ASM_ARCH_OMAP7XX_H
+
+/*
+ * ----------------------------------------------------------------------------
+ * Base addresses
+ * ----------------------------------------------------------------------------
+ */
+
+/* Syntax: XX_BASE = Virtual base address, XX_START = Physical base address */
+
+#define OMAP7XX_DSP_BASE	0xE0000000
+#define OMAP7XX_DSP_SIZE	0x50000
+#define OMAP7XX_DSP_START	0xE0000000
+
+#define OMAP7XX_DSPREG_BASE	0xE1000000
+#define OMAP7XX_DSPREG_SIZE	SZ_128K
+#define OMAP7XX_DSPREG_START	0xE1000000
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP7XX specific configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP7XX_CONFIG_BASE	0xfffe1000
+#define OMAP7XX_IO_CONF_0	0xfffe1070
+#define OMAP7XX_IO_CONF_1	0xfffe1074
+#define OMAP7XX_IO_CONF_2	0xfffe1078
+#define OMAP7XX_IO_CONF_3	0xfffe107c
+#define OMAP7XX_IO_CONF_4	0xfffe1080
+#define OMAP7XX_IO_CONF_5	0xfffe1084
+#define OMAP7XX_IO_CONF_6	0xfffe1088
+#define OMAP7XX_IO_CONF_7	0xfffe108c
+#define OMAP7XX_IO_CONF_8	0xfffe1090
+#define OMAP7XX_IO_CONF_9	0xfffe1094
+#define OMAP7XX_IO_CONF_10	0xfffe1098
+#define OMAP7XX_IO_CONF_11	0xfffe109c
+#define OMAP7XX_IO_CONF_12	0xfffe10a0
+#define OMAP7XX_IO_CONF_13	0xfffe10a4
+
+#define OMAP7XX_MODE_1		0xfffe1010
+#define OMAP7XX_MODE_2		0xfffe1014
+
+/* CSMI specials: in terms of base + offset */
+#define OMAP7XX_MODE2_OFFSET	0x14
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP7XX traffic controller configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP7XX_FLASH_CFG_0	0xfffecc10
+#define OMAP7XX_FLASH_ACFG_0	0xfffecc50
+#define OMAP7XX_FLASH_CFG_1	0xfffecc14
+#define OMAP7XX_FLASH_ACFG_1	0xfffecc54
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP7XX DSP control registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP7XX_ICR_BASE	0xfffbb800
+#define OMAP7XX_DSP_M_CTL	0xfffbb804
+#define OMAP7XX_DSP_MMU_BASE	0xfffed200
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP7XX PCC_UPLD configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP7XX_PCC_UPLD_CTRL_BASE	(0xfffe0900)
+#define OMAP7XX_PCC_UPLD_CTRL		(OMAP7XX_PCC_UPLD_CTRL_BASE + 0x00)
+
+#endif /*  __ASM_ARCH_OMAP7XX_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap850.h
@@ -0,0 +1,102 @@
+/* arch/arm/plat-omap/include/mach/omap850.h
+ *
+ * Hardware definitions for TI OMAP850 processor.
+ *
+ * Derived from omap730.h by Zebediah C. McClure <zmc@lurian.net>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __ASM_ARCH_OMAP850_H
+#define __ASM_ARCH_OMAP850_H
+
+/*
+ * ----------------------------------------------------------------------------
+ * Base addresses
+ * ----------------------------------------------------------------------------
+ */
+
+/* Syntax: XX_BASE = Virtual base address, XX_START = Physical base address */
+
+#define OMAP850_DSP_BASE	0xE0000000
+#define OMAP850_DSP_SIZE	0x50000
+#define OMAP850_DSP_START	0xE0000000
+
+#define OMAP850_DSPREG_BASE	0xE1000000
+#define OMAP850_DSPREG_SIZE	SZ_128K
+#define OMAP850_DSPREG_START	0xE1000000
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP850 specific configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP850_CONFIG_BASE	0xfffe1000
+#define OMAP850_IO_CONF_0	0xfffe1070
+#define OMAP850_IO_CONF_1	0xfffe1074
+#define OMAP850_IO_CONF_2	0xfffe1078
+#define OMAP850_IO_CONF_3	0xfffe107c
+#define OMAP850_IO_CONF_4	0xfffe1080
+#define OMAP850_IO_CONF_5	0xfffe1084
+#define OMAP850_IO_CONF_6	0xfffe1088
+#define OMAP850_IO_CONF_7	0xfffe108c
+#define OMAP850_IO_CONF_8	0xfffe1090
+#define OMAP850_IO_CONF_9	0xfffe1094
+#define OMAP850_IO_CONF_10	0xfffe1098
+#define OMAP850_IO_CONF_11	0xfffe109c
+#define OMAP850_IO_CONF_12	0xfffe10a0
+#define OMAP850_IO_CONF_13	0xfffe10a4
+
+#define OMAP850_MODE_1		0xfffe1010
+#define OMAP850_MODE_2		0xfffe1014
+
+/* CSMI specials: in terms of base + offset */
+#define OMAP850_MODE2_OFFSET	0x14
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP850 traffic controller configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP850_FLASH_CFG_0	0xfffecc10
+#define OMAP850_FLASH_ACFG_0	0xfffecc50
+#define OMAP850_FLASH_CFG_1	0xfffecc14
+#define OMAP850_FLASH_ACFG_1	0xfffecc54
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP850 DSP control registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP850_ICR_BASE	0xfffbb800
+#define OMAP850_DSP_M_CTL	0xfffbb804
+#define OMAP850_DSP_MMU_BASE	0xfffed200
+
+/*
+ * ----------------------------------------------------------------------------
+ * OMAP850 PCC_UPLD configuration registers
+ * ----------------------------------------------------------------------------
+ */
+#define OMAP850_PCC_UPLD_CTRL_BASE	(0xfffe0900)
+#define OMAP850_PCC_UPLD_CTRL		(OMAP850_PCC_UPLD_CTRL_BASE + 0x00)
+
+#endif /*  __ASM_ARCH_OMAP850_H */
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap-alsa.h
@@ -0,0 +1,123 @@
+/*
+ * arch/arm/plat-omap/include/mach/omap-alsa.h
+ *
+ * Alsa Driver for AIC23 and TSC2101 codecs on OMAP platform boards.
+ *
+ * Copyright (C) 2006 Mika Laitio <lamikr@cc.jyu.fi>
+ *
+ * Copyright (C) 2005 Instituto Nokia de Tecnologia - INdT - Manaus Brazil
+ * Written by Daniel Petrini, David Cohen, Anderson Briglia
+ *            {daniel.petrini, david.cohen, anderson.briglia}@indt.org.br
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ *  History
+ *  -------
+ *
+ *  2005/07/25 INdT-10LE Kernel Team - 	Alsa driver for omap osk,
+ *  					original version based in sa1100 driver
+ *  					and omap oss driver.
+ */
+
+#ifndef __OMAP_ALSA_H
+#define __OMAP_ALSA_H
+
+#include <plat/dma.h>
+#include <sound/core.h>
+#include <sound/pcm.h>
+#include <plat/mcbsp.h>
+#include <linux/platform_device.h>
+
+#define DMA_BUF_SIZE	(1024 * 8)
+
+/*
+ * Buffer management for alsa and dma
+ */
+struct audio_stream {
+	char *id;		/* identification string */
+	int stream_id;		/* numeric identification */
+	int dma_dev;		/* dma number of that device */
+	int *lch;		/* Chain of channels this stream is linked to */
+	char started;		/* to store if the chain was started or not */
+	int dma_q_head;		/* DMA Channel Q Head */
+	int dma_q_tail;		/* DMA Channel Q Tail */
+	char dma_q_count;	/* DMA Channel Q Count */
+	int active:1;		/* we are using this stream for transfer now */
+	int period;		/* current transfer period */
+	int periods;		/* current count of periods registerd in the DMA engine */
+	spinlock_t dma_lock;	/* for locking in DMA operations */
+	struct snd_pcm_substream *stream;	/* the pcm stream */
+	unsigned linked:1;	/* dma channels linked */
+	int offset;		/* store start position of the last period in the alsa buffer */
+	int (*hw_start)(void);  /* interface to start HW interface, e.g. McBSP */
+	int (*hw_stop)(void);   /* interface to stop HW interface, e.g. McBSP */
+};
+
+/*
+ * Alsa card structure for aic23
+ */
+struct snd_card_omap_codec {
+	struct snd_card *card;
+	struct snd_pcm *pcm;
+	long samplerate;
+	struct audio_stream s[2];	/* playback & capture */
+};
+
+/* Codec specific information and function pointers.
+ * Codec (omap-alsa-aic23.c and omap-alsa-tsc2101.c)
+ * are responsible for defining the function pointers.
+ */
+struct omap_alsa_codec_config {
+	char 	*name;
+	struct	omap_mcbsp_reg_cfg *mcbsp_regs_alsa;
+	struct	snd_pcm_hw_constraint_list *hw_constraints_rates;
+	struct	snd_pcm_hardware *snd_omap_alsa_playback;
+	struct	snd_pcm_hardware *snd_omap_alsa_capture;
+	void	(*codec_configure_dev)(void);
+	void	(*codec_set_samplerate)(long);
+	void	(*codec_clock_setup)(void);
+	int	(*codec_clock_on)(void);
+	int 	(*codec_clock_off)(void);
+	int	(*get_default_samplerate)(void);
+};
+
+/*********** Mixer function prototypes *************************/
+int snd_omap_mixer(struct snd_card_omap_codec *);
+void snd_omap_init_mixer(void);
+
+#ifdef CONFIG_PM
+void snd_omap_suspend_mixer(void);
+void snd_omap_resume_mixer(void);
+#endif
+
+int snd_omap_alsa_post_probe(struct platform_device *pdev, struct omap_alsa_codec_config *config);
+int snd_omap_alsa_remove(struct platform_device *pdev);
+#ifdef CONFIG_PM
+int snd_omap_alsa_suspend(struct platform_device *pdev, pm_message_t state);
+int snd_omap_alsa_resume(struct platform_device *pdev);
+#else
+#define snd_omap_alsa_suspend	NULL
+#define snd_omap_alsa_resume	NULL
+#endif
+
+void callback_omap_alsa_sound_dma(void *);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap_device.h
@@ -0,0 +1,143 @@
+/*
+ * omap_device headers
+ *
+ * Copyright (C) 2009 Nokia Corporation
+ * Paul Walmsley
+ *
+ * Developed in collaboration with (alphabetical order): Benoit
+ * Cousson, Kevin Hilman, Tony Lindgren, Rajendra Nayak, Vikram
+ * Pandita, Sakari Poussa, Anand Sawant, Santosh Shilimkar, Richard
+ * Woodruff
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * Eventually this type of functionality should either be
+ * a) implemented via arch-specific pointers in platform_device
+ * or
+ * b) implemented as a proper omap_bus/omap_device in Linux, no more
+ *    platform_device
+ *
+ * omap_device differs from omap_hwmod in that it includes external
+ * (e.g., board- and system-level) integration details.  omap_hwmod
+ * stores hardware data that is invariant for a given OMAP chip.
+ *
+ * To do:
+ * - GPIO integration
+ * - regulator integration
+ *
+ */
+#ifndef __ARCH_ARM_PLAT_OMAP_INCLUDE_MACH_OMAP_DEVICE_H
+#define __ARCH_ARM_PLAT_OMAP_INCLUDE_MACH_OMAP_DEVICE_H
+
+#include <linux/kernel.h>
+#include <linux/platform_device.h>
+
+#include <plat/omap_hwmod.h>
+
+/* omap_device._state values */
+#define OMAP_DEVICE_STATE_UNKNOWN	0
+#define OMAP_DEVICE_STATE_ENABLED	1
+#define OMAP_DEVICE_STATE_IDLE		2
+#define OMAP_DEVICE_STATE_SHUTDOWN	3
+
+/**
+ * struct omap_device - omap_device wrapper for platform_devices
+ * @pdev: platform_device
+ * @hwmods: (one .. many per omap_device)
+ * @hwmods_cnt: ARRAY_SIZE() of @hwmods
+ * @pm_lats: ptr to an omap_device_pm_latency table
+ * @pm_lats_cnt: ARRAY_SIZE() of what is passed to @pm_lats
+ * @pm_lat_level: array index of the last odpl entry executed - -1 if never
+ * @dev_wakeup_lat: dev wakeup latency in nanoseconds
+ * @_dev_wakeup_lat_limit: dev wakeup latency limit in nsec - set by OMAP PM
+ * @_state: one of OMAP_DEVICE_STATE_* (see above)
+ * @flags: device flags
+ *
+ * Integrates omap_hwmod data into Linux platform_device.
+ *
+ * Field names beginning with underscores are for the internal use of
+ * the omap_device code.
+ *
+ */
+struct omap_device {
+	struct platform_device		pdev;
+	struct omap_hwmod		**hwmods;
+	struct omap_device_pm_latency	*pm_lats;
+	u32				dev_wakeup_lat;
+	u32				_dev_wakeup_lat_limit;
+	u8				pm_lats_cnt;
+	s8				pm_lat_level;
+	u8				hwmods_cnt;
+	u8				_state;
+};
+
+/* Device driver interface (call via platform_data fn ptrs) */
+
+int omap_device_enable(struct platform_device *pdev);
+int omap_device_idle(struct platform_device *pdev);
+int omap_device_shutdown(struct platform_device *pdev);
+
+/* Core code interface */
+
+int omap_device_count_resources(struct omap_device *od);
+int omap_device_fill_resources(struct omap_device *od, struct resource *res);
+
+struct omap_device *omap_device_build(const char *pdev_name, int pdev_id,
+				      struct omap_hwmod *oh, void *pdata,
+				      int pdata_len,
+				      struct omap_device_pm_latency *pm_lats,
+				      int pm_lats_cnt);
+
+struct omap_device *omap_device_build_ss(const char *pdev_name, int pdev_id,
+					 struct omap_hwmod **oh, int oh_cnt,
+					 void *pdata, int pdata_len,
+					 struct omap_device_pm_latency *pm_lats,
+					 int pm_lats_cnt);
+
+int omap_device_register(struct omap_device *od);
+
+/* OMAP PM interface */
+int omap_device_align_pm_lat(struct platform_device *pdev,
+			     u32 new_wakeup_lat_limit);
+struct powerdomain *omap_device_get_pwrdm(struct omap_device *od);
+
+/* Other */
+
+int omap_device_idle_hwmods(struct omap_device *od);
+int omap_device_enable_hwmods(struct omap_device *od);
+
+int omap_device_disable_clocks(struct omap_device *od);
+int omap_device_enable_clocks(struct omap_device *od);
+
+
+/*
+ * Entries should be kept in latency order ascending
+ *
+ * deact_lat is the maximum number of microseconds required to complete
+ * deactivate_func() at the device's slowest OPP.
+ *
+ * act_lat is the maximum number of microseconds required to complete
+ * activate_func() at the device's slowest OPP.
+ *
+ * This will result in some suboptimal power management decisions at fast
+ * OPPs, but avoids having to recompute all device power management decisions
+ * if the system shifts from a fast OPP to a slow OPP (in order to meet
+ * latency requirements).
+ *
+ * XXX should deactivate_func/activate_func() take platform_device pointers
+ * rather than omap_device pointers?
+ */
+struct omap_device_pm_latency {
+	u32 deactivate_lat;
+	int (*deactivate_func)(struct omap_device *od);
+	u32 activate_lat;
+	int (*activate_func)(struct omap_device *od);
+};
+
+
+/* Get omap_device pointer from platform_device pointer */
+#define to_omap_device(x) container_of((x), struct omap_device, pdev)
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap_hwmod.h
@@ -0,0 +1,467 @@
+/*
+ * omap_hwmod macros, structures
+ *
+ * Copyright (C) 2009 Nokia Corporation
+ * Paul Walmsley
+ *
+ * Created in collaboration with (alphabetical order): Benoit Cousson,
+ * Kevin Hilman, Tony Lindgren, Rajendra Nayak, Vikram Pandita, Sakari
+ * Poussa, Anand Sawant, Santosh Shilimkar, Richard Woodruff
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * These headers and macros are used to define OMAP on-chip module
+ * data and their integration with other OMAP modules and Linux.
+ *
+ * References:
+ * - OMAP2420 Multimedia Processor Silicon Revision 2.1.1, 2.2 (SWPU064)
+ * - OMAP2430 Multimedia Device POP Silicon Revision 2.1 (SWPU090)
+ * - OMAP34xx Multimedia Device Silicon Revision 3.1 (SWPU108)
+ * - OMAP4430 Multimedia Device Silicon Revision 1.0 (SWPU140)
+ * - Open Core Protocol Specification 2.2
+ *
+ * To do:
+ * - add interconnect error log structures
+ * - add pinmuxing
+ * - init_conn_id_bit (CONNID_BIT_VECTOR)
+ * - implement default hwmod SMS/SDRC flags?
+ *
+ */
+#ifndef __ARCH_ARM_PLAT_OMAP_INCLUDE_MACH_OMAP_HWMOD_H
+#define __ARCH_ARM_PLAT_OMAP_INCLUDE_MACH_OMAP_HWMOD_H
+
+#include <linux/kernel.h>
+#include <linux/ioport.h>
+
+#include <plat/cpu.h>
+
+struct omap_device;
+
+/* OCP SYSCONFIG bit shifts/masks */
+#define SYSC_MIDLEMODE_SHIFT		12
+#define SYSC_MIDLEMODE_MASK		(0x3 << SYSC_MIDLEMODE_SHIFT)
+#define SYSC_CLOCKACTIVITY_SHIFT	8
+#define SYSC_CLOCKACTIVITY_MASK		(0x3 << SYSC_CLOCKACTIVITY_SHIFT)
+#define SYSC_SIDLEMODE_SHIFT		3
+#define SYSC_SIDLEMODE_MASK		(0x3 << SYSC_SIDLEMODE_SHIFT)
+#define SYSC_ENAWAKEUP_SHIFT		2
+#define SYSC_ENAWAKEUP_MASK		(1 << SYSC_ENAWAKEUP_SHIFT)
+#define SYSC_SOFTRESET_SHIFT		1
+#define SYSC_SOFTRESET_MASK		(1 << SYSC_SOFTRESET_SHIFT)
+#define SYSC_AUTOIDLE_SHIFT		0
+#define SYSC_AUTOIDLE_MASK		(1 << SYSC_AUTOIDLE_SHIFT)
+
+/* OCP SYSSTATUS bit shifts/masks */
+#define SYSS_RESETDONE_SHIFT		0
+#define SYSS_RESETDONE_MASK		(1 << SYSS_RESETDONE_SHIFT)
+
+/* Master standby/slave idle mode flags */
+#define HWMOD_IDLEMODE_FORCE		(1 << 0)
+#define HWMOD_IDLEMODE_NO		(1 << 1)
+#define HWMOD_IDLEMODE_SMART		(1 << 2)
+
+
+/**
+ * struct omap_hwmod_irq_info - MPU IRQs used by the hwmod
+ * @name: name of the IRQ channel (module local name)
+ * @irq_ch: IRQ channel ID
+ *
+ * @name should be something short, e.g., "tx" or "rx".  It is for use
+ * by platform_get_resource_byname().  It is defined locally to the
+ * hwmod.
+ */
+struct omap_hwmod_irq_info {
+	const char	*name;
+	u16		irq;
+};
+
+/**
+ * struct omap_hwmod_dma_info - DMA channels used by the hwmod
+ * @name: name of the DMA channel (module local name)
+ * @dma_ch: DMA channel ID
+ *
+ * @name should be something short, e.g., "tx" or "rx".  It is for use
+ * by platform_get_resource_byname().  It is defined locally to the
+ * hwmod.
+ */
+struct omap_hwmod_dma_info {
+	const char	*name;
+	u16		dma_ch;
+};
+
+/**
+ * struct omap_hwmod_opt_clk - optional clocks used by this hwmod
+ * @role: "sys", "32k", "tv", etc -- for use in clk_get()
+ * @clkdev_dev_id: opt clock: clkdev dev_id string
+ * @clkdev_con_id: opt clock: clkdev con_id string
+ * @_clk: pointer to the struct clk (filled in at runtime)
+ *
+ * The module's interface clock and main functional clock should not
+ * be added as optional clocks.
+ */
+struct omap_hwmod_opt_clk {
+	const char	*role;
+	const char	*clkdev_dev_id;
+	const char	*clkdev_con_id;
+	struct clk	*_clk;
+};
+
+
+/* omap_hwmod_omap2_firewall.flags bits */
+#define OMAP_FIREWALL_L3		(1 << 0)
+#define OMAP_FIREWALL_L4		(1 << 1)
+
+/**
+ * struct omap_hwmod_omap2_firewall - OMAP2/3 device firewall data
+ * @l3_perm_bit: bit shift for L3_PM_*_PERMISSION_*
+ * @l4_fw_region: L4 firewall region ID
+ * @l4_prot_group: L4 protection group ID
+ * @flags: (see omap_hwmod_omap2_firewall.flags macros above)
+ */
+struct omap_hwmod_omap2_firewall {
+	u8 l3_perm_bit;
+	u8 l4_fw_region;
+	u8 l4_prot_group;
+	u8 flags;
+};
+
+
+/*
+ * omap_hwmod_addr_space.flags bits
+ *
+ * ADDR_MAP_ON_INIT: Map this address space during omap_hwmod init.
+ * ADDR_TYPE_RT: Address space contains module register target data.
+ */
+#define ADDR_MAP_ON_INIT	(1 << 0)
+#define ADDR_TYPE_RT		(1 << 1)
+
+/**
+ * struct omap_hwmod_addr_space - MPU address space handled by the hwmod
+ * @pa_start: starting physical address
+ * @pa_end: ending physical address
+ * @flags: (see omap_hwmod_addr_space.flags macros above)
+ *
+ * Address space doesn't necessarily follow physical interconnect
+ * structure.  GPMC is one example.
+ */
+struct omap_hwmod_addr_space {
+	u32 pa_start;
+	u32 pa_end;
+	u8 flags;
+};
+
+
+/*
+ * omap_hwmod_ocp_if.user bits: these indicate the initiators that use this
+ * interface to interact with the hwmod.  Used to add sleep dependencies
+ * when the module is enabled or disabled.
+ */
+#define OCP_USER_MPU			(1 << 0)
+#define OCP_USER_SDMA			(1 << 1)
+
+/* omap_hwmod_ocp_if.flags bits */
+#define OCPIF_HAS_IDLEST		(1 << 0)
+#define OCPIF_SWSUP_IDLE		(1 << 1)
+#define OCPIF_CAN_BURST			(1 << 2)
+
+/**
+ * struct omap_hwmod_ocp_if - OCP interface data
+ * @master: struct omap_hwmod that initiates OCP transactions on this link
+ * @slave: struct omap_hwmod that responds to OCP transactions on this link
+ * @addr: address space associated with this link
+ * @clkdev_dev_id: interface clock: clkdev dev_id string
+ * @clkdev_con_id: interface clock: clkdev con_id string
+ * @_clk: pointer to the interface struct clk (filled in at runtime)
+ * @fw: interface firewall data
+ * @addr_cnt: ARRAY_SIZE(@addr)
+ * @width: OCP data width
+ * @thread_cnt: number of threads
+ * @max_burst_len: maximum burst length in @width sized words (0 if unlimited)
+ * @user: initiators using this interface (see OCP_USER_* macros above)
+ * @flags: OCP interface flags (see OCPIF_* macros above)
+ *
+ * It may also be useful to add a tag_cnt field for OCP2.x devices.
+ *
+ * Parameter names beginning with an underscore are managed internally by
+ * the omap_hwmod code and should not be set during initialization.
+ */
+struct omap_hwmod_ocp_if {
+	struct omap_hwmod		*master;
+	struct omap_hwmod		*slave;
+	struct omap_hwmod_addr_space	*addr;
+	const char			*clkdev_dev_id;
+	const char			*clkdev_con_id;
+	struct clk			*_clk;
+	union {
+		struct omap_hwmod_omap2_firewall omap2;
+	}				fw;
+	u8				addr_cnt;
+	u8				width;
+	u8				thread_cnt;
+	u8				max_burst_len;
+	u8				user;
+	u8				flags;
+};
+
+
+/* Macros for use in struct omap_hwmod_sysconfig */
+
+/* Flags for use in omap_hwmod_sysconfig.idlemodes */
+#define MASTER_STANDBY_SHIFT	2
+#define SLAVE_IDLE_SHIFT	0
+#define SIDLE_FORCE		(HWMOD_IDLEMODE_FORCE << SLAVE_IDLE_SHIFT)
+#define SIDLE_NO		(HWMOD_IDLEMODE_NO << SLAVE_IDLE_SHIFT)
+#define SIDLE_SMART		(HWMOD_IDLEMODE_SMART << SLAVE_IDLE_SHIFT)
+#define MSTANDBY_FORCE		(HWMOD_IDLEMODE_FORCE << MASTER_STANDBY_SHIFT)
+#define MSTANDBY_NO		(HWMOD_IDLEMODE_NO << MASTER_STANDBY_SHIFT)
+#define MSTANDBY_SMART		(HWMOD_IDLEMODE_SMART << MASTER_STANDBY_SHIFT)
+
+/* omap_hwmod_sysconfig.sysc_flags capability flags */
+#define SYSC_HAS_AUTOIDLE	(1 << 0)
+#define SYSC_HAS_SOFTRESET	(1 << 1)
+#define SYSC_HAS_ENAWAKEUP	(1 << 2)
+#define SYSC_HAS_EMUFREE	(1 << 3)
+#define SYSC_HAS_CLOCKACTIVITY	(1 << 4)
+#define SYSC_HAS_SIDLEMODE	(1 << 5)
+#define SYSC_HAS_MIDLEMODE	(1 << 6)
+#define SYSS_MISSING		(1 << 7)
+
+/* omap_hwmod_sysconfig.clockact flags */
+#define CLOCKACT_TEST_BOTH	0x0
+#define CLOCKACT_TEST_MAIN	0x1
+#define CLOCKACT_TEST_ICLK	0x2
+#define CLOCKACT_TEST_NONE	0x3
+
+/**
+ * struct omap_hwmod_sysconfig - hwmod OCP_SYSCONFIG/OCP_SYSSTATUS data
+ * @rev_offs: IP block revision register offset (from module base addr)
+ * @sysc_offs: OCP_SYSCONFIG register offset (from module base addr)
+ * @syss_offs: OCP_SYSSTATUS register offset (from module base addr)
+ * @idlemodes: One or more of {SIDLE,MSTANDBY}_{OFF,FORCE,SMART}
+ * @sysc_flags: SYS{C,S}_HAS* flags indicating SYSCONFIG bits supported
+ * @clockact: the default value of the module CLOCKACTIVITY bits
+ *
+ * @clockact describes to the module which clocks are likely to be
+ * disabled when the PRCM issues its idle request to the module.  Some
+ * modules have separate clockdomains for the interface clock and main
+ * functional clock, and can check whether they should acknowledge the
+ * idle request based on the internal module functionality that has
+ * been associated with the clocks marked in @clockact.  This field is
+ * only used if HWMOD_SET_DEFAULT_CLOCKACT is set (see below)
+ *
+ */
+struct omap_hwmod_sysconfig {
+	u16 rev_offs;
+	u16 sysc_offs;
+	u16 syss_offs;
+	u8 idlemodes;
+	u8 sysc_flags;
+	u8 clockact;
+};
+
+/**
+ * struct omap_hwmod_omap2_prcm - OMAP2/3-specific PRCM data
+ * @module_offs: PRCM submodule offset from the start of the PRM/CM
+ * @prcm_reg_id: PRCM register ID (e.g., 3 for CM_AUTOIDLE3)
+ * @module_bit: register bit shift for AUTOIDLE, WKST, WKEN, GRPSEL regs
+ * @idlest_reg_id: IDLEST register ID (e.g., 3 for CM_IDLEST3)
+ * @idlest_idle_bit: register bit shift for CM_IDLEST slave idle bit
+ * @idlest_stdby_bit: register bit shift for CM_IDLEST master standby bit
+ *
+ * @prcm_reg_id and @module_bit are specific to the AUTOIDLE, WKST,
+ * WKEN, GRPSEL registers.  In an ideal world, no extra information
+ * would be needed for IDLEST information, but alas, there are some
+ * exceptions, so @idlest_reg_id, @idlest_idle_bit, @idlest_stdby_bit
+ * are needed for the IDLEST registers (c.f. 2430 I2CHS, 3430 USBHOST)
+ */
+struct omap_hwmod_omap2_prcm {
+	s16 module_offs;
+	u8 prcm_reg_id;
+	u8 module_bit;
+	u8 idlest_reg_id;
+	u8 idlest_idle_bit;
+	u8 idlest_stdby_bit;
+};
+
+
+/**
+ * struct omap_hwmod_omap4_prcm - OMAP4-specific PRCM data
+ * @module_offs: PRCM submodule offset from the start of the PRM/CM1/CM2
+ * @device_offs: device register offset from @module_offs
+ * @submodule_wkdep_bit: bit shift of the WKDEP range
+ */
+struct omap_hwmod_omap4_prcm {
+	u32 module_offs;
+	u16 device_offs;
+	u8 submodule_wkdep_bit;
+};
+
+
+/*
+ * omap_hwmod.flags definitions
+ *
+ * HWMOD_SWSUP_SIDLE: omap_hwmod code should manually bring module in and out
+ *     of idle, rather than relying on module smart-idle
+ * HWMOD_SWSUP_MSTDBY: omap_hwmod code should manually bring module in and out
+ *     of standby, rather than relying on module smart-standby
+ * HWMOD_INIT_NO_RESET: don't reset this module at boot - important for
+ *     SDRAM controller, etc.
+ * HWMOD_INIT_NO_IDLE: don't idle this module at boot - important for SDRAM
+ *     controller, etc.
+ * HWMOD_NO_AUTOIDLE: disable module autoidle (OCP_SYSCONFIG.AUTOIDLE)
+ *     when module is enabled, rather than the default, which is to
+ *     enable autoidle
+ * HWMOD_SET_DEFAULT_CLOCKACT: program CLOCKACTIVITY bits at startup
+ */
+#define HWMOD_SWSUP_SIDLE			(1 << 0)
+#define HWMOD_SWSUP_MSTANDBY			(1 << 1)
+#define HWMOD_INIT_NO_RESET			(1 << 2)
+#define HWMOD_INIT_NO_IDLE			(1 << 3)
+#define HWMOD_NO_OCP_AUTOIDLE			(1 << 4)
+#define HWMOD_SET_DEFAULT_CLOCKACT		(1 << 5)
+
+/*
+ * omap_hwmod._int_flags definitions
+ * These are for internal use only and are managed by the omap_hwmod code.
+ *
+ * _HWMOD_NO_MPU_PORT: no path exists for the MPU to write to this module
+ * _HWMOD_WAKEUP_ENABLED: set when the omap_hwmod code has enabled ENAWAKEUP
+ * _HWMOD_SYSCONFIG_LOADED: set when the OCP_SYSCONFIG value has been cached
+ */
+#define _HWMOD_NO_MPU_PORT			(1 << 0)
+#define _HWMOD_WAKEUP_ENABLED			(1 << 1)
+#define _HWMOD_SYSCONFIG_LOADED			(1 << 2)
+
+/*
+ * omap_hwmod._state definitions
+ *
+ * INITIALIZED: reset (optionally), initialized, enabled, disabled
+ *              (optionally)
+ *
+ *
+ */
+#define _HWMOD_STATE_UNKNOWN			0
+#define _HWMOD_STATE_REGISTERED			1
+#define _HWMOD_STATE_CLKS_INITED		2
+#define _HWMOD_STATE_INITIALIZED		3
+#define _HWMOD_STATE_ENABLED			4
+#define _HWMOD_STATE_IDLE			5
+#define _HWMOD_STATE_DISABLED			6
+
+/**
+ * struct omap_hwmod - integration data for OMAP hardware "modules" (IP blocks)
+ * @name: name of the hwmod
+ * @od: struct omap_device currently associated with this hwmod (internal use)
+ * @mpu_irqs: ptr to an array of MPU IRQs (see also mpu_irqs_cnt)
+ * @sdma_chs: ptr to an array of SDMA channel IDs (see also sdma_chs_cnt)
+ * @prcm: PRCM data pertaining to this hwmod
+ * @clkdev_dev_id: main clock: clkdev dev_id string
+ * @clkdev_con_id: main clock: clkdev con_id string
+ * @_clk: pointer to the main struct clk (filled in at runtime)
+ * @opt_clks: other device clocks that drivers can request (0..*)
+ * @masters: ptr to array of OCP ifs that this hwmod can initiate on
+ * @slaves: ptr to array of OCP ifs that this hwmod can respond on
+ * @sysconfig: device SYSCONFIG/SYSSTATUS register data
+ * @dev_attr: arbitrary device attributes that can be passed to the driver
+ * @_sysc_cache: internal-use hwmod flags
+ * @_rt_va: cached register target start address (internal use)
+ * @_mpu_port_index: cached MPU register target slave ID (internal use)
+ * @msuspendmux_reg_id: CONTROL_MSUSPENDMUX register ID (1-6)
+ * @msuspendmux_shift: CONTROL_MSUSPENDMUX register bit shift
+ * @mpu_irqs_cnt: number of @mpu_irqs
+ * @sdma_chs_cnt: number of @sdma_chs
+ * @opt_clks_cnt: number of @opt_clks
+ * @master_cnt: number of @master entries
+ * @slaves_cnt: number of @slave entries
+ * @response_lat: device OCP response latency (in interface clock cycles)
+ * @_int_flags: internal-use hwmod flags
+ * @_state: internal-use hwmod state
+ * @flags: hwmod flags (documented below)
+ * @omap_chip: OMAP chips this hwmod is present on
+ * @node: list node for hwmod list (internal use)
+ *
+ * @clkdev_dev_id, @clkdev_con_id, and @clk all refer to this module's "main
+ * clock," which for our purposes is defined as "the functional clock needed
+ * for register accesses to complete."  Modules may not have a main clock if
+ * the interface clock also serves as a main clock.
+ *
+ * Parameter names beginning with an underscore are managed internally by
+ * the omap_hwmod code and should not be set during initialization.
+ */
+struct omap_hwmod {
+	const char			*name;
+	struct omap_device		*od;
+	struct omap_hwmod_irq_info	*mpu_irqs;
+	struct omap_hwmod_dma_info	*sdma_chs;
+	union {
+		struct omap_hwmod_omap2_prcm omap2;
+		struct omap_hwmod_omap4_prcm omap4;
+	}				prcm;
+	const char			*clkdev_dev_id;
+	const char			*clkdev_con_id;
+	struct clk			*_clk;
+	struct omap_hwmod_opt_clk	*opt_clks;
+	struct omap_hwmod_ocp_if	**masters; /* connect to *_IA */
+	struct omap_hwmod_ocp_if	**slaves;  /* connect to *_TA */
+	struct omap_hwmod_sysconfig	*sysconfig;
+	void				*dev_attr;
+	u32				_sysc_cache;
+	void __iomem			*_rt_va;
+	struct list_head		node;
+	u16				flags;
+	u8				_mpu_port_index;
+	u8				msuspendmux_reg_id;
+	u8				msuspendmux_shift;
+	u8				response_lat;
+	u8				mpu_irqs_cnt;
+	u8				sdma_chs_cnt;
+	u8				opt_clks_cnt;
+	u8				masters_cnt;
+	u8				slaves_cnt;
+	u8				hwmods_cnt;
+	u8				_int_flags;
+	u8				_state;
+	const struct omap_chip_id	omap_chip;
+};
+
+int omap_hwmod_init(struct omap_hwmod **ohs);
+int omap_hwmod_register(struct omap_hwmod *oh);
+int omap_hwmod_unregister(struct omap_hwmod *oh);
+struct omap_hwmod *omap_hwmod_lookup(const char *name);
+int omap_hwmod_for_each(int (*fn)(struct omap_hwmod *oh));
+int omap_hwmod_late_init(void);
+
+int omap_hwmod_enable(struct omap_hwmod *oh);
+int omap_hwmod_idle(struct omap_hwmod *oh);
+int omap_hwmod_shutdown(struct omap_hwmod *oh);
+
+int omap_hwmod_enable_clocks(struct omap_hwmod *oh);
+int omap_hwmod_disable_clocks(struct omap_hwmod *oh);
+
+int omap_hwmod_reset(struct omap_hwmod *oh);
+void omap_hwmod_ocp_barrier(struct omap_hwmod *oh);
+
+void omap_hwmod_writel(u32 v, struct omap_hwmod *oh, u16 reg_offs);
+u32 omap_hwmod_readl(struct omap_hwmod *oh, u16 reg_offs);
+
+int omap_hwmod_count_resources(struct omap_hwmod *oh);
+int omap_hwmod_fill_resources(struct omap_hwmod *oh, struct resource *res);
+
+struct powerdomain *omap_hwmod_get_pwrdm(struct omap_hwmod *oh);
+
+int omap_hwmod_add_initiator_dep(struct omap_hwmod *oh,
+				 struct omap_hwmod *init_oh);
+int omap_hwmod_del_initiator_dep(struct omap_hwmod *oh,
+				 struct omap_hwmod *init_oh);
+
+int omap_hwmod_set_clockact_both(struct omap_hwmod *oh);
+int omap_hwmod_set_clockact_main(struct omap_hwmod *oh);
+int omap_hwmod_set_clockact_iclk(struct omap_hwmod *oh);
+int omap_hwmod_set_clockact_none(struct omap_hwmod *oh);
+
+int omap_hwmod_enable_wakeup(struct omap_hwmod *oh);
+int omap_hwmod_disable_wakeup(struct omap_hwmod *oh);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/omap-pm.h
@@ -0,0 +1,301 @@
+/*
+ * omap-pm.h - OMAP power management interface
+ *
+ * Copyright (C) 2008-2009 Texas Instruments, Inc.
+ * Copyright (C) 2008-2009 Nokia Corporation
+ * Paul Walmsley
+ *
+ * Interface developed by (in alphabetical order): Karthik Dasu, Jouni
+ * HÃ¶gander, Tony Lindgren, Rajendra Nayak, Sakari Poussa,
+ * Veeramanikandan Raju, Anand Sawant, Igor Stoppa, Paul Walmsley,
+ * Richard Woodruff
+ */
+
+#ifndef ASM_ARM_ARCH_OMAP_OMAP_PM_H
+#define ASM_ARM_ARCH_OMAP_OMAP_PM_H
+
+#include <linux/device.h>
+#include <linux/cpufreq.h>
+
+#include "powerdomain.h"
+
+/**
+ * struct omap_opp - clock frequency-to-OPP ID table for DSP, MPU
+ * @rate: target clock rate
+ * @opp_id: OPP ID
+ * @min_vdd: minimum VDD1 voltage (in millivolts) for this OPP
+ *
+ * Operating performance point data.  Can vary by OMAP chip and board.
+ */
+struct omap_opp {
+	unsigned long rate;
+	u8 opp_id;
+	u16 min_vdd;
+};
+
+extern struct omap_opp *mpu_opps;
+extern struct omap_opp *dsp_opps;
+extern struct omap_opp *l3_opps;
+
+/*
+ * agent_id values for use with omap_pm_set_min_bus_tput():
+ *
+ * OCP_INITIATOR_AGENT is only valid for devices that can act as
+ * initiators -- it represents the device's L3 interconnect
+ * connection.  OCP_TARGET_AGENT represents the device's L4
+ * interconnect connection.
+ */
+#define OCP_TARGET_AGENT		1
+#define OCP_INITIATOR_AGENT		2
+
+/**
+ * omap_pm_if_early_init - OMAP PM init code called before clock fw init
+ * @mpu_opp_table: array ptr to struct omap_opp for MPU
+ * @dsp_opp_table: array ptr to struct omap_opp for DSP
+ * @l3_opp_table : array ptr to struct omap_opp for CORE
+ *
+ * Initialize anything that must be configured before the clock
+ * framework starts.  The "_if_" is to avoid name collisions with the
+ * PM idle-loop code.
+ */
+int __init omap_pm_if_early_init(struct omap_opp *mpu_opp_table,
+				 struct omap_opp *dsp_opp_table,
+				 struct omap_opp *l3_opp_table);
+
+/**
+ * omap_pm_if_init - OMAP PM init code called after clock fw init
+ *
+ * The main initialization code.  OPP tables are passed in here.  The
+ * "_if_" is to avoid name collisions with the PM idle-loop code.
+ */
+int __init omap_pm_if_init(void);
+
+/**
+ * omap_pm_if_exit - OMAP PM exit code
+ *
+ * Exit code; currently unused.  The "_if_" is to avoid name
+ * collisions with the PM idle-loop code.
+ */
+void omap_pm_if_exit(void);
+
+/*
+ * Device-driver-originated constraints (via board-*.c files, platform_data)
+ */
+
+
+/**
+ * omap_pm_set_max_mpu_wakeup_lat - set the maximum MPU wakeup latency
+ * @dev: struct device * requesting the constraint
+ * @t: maximum MPU wakeup latency in microseconds
+ *
+ * Request that the maximum interrupt latency for the MPU to be no
+ * greater than 't' microseconds. "Interrupt latency" in this case is
+ * defined as the elapsed time from the occurrence of a hardware or
+ * timer interrupt to the time when the device driver's interrupt
+ * service routine has been entered by the MPU.
+ *
+ * It is intended that underlying PM code will use this information to
+ * determine what power state to put the MPU powerdomain into, and
+ * possibly the CORE powerdomain as well, since interrupt handling
+ * code currently runs from SDRAM.  Advanced PM or board*.c code may
+ * also configure interrupt controller priorities, OCP bus priorities,
+ * CPU speed(s), etc.
+ *
+ * This function will not affect device wakeup latency, e.g., time
+ * elapsed from when a device driver enables a hardware device with
+ * clk_enable(), to when the device is ready for register access or
+ * other use.  To control this device wakeup latency, use
+ * set_max_dev_wakeup_lat()
+ *
+ * Multiple calls to set_max_mpu_wakeup_lat() will replace the
+ * previous t value.  To remove the latency target for the MPU, call
+ * with t = -1.
+ *
+ * No return value.
+ */
+void omap_pm_set_max_mpu_wakeup_lat(struct device *dev, long t);
+
+
+/**
+ * omap_pm_set_min_bus_tput - set minimum bus throughput needed by device
+ * @dev: struct device * requesting the constraint
+ * @tbus_id: interconnect to operate on (OCP_{INITIATOR,TARGET}_AGENT)
+ * @r: minimum throughput (in KiB/s)
+ *
+ * Request that the minimum data throughput on the OCP interconnect
+ * attached to device 'dev' interconnect agent 'tbus_id' be no less
+ * than 'r' KiB/s.
+ *
+ * It is expected that the OMAP PM or bus code will use this
+ * information to set the interconnect clock to run at the lowest
+ * possible speed that satisfies all current system users.  The PM or
+ * bus code will adjust the estimate based on its model of the bus, so
+ * device driver authors should attempt to specify an accurate
+ * quantity for their device use case, and let the PM or bus code
+ * overestimate the numbers as necessary to handle request/response
+ * latency, other competing users on the system, etc.  On OMAP2/3, if
+ * a driver requests a minimum L4 interconnect speed constraint, the
+ * code will also need to add an minimum L3 interconnect speed
+ * constraint,
+ *
+ * Multiple calls to set_min_bus_tput() will replace the previous rate
+ * value for this device.  To remove the interconnect throughput
+ * restriction for this device, call with r = 0.
+ *
+ * No return value.
+ */
+void omap_pm_set_min_bus_tput(struct device *dev, u8 agent_id, unsigned long r);
+
+
+/**
+ * omap_pm_set_max_dev_wakeup_lat - set the maximum device enable latency
+ * @dev: struct device *
+ * @t: maximum device wakeup latency in microseconds
+ *
+ * Request that the maximum amount of time necessary for a device to
+ * become accessible after its clocks are enabled should be no greater
+ * than 't' microseconds.  Specifically, this represents the time from
+ * when a device driver enables device clocks with clk_enable(), to
+ * when the register reads and writes on the device will succeed.
+ * This function should be called before clk_disable() is called,
+ * since the power state transition decision may be made during
+ * clk_disable().
+ *
+ * It is intended that underlying PM code will use this information to
+ * determine what power state to put the powerdomain enclosing this
+ * device into.
+ *
+ * Multiple calls to set_max_dev_wakeup_lat() will replace the
+ * previous wakeup latency values for this device.  To remove the wakeup
+ * latency restriction for this device, call with t = -1.
+ *
+ * No return value.
+ */
+void omap_pm_set_max_dev_wakeup_lat(struct device *dev, long t);
+
+
+/**
+ * omap_pm_set_max_sdma_lat - set the maximum system DMA transfer start latency
+ * @dev: struct device *
+ * @t: maximum DMA transfer start latency in microseconds
+ *
+ * Request that the maximum system DMA transfer start latency for this
+ * device 'dev' should be no greater than 't' microseconds.  "DMA
+ * transfer start latency" here is defined as the elapsed time from
+ * when a device (e.g., McBSP) requests that a system DMA transfer
+ * start or continue, to the time at which data starts to flow into
+ * that device from the system DMA controller.
+ *
+ * It is intended that underlying PM code will use this information to
+ * determine what power state to put the CORE powerdomain into.
+ *
+ * Since system DMA transfers may not involve the MPU, this function
+ * will not affect MPU wakeup latency.  Use set_max_cpu_lat() to do
+ * so.  Similarly, this function will not affect device wakeup latency
+ * -- use set_max_dev_wakeup_lat() to affect that.
+ *
+ * Multiple calls to set_max_sdma_lat() will replace the previous t
+ * value for this device.  To remove the maximum DMA latency for this
+ * device, call with t = -1.
+ *
+ * No return value.
+ */
+void omap_pm_set_max_sdma_lat(struct device *dev, long t);
+
+
+/*
+ * DSP Bridge-specific constraints
+ */
+
+/**
+ * omap_pm_dsp_get_opp_table - get OPP->DSP clock frequency table
+ *
+ * Intended for use by DSPBridge.  Returns an array of OPP->DSP clock
+ * frequency entries.  The final item in the array should have .rate =
+ * .opp_id = 0.
+ */
+const struct omap_opp *omap_pm_dsp_get_opp_table(void);
+
+/**
+ * omap_pm_dsp_set_min_opp - receive desired OPP target ID from DSP Bridge
+ * @opp_id: target DSP OPP ID
+ *
+ * Set a minimum OPP ID for the DSP.  This is intended to be called
+ * only from the DSP Bridge MPU-side driver.  Unfortunately, the only
+ * information that code receives from the DSP/BIOS load estimator is the
+ * target OPP ID; hence, this interface.  No return value.
+ */
+void omap_pm_dsp_set_min_opp(u8 opp_id);
+
+/**
+ * omap_pm_dsp_get_opp - report the current DSP OPP ID
+ *
+ * Report the current OPP for the DSP.  Since on OMAP3, the DSP and
+ * MPU share a single voltage domain, the OPP ID returned back may
+ * represent a higher DSP speed than the OPP requested via
+ * omap_pm_dsp_set_min_opp().
+ *
+ * Returns the current VDD1 OPP ID, or 0 upon error.
+ */
+u8 omap_pm_dsp_get_opp(void);
+
+
+/*
+ * CPUFreq-originated constraint
+ *
+ * In the future, this should be handled by custom OPP clocktype
+ * functions.
+ */
+
+/**
+ * omap_pm_cpu_get_freq_table - return a cpufreq_frequency_table array ptr
+ *
+ * Provide a frequency table usable by CPUFreq for the current chip/board.
+ * Returns a pointer to a struct cpufreq_frequency_table array or NULL
+ * upon error.
+ */
+struct cpufreq_frequency_table **omap_pm_cpu_get_freq_table(void);
+
+/**
+ * omap_pm_cpu_set_freq - set the current minimum MPU frequency
+ * @f: MPU frequency in Hz
+ *
+ * Set the current minimum CPU frequency.  The actual CPU frequency
+ * used could end up higher if the DSP requested a higher OPP.
+ * Intended to be called by plat-omap/cpu_omap.c:omap_target().  No
+ * return value.
+ */
+void omap_pm_cpu_set_freq(unsigned long f);
+
+/**
+ * omap_pm_cpu_get_freq - report the current CPU frequency
+ *
+ * Returns the current MPU frequency, or 0 upon error.
+ */
+unsigned long omap_pm_cpu_get_freq(void);
+
+
+/*
+ * Device context loss tracking
+ */
+
+/**
+ * omap_pm_get_dev_context_loss_count - return count of times dev has lost ctx
+ * @dev: struct device *
+ *
+ * This function returns the number of times that the device @dev has
+ * lost its internal context.  This generally occurs on a powerdomain
+ * transition to OFF.  Drivers use this as an optimization to avoid restoring
+ * context if the device hasn't lost it.  To use, drivers should initially
+ * call this in their context save functions and store the result.  Early in
+ * the driver's context restore function, the driver should call this function
+ * again, and compare the result to the stored counter.  If they differ, the
+ * driver must restore device context.   If the number of context losses
+ * exceeds the maximum positive integer, the function will wrap to 0 and
+ * continue counting.  Returns the number of context losses for this device,
+ * or -EINVAL upon error.
+ */
+int omap_pm_get_dev_context_loss_count(struct device *dev);
+
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/onenand.h
@@ -0,0 +1,43 @@
+/*
+ * arch/arm/plat-omap/include/mach/onenand.h
+ *
+ * Copyright (C) 2006 Nokia Corporation
+ * Author: Juha Yrjola
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+
+#define ONENAND_SYNC_READ	(1 << 0)
+#define ONENAND_SYNC_READWRITE	(1 << 1)
+
+struct omap_onenand_platform_data {
+	int			cs;
+	int			gpio_irq;
+	struct mtd_partition	*parts;
+	int			nr_parts;
+	int                     (*onenand_setup)(void __iomem *, int freq);
+	int			dma_channel;
+	u8			flags;
+};
+
+#define ONENAND_MAX_PARTITIONS 8
+
+#if defined(CONFIG_MTD_ONENAND_OMAP2) || \
+	defined(CONFIG_MTD_ONENAND_OMAP2_MODULE)
+
+extern void gpmc_onenand_init(struct omap_onenand_platform_data *d);
+
+#else
+
+#define board_onenand_data	NULL
+
+static inline void gpmc_onenand_init(struct omap_onenand_platform_data *d)
+{
+}
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/param.h
@@ -0,0 +1,8 @@
+/*
+ *  arch/arm/plat-omap/include/mach/param.h
+ *
+ */
+
+#ifdef CONFIG_OMAP_32K_TIMER_HZ
+#define HZ	CONFIG_OMAP_32K_TIMER_HZ
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/powerdomain.h
@@ -0,0 +1,187 @@
+/*
+ * OMAP2/3 powerdomain control
+ *
+ * Copyright (C) 2007-8 Texas Instruments, Inc.
+ * Copyright (C) 2007-8 Nokia Corporation
+ *
+ * Written by Paul Walmsley
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef ASM_ARM_ARCH_OMAP_POWERDOMAIN
+#define ASM_ARM_ARCH_OMAP_POWERDOMAIN
+
+#include <linux/types.h>
+#include <linux/list.h>
+
+#include <asm/atomic.h>
+
+#include <plat/cpu.h>
+
+
+/* Powerdomain basic power states */
+#define PWRDM_POWER_OFF		0x0
+#define PWRDM_POWER_RET		0x1
+#define PWRDM_POWER_INACTIVE	0x2
+#define PWRDM_POWER_ON		0x3
+
+#define PWRDM_MAX_PWRSTS	4
+
+/* Powerdomain allowable state bitfields */
+#define PWRSTS_OFF_ON		((1 << PWRDM_POWER_OFF) | \
+				 (1 << PWRDM_POWER_ON))
+
+#define PWRSTS_OFF_RET		((1 << PWRDM_POWER_OFF) | \
+				 (1 << PWRDM_POWER_RET))
+
+#define PWRSTS_OFF_RET_ON	(PWRSTS_OFF_RET | (1 << PWRDM_POWER_ON))
+
+
+/* Powerdomain flags */
+#define PWRDM_HAS_HDWR_SAR	(1 << 0) /* hardware save-and-restore support */
+#define PWRDM_HAS_MPU_QUIRK	(1 << 1) /* MPU pwr domain has MEM bank 0 bits
+					  * in MEM bank 1 position. This is
+					  * true for OMAP3430
+					  */
+
+/*
+ * Number of memory banks that are power-controllable.	On OMAP3430, the
+ * maximum is 4.
+ */
+#define PWRDM_MAX_MEM_BANKS	4
+
+/*
+ * Maximum number of clockdomains that can be associated with a powerdomain.
+ * CORE powerdomain on OMAP3 is the worst case
+ */
+#define PWRDM_MAX_CLKDMS	4
+
+/* XXX A completely arbitrary number. What is reasonable here? */
+#define PWRDM_TRANSITION_BAILOUT 100000
+
+struct clockdomain;
+struct powerdomain;
+
+/* Encodes dependencies between powerdomains - statically defined */
+struct pwrdm_dep {
+
+	/* Powerdomain name */
+	const char *pwrdm_name;
+
+	/* Powerdomain pointer - resolved by the powerdomain code */
+	struct powerdomain *pwrdm;
+
+	/* Flags to mark OMAP chip restrictions, etc. */
+	const struct omap_chip_id omap_chip;
+
+};
+
+struct powerdomain {
+
+	/* Powerdomain name */
+	const char *name;
+
+	/* the address offset from CM_BASE/PRM_BASE */
+	const s16 prcm_offs;
+
+	/* Used to represent the OMAP chip types containing this pwrdm */
+	const struct omap_chip_id omap_chip;
+
+	/* Powerdomains that can be told to wake this powerdomain up */
+	struct pwrdm_dep *wkdep_srcs;
+
+	/* Powerdomains that can be told to keep this pwrdm from inactivity */
+	struct pwrdm_dep *sleepdep_srcs;
+
+	/* Bit shift of this powerdomain's PM_WKDEP/CM_SLEEPDEP bit */
+	const u8 dep_bit;
+
+	/* Possible powerdomain power states */
+	const u8 pwrsts;
+
+	/* Possible logic power states when pwrdm in RETENTION */
+	const u8 pwrsts_logic_ret;
+
+	/* Powerdomain flags */
+	const u8 flags;
+
+	/* Number of software-controllable memory banks in this powerdomain */
+	const u8 banks;
+
+	/* Possible memory bank pwrstates when pwrdm in RETENTION */
+	const u8 pwrsts_mem_ret[PWRDM_MAX_MEM_BANKS];
+
+	/* Possible memory bank pwrstates when pwrdm is ON */
+	const u8 pwrsts_mem_on[PWRDM_MAX_MEM_BANKS];
+
+	/* Clockdomains in this powerdomain */
+	struct clockdomain *pwrdm_clkdms[PWRDM_MAX_CLKDMS];
+
+	struct list_head node;
+
+	int state;
+	unsigned state_counter[PWRDM_MAX_PWRSTS];
+
+#ifdef CONFIG_PM_DEBUG
+	s64 timer;
+	s64 state_timer[PWRDM_MAX_PWRSTS];
+#endif
+};
+
+
+void pwrdm_init(struct powerdomain **pwrdm_list);
+
+int pwrdm_register(struct powerdomain *pwrdm);
+int pwrdm_unregister(struct powerdomain *pwrdm);
+struct powerdomain *pwrdm_lookup(const char *name);
+
+int pwrdm_for_each(int (*fn)(struct powerdomain *pwrdm, void *user),
+			void *user);
+int pwrdm_for_each_nolock(int (*fn)(struct powerdomain *pwrdm, void *user),
+			void *user);
+
+int pwrdm_add_clkdm(struct powerdomain *pwrdm, struct clockdomain *clkdm);
+int pwrdm_del_clkdm(struct powerdomain *pwrdm, struct clockdomain *clkdm);
+int pwrdm_for_each_clkdm(struct powerdomain *pwrdm,
+			 int (*fn)(struct powerdomain *pwrdm,
+				   struct clockdomain *clkdm));
+
+int pwrdm_add_wkdep(struct powerdomain *pwrdm1, struct powerdomain *pwrdm2);
+int pwrdm_del_wkdep(struct powerdomain *pwrdm1, struct powerdomain *pwrdm2);
+int pwrdm_read_wkdep(struct powerdomain *pwrdm1, struct powerdomain *pwrdm2);
+int pwrdm_add_sleepdep(struct powerdomain *pwrdm1, struct powerdomain *pwrdm2);
+int pwrdm_del_sleepdep(struct powerdomain *pwrdm1, struct powerdomain *pwrdm2);
+int pwrdm_read_sleepdep(struct powerdomain *pwrdm1, struct powerdomain *pwrdm2);
+
+int pwrdm_get_mem_bank_count(struct powerdomain *pwrdm);
+
+int pwrdm_set_next_pwrst(struct powerdomain *pwrdm, u8 pwrst);
+int pwrdm_read_next_pwrst(struct powerdomain *pwrdm);
+int pwrdm_read_pwrst(struct powerdomain *pwrdm);
+int pwrdm_read_prev_pwrst(struct powerdomain *pwrdm);
+int pwrdm_clear_all_prev_pwrst(struct powerdomain *pwrdm);
+
+int pwrdm_set_logic_retst(struct powerdomain *pwrdm, u8 pwrst);
+int pwrdm_set_mem_onst(struct powerdomain *pwrdm, u8 bank, u8 pwrst);
+int pwrdm_set_mem_retst(struct powerdomain *pwrdm, u8 bank, u8 pwrst);
+
+int pwrdm_read_logic_pwrst(struct powerdomain *pwrdm);
+int pwrdm_read_prev_logic_pwrst(struct powerdomain *pwrdm);
+int pwrdm_read_mem_pwrst(struct powerdomain *pwrdm, u8 bank);
+int pwrdm_read_prev_mem_pwrst(struct powerdomain *pwrdm, u8 bank);
+
+int pwrdm_enable_hdwr_sar(struct powerdomain *pwrdm);
+int pwrdm_disable_hdwr_sar(struct powerdomain *pwrdm);
+bool pwrdm_has_hdwr_sar(struct powerdomain *pwrdm);
+
+int pwrdm_wait_transition(struct powerdomain *pwrdm);
+
+int pwrdm_state_switch(struct powerdomain *pwrdm);
+int pwrdm_clkdm_state_switch(struct clockdomain *clkdm);
+int pwrdm_pre_transition(void);
+int pwrdm_post_transition(void);
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/prcm.h
@@ -0,0 +1,39 @@
+/*
+ * arch/arm/plat-omap/include/mach/prcm.h
+ *
+ * Access definations for use in OMAP24XX clock and power management
+ *
+ * Copyright (C) 2005 Texas Instruments, Inc.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
+ */
+
+#ifndef __ASM_ARM_ARCH_OMAP_PRCM_H
+#define __ASM_ARM_ARCH_OMAP_PRCM_H
+
+u32 omap_prcm_get_reset_sources(void);
+void omap_prcm_arch_reset(char mode);
+int omap2_cm_wait_idlest(void __iomem *reg, u32 mask, const char *name);
+
+#define START_PADCONF_SAVE 0x2
+#define PADCONF_SAVE_DONE  0x1
+
+void omap3_prcm_save_context(void);
+void omap3_prcm_restore_context(void);
+
+#endif
+
+
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/sdrc.h
@@ -0,0 +1,158 @@
+#ifndef ____ASM_ARCH_SDRC_H
+#define ____ASM_ARCH_SDRC_H
+
+/*
+ * OMAP2/3 SDRC/SMS register definitions
+ *
+ * Copyright (C) 2007-2008 Texas Instruments, Inc.
+ * Copyright (C) 2007-2008 Nokia Corporation
+ *
+ * Tony Lindgren
+ * Paul Walmsley
+ * Richard Woodruff
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <mach/io.h>
+
+/* SDRC register offsets - read/write with sdrc_{read,write}_reg() */
+
+#define SDRC_SYSCONFIG		0x010
+#define SDRC_CS_CFG		0x040
+#define SDRC_SHARING		0x044
+#define SDRC_ERR_TYPE		0x04C
+#define SDRC_DLLA_CTRL		0x060
+#define SDRC_DLLA_STATUS	0x064
+#define SDRC_DLLB_CTRL		0x068
+#define SDRC_DLLB_STATUS	0x06C
+#define SDRC_POWER		0x070
+#define SDRC_MCFG_0		0x080
+#define SDRC_MR_0		0x084
+#define SDRC_EMR2_0		0x08c
+#define SDRC_ACTIM_CTRL_A_0	0x09c
+#define SDRC_ACTIM_CTRL_B_0	0x0a0
+#define SDRC_RFR_CTRL_0		0x0a4
+#define SDRC_MANUAL_0		0x0a8
+#define SDRC_MCFG_1		0x0B0
+#define SDRC_MR_1		0x0B4
+#define SDRC_EMR2_1		0x0BC
+#define SDRC_ACTIM_CTRL_A_1	0x0C4
+#define SDRC_ACTIM_CTRL_B_1	0x0C8
+#define SDRC_RFR_CTRL_1		0x0D4
+#define SDRC_MANUAL_1		0x0D8
+
+#define SDRC_POWER_AUTOCOUNT_SHIFT	8
+#define SDRC_POWER_AUTOCOUNT_MASK	(0xffff << SDRC_POWER_AUTOCOUNT_SHIFT)
+#define SDRC_POWER_CLKCTRL_SHIFT	4
+#define SDRC_POWER_CLKCTRL_MASK		(0x3 << SDRC_POWER_CLKCTRL_SHIFT)
+#define SDRC_SELF_REFRESH_ON_AUTOCOUNT	(0x2 << SDRC_POWER_CLKCTRL_SHIFT)
+
+/*
+ * These values represent the number of memory clock cycles between
+ * autorefresh initiation.  They assume 1 refresh per 64 ms (JEDEC), 8192
+ * rows per device, and include a subtraction of a 50 cycle window in the
+ * event that the autorefresh command is delayed due to other SDRC activity.
+ * The '| 1' sets the ARE field to send one autorefresh when the autorefresh
+ * counter reaches 0.
+ *
+ * These represent optimal values for common parts, it won't work for all.
+ * As long as you scale down, most parameters are still work, they just
+ * become sub-optimal. The RFR value goes in the opposite direction. If you
+ * don't adjust it down as your clock period increases the refresh interval
+ * will not be met. Setting all parameters for complete worst case may work,
+ * but may cut memory performance by 2x. Due to errata the DLLs need to be
+ * unlocked and their value needs run time calibration.	A dynamic call is
+ * need for that as no single right value exists acorss production samples.
+ *
+ * Only the FULL speed values are given. Current code is such that rate
+ * changes must be made at DPLLoutx2. The actual value adjustment for low
+ * frequency operation will be handled by omap_set_performance()
+ *
+ * By having the boot loader boot up in the fastest L4 speed available likely
+ * will result in something which you can switch between.
+ */
+#define SDRC_RFR_CTRL_165MHz	(0x00044c00 | 1)
+#define SDRC_RFR_CTRL_133MHz	(0x0003de00 | 1)
+#define SDRC_RFR_CTRL_100MHz	(0x0002da01 | 1)
+#define SDRC_RFR_CTRL_110MHz	(0x0002da01 | 1) /* Need to calc */
+#define SDRC_RFR_CTRL_BYPASS	(0x00005000 | 1) /* Need to calc */
+
+
+/*
+ * SMS register access
+ */
+
+#define OMAP242X_SMS_REGADDR(reg)					\
+		(void __iomem *)OMAP2_L3_IO_ADDRESS(OMAP2420_SMS_BASE + reg)
+#define OMAP243X_SMS_REGADDR(reg)					\
+		(void __iomem *)OMAP2_L3_IO_ADDRESS(OMAP243X_SMS_BASE + reg)
+#define OMAP343X_SMS_REGADDR(reg)					\
+		(void __iomem *)OMAP2_L3_IO_ADDRESS(OMAP343X_SMS_BASE + reg)
+
+/* SMS register offsets - read/write with sms_{read,write}_reg() */
+
+#define SMS_SYSCONFIG			0x010
+#define SMS_ROT_CONTROL(context)	(0x180 + 0x10 * context)
+#define SMS_ROT_SIZE(context)		(0x184 + 0x10 * context)
+#define SMS_ROT_PHYSICAL_BA(context)	(0x188 + 0x10 * context)
+/* REVISIT: fill in other SMS registers here */
+
+
+#ifndef __ASSEMBLER__
+
+/**
+ * struct omap_sdrc_params - SDRC parameters for a given SDRC clock rate
+ * @rate: SDRC clock rate (in Hz)
+ * @actim_ctrla: Value to program to SDRC_ACTIM_CTRLA for this rate
+ * @actim_ctrlb: Value to program to SDRC_ACTIM_CTRLB for this rate
+ * @rfr_ctrl: Value to program to SDRC_RFR_CTRL for this rate
+ * @mr: Value to program to SDRC_MR for this rate
+ *
+ * This structure holds a pre-computed set of register values for the
+ * SDRC for a given SDRC clock rate and SDRAM chip.  These are
+ * intended to be pre-computed and specified in an array in the board-*.c
+ * files.  The structure is keyed off the 'rate' field.
+ */
+struct omap_sdrc_params {
+	unsigned long rate;
+	u32 actim_ctrla;
+	u32 actim_ctrlb;
+	u32 rfr_ctrl;
+	u32 mr;
+};
+
+void __init omap2_sdrc_init(struct omap_sdrc_params *sdrc_cs0,
+			    struct omap_sdrc_params *sdrc_cs1);
+int omap2_sdrc_get_params(unsigned long r,
+			  struct omap_sdrc_params **sdrc_cs0,
+			  struct omap_sdrc_params **sdrc_cs1);
+void omap2_sms_save_context(void);
+void omap2_sms_restore_context(void);
+
+void omap2_sms_write_rot_control(u32 val, unsigned ctx);
+void omap2_sms_write_rot_size(u32 val, unsigned ctx);
+void omap2_sms_write_rot_physical_ba(u32 val, unsigned ctx);
+
+#ifdef CONFIG_ARCH_OMAP2
+
+struct memory_timings {
+	u32 m_type;		/* ddr = 1, sdr = 0 */
+	u32 dll_mode;		/* use lock mode = 1, unlock mode = 0 */
+	u32 slow_dll_ctrl;	/* unlock mode, dll value for slow speed */
+	u32 fast_dll_ctrl;	/* unlock mode, dll value for fast speed */
+	u32 base_cs;		/* base chip select to use for calculations */
+};
+
+extern void omap2xxx_sdrc_init_params(u32 force_lock_to_unlock_mode);
+
+u32 omap2xxx_sdrc_dll_is_unlocked(void);
+u32 omap2xxx_sdrc_reprogram(u32 level, u32 force);
+
+#endif  /* CONFIG_ARCH_OMAP2 */
+
+#endif  /* __ASSEMBLER__ */
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/serial.h
@@ -0,0 +1,65 @@
+/*
+ * arch/arm/plat-omap/include/mach/serial.h
+ *
+ * Copyright (C) 2009 Texas Instruments
+ * Addded OMAP4 support- Santosh Shilimkar <santosh.shilimkar@ti.com>
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+ * GNU General Public License for more details.
+ */
+
+#ifndef __ASM_ARCH_SERIAL_H
+#define __ASM_ARCH_SERIAL_H
+
+#include <linux/init.h>
+
+#if defined(CONFIG_ARCH_OMAP1)
+/* OMAP1 serial ports */
+#define OMAP_UART1_BASE		0xfffb0000
+#define OMAP_UART2_BASE		0xfffb0800
+#define OMAP_UART3_BASE		0xfffb9800
+#elif defined(CONFIG_ARCH_OMAP2)
+/* OMAP2 serial ports */
+#define OMAP_UART1_BASE		0x4806a000
+#define OMAP_UART2_BASE		0x4806c000
+#define OMAP_UART3_BASE		0x4806e000
+#elif defined(CONFIG_ARCH_OMAP3)
+/* OMAP3 serial ports */
+#define OMAP_UART1_BASE		0x4806a000
+#define OMAP_UART2_BASE		0x4806c000
+#define OMAP_UART3_BASE		0x49020000
+#elif defined(CONFIG_ARCH_OMAP4)
+/* OMAP4 serial ports */
+#define OMAP_UART1_BASE		0x4806a000
+#define OMAP_UART2_BASE		0x4806c000
+#define OMAP_UART3_BASE		0x48020000
+#define OMAP_UART4_BASE		0x4806e000
+#endif
+
+#define OMAP1510_BASE_BAUD	(12000000/16)
+#define OMAP16XX_BASE_BAUD	(48000000/16)
+#define OMAP24XX_BASE_BAUD	(48000000/16)
+
+#define is_omap_port(pt)	({int __ret = 0;			\
+			if ((pt)->port.mapbase == OMAP_UART1_BASE ||	\
+			    (pt)->port.mapbase == OMAP_UART2_BASE ||	\
+			    (pt)->port.mapbase == OMAP_UART3_BASE)	\
+				__ret = 1;				\
+			__ret;						\
+			})
+
+#ifndef __ASSEMBLER__
+extern void __init omap_serial_early_init(void);
+extern void omap_serial_init(void);
+extern void omap_serial_init_port(int port);
+extern int omap_uart_can_sleep(void);
+extern void omap_uart_check_wakeup(void);
+extern void omap_uart_prepare_suspend(void);
+extern void omap_uart_prepare_idle(int num);
+extern void omap_uart_resume_idle(int num);
+extern void omap_uart_enable_irqs(int enable);
+#endif
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/smp.h
@@ -0,0 +1,53 @@
+/*
+ * OMAP4 machine specific smp.h
+ *
+ * Copyright (C) 2009 Texas Instruments, Inc.
+ *
+ * Author:
+ *	Santosh Shilimkar <santosh.shilimkar@ti.com>
+ *
+ * Interface functions needed for the SMP. This file is based on arm
+ * realview smp platform.
+ * Copyright (c) 2003 ARM Limited.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+#ifndef OMAP_ARCH_SMP_H
+#define OMAP_ARCH_SMP_H
+
+#include <asm/hardware/gic.h>
+
+/*
+ * set_event() is used to wake up secondary core from wfe using sev. ROM
+ * code puts the second core into wfe(standby).
+ *
+ */
+#define set_event()	__asm__ __volatile__ ("sev" : : : "memory")
+
+/* Needed for secondary core boot */
+extern void omap_secondary_startup(void);
+extern u32 omap_modify_auxcoreboot0(u32 set_mask, u32 clear_mask);
+extern void omap_auxcoreboot_addr(u32 cpu_addr);
+
+/*
+ * We use Soft IRQ1 as the IPI
+ */
+static inline void smp_cross_call(const struct cpumask *mask)
+{
+	gic_raise_softirq(mask, 1);
+}
+
+/*
+ * Read MPIDR: Multiprocessor affinity register
+ */
+#define hard_smp_processor_id()			\
+	({						\
+		unsigned int cpunum;			\
+		__asm__("mrc p15, 0, %0, c0, c0, 5"	\
+			: "=r" (cpunum));		\
+		cpunum &= 0x0F;				\
+	})
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/sram.h
@@ -0,0 +1,78 @@
+/*
+ * arch/arm/plat-omap/include/mach/sram.h
+ *
+ * Interface for functions that need to be run in internal SRAM
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#ifndef __ARCH_ARM_OMAP_SRAM_H
+#define __ARCH_ARM_OMAP_SRAM_H
+
+extern int __init omap_sram_init(void);
+extern void * omap_sram_push(void * start, unsigned long size);
+extern void omap_sram_reprogram_clock(u32 dpllctl, u32 ckctl);
+
+extern void omap2_sram_ddr_init(u32 *slow_dll_ctrl, u32 fast_dll_ctrl,
+				u32 base_cs, u32 force_unlock);
+extern void omap2_sram_reprogram_sdrc(u32 perf_level, u32 dll_val,
+				      u32 mem_type);
+extern u32 omap2_set_prcm(u32 dpll_ctrl_val, u32 sdrc_rfr_val, int bypass);
+
+extern u32 omap3_configure_core_dpll(
+			u32 m2, u32 unlock_dll, u32 f, u32 inc,
+			u32 sdrc_rfr_ctrl_0, u32 sdrc_actim_ctrl_a_0,
+			u32 sdrc_actim_ctrl_b_0, u32 sdrc_mr_0,
+			u32 sdrc_rfr_ctrl_1, u32 sdrc_actim_ctrl_a_1,
+			u32 sdrc_actim_ctrl_b_1, u32 sdrc_mr_1);
+extern void omap3_sram_restore_context(void);
+
+/* Do not use these */
+extern void omap1_sram_reprogram_clock(u32 ckctl, u32 dpllctl);
+extern unsigned long omap1_sram_reprogram_clock_sz;
+
+extern void omap24xx_sram_reprogram_clock(u32 ckctl, u32 dpllctl);
+extern unsigned long omap24xx_sram_reprogram_clock_sz;
+
+extern void omap242x_sram_ddr_init(u32 *slow_dll_ctrl, u32 fast_dll_ctrl,
+						u32 base_cs, u32 force_unlock);
+extern unsigned long omap242x_sram_ddr_init_sz;
+
+extern u32 omap242x_sram_set_prcm(u32 dpll_ctrl_val, u32 sdrc_rfr_val,
+						int bypass);
+extern unsigned long omap242x_sram_set_prcm_sz;
+
+extern void omap242x_sram_reprogram_sdrc(u32 perf_level, u32 dll_val,
+						u32 mem_type);
+extern unsigned long omap242x_sram_reprogram_sdrc_sz;
+
+
+extern void omap243x_sram_ddr_init(u32 *slow_dll_ctrl, u32 fast_dll_ctrl,
+						u32 base_cs, u32 force_unlock);
+extern unsigned long omap243x_sram_ddr_init_sz;
+
+extern u32 omap243x_sram_set_prcm(u32 dpll_ctrl_val, u32 sdrc_rfr_val,
+						int bypass);
+extern unsigned long omap243x_sram_set_prcm_sz;
+
+extern void omap243x_sram_reprogram_sdrc(u32 perf_level, u32 dll_val,
+						u32 mem_type);
+extern unsigned long omap243x_sram_reprogram_sdrc_sz;
+
+extern u32 omap3_sram_configure_core_dpll(
+			u32 m2, u32 unlock_dll, u32 f, u32 inc,
+			u32 sdrc_rfr_ctrl_0, u32 sdrc_actim_ctrl_a_0,
+			u32 sdrc_actim_ctrl_b_0, u32 sdrc_mr_0,
+			u32 sdrc_rfr_ctrl_1, u32 sdrc_actim_ctrl_a_1,
+			u32 sdrc_actim_ctrl_b_1, u32 sdrc_mr_1);
+extern unsigned long omap3_sram_configure_core_dpll_sz;
+
+#ifdef CONFIG_PM
+extern void omap_push_sram_idle(void);
+#else
+static inline void omap_push_sram_idle(void) {}
+#endif /* CONFIG_PM */
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/system.h
@@ -0,0 +1,51 @@
+/*
+ * Copied from arch/arm/mach-sa1100/include/mach/system.h
+ * Copyright (c) 1999 Nicolas Pitre <nico@fluxnic.net>
+ */
+#ifndef __ASM_ARCH_SYSTEM_H
+#define __ASM_ARCH_SYSTEM_H
+#include <linux/clk.h>
+
+#include <asm/mach-types.h>
+#include <mach/hardware.h>
+
+#include <plat/prcm.h>
+
+#ifndef CONFIG_MACH_VOICEBLUE
+#define voiceblue_reset()		do {} while (0)
+#else
+extern void voiceblue_reset(void);
+#endif
+
+static inline void arch_idle(void)
+{
+	cpu_do_idle();
+}
+
+static inline void omap1_arch_reset(char mode)
+{
+	/*
+	 * Workaround for 5912/1611b bug mentioned in sprz209d.pdf p. 28
+	 * "Global Software Reset Affects Traffic Controller Frequency".
+	 */
+	if (cpu_is_omap5912()) {
+		omap_writew(omap_readw(DPLL_CTL) & ~(1 << 4),
+				 DPLL_CTL);
+		omap_writew(0x8, ARM_RSTCT1);
+	}
+
+	if (machine_is_voiceblue())
+		voiceblue_reset();
+	else
+		omap_writew(1, ARM_RSTCT1);
+}
+
+static inline void arch_reset(char mode, const char *cmd)
+{
+	if (!cpu_class_is_omap2())
+		omap1_arch_reset(mode);
+	else
+		omap_prcm_arch_reset(mode);
+}
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/tc.h
@@ -0,0 +1,106 @@
+/*
+ * arch/arm/plat-omap/include/mach/tc.h
+ *
+ * OMAP Traffic Controller
+ *
+ * Copyright (C) 2004 Nokia Corporation
+ * Author: Imre Deak <imre.deak@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 59 Temple Place - Suite 330, Boston, MA  02111-1307, USA.
+ */
+
+#ifndef __ASM_ARCH_TC_H
+#define __ASM_ARCH_TC_H
+
+#define TCMIF_BASE		0xfffecc00
+#define OMAP_TC_OCPT1_PRIOR	(TCMIF_BASE + 0x00)
+#define OMAP_TC_EMIFS_PRIOR	(TCMIF_BASE + 0x04)
+#define OMAP_TC_EMIFF_PRIOR	(TCMIF_BASE + 0x08)
+#define EMIFS_CONFIG		(TCMIF_BASE + 0x0c)
+#define EMIFS_CS0_CONFIG	(TCMIF_BASE + 0x10)
+#define EMIFS_CS1_CONFIG	(TCMIF_BASE + 0x14)
+#define EMIFS_CS2_CONFIG	(TCMIF_BASE + 0x18)
+#define EMIFS_CS3_CONFIG	(TCMIF_BASE + 0x1c)
+#define EMIFF_SDRAM_CONFIG	(TCMIF_BASE + 0x20)
+#define EMIFF_MRS		(TCMIF_BASE + 0x24)
+#define TC_TIMEOUT1		(TCMIF_BASE + 0x28)
+#define TC_TIMEOUT2		(TCMIF_BASE + 0x2c)
+#define TC_TIMEOUT3		(TCMIF_BASE + 0x30)
+#define TC_ENDIANISM		(TCMIF_BASE + 0x34)
+#define EMIFF_SDRAM_CONFIG_2	(TCMIF_BASE + 0x3c)
+#define EMIF_CFG_DYNAMIC_WS	(TCMIF_BASE + 0x40)
+#define EMIFS_ACS0		(TCMIF_BASE + 0x50)
+#define EMIFS_ACS1		(TCMIF_BASE + 0x54)
+#define EMIFS_ACS2		(TCMIF_BASE + 0x58)
+#define EMIFS_ACS3		(TCMIF_BASE + 0x5c)
+#define OMAP_TC_OCPT2_PRIOR	(TCMIF_BASE + 0xd0)
+
+/* external EMIFS chipselect regions */
+#define	OMAP_CS0_PHYS		0x00000000
+#define	OMAP_CS0_SIZE		SZ_64M
+
+#define	OMAP_CS1_PHYS		0x04000000
+#define	OMAP_CS1_SIZE		SZ_64M
+
+#define	OMAP_CS1A_PHYS		OMAP_CS1_PHYS
+#define	OMAP_CS1A_SIZE		SZ_32M
+
+#define	OMAP_CS1B_PHYS		(OMAP_CS1A_PHYS + OMAP_CS1A_SIZE)
+#define	OMAP_CS1B_SIZE		SZ_32M
+
+#define	OMAP_CS2_PHYS		0x08000000
+#define	OMAP_CS2_SIZE		SZ_64M
+
+#define	OMAP_CS2A_PHYS		OMAP_CS2_PHYS
+#define	OMAP_CS2A_SIZE		SZ_32M
+
+#define	OMAP_CS2B_PHYS		(OMAP_CS2A_PHYS + OMAP_CS2A_SIZE)
+#define	OMAP_CS2B_SIZE		SZ_32M
+
+#define	OMAP_CS3_PHYS		0x0c000000
+#define	OMAP_CS3_SIZE		SZ_64M
+
+#ifndef	__ASSEMBLER__
+
+/* EMIF Slow Interface Configuration Register */
+#define OMAP_EMIFS_CONFIG_FR		(1 << 4)
+#define OMAP_EMIFS_CONFIG_PDE		(1 << 3)
+#define OMAP_EMIFS_CONFIG_PWD_EN	(1 << 2)
+#define OMAP_EMIFS_CONFIG_BM		(1 << 1)
+#define OMAP_EMIFS_CONFIG_WP		(1 << 0)
+
+#define EMIFS_CCS(n)		(EMIFS_CS0_CONFIG + (4 * (n)))
+#define EMIFS_ACS(n)		(EMIFS_ACS0 + (4 * (n)))
+
+/* Almost all documentation for chip and board memory maps assumes
+ * BM is clear.  Most devel boards have a switch to control booting
+ * from NOR flash (using external chipselect 3) rather than mask ROM,
+ * which uses BM to interchange the physical CS0 and CS3 addresses.
+ */
+static inline u32 omap_cs0_phys(void)
+{
+	return (omap_readl(EMIFS_CONFIG) & OMAP_EMIFS_CONFIG_BM)
+			?  OMAP_CS3_PHYS : 0;
+}
+
+static inline u32 omap_cs3_phys(void)
+{
+	return (omap_readl(EMIFS_CONFIG) & OMAP_EMIFS_CONFIG_BM)
+			? 0 : OMAP_CS3_PHYS;
+}
+
+#endif	/* __ASSEMBLER__ */
+
+#endif	/* __ASM_ARCH_TC_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/timer-gp.h
@@ -0,0 +1,17 @@
+/*
+ * OMAP2/3 GPTIMER support.headers
+ *
+ * Copyright (C) 2009 Nokia Corporation
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License. See the file "COPYING" in the main directory of this archive
+ * for more details.
+ */
+
+#ifndef __ARCH_ARM_PLAT_OMAP_INCLUDE_MACH_TIMER_GP_H
+#define __ARCH_ARM_PLAT_OMAP_INCLUDE_MACH_TIMER_GP_H
+
+int __init omap2_gp_clockevent_set_gptimer(u8 id);
+
+#endif
+
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/timex.h
@@ -0,0 +1,41 @@
+/*
+ * arch/arm/plat-omap/include/mach/timex.h
+ *
+ * Copyright (C) 2000 RidgeRun, Inc.
+ * Author:  Greg Lonnon <glonnon@ridgerun.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * THIS SOFTWARE IS PROVIDED ``AS IS'' AND ANY EXPRESS OR IMPLIED
+ * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN
+ * NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY DIRECT, INDIRECT,
+ * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
+ * NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
+ * USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
+ * ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
+ * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ *
+ * You should have received a copy of the  GNU General Public License along
+ * with this program; if not, write  to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#if !defined(__ASM_ARCH_OMAP_TIMEX_H)
+#define __ASM_ARCH_OMAP_TIMEX_H
+
+/*
+ * OMAP 32KHz timer updates time one jiffie at a time from a secondary timer,
+ * and that's why the CLOCK_TICK_RATE is not 32768.
+ */
+#ifdef CONFIG_OMAP_32K_TIMER
+#define CLOCK_TICK_RATE		(CONFIG_OMAP_32K_TIMER_HZ)
+#else
+#define CLOCK_TICK_RATE		(HZ * 100000UL)
+#endif
+
+#endif /* __ASM_ARCH_OMAP_TIMEX_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/uncompress.h
@@ -0,0 +1,88 @@
+/*
+ * arch/arm/plat-omap/include/mach/uncompress.h
+ *
+ * Serial port stubs for kernel decompress status messages
+ *
+ * Initially based on:
+ * linux-2.4.15-rmk1-dsplinux1.6/arch/arm/plat-omap/include/mach1510/uncompress.h
+ * Copyright (C) 2000 RidgeRun, Inc.
+ * Author: Greg Lonnon <glonnon@ridgerun.com>
+ *
+ * Rewritten by:
+ * Author: <source@mvista.com>
+ * 2004 (c) MontaVista Software, Inc.
+ *
+ * This file is licensed under the terms of the GNU General Public License
+ * version 2. This program is licensed "as is" without any warranty of any
+ * kind, whether express or implied.
+ */
+
+#include <linux/types.h>
+#include <linux/serial_reg.h>
+#include <plat/serial.h>
+
+unsigned int system_rev;
+
+#define UART_OMAP_MDR1		0x08	/* mode definition register */
+#define OMAP_ID_730		0x355F
+#define OMAP_ID_850		0x362C
+#define ID_MASK			0x7fff
+#define check_port(base, shift) ((base[UART_OMAP_MDR1 << shift] & 7) == 0)
+#define omap_get_id() ((*(volatile unsigned int *)(0xfffed404)) >> 12) & ID_MASK
+
+static void putc(int c)
+{
+	volatile u8 * uart = 0;
+	int shift = 2;
+
+#ifdef CONFIG_MACH_OMAP_PALMTE
+	return;
+#endif
+
+#ifdef CONFIG_ARCH_OMAP
+#ifdef	CONFIG_OMAP_LL_DEBUG_UART3
+	uart = (volatile u8 *)(OMAP_UART3_BASE);
+#elif defined(CONFIG_OMAP_LL_DEBUG_UART2)
+	uart = (volatile u8 *)(OMAP_UART2_BASE);
+#elif defined(CONFIG_OMAP_LL_DEBUG_UART1)
+	uart = (volatile u8 *)(OMAP_UART1_BASE);
+#elif defined(CONFIG_OMAP_LL_DEBUG_NONE)
+	return;
+#else
+	return;
+#endif
+
+#ifdef CONFIG_ARCH_OMAP1
+	/* Determine which serial port to use */
+	do {
+		/* MMU is not on, so cpu_is_omapXXXX() won't work here */
+		unsigned int omap_id = omap_get_id();
+
+		if (omap_id == OMAP_ID_730 || omap_id == OMAP_ID_850)
+			shift = 0;
+
+		if (check_port(uart, shift))
+			break;
+		/* Silent boot if no serial ports are enabled. */
+		return;
+	} while (0);
+#endif /* CONFIG_ARCH_OMAP1 */
+#endif
+
+	/*
+	 * Now, xmit each character
+	 */
+	while (!(uart[UART_LSR << shift] & UART_LSR_THRE))
+		barrier();
+	uart[UART_TX << shift] = c;
+}
+
+static inline void flush(void)
+{
+}
+
+/*
+ * nothing to do
+ */
+#define arch_decomp_setup()
+#define arch_decomp_wdog()
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/usb.h
@@ -0,0 +1,162 @@
+// include/asm-arm/mach-omap/usb.h
+
+#ifndef	__ASM_ARCH_OMAP_USB_H
+#define	__ASM_ARCH_OMAP_USB_H
+
+#include <plat/board.h>
+
+#define OMAP3_HS_USB_PORTS	3
+enum ehci_hcd_omap_mode {
+	EHCI_HCD_OMAP_MODE_UNKNOWN,
+	EHCI_HCD_OMAP_MODE_PHY,
+	EHCI_HCD_OMAP_MODE_TLL,
+};
+
+struct ehci_hcd_omap_platform_data {
+	enum ehci_hcd_omap_mode		port_mode[OMAP3_HS_USB_PORTS];
+	unsigned			phy_reset:1;
+
+	/* have to be valid if phy_reset is true and portx is in phy mode */
+	int	reset_gpio_port[OMAP3_HS_USB_PORTS];
+};
+
+/*-------------------------------------------------------------------------*/
+
+#define OMAP1_OTG_BASE			0xfffb0400
+#define OMAP1_UDC_BASE			0xfffb4000
+#define OMAP1_OHCI_BASE			0xfffba000
+
+#define OMAP2_OHCI_BASE			0x4805e000
+#define OMAP2_UDC_BASE			0x4805e200
+#define OMAP2_OTG_BASE			0x4805e300
+
+#ifdef CONFIG_ARCH_OMAP1
+
+#define OTG_BASE			OMAP1_OTG_BASE
+#define UDC_BASE			OMAP1_UDC_BASE
+#define OMAP_OHCI_BASE			OMAP1_OHCI_BASE
+
+#else
+
+#define OTG_BASE			OMAP2_OTG_BASE
+#define UDC_BASE			OMAP2_UDC_BASE
+#define OMAP_OHCI_BASE			OMAP2_OHCI_BASE
+
+extern void usb_musb_init(void);
+
+extern void usb_ehci_init(struct ehci_hcd_omap_platform_data *pdata);
+
+#endif
+
+void omap_usb_init(struct omap_usb_config *pdata);
+
+/*-------------------------------------------------------------------------*/
+
+/*
+ * OTG and transceiver registers, for OMAPs starting with ARM926
+ */
+#define OTG_REV				(OTG_BASE + 0x00)
+#define OTG_SYSCON_1			(OTG_BASE + 0x04)
+#	define	 USB2_TRX_MODE(w)	(((w)>>24)&0x07)
+#	define	 USB1_TRX_MODE(w)	(((w)>>20)&0x07)
+#	define	 USB0_TRX_MODE(w)	(((w)>>16)&0x07)
+#	define	 OTG_IDLE_EN		(1 << 15)
+#	define	 HST_IDLE_EN		(1 << 14)
+#	define	 DEV_IDLE_EN		(1 << 13)
+#	define	 OTG_RESET_DONE		(1 << 2)
+#	define	 OTG_SOFT_RESET		(1 << 1)
+#define OTG_SYSCON_2			(OTG_BASE + 0x08)
+#	define	 OTG_EN			(1 << 31)
+#	define	 USBX_SYNCHRO		(1 << 30)
+#	define	 OTG_MST16		(1 << 29)
+#	define	 SRP_GPDATA		(1 << 28)
+#	define	 SRP_GPDVBUS		(1 << 27)
+#	define	 SRP_GPUVBUS(w)		(((w)>>24)&0x07)
+#	define	 A_WAIT_VRISE(w)	(((w)>>20)&0x07)
+#	define	 B_ASE_BRST(w)		(((w)>>16)&0x07)
+#	define	 SRP_DPW		(1 << 14)
+#	define	 SRP_DATA		(1 << 13)
+#	define	 SRP_VBUS		(1 << 12)
+#	define	 OTG_PADEN		(1 << 10)
+#	define	 HMC_PADEN		(1 << 9)
+#	define	 UHOST_EN		(1 << 8)
+#	define	 HMC_TLLSPEED		(1 << 7)
+#	define	 HMC_TLLATTACH		(1 << 6)
+#	define	 OTG_HMC(w)		(((w)>>0)&0x3f)
+#define OTG_CTRL			(OTG_BASE + 0x0c)
+#	define	 OTG_USB2_EN		(1 << 29)
+#	define	 OTG_USB2_DP		(1 << 28)
+#	define	 OTG_USB2_DM		(1 << 27)
+#	define	 OTG_USB1_EN		(1 << 26)
+#	define	 OTG_USB1_DP		(1 << 25)
+#	define	 OTG_USB1_DM		(1 << 24)
+#	define	 OTG_USB0_EN		(1 << 23)
+#	define	 OTG_USB0_DP		(1 << 22)
+#	define	 OTG_USB0_DM		(1 << 21)
+#	define	 OTG_ASESSVLD		(1 << 20)
+#	define	 OTG_BSESSEND		(1 << 19)
+#	define	 OTG_BSESSVLD		(1 << 18)
+#	define	 OTG_VBUSVLD		(1 << 17)
+#	define	 OTG_ID			(1 << 16)
+#	define	 OTG_DRIVER_SEL		(1 << 15)
+#	define	 OTG_A_SETB_HNPEN	(1 << 12)
+#	define	 OTG_A_BUSREQ		(1 << 11)
+#	define	 OTG_B_HNPEN		(1 << 9)
+#	define	 OTG_B_BUSREQ		(1 << 8)
+#	define	 OTG_BUSDROP		(1 << 7)
+#	define	 OTG_PULLDOWN		(1 << 5)
+#	define	 OTG_PULLUP		(1 << 4)
+#	define	 OTG_DRV_VBUS		(1 << 3)
+#	define	 OTG_PD_VBUS		(1 << 2)
+#	define	 OTG_PU_VBUS		(1 << 1)
+#	define	 OTG_PU_ID		(1 << 0)
+#define OTG_IRQ_EN			(OTG_BASE + 0x10)	/* 16-bit */
+#	define	 DRIVER_SWITCH		(1 << 15)
+#	define	 A_VBUS_ERR		(1 << 13)
+#	define	 A_REQ_TMROUT		(1 << 12)
+#	define	 A_SRP_DETECT		(1 << 11)
+#	define	 B_HNP_FAIL		(1 << 10)
+#	define	 B_SRP_TMROUT		(1 << 9)
+#	define	 B_SRP_DONE		(1 << 8)
+#	define	 B_SRP_STARTED		(1 << 7)
+#	define	 OPRT_CHG		(1 << 0)
+#define OTG_IRQ_SRC			(OTG_BASE + 0x14)	/* 16-bit */
+	// same bits as in IRQ_EN
+#define OTG_OUTCTRL			(OTG_BASE + 0x18)	/* 16-bit */
+#	define	 OTGVPD			(1 << 14)
+#	define	 OTGVPU			(1 << 13)
+#	define	 OTGPUID		(1 << 12)
+#	define	 USB2VDR		(1 << 10)
+#	define	 USB2PDEN		(1 << 9)
+#	define	 USB2PUEN		(1 << 8)
+#	define	 USB1VDR		(1 << 6)
+#	define	 USB1PDEN		(1 << 5)
+#	define	 USB1PUEN		(1 << 4)
+#	define	 USB0VDR		(1 << 2)
+#	define	 USB0PDEN		(1 << 1)
+#	define	 USB0PUEN		(1 << 0)
+#define OTG_TEST			(OTG_BASE + 0x20)	/* 16-bit */
+#define OTG_VENDOR_CODE			(OTG_BASE + 0xfc)	/* 16-bit */
+
+/*-------------------------------------------------------------------------*/
+
+/* OMAP1 */
+#define	USB_TRANSCEIVER_CTRL		(0xfffe1000 + 0x0064)
+#	define	CONF_USB2_UNI_R		(1 << 8)
+#	define	CONF_USB1_UNI_R		(1 << 7)
+#	define	CONF_USB_PORT0_R(x)	(((x)>>4)&0x7)
+#	define	CONF_USB0_ISOLATE_R	(1 << 3)
+#	define	CONF_USB_PWRDN_DM_R	(1 << 2)
+#	define	CONF_USB_PWRDN_DP_R	(1 << 1)
+
+/* OMAP2 */
+#	define	USB_UNIDIR			0x0
+#	define	USB_UNIDIR_TLL			0x1
+#	define	USB_BIDIR			0x2
+#	define	USB_BIDIR_TLL			0x3
+#	define	USBTXWRMODEI(port, x)	((x) << (22 - (port * 2)))
+#	define	USBT2TLL5PI		(1 << 17)
+#	define	USB0PUENACTLOI		(1 << 16)
+#	define	USBSTANDBYCTRL		(1 << 15)
+
+#endif	/* __ASM_ARCH_OMAP_USB_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/vram.h
@@ -0,0 +1,62 @@
+/*
+ * VRAM manager for OMAP
+ *
+ * Copyright (C) 2009 Nokia Corporation
+ * Author: Tomi Valkeinen <tomi.valkeinen@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 59 Temple Place - Suite 330, Boston, MA  02111-1307, USA.
+ */
+
+#ifndef __OMAP_VRAM_H__
+#define __OMAP_VRAM_H__
+
+#include <linux/types.h>
+
+#define OMAP_VRAM_MEMTYPE_SDRAM		0
+#define OMAP_VRAM_MEMTYPE_SRAM		1
+#define OMAP_VRAM_MEMTYPE_MAX		1
+
+extern int omap_vram_add_region(unsigned long paddr, size_t size);
+extern int omap_vram_free(unsigned long paddr, size_t size);
+extern int omap_vram_alloc(int mtype, size_t size, unsigned long *paddr);
+extern int omap_vram_reserve(unsigned long paddr, size_t size);
+extern void omap_vram_get_info(unsigned long *vram, unsigned long *free_vram,
+		unsigned long *largest_free_block);
+
+#ifdef CONFIG_OMAP2_VRAM
+extern void omap_vram_set_sdram_vram(u32 size, u32 start);
+extern void omap_vram_set_sram_vram(u32 size, u32 start);
+
+extern void omap_vram_reserve_sdram(void);
+extern unsigned long omap_vram_reserve_sram(unsigned long sram_pstart,
+					    unsigned long sram_vstart,
+					    unsigned long sram_size,
+					    unsigned long pstart_avail,
+					    unsigned long size_avail);
+#else
+static inline void omap_vram_set_sdram_vram(u32 size, u32 start) { }
+static inline void omap_vram_set_sram_vram(u32 size, u32 start) { }
+
+static inline void omap_vram_reserve_sdram(void) { }
+static inline unsigned long omap_vram_reserve_sram(unsigned long sram_pstart,
+					    unsigned long sram_vstart,
+					    unsigned long sram_size,
+					    unsigned long pstart_avail,
+					    unsigned long size_avail)
+{
+	return 0;
+}
+#endif
+
+#endif
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/mach/vrfb.h
@@ -0,0 +1,50 @@
+/*
+ * VRFB Rotation Engine
+ *
+ * Copyright (C) 2009 Nokia Corporation
+ * Author: Tomi Valkeinen <tomi.valkeinen@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 59 Temple Place - Suite 330, Boston, MA  02111-1307, USA.
+ */
+
+#ifndef __OMAP_VRFB_H__
+#define __OMAP_VRFB_H__
+
+#define OMAP_VRFB_LINE_LEN 2048
+
+struct vrfb {
+	u8 context;
+	void __iomem *vaddr[4];
+	unsigned long paddr[4];
+	u16 xres;
+	u16 yres;
+	u16 xoffset;
+	u16 yoffset;
+	u8 bytespp;
+	bool yuv_mode;
+};
+
+extern int omap_vrfb_request_ctx(struct vrfb *vrfb);
+extern void omap_vrfb_release_ctx(struct vrfb *vrfb);
+extern void omap_vrfb_adjust_size(u16 *width, u16 *height,
+		u8 bytespp);
+extern u32 omap_vrfb_min_phys_size(u16 width, u16 height, u8 bytespp);
+extern u16 omap_vrfb_max_height(u32 phys_size, u16 width, u8 bytespp);
+extern void omap_vrfb_setup(struct vrfb *vrfb, unsigned long paddr,
+		u16 width, u16 height,
+		unsigned bytespp, bool yuv_mode);
+extern int omap_vrfb_map_angle(struct vrfb *vrfb, u16 height, u8 rot);
+extern void omap_vrfb_restore_context(void);
+
+#endif /* __VRFB_H */
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/plat/cbus.h
@@ -0,0 +1,31 @@
+/*
+ * cbus.h - CBUS platform_data definition
+ *
+ * Copyright (C) 2004 - 2009 Nokia Corporation
+ *
+ * Written by Felipe Balbi <felipe.balbi@nokia.com>
+ *
+ * This file is subject to the terms and conditions of the GNU General
+ * Public License. See the file "COPYING" in the main directory of this
+ * archive for more details.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ */
+
+#ifndef __PLAT_CBUS_H
+#define __PLAT_CBUS_H
+
+struct cbus_host_platform_data {
+	int	dat_gpio;
+	int	clk_gpio;
+	int	sel_gpio;
+};
+
+#endif /* __PLAT_CBUS_H */
--- linux-2.6.36-rc4.orig/arch/arm/plat-omap/Kconfig
+++ linux-2.6.36-rc4/arch/arm/plat-omap/Kconfig
@@ -47,6 +47,38 @@ config OMAP_RESET_CLOCKS
 	  probably do not want this option enabled until your
 	  device drivers work properly.
 
+config OMAP_BOOT_TAG
+	bool "OMAP bootloader information passing"
+        depends on ARCH_OMAP
+        default n
+        help
+          Say Y, if you have a bootloader which passes information
+          about your board and its peripheral configuration.
+
+config OMAP_BOOT_REASON
+	bool "Support for boot reason"
+        depends on OMAP_BOOT_TAG
+        default n
+        help
+          Say Y, if you want to have a procfs entry for reading the boot
+          reason in user-space.
+
+config OMAP_COMPONENT_VERSION
+	bool "Support for component version display"
+	depends on OMAP_BOOT_TAG && PROC_FS
+	default n
+	help
+	  Say Y, if you want to have a procfs entry for reading component
+	  versions (supplied by the bootloader) in user-space.
+
+config OMAP_GPIO_SWITCH
+	bool "GPIO switch support"
+	help
+	  Say Y, if you want to have support for reporting of GPIO
+	  switches (e.g. cover switches) via sysfs. Your bootloader has
+	  to provide information about the switches to the kernel via the
+	  ATAG_BOARD mechanism if they're not defined by the board config.
+
 config OMAP_MUX
 	bool "OMAP multiplexing support"
 	depends on ARCH_OMAP
--- linux-2.6.36-rc4.orig/arch/arm/plat-omap/Makefile
+++ linux-2.6.36-rc4/arch/arm/plat-omap/Makefile
@@ -23,6 +23,9 @@ obj-$(CONFIG_OMAP_IOMMU_DEBUG) += iommu-
 
 obj-$(CONFIG_CPU_FREQ) += cpu-omap.o
 obj-$(CONFIG_OMAP_DM_TIMER) += dmtimer.o
+obj-$(CONFIG_OMAP_BOOT_REASON) += bootreason.o
+obj-$(CONFIG_OMAP_COMPONENT_VERSION) += component-version.o
+obj-$(CONFIG_OMAP_GPIO_SWITCH) += gpio-switch.o
 obj-$(CONFIG_OMAP_DEBUG_DEVICES) += debug-devices.o
 obj-$(CONFIG_OMAP_DEBUG_LEDS) += debug-leds.o
 i2c-omap-$(CONFIG_I2C_OMAP) := i2c.o
@@ -31,4 +34,4 @@ obj-y += $(i2c-omap-m) $(i2c-omap-y)
 # OMAP mailbox framework
 obj-$(CONFIG_OMAP_MBOX_FWK) += mailbox.o
 
-obj-$(CONFIG_OMAP_PM_NOOP) += omap-pm-noop.o
\ No newline at end of file
+obj-$(CONFIG_OMAP_PM_NOOP) += omap-pm-noop.o
--- linux-2.6.36-rc4.orig/arch/arm/include/asm/setup.h
+++ linux-2.6.36-rc4/arch/arm/include/asm/setup.h
@@ -136,6 +136,13 @@ struct tag_acorn {
 	__u8 adfsdrives;
 };
 
+/* TI OMAP specific information */
+#define ATAG_BOARD       0x414f4d50
+
+struct tag_omap {
+	u8 data[0];
+};
+
 /* footbridge memory clock, see arch/arm/mach-footbridge/arch.c */
 #define ATAG_MEMCLK	0x41000402
 
@@ -162,6 +169,11 @@ struct tag {
 		struct tag_acorn	acorn;
 
 		/*
+		 * OMAP specific
+                 */
+                struct tag_omap         omap;
+
+		/*
 		 * DC21285 specific
 		 */
 		struct tag_memclk	memclk;
--- /dev/null
+++ linux-2.6.36-rc4/arch/arm/plat-omap/gpio-switch.c
@@ -0,0 +1,554 @@
+/*
+ *  linux/arch/arm/plat-omap/gpio-switch.c
+ *
+ *  Copyright (C) 2004-2006 Nokia Corporation
+ *  Written by Juha Yrjölä <juha.yrjola@nokia.com>
+ *         and Paul Mundt <paul.mundt@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/sched.h>
+#include <linux/init.h>
+#include <linux/list.h>
+#include <linux/irq.h>
+#include <linux/interrupt.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/timer.h>
+#include <linux/err.h>
+#include <linux/slab.h>
+#include <linux/gpio.h>
+#include <plat/hardware.h>
+#include <plat/irqs.h>
+#include <plat/mux.h>
+#include <plat/board.h>
+#include <plat/gpio-switch.h>
+
+struct gpio_switch {
+	char		name[14];
+	u16		gpio;
+	unsigned	flags:4;
+	unsigned	type:4;
+	unsigned	state:1;
+	unsigned	both_edges:1;
+
+	u16		debounce_rising;
+	u16		debounce_falling;
+
+	void (* notify)(void *data, int state);
+	void *notify_data;
+
+	struct work_struct	work;
+	struct timer_list	timer;
+	struct platform_device	pdev;
+
+	struct list_head	node;
+};
+
+static LIST_HEAD(gpio_switches);
+static struct platform_device *gpio_sw_platform_dev;
+static struct platform_driver gpio_sw_driver;
+
+static const struct omap_gpio_switch *board_gpio_sw_table;
+static int board_gpio_sw_count;
+
+static const char *cover_str[2] = { "open", "closed" };
+static const char *connection_str[2] = { "disconnected", "connected" };
+static const char *activity_str[2] = { "inactive", "active" };
+
+/*
+ * GPIO switch state default debounce delay in ms
+ */
+#define OMAP_GPIO_SW_DEFAULT_DEBOUNCE		10
+
+static const char **get_sw_str(struct gpio_switch *sw)
+{
+	switch (sw->type) {
+	case OMAP_GPIO_SWITCH_TYPE_COVER:
+		return cover_str;
+	case OMAP_GPIO_SWITCH_TYPE_CONNECTION:
+		return connection_str;
+	case OMAP_GPIO_SWITCH_TYPE_ACTIVITY:
+		return activity_str;
+	default:
+		BUG();
+		return NULL;
+	}
+}
+
+static const char *get_sw_type(struct gpio_switch *sw)
+{
+	switch (sw->type) {
+	case OMAP_GPIO_SWITCH_TYPE_COVER:
+		return "cover";
+	case OMAP_GPIO_SWITCH_TYPE_CONNECTION:
+		return "connection";
+	case OMAP_GPIO_SWITCH_TYPE_ACTIVITY:
+		return "activity";
+	default:
+		BUG();
+		return NULL;
+	}
+}
+
+static void print_sw_state(struct gpio_switch *sw, int state)
+{
+	const char **str;
+
+	str = get_sw_str(sw);
+	if (str != NULL)
+		printk(KERN_INFO "%s (GPIO %d) is now %s\n", sw->name, sw->gpio, str[state]);
+}
+
+static int gpio_sw_get_state(struct gpio_switch *sw)
+{
+	int state;
+
+	state = gpio_get_value(sw->gpio);
+	if (sw->flags & OMAP_GPIO_SWITCH_FLAG_INVERTED)
+		state = !state;
+
+	return state;
+}
+
+static ssize_t gpio_sw_state_store(struct device *dev,
+				   struct device_attribute *attr,
+				   const char *buf,
+				   size_t count)
+{
+	struct gpio_switch *sw = dev_get_drvdata(dev);
+	const char **str;
+	char state[16];
+	int enable;
+
+	if (!(sw->flags & OMAP_GPIO_SWITCH_FLAG_OUTPUT))
+		return -EPERM;
+
+	if (sscanf(buf, "%15s", state) != 1)
+		return -EINVAL;
+
+	str = get_sw_str(sw);
+	if (strcmp(state, str[0]) == 0)
+		sw->state = enable = 0;
+	else if (strcmp(state, str[1]) == 0)
+		sw->state = enable = 1;
+	else
+		return -EINVAL;
+
+	if (sw->flags & OMAP_GPIO_SWITCH_FLAG_INVERTED)
+		enable = !enable;
+	gpio_set_value(sw->gpio, enable);
+
+	return count;
+}
+
+static ssize_t gpio_sw_state_show(struct device *dev,
+				  struct device_attribute *attr,
+				  char *buf)
+{
+	struct gpio_switch *sw = dev_get_drvdata(dev);
+	const char **str;
+
+	str = get_sw_str(sw);
+	return sprintf(buf, "%s\n", str[sw->state]);
+}
+
+static DEVICE_ATTR(state, S_IRUGO | S_IWUSR, gpio_sw_state_show,
+		   gpio_sw_state_store);
+
+static ssize_t gpio_sw_type_show(struct device *dev,
+				 struct device_attribute *attr,
+				 char *buf)
+{
+	struct gpio_switch *sw = dev_get_drvdata(dev);
+
+	return sprintf(buf, "%s\n", get_sw_type(sw));
+}
+
+static DEVICE_ATTR(type, S_IRUGO, gpio_sw_type_show, NULL);
+
+static ssize_t gpio_sw_direction_show(struct device *dev,
+				      struct device_attribute *attr,
+				      char *buf)
+{
+	struct gpio_switch *sw = dev_get_drvdata(dev);
+	int is_output;
+
+	is_output = sw->flags & OMAP_GPIO_SWITCH_FLAG_OUTPUT;
+	return sprintf(buf, "%s\n", is_output ? "output" : "input");
+}
+
+static DEVICE_ATTR(direction, S_IRUGO, gpio_sw_direction_show, NULL);
+
+
+static irqreturn_t gpio_sw_irq_handler(int irq, void *arg)
+{
+	struct gpio_switch *sw = arg;
+	unsigned long timeout;
+	int state;
+
+	if (!sw->both_edges) {
+		if (gpio_get_value(sw->gpio))
+			set_irq_type(OMAP_GPIO_IRQ(sw->gpio), IRQ_TYPE_EDGE_FALLING);
+		else
+			set_irq_type(OMAP_GPIO_IRQ(sw->gpio), IRQ_TYPE_EDGE_RISING);
+	}
+
+	state = gpio_sw_get_state(sw);
+	if (sw->state == state)
+		return IRQ_HANDLED;
+
+	if (state)
+		timeout = sw->debounce_rising;
+	else
+		timeout = sw->debounce_falling;
+	if (!timeout)
+		schedule_work(&sw->work);
+	else
+		mod_timer(&sw->timer, jiffies + msecs_to_jiffies(timeout));
+
+	return IRQ_HANDLED;
+}
+
+static void gpio_sw_timer(unsigned long arg)
+{
+	struct gpio_switch *sw = (struct gpio_switch *) arg;
+
+	schedule_work(&sw->work);
+}
+
+static void gpio_sw_handler(struct work_struct *work)
+{
+	struct gpio_switch *sw = container_of(work, struct gpio_switch, work);
+	int state;
+
+	state = gpio_sw_get_state(sw);
+	if (sw->state == state)
+		return;
+
+	sw->state = state;
+	if (sw->notify != NULL)
+		sw->notify(sw->notify_data, state);
+	sysfs_notify(&sw->pdev.dev.kobj, NULL, "state");
+	print_sw_state(sw, state);
+}
+
+static int __init can_do_both_edges(struct gpio_switch *sw)
+{
+	if (!cpu_class_is_omap1())
+		return 1;
+	if (OMAP_GPIO_IS_MPUIO(sw->gpio))
+		return 0;
+	else
+		return 1;
+}
+
+static void gpio_sw_release(struct device *dev)
+{
+}
+
+static int __init new_switch(struct gpio_switch *sw)
+{
+	int r, direction, trigger;
+
+	switch (sw->type) {
+	case OMAP_GPIO_SWITCH_TYPE_COVER:
+	case OMAP_GPIO_SWITCH_TYPE_CONNECTION:
+	case OMAP_GPIO_SWITCH_TYPE_ACTIVITY:
+		break;
+	default:
+		printk(KERN_ERR "invalid GPIO switch type: %d\n", sw->type);
+		return -EINVAL;
+	}
+
+	sw->pdev.name	= sw->name;
+	sw->pdev.id	= -1;
+
+	sw->pdev.dev.parent = &gpio_sw_platform_dev->dev;
+	sw->pdev.dev.driver = &gpio_sw_driver.driver;
+	sw->pdev.dev.release = gpio_sw_release;
+
+	r = platform_device_register(&sw->pdev);
+	if (r) {
+		printk(KERN_ERR "gpio-switch: platform device registration "
+		       "failed for %s", sw->name);
+		return r;
+	}
+	dev_set_drvdata(&sw->pdev.dev, sw);
+
+	r = gpio_request(sw->gpio, "gpio-switch");
+	if (r < 0) {
+		platform_device_unregister(&sw->pdev);
+		return r;
+	}
+
+	/* input: 1, output: 0 */
+	direction = !(sw->flags & OMAP_GPIO_SWITCH_FLAG_OUTPUT);
+	if (direction)
+		gpio_direction_input(sw->gpio);
+	else
+		gpio_direction_output(sw->gpio, 0);
+
+	sw->state = gpio_sw_get_state(sw);
+
+	r = 0;
+	r |= device_create_file(&sw->pdev.dev, &dev_attr_state);
+	r |= device_create_file(&sw->pdev.dev, &dev_attr_type);
+	r |= device_create_file(&sw->pdev.dev, &dev_attr_direction);
+	if (r)
+		printk(KERN_ERR "gpio-switch: attribute file creation "
+		       "failed for %s\n", sw->name);
+
+	if (!direction)
+		return 0;
+
+	if (can_do_both_edges(sw)) {
+		trigger = IRQF_TRIGGER_FALLING | IRQF_TRIGGER_RISING;
+		sw->both_edges = 1;
+	} else {
+		if (gpio_get_value(sw->gpio))
+			trigger = IRQF_TRIGGER_FALLING;
+		else
+			trigger = IRQF_TRIGGER_RISING;
+	}
+	r = request_irq(OMAP_GPIO_IRQ(sw->gpio), gpio_sw_irq_handler,
+			IRQF_SHARED | trigger, sw->name, sw);
+	if (r < 0) {
+		printk(KERN_ERR "gpio-switch: request_irq() failed "
+		       "for GPIO %d\n", sw->gpio);
+		platform_device_unregister(&sw->pdev);
+		gpio_free(sw->gpio);
+		return r;
+	}
+
+	INIT_WORK(&sw->work, gpio_sw_handler);
+	init_timer(&sw->timer);
+
+	sw->timer.function = gpio_sw_timer;
+	sw->timer.data = (unsigned long)sw;
+
+	list_add(&sw->node, &gpio_switches);
+
+	return 0;
+}
+
+static int __init add_atag_switches(void)
+{
+	const struct omap_gpio_switch_config *cfg;
+	struct gpio_switch *sw;
+	int i, r;
+
+	for (i = 0; ; i++) {
+		cfg = omap_get_nr_config(OMAP_TAG_GPIO_SWITCH,
+					 struct omap_gpio_switch_config, i);
+		if (cfg == NULL)
+			break;
+		sw = kzalloc(sizeof(*sw), GFP_KERNEL);
+		if (sw == NULL) {
+			printk(KERN_ERR "gpio-switch: kmalloc failed\n");
+			return -ENOMEM;
+		}
+		strncpy(sw->name, cfg->name, sizeof(cfg->name));
+		sw->gpio = cfg->gpio;
+		sw->flags = cfg->flags;
+		sw->type = cfg->type;
+		sw->debounce_rising = OMAP_GPIO_SW_DEFAULT_DEBOUNCE;
+		sw->debounce_falling = OMAP_GPIO_SW_DEFAULT_DEBOUNCE;
+		if ((r = new_switch(sw)) < 0) {
+			kfree(sw);
+			return r;
+		}
+	}
+	return 0;
+}
+
+static struct gpio_switch * __init find_switch(int gpio, const char *name)
+{
+	struct gpio_switch *sw;
+
+	list_for_each_entry(sw, &gpio_switches, node) {
+		if ((gpio < 0 || sw->gpio != gpio) &&
+		    (name == NULL || strcmp(sw->name, name) != 0))
+			continue;
+
+		if (gpio < 0 || name == NULL)
+			goto no_check;
+
+		if (strcmp(sw->name, name) != 0)
+			printk("gpio-switch: name mismatch for %d (%s, %s)\n",
+			       gpio, name, sw->name);
+		else if (sw->gpio != gpio)
+			printk("gpio-switch: GPIO mismatch for %s (%d, %d)\n",
+			       name, gpio, sw->gpio);
+no_check:
+		return sw;
+	}
+	return NULL;
+}
+
+static int __init add_board_switches(void)
+{
+	int i;
+
+	for (i = 0; i < board_gpio_sw_count; i++) {
+		const struct omap_gpio_switch *cfg;
+		struct gpio_switch *sw;
+		int r;
+
+		cfg = board_gpio_sw_table + i;
+		if (strlen(cfg->name) > sizeof(sw->name) - 1)
+			return -EINVAL;
+		/* Check whether we only update an existing switch
+		 * or add a new switch. */
+		sw = find_switch(cfg->gpio, cfg->name);
+		if (sw != NULL) {
+			sw->debounce_rising = cfg->debounce_rising;
+			sw->debounce_falling = cfg->debounce_falling;
+			sw->notify = cfg->notify;
+			sw->notify_data = cfg->notify_data;
+			continue;
+		} else {
+			if (cfg->gpio < 0 || cfg->name == NULL) {
+				printk("gpio-switch: required switch not "
+				       "found (%d, %s)\n", cfg->gpio,
+				       cfg->name);
+				continue;
+			}
+		}
+		sw = kzalloc(sizeof(*sw), GFP_KERNEL);
+		if (sw == NULL) {
+			printk(KERN_ERR "gpio-switch: kmalloc failed\n");
+			return -ENOMEM;
+		}
+		strlcpy(sw->name, cfg->name, sizeof(sw->name));
+		sw->gpio = cfg->gpio;
+		sw->flags = cfg->flags;
+		sw->type = cfg->type;
+		sw->debounce_rising = cfg->debounce_rising;
+		sw->debounce_falling = cfg->debounce_falling;
+		sw->notify = cfg->notify;
+		sw->notify_data = cfg->notify_data;
+		if ((r = new_switch(sw)) < 0) {
+			kfree(sw);
+			return r;
+		}
+	}
+	return 0;
+}
+
+static void gpio_sw_cleanup(void)
+{
+	struct gpio_switch *sw = NULL, *old = NULL;
+
+	list_for_each_entry(sw, &gpio_switches, node) {
+		if (old != NULL)
+			kfree(old);
+		flush_scheduled_work();
+		del_timer_sync(&sw->timer);
+
+		free_irq(OMAP_GPIO_IRQ(sw->gpio), sw);
+
+		device_remove_file(&sw->pdev.dev, &dev_attr_state);
+		device_remove_file(&sw->pdev.dev, &dev_attr_type);
+		device_remove_file(&sw->pdev.dev, &dev_attr_direction);
+
+		platform_device_unregister(&sw->pdev);
+		gpio_free(sw->gpio);
+		old = sw;
+	}
+	kfree(old);
+}
+
+static void __init report_initial_state(void)
+{
+	struct gpio_switch *sw;
+
+	list_for_each_entry(sw, &gpio_switches, node) {
+		int state;
+
+		state = gpio_get_value(sw->gpio);
+		if (sw->flags & OMAP_GPIO_SWITCH_FLAG_INVERTED)
+			state = !state;
+		if (sw->notify != NULL)
+			sw->notify(sw->notify_data, state);
+		print_sw_state(sw, state);
+	}
+}
+
+static int gpio_sw_remove(struct platform_device *dev)
+{
+	return 0;
+}
+
+static struct platform_driver gpio_sw_driver = {
+	.remove		= gpio_sw_remove,
+	.driver		= {
+		.name	= "gpio-switch",
+	},
+};
+
+void __init omap_register_gpio_switches(const struct omap_gpio_switch *tbl,
+					int count)
+{
+	BUG_ON(board_gpio_sw_table != NULL);
+
+	board_gpio_sw_table = tbl;
+	board_gpio_sw_count = count;
+}
+
+static int __init gpio_sw_init(void)
+{
+	int r;
+
+	printk(KERN_INFO "OMAP GPIO switch handler initializing\n");
+
+	r = platform_driver_register(&gpio_sw_driver);
+	if (r)
+		return r;
+
+	gpio_sw_platform_dev = platform_device_register_simple("gpio-switch",
+							       -1, NULL, 0);
+	if (IS_ERR(gpio_sw_platform_dev)) {
+		r = PTR_ERR(gpio_sw_platform_dev);
+		goto err1;
+	}
+
+	r = add_atag_switches();
+	if (r < 0)
+		goto err2;
+
+	r = add_board_switches();
+	if (r < 0)
+		goto err2;
+
+	report_initial_state();
+
+	return 0;
+err2:
+	gpio_sw_cleanup();
+	platform_device_unregister(gpio_sw_platform_dev);
+err1:
+	platform_driver_unregister(&gpio_sw_driver);
+	return r;
+}
+
+static void __exit gpio_sw_exit(void)
+{
+	gpio_sw_cleanup();
+	platform_device_unregister(gpio_sw_platform_dev);
+	platform_driver_unregister(&gpio_sw_driver);
+}
+
+#ifndef MODULE
+late_initcall(gpio_sw_init);
+#else
+module_init(gpio_sw_init);
+#endif
+module_exit(gpio_sw_exit);
+
+MODULE_AUTHOR("Juha Yrjölä <juha.yrjola@nokia.com>, Paul Mundt <paul.mundt@nokia.com");
+MODULE_DESCRIPTION("GPIO switch driver");
+MODULE_LICENSE("GPL");
--- linux-2.6.36-rc4.orig/arch/arm/plat-omap/include/plat/board.h
+++ linux-2.6.36-rc4/arch/arm/plat-omap/include/plat/board.h
@@ -151,6 +151,14 @@ struct omap_board_config_kernel {
 	const void *data;
 };
 
+struct omap_gpio_switch_config {
+	char name[12];
+	u16 gpio;
+	int flags:4;
+	int type:4;
+	int key_code:24; /* Linux key code */
+};
+
 extern const void *__omap_get_config(u16 tag, size_t len, int nr);
 
 #define omap_get_config(tag, type) \
