--- a/arch/arm/mach-gemini/board-wbd111.c
+++ b/arch/arm/mach-gemini/board-wbd111.c
@@ -16,6 +16,8 @@
 #include <linux/skbuff.h>
 #include <linux/gpio_keys.h>
 #include <linux/mdio-gpio.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
 #include <asm/mach-types.h>
 #include <asm/mach/arch.h>
 #include <asm/mach/time.h>
@@ -102,12 +104,51 @@ static struct sys_timer wbd111_timer = {
 	.init	= gemini_timer_init,
 };
 
+#ifdef CONFIG_MTD_PARTITIONS
+static struct mtd_partition wbd111_partitions[] = {
+	{
+		.name		= "RedBoot",
+		.offset		= 0,
+		.size		= 0x020000,
+		.mask_flags	= MTD_WRITEABLE,
+	} , {
+		.name		= "kernel",
+		.offset		= 0x020000,
+		.size		= 0x100000,
+	} , {
+		.name		= "rootfs",
+		.offset		= 0x120000,
+		.size		= 0x6a0000,
+	} , {
+		.name		= "VCTL",
+		.offset		= 0x7c0000,
+		.size		= 0x010000,
+		.mask_flags	= MTD_WRITEABLE,
+	} , {
+		.name		= "cfg",
+		.offset		= 0x7d0000,
+		.size		= 0x010000,
+		.mask_flags	= MTD_WRITEABLE,
+	} , {
+		.name		= "FIS",
+		.offset		= 0x7e0000,
+		.size		= 0x010000,
+		.mask_flags	= MTD_WRITEABLE,
+	}
+};
+#define wbd111_num_partitions	ARRAY_SIZE(wbd111_partitions)
+#else
+#define wbd111_partitions	NULL
+#define wbd111_num_partitions	0
+#endif /* CONFIG_MTD_PARTITIONS */
+
 static void __init wbd111_init(void)
 {
 	gemini_gpio_init();
 	platform_register_uart();
 	platform_register_watchdog();
-	platform_register_pflash(SZ_8M, NULL, 0);
+	platform_register_pflash(SZ_8M, wbd111_partitions,
+				 wbd111_num_partitions);
 	platform_device_register(&wbd111_leds_device);
 	platform_device_register(&wbd111_keys_device);
 	platform_device_register(&wbd111_phy_device);
