--- a/drivers/ssb/main.c
+++ b/drivers/ssb/main.c
@@ -3,7 +3,7 @@
  * Subsystem core
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -12,6 +12,7 @@
 
 #include <linux/delay.h>
 #include <linux/io.h>
+#include <linux/module.h>
 #include <linux/ssb/ssb.h>
 #include <linux/ssb/ssb_regs.h>
 #include <linux/ssb/ssb_driver_gige.h>
@@ -139,19 +140,6 @@ static void ssb_device_put(struct ssb_de
 		put_device(dev->dev);
 }
 
-static inline struct ssb_driver *ssb_driver_get(struct ssb_driver *drv)
-{
-	if (drv)
-		get_driver(&drv->drv);
-	return drv;
-}
-
-static inline void ssb_driver_put(struct ssb_driver *drv)
-{
-	if (drv)
-		put_driver(&drv->drv);
-}
-
 static int ssb_device_resume(struct device *dev)
 {
 	struct ssb_device *ssb_dev = dev_to_ssb_dev(dev);
@@ -249,11 +237,9 @@ int ssb_devices_freeze(struct ssb_bus *b
 			ssb_device_put(sdev);
 			continue;
 		}
-		sdrv = ssb_driver_get(drv_to_ssb_drv(sdev->dev->driver));
-		if (!sdrv || SSB_WARN_ON(!sdrv->remove)) {
-			ssb_device_put(sdev);
+		sdrv = drv_to_ssb_drv(sdev->dev->driver);
+		if (SSB_WARN_ON(!sdrv->remove))
 			continue;
-		}
 		sdrv->remove(sdev);
 		ctx->device_frozen[i] = 1;
 	}
@@ -292,7 +278,6 @@ int ssb_devices_thaw(struct ssb_freeze_c
 				   dev_name(sdev->dev));
 			result = err;
 		}
-		ssb_driver_put(sdrv);
 		ssb_device_put(sdev);
 	}
 
@@ -557,7 +542,7 @@ error:
 }
 
 /* Needs ssb_buses_lock() */
-static int ssb_attach_queued_buses(void)
+static int __devinit ssb_attach_queued_buses(void)
 {
 	struct ssb_bus *bus, *n;
 	int err = 0;
@@ -768,9 +753,9 @@ out:
 	return err;
 }
 
-static int ssb_bus_register(struct ssb_bus *bus,
-			    ssb_invariants_func_t get_invariants,
-			    unsigned long baseaddr)
+static int __devinit ssb_bus_register(struct ssb_bus *bus,
+				      ssb_invariants_func_t get_invariants,
+				      unsigned long baseaddr)
 {
 	int err;
 
@@ -851,8 +836,8 @@ err_disable_xtal:
 }
 
 #ifdef CONFIG_SSB_PCIHOST
-int ssb_bus_pcibus_register(struct ssb_bus *bus,
-			    struct pci_dev *host_pci)
+int __devinit ssb_bus_pcibus_register(struct ssb_bus *bus,
+				      struct pci_dev *host_pci)
 {
 	int err;
 
@@ -875,9 +860,9 @@ EXPORT_SYMBOL(ssb_bus_pcibus_register);
 #endif /* CONFIG_SSB_PCIHOST */
 
 #ifdef CONFIG_SSB_PCMCIAHOST
-int ssb_bus_pcmciabus_register(struct ssb_bus *bus,
-			       struct pcmcia_device *pcmcia_dev,
-			       unsigned long baseaddr)
+int __devinit ssb_bus_pcmciabus_register(struct ssb_bus *bus,
+					 struct pcmcia_device *pcmcia_dev,
+					 unsigned long baseaddr)
 {
 	int err;
 
@@ -897,8 +882,9 @@ EXPORT_SYMBOL(ssb_bus_pcmciabus_register
 #endif /* CONFIG_SSB_PCMCIAHOST */
 
 #ifdef CONFIG_SSB_SDIOHOST
-int ssb_bus_sdiobus_register(struct ssb_bus *bus, struct sdio_func *func,
-			     unsigned int quirks)
+int __devinit ssb_bus_sdiobus_register(struct ssb_bus *bus,
+				       struct sdio_func *func,
+				       unsigned int quirks)
 {
 	int err;
 
@@ -918,9 +904,9 @@ int ssb_bus_sdiobus_register(struct ssb_
 EXPORT_SYMBOL(ssb_bus_sdiobus_register);
 #endif /* CONFIG_SSB_PCMCIAHOST */
 
-int ssb_bus_ssbbus_register(struct ssb_bus *bus,
-			    unsigned long baseaddr,
-			    ssb_invariants_func_t get_invariants)
+int __devinit ssb_bus_ssbbus_register(struct ssb_bus *bus,
+				      unsigned long baseaddr,
+				      ssb_invariants_func_t get_invariants)
 {
 	int err;
 
@@ -1001,8 +987,8 @@ u32 ssb_calc_clock_rate(u32 plltype, u32
 	switch (plltype) {
 	case SSB_PLLTYPE_6: /* 100/200 or 120/240 only */
 		if (m & SSB_CHIPCO_CLK_T6_MMASK)
-			return SSB_CHIPCO_CLK_T6_M0;
-		return SSB_CHIPCO_CLK_T6_M1;
+			return SSB_CHIPCO_CLK_T6_M1;
+		return SSB_CHIPCO_CLK_T6_M0;
 	case SSB_PLLTYPE_1: /* 48Mhz base, 3 dividers */
 	case SSB_PLLTYPE_3: /* 25Mhz, 2 dividers */
 	case SSB_PLLTYPE_4: /* 48Mhz, 4 dividers */
@@ -1092,6 +1078,9 @@ u32 ssb_clockspeed(struct ssb_bus *bus)
 	u32 plltype;
 	u32 clkctl_n, clkctl_m;
 
+	if (bus->chipco.capabilities & SSB_CHIPCO_CAP_PMU)
+		return ssb_pmu_get_controlclock(&bus->chipco);
+
 	if (ssb_extif_available(&bus->extif))
 		ssb_extif_get_clockcontrol(&bus->extif, &plltype,
 					   &clkctl_n, &clkctl_m);
@@ -1117,23 +1106,22 @@ static u32 ssb_tmslow_reject_bitmask(str
 {
 	u32 rev = ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_SSBREV;
 
-	/* The REJECT bit changed position in TMSLOW between
-	 * Backplane revisions. */
+	/* The REJECT bit seems to be different for Backplane rev 2.3 */
 	switch (rev) {
 	case SSB_IDLOW_SSBREV_22:
-		return SSB_TMSLOW_REJECT_22;
+	case SSB_IDLOW_SSBREV_24:
+	case SSB_IDLOW_SSBREV_26:
+		return SSB_TMSLOW_REJECT;
 	case SSB_IDLOW_SSBREV_23:
 		return SSB_TMSLOW_REJECT_23;
-	case SSB_IDLOW_SSBREV_24:     /* TODO - find the proper REJECT bits */
-	case SSB_IDLOW_SSBREV_25:     /* same here */
-	case SSB_IDLOW_SSBREV_26:     /* same here */
+	case SSB_IDLOW_SSBREV_25:     /* TODO - find the proper REJECT bit */
 	case SSB_IDLOW_SSBREV_27:     /* same here */
-		return SSB_TMSLOW_REJECT_23;	/* this is a guess */
+		return SSB_TMSLOW_REJECT;	/* this is a guess */
 	default:
 		printk(KERN_INFO "ssb: Backplane Revision 0x%.8X\n", rev);
 		WARN_ON(1);
 	}
-	return (SSB_TMSLOW_REJECT_22 | SSB_TMSLOW_REJECT_23);
+	return (SSB_TMSLOW_REJECT | SSB_TMSLOW_REJECT_23);
 }
 
 int ssb_device_is_enabled(struct ssb_device *dev)
@@ -1192,10 +1180,10 @@ void ssb_device_enable(struct ssb_device
 }
 EXPORT_SYMBOL(ssb_device_enable);
 
-/* Wait for a bit in a register to get set or unset.
+/* Wait for bitmask in a register to get set or cleared.
  * timeout is in units of ten-microseconds */
-static int ssb_wait_bit(struct ssb_device *dev, u16 reg, u32 bitmask,
-			int timeout, int set)
+static int ssb_wait_bits(struct ssb_device *dev, u16 reg, u32 bitmask,
+			 int timeout, int set)
 {
 	int i;
 	u32 val;
@@ -1203,7 +1191,7 @@ static int ssb_wait_bit(struct ssb_devic
 	for (i = 0; i < timeout; i++) {
 		val = ssb_read32(dev, reg);
 		if (set) {
-			if (val & bitmask)
+			if ((val & bitmask) == bitmask)
 				return 0;
 		} else {
 			if (!(val & bitmask))
@@ -1220,20 +1208,38 @@ static int ssb_wait_bit(struct ssb_devic
 
 void ssb_device_disable(struct ssb_device *dev, u32 core_specific_flags)
 {
-	u32 reject;
+	u32 reject, val;
 
 	if (ssb_read32(dev, SSB_TMSLOW) & SSB_TMSLOW_RESET)
 		return;
 
 	reject = ssb_tmslow_reject_bitmask(dev);
-	ssb_write32(dev, SSB_TMSLOW, reject | SSB_TMSLOW_CLOCK);
-	ssb_wait_bit(dev, SSB_TMSLOW, reject, 1000, 1);
-	ssb_wait_bit(dev, SSB_TMSHIGH, SSB_TMSHIGH_BUSY, 1000, 0);
-	ssb_write32(dev, SSB_TMSLOW,
-		    SSB_TMSLOW_FGC | SSB_TMSLOW_CLOCK |
-		    reject | SSB_TMSLOW_RESET |
-		    core_specific_flags);
-	ssb_flush_tmslow(dev);
+
+	if (ssb_read32(dev, SSB_TMSLOW) & SSB_TMSLOW_CLOCK) {
+		ssb_write32(dev, SSB_TMSLOW, reject | SSB_TMSLOW_CLOCK);
+		ssb_wait_bits(dev, SSB_TMSLOW, reject, 1000, 1);
+		ssb_wait_bits(dev, SSB_TMSHIGH, SSB_TMSHIGH_BUSY, 1000, 0);
+
+		if (ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_INITIATOR) {
+			val = ssb_read32(dev, SSB_IMSTATE);
+			val |= SSB_IMSTATE_REJECT;
+			ssb_write32(dev, SSB_IMSTATE, val);
+			ssb_wait_bits(dev, SSB_IMSTATE, SSB_IMSTATE_BUSY, 1000,
+				      0);
+		}
+
+		ssb_write32(dev, SSB_TMSLOW,
+			SSB_TMSLOW_FGC | SSB_TMSLOW_CLOCK |
+			reject | SSB_TMSLOW_RESET |
+			core_specific_flags);
+		ssb_flush_tmslow(dev);
+
+		if (ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_INITIATOR) {
+			val = ssb_read32(dev, SSB_IMSTATE);
+			val &= ~SSB_IMSTATE_REJECT;
+			ssb_write32(dev, SSB_IMSTATE, val);
+		}
+	}
 
 	ssb_write32(dev, SSB_TMSLOW,
 		    reject | SSB_TMSLOW_RESET |
@@ -1242,13 +1248,34 @@ void ssb_device_disable(struct ssb_devic
 }
 EXPORT_SYMBOL(ssb_device_disable);
 
+/* Some chipsets need routing known for PCIe and 64-bit DMA */
+static bool ssb_dma_translation_special_bit(struct ssb_device *dev)
+{
+	u16 chip_id = dev->bus->chip_id;
+
+	if (dev->id.coreid == SSB_DEV_80211) {
+		return (chip_id == 0x4322 || chip_id == 43221 ||
+			chip_id == 43231 || chip_id == 43222);
+	}
+
+	return 0;
+}
+
 u32 ssb_dma_translation(struct ssb_device *dev)
 {
 	switch (dev->bus->bustype) {
 	case SSB_BUSTYPE_SSB:
 		return 0;
 	case SSB_BUSTYPE_PCI:
-		return SSB_PCI_DMA;
+		if (pci_is_pcie(dev->bus->host_pci) &&
+		    ssb_read32(dev, SSB_TMSHIGH) & SSB_TMSHIGH_DMA64) {
+			return SSB_PCIE_DMA_H32;
+		} else {
+			if (ssb_dma_translation_special_bit(dev))
+				return SSB_PCIE_DMA_H32;
+			else
+				return SSB_PCI_DMA;
+		}
 	default:
 		__ssb_dma_not_implemented(dev);
 	}
@@ -1291,20 +1318,20 @@ EXPORT_SYMBOL(ssb_bus_may_powerdown);
 
 int ssb_bus_powerup(struct ssb_bus *bus, bool dynamic_pctl)
 {
-	struct ssb_chipcommon *cc;
 	int err;
 	enum ssb_clkmode mode;
 
 	err = ssb_pci_xtal(bus, SSB_GPIO_XTAL | SSB_GPIO_PLL, 1);
 	if (err)
 		goto error;
-	cc = &bus->chipco;
-	mode = dynamic_pctl ? SSB_CLKMODE_DYNAMIC : SSB_CLKMODE_FAST;
-	ssb_chipco_set_clockmode(cc, mode);
 
 #ifdef CONFIG_SSB_DEBUG
 	bus->powered_up = 1;
 #endif
+
+	mode = dynamic_pctl ? SSB_CLKMODE_DYNAMIC : SSB_CLKMODE_FAST;
+	ssb_chipco_set_clockmode(&bus->chipco, mode);
+
 	return 0;
 error:
 	ssb_printk(KERN_ERR PFX "Bus powerup failed\n");
@@ -1312,6 +1339,37 @@ error:
 }
 EXPORT_SYMBOL(ssb_bus_powerup);
 
+static void ssb_broadcast_value(struct ssb_device *dev,
+				u32 address, u32 data)
+{
+#ifdef CONFIG_SSB_DRIVER_PCICORE
+	/* This is used for both, PCI and ChipCommon core, so be careful. */
+	BUILD_BUG_ON(SSB_PCICORE_BCAST_ADDR != SSB_CHIPCO_BCAST_ADDR);
+	BUILD_BUG_ON(SSB_PCICORE_BCAST_DATA != SSB_CHIPCO_BCAST_DATA);
+#endif
+
+	ssb_write32(dev, SSB_CHIPCO_BCAST_ADDR, address);
+	ssb_read32(dev, SSB_CHIPCO_BCAST_ADDR); /* flush */
+	ssb_write32(dev, SSB_CHIPCO_BCAST_DATA, data);
+	ssb_read32(dev, SSB_CHIPCO_BCAST_DATA); /* flush */
+}
+
+void ssb_commit_settings(struct ssb_bus *bus)
+{
+	struct ssb_device *dev;
+
+#ifdef CONFIG_SSB_DRIVER_PCICORE
+	dev = bus->chipco.dev ? bus->chipco.dev : bus->pcicore.dev;
+#else
+	dev = bus->chipco.dev;
+#endif
+	if (WARN_ON(!dev))
+		return;
+	/* This forces an update of the cached registers. */
+	ssb_broadcast_value(dev, 0xFD8, 0);
+}
+EXPORT_SYMBOL(ssb_commit_settings);
+
 u32 ssb_admatch_base(u32 adm)
 {
 	u32 base = 0;
--- a/drivers/ssb/pci.c
+++ b/drivers/ssb/pci.c
@@ -1,7 +1,7 @@
 /*
  * Sonics Silicon Backplane PCI-Hostbus related functions.
  *
- * Copyright (C) 2005-2006 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2006 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -331,7 +331,6 @@ static void sprom_extract_r123(struct ss
 {
 	int i;
 	u16 v;
-	s8 gain;
 	u16 loc[3];
 
 	if (out->revision == 3)			/* rev 3 moved MAC */
@@ -390,20 +389,12 @@ static void sprom_extract_r123(struct ss
 		SPEX(boardflags_hi, SSB_SPROM2_BFLHI, 0xFFFF, 0);
 
 	/* Extract the antenna gain values. */
-	gain = r123_extract_antgain(out->revision, in,
-				    SSB_SPROM1_AGAIN_BG,
-				    SSB_SPROM1_AGAIN_BG_SHIFT);
-	out->antenna_gain.ghz24.a0 = gain;
-	out->antenna_gain.ghz24.a1 = gain;
-	out->antenna_gain.ghz24.a2 = gain;
-	out->antenna_gain.ghz24.a3 = gain;
-	gain = r123_extract_antgain(out->revision, in,
-				    SSB_SPROM1_AGAIN_A,
-				    SSB_SPROM1_AGAIN_A_SHIFT);
-	out->antenna_gain.ghz5.a0 = gain;
-	out->antenna_gain.ghz5.a1 = gain;
-	out->antenna_gain.ghz5.a2 = gain;
-	out->antenna_gain.ghz5.a3 = gain;
+	out->antenna_gain.a0 = r123_extract_antgain(out->revision, in,
+						    SSB_SPROM1_AGAIN_BG,
+						    SSB_SPROM1_AGAIN_BG_SHIFT);
+	out->antenna_gain.a1 = r123_extract_antgain(out->revision, in,
+						    SSB_SPROM1_AGAIN_A,
+						    SSB_SPROM1_AGAIN_A_SHIFT);
 }
 
 /* Revs 4 5 and 8 have partially shared layout */
@@ -468,10 +459,14 @@ static void sprom_extract_r45(struct ssb
 		SPEX(country_code, SSB_SPROM4_CCODE, 0xFFFF, 0);
 		SPEX(boardflags_lo, SSB_SPROM4_BFLLO, 0xFFFF, 0);
 		SPEX(boardflags_hi, SSB_SPROM4_BFLHI, 0xFFFF, 0);
+		SPEX(boardflags2_lo, SSB_SPROM4_BFL2LO, 0xFFFF, 0);
+		SPEX(boardflags2_hi, SSB_SPROM4_BFL2HI, 0xFFFF, 0);
 	} else {
 		SPEX(country_code, SSB_SPROM5_CCODE, 0xFFFF, 0);
 		SPEX(boardflags_lo, SSB_SPROM5_BFLLO, 0xFFFF, 0);
 		SPEX(boardflags_hi, SSB_SPROM5_BFLHI, 0xFFFF, 0);
+		SPEX(boardflags2_lo, SSB_SPROM5_BFL2LO, 0xFFFF, 0);
+		SPEX(boardflags2_hi, SSB_SPROM5_BFL2HI, 0xFFFF, 0);
 	}
 	SPEX(ant_available_a, SSB_SPROM4_ANTAVAIL, SSB_SPROM4_ANTAVAIL_A,
 	     SSB_SPROM4_ANTAVAIL_A_SHIFT);
@@ -500,16 +495,14 @@ static void sprom_extract_r45(struct ssb
 	}
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.ghz24.a0, SSB_SPROM4_AGAIN01,
+	SPEX(antenna_gain.a0, SSB_SPROM4_AGAIN01,
 	     SSB_SPROM4_AGAIN0, SSB_SPROM4_AGAIN0_SHIFT);
-	SPEX(antenna_gain.ghz24.a1, SSB_SPROM4_AGAIN01,
+	SPEX(antenna_gain.a1, SSB_SPROM4_AGAIN01,
 	     SSB_SPROM4_AGAIN1, SSB_SPROM4_AGAIN1_SHIFT);
-	SPEX(antenna_gain.ghz24.a2, SSB_SPROM4_AGAIN23,
+	SPEX(antenna_gain.a2, SSB_SPROM4_AGAIN23,
 	     SSB_SPROM4_AGAIN2, SSB_SPROM4_AGAIN2_SHIFT);
-	SPEX(antenna_gain.ghz24.a3, SSB_SPROM4_AGAIN23,
+	SPEX(antenna_gain.a3, SSB_SPROM4_AGAIN23,
 	     SSB_SPROM4_AGAIN3, SSB_SPROM4_AGAIN3_SHIFT);
-	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
-	       sizeof(out->antenna_gain.ghz5));
 
 	sprom_extract_r458(out, in);
 
@@ -519,7 +512,13 @@ static void sprom_extract_r45(struct ssb
 static void sprom_extract_r8(struct ssb_sprom *out, const u16 *in)
 {
 	int i;
-	u16 v;
+	u16 v, o;
+	u16 pwr_info_offset[] = {
+		SSB_SROM8_PWR_INFO_CORE0, SSB_SROM8_PWR_INFO_CORE1,
+		SSB_SROM8_PWR_INFO_CORE2, SSB_SROM8_PWR_INFO_CORE3
+	};
+	BUILD_BUG_ON(ARRAY_SIZE(pwr_info_offset) !=
+			ARRAY_SIZE(out->core_pwr_info));
 
 	/* extract the MAC address */
 	for (i = 0; i < 3; i++) {
@@ -592,16 +591,69 @@ static void sprom_extract_r8(struct ssb_
 	SPEX32(ofdm5ghpo, SSB_SPROM8_OFDM5GHPO, 0xFFFFFFFF, 0);
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.ghz24.a0, SSB_SPROM8_AGAIN01,
+	SPEX(antenna_gain.a0, SSB_SPROM8_AGAIN01,
 	     SSB_SPROM8_AGAIN0, SSB_SPROM8_AGAIN0_SHIFT);
-	SPEX(antenna_gain.ghz24.a1, SSB_SPROM8_AGAIN01,
+	SPEX(antenna_gain.a1, SSB_SPROM8_AGAIN01,
 	     SSB_SPROM8_AGAIN1, SSB_SPROM8_AGAIN1_SHIFT);
-	SPEX(antenna_gain.ghz24.a2, SSB_SPROM8_AGAIN23,
+	SPEX(antenna_gain.a2, SSB_SPROM8_AGAIN23,
 	     SSB_SPROM8_AGAIN2, SSB_SPROM8_AGAIN2_SHIFT);
-	SPEX(antenna_gain.ghz24.a3, SSB_SPROM8_AGAIN23,
+	SPEX(antenna_gain.a3, SSB_SPROM8_AGAIN23,
 	     SSB_SPROM8_AGAIN3, SSB_SPROM8_AGAIN3_SHIFT);
-	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
-	       sizeof(out->antenna_gain.ghz5));
+
+	/* Extract cores power info info */
+	for (i = 0; i < ARRAY_SIZE(pwr_info_offset); i++) {
+		o = pwr_info_offset[i];
+		SPEX(core_pwr_info[i].itssi_2g, o + SSB_SROM8_2G_MAXP_ITSSI,
+			SSB_SPROM8_2G_ITSSI, SSB_SPROM8_2G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_2g, o + SSB_SROM8_2G_MAXP_ITSSI,
+			SSB_SPROM8_2G_MAXP, 0);
+
+		SPEX(core_pwr_info[i].pa_2g[0], o + SSB_SROM8_2G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[1], o + SSB_SROM8_2G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[2], o + SSB_SROM8_2G_PA_2, ~0, 0);
+
+		SPEX(core_pwr_info[i].itssi_5g, o + SSB_SROM8_5G_MAXP_ITSSI,
+			SSB_SPROM8_5G_ITSSI, SSB_SPROM8_5G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_5g, o + SSB_SROM8_5G_MAXP_ITSSI,
+			SSB_SPROM8_5G_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gh, o + SSB_SPROM8_5GHL_MAXP,
+			SSB_SPROM8_5GH_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gl, o + SSB_SPROM8_5GHL_MAXP,
+			SSB_SPROM8_5GL_MAXP, SSB_SPROM8_5GL_MAXP_SHIFT);
+
+		SPEX(core_pwr_info[i].pa_5gl[0], o + SSB_SROM8_5GL_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[1], o + SSB_SROM8_5GL_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[2], o + SSB_SROM8_5GL_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[0], o + SSB_SROM8_5G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[1], o + SSB_SROM8_5G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[2], o + SSB_SROM8_5G_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[0], o + SSB_SROM8_5GH_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[1], o + SSB_SROM8_5GH_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[2], o + SSB_SROM8_5GH_PA_2, ~0, 0);
+	}
+
+	/* Extract FEM info */
+	SPEX(fem.ghz2.tssipos, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_TSSIPOS, SSB_SROM8_FEM_TSSIPOS_SHIFT);
+	SPEX(fem.ghz2.extpa_gain, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_EXTPA_GAIN, SSB_SROM8_FEM_EXTPA_GAIN_SHIFT);
+	SPEX(fem.ghz2.pdet_range, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_PDET_RANGE, SSB_SROM8_FEM_PDET_RANGE_SHIFT);
+	SPEX(fem.ghz2.tr_iso, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_TR_ISO, SSB_SROM8_FEM_TR_ISO_SHIFT);
+	SPEX(fem.ghz2.antswlut, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_ANTSWLUT, SSB_SROM8_FEM_ANTSWLUT_SHIFT);
+
+	SPEX(fem.ghz5.tssipos, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_TSSIPOS, SSB_SROM8_FEM_TSSIPOS_SHIFT);
+	SPEX(fem.ghz5.extpa_gain, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_EXTPA_GAIN, SSB_SROM8_FEM_EXTPA_GAIN_SHIFT);
+	SPEX(fem.ghz5.pdet_range, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_PDET_RANGE, SSB_SROM8_FEM_PDET_RANGE_SHIFT);
+	SPEX(fem.ghz5.tr_iso, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_TR_ISO, SSB_SROM8_FEM_TR_ISO_SHIFT);
+	SPEX(fem.ghz5.antswlut, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_ANTSWLUT, SSB_SROM8_FEM_ANTSWLUT_SHIFT);
 
 	sprom_extract_r458(out, in);
 
@@ -641,7 +693,7 @@ static int sprom_extract(struct ssb_bus
 		break;
 	default:
 		ssb_printk(KERN_WARNING PFX "Unsupported SPROM"
-			   "  revision %d detected. Will extract"
+			   " revision %d detected. Will extract"
 			   " v1\n", out->revision);
 		out->revision = 1;
 		sprom_extract_r123(out, in);
@@ -658,7 +710,6 @@ static int sprom_extract(struct ssb_bus
 static int ssb_pci_sprom_get(struct ssb_bus *bus,
 			     struct ssb_sprom *sprom)
 {
-	const struct ssb_sprom *fallback;
 	int err;
 	u16 *buf;
 
@@ -666,7 +717,7 @@ static int ssb_pci_sprom_get(struct ssb_
 		ssb_printk(KERN_ERR PFX "No SPROM available!\n");
 		return -ENODEV;
 	}
-	if (bus->chipco.dev) {	/* can be unavailible! */
+	if (bus->chipco.dev) {	/* can be unavailable! */
 		/*
 		 * get SPROM offset: SSB_SPROM_BASE1 except for
 		 * chipcommon rev >= 31 or chip ID is 0x4312 and
@@ -703,10 +754,17 @@ static int ssb_pci_sprom_get(struct ssb_
 		if (err) {
 			/* All CRC attempts failed.
 			 * Maybe there is no SPROM on the device?
-			 * If we have a fallback, use that. */
-			fallback = ssb_get_fallback_sprom();
-			if (fallback) {
-				memcpy(sprom, fallback, sizeof(*sprom));
+			 * Now we ask the arch code if there is some sprom
+			 * available for this device in some other storage */
+			err = ssb_fill_sprom_with_fallback(bus, sprom);
+			if (err) {
+				ssb_printk(KERN_WARNING PFX "WARNING: Using"
+					   " fallback SPROM failed (err %d)\n",
+					   err);
+			} else {
+				ssb_dprintk(KERN_DEBUG PFX "Using SPROM"
+					    " revision %d provided by"
+					    " platform.\n", sprom->revision);
 				err = 0;
 				goto out_free;
 			}
@@ -724,12 +782,9 @@ out_free:
 static void ssb_pci_get_boardinfo(struct ssb_bus *bus,
 				  struct ssb_boardinfo *bi)
 {
-	pci_read_config_word(bus->host_pci, PCI_SUBSYSTEM_VENDOR_ID,
-			     &bi->vendor);
-	pci_read_config_word(bus->host_pci, PCI_SUBSYSTEM_ID,
-			     &bi->type);
-	pci_read_config_word(bus->host_pci, PCI_REVISION_ID,
-			     &bi->rev);
+	bi->vendor = bus->host_pci->subsystem_vendor;
+	bi->type = bus->host_pci->subsystem_device;
+	bi->rev = bus->host_pci->revision;
 }
 
 int ssb_pci_get_invariants(struct ssb_bus *bus,
--- a/include/linux/ssb/ssb_regs.h
+++ b/include/linux/ssb/ssb_regs.h
@@ -85,6 +85,8 @@
 #define  SSB_IMSTATE_AP_RSV	0x00000030 /* Reserved */
 #define  SSB_IMSTATE_IBE	0x00020000 /* In Band Error */
 #define  SSB_IMSTATE_TO		0x00040000 /* Timeout */
+#define  SSB_IMSTATE_BUSY	0x01800000 /* Busy (Backplane rev >= 2.3 only) */
+#define  SSB_IMSTATE_REJECT	0x02000000 /* Reject (Backplane rev >= 2.3 only) */
 #define SSB_INTVEC		0x0F94     /* SB Interrupt Mask */
 #define  SSB_INTVEC_PCI		0x00000001 /* Enable interrupts for PCI */
 #define  SSB_INTVEC_ENET0	0x00000002 /* Enable interrupts for enet 0 */
@@ -95,9 +97,8 @@
 #define  SSB_INTVEC_ENET1	0x00000040 /* Enable interrupts for enet 1 */
 #define SSB_TMSLOW		0x0F98     /* SB Target State Low */
 #define  SSB_TMSLOW_RESET	0x00000001 /* Reset */
-#define  SSB_TMSLOW_REJECT_22	0x00000002 /* Reject (Backplane rev 2.2) */
+#define  SSB_TMSLOW_REJECT	0x00000002 /* Reject (Standard Backplane) */
 #define  SSB_TMSLOW_REJECT_23	0x00000004 /* Reject (Backplane rev 2.3) */
-#define  SSB_TMSLOW_PHYCLK	0x00000010 /* MAC PHY Clock Control Enable */
 #define  SSB_TMSLOW_CLOCK	0x00010000 /* Clock Enable */
 #define  SSB_TMSLOW_FGC		0x00020000 /* Force Gated Clocks On */
 #define  SSB_TMSLOW_PE		0x40000000 /* Power Management Enable */
@@ -268,6 +269,8 @@
 /* SPROM Revision 4 */
 #define SSB_SPROM4_BFLLO		0x0044	/* Boardflags (low 16 bits) */
 #define SSB_SPROM4_BFLHI		0x0046  /* Board Flags Hi */
+#define SSB_SPROM4_BFL2LO		0x0048	/* Board flags 2 (low 16 bits) */
+#define SSB_SPROM4_BFL2HI		0x004A	/* Board flags 2 Hi */
 #define SSB_SPROM4_IL0MAC		0x004C	/* 6 byte MAC address for a/b/g/n */
 #define SSB_SPROM4_CCODE		0x0052	/* Country Code (2 bytes) */
 #define SSB_SPROM4_GPIOA		0x0056	/* Gen. Purpose IO # 0 and 1 */
@@ -358,6 +361,8 @@
 #define SSB_SPROM5_CCODE		0x0044	/* Country Code (2 bytes) */
 #define SSB_SPROM5_BFLLO		0x004A	/* Boardflags (low 16 bits) */
 #define SSB_SPROM5_BFLHI		0x004C  /* Board Flags Hi */
+#define SSB_SPROM5_BFL2LO		0x004E	/* Board flags 2 (low 16 bits) */
+#define SSB_SPROM5_BFL2HI		0x0050	/* Board flags 2 Hi */
 #define SSB_SPROM5_IL0MAC		0x0052	/* 6 byte MAC address for a/b/g/n */
 #define SSB_SPROM5_GPIOA		0x0076	/* Gen. Purpose IO # 0 and 1 */
 #define  SSB_SPROM5_GPIOA_P0		0x00FF	/* Pin 0 */
@@ -427,6 +432,56 @@
 #define  SSB_SPROM8_RXPO2G		0x00FF	/* 2GHz RX power offset */
 #define  SSB_SPROM8_RXPO5G		0xFF00	/* 5GHz RX power offset */
 #define  SSB_SPROM8_RXPO5G_SHIFT	8
+#define SSB_SPROM8_FEM2G		0x00AE
+#define SSB_SPROM8_FEM5G		0x00B0
+#define  SSB_SROM8_FEM_TSSIPOS		0x0001
+#define  SSB_SROM8_FEM_TSSIPOS_SHIFT	0
+#define  SSB_SROM8_FEM_EXTPA_GAIN	0x0006
+#define  SSB_SROM8_FEM_EXTPA_GAIN_SHIFT	1
+#define  SSB_SROM8_FEM_PDET_RANGE	0x00F8
+#define  SSB_SROM8_FEM_PDET_RANGE_SHIFT	3
+#define  SSB_SROM8_FEM_TR_ISO		0x0700
+#define  SSB_SROM8_FEM_TR_ISO_SHIFT	8
+#define  SSB_SROM8_FEM_ANTSWLUT		0xF800
+#define  SSB_SROM8_FEM_ANTSWLUT_SHIFT	11
+#define SSB_SPROM8_THERMAL		0x00B2
+#define SSB_SPROM8_MPWR_RAWTS		0x00B4
+#define SSB_SPROM8_TS_SLP_OPT_CORRX	0x00B6
+#define SSB_SPROM8_FOC_HWIQ_IQSWP	0x00B8
+#define SSB_SPROM8_PHYCAL_TEMPDELTA	0x00BA
+
+/* There are 4 blocks with power info sharing the same layout */
+#define SSB_SROM8_PWR_INFO_CORE0	0x00C0
+#define SSB_SROM8_PWR_INFO_CORE1	0x00E0
+#define SSB_SROM8_PWR_INFO_CORE2	0x0100
+#define SSB_SROM8_PWR_INFO_CORE3	0x0120
+
+#define SSB_SROM8_2G_MAXP_ITSSI		0x00
+#define  SSB_SPROM8_2G_MAXP		0x00FF
+#define  SSB_SPROM8_2G_ITSSI		0xFF00
+#define  SSB_SPROM8_2G_ITSSI_SHIFT	8
+#define SSB_SROM8_2G_PA_0		0x02	/* 2GHz power amp settings */
+#define SSB_SROM8_2G_PA_1		0x04
+#define SSB_SROM8_2G_PA_2		0x06
+#define SSB_SROM8_5G_MAXP_ITSSI		0x08	/* 5GHz ITSSI and 5.3GHz Max Power */
+#define  SSB_SPROM8_5G_MAXP		0x00FF
+#define  SSB_SPROM8_5G_ITSSI		0xFF00
+#define  SSB_SPROM8_5G_ITSSI_SHIFT	8
+#define SSB_SPROM8_5GHL_MAXP		0x0A	/* 5.2GHz and 5.8GHz Max Power */
+#define  SSB_SPROM8_5GH_MAXP		0x00FF
+#define  SSB_SPROM8_5GL_MAXP		0xFF00
+#define  SSB_SPROM8_5GL_MAXP_SHIFT	8
+#define SSB_SROM8_5G_PA_0		0x0C	/* 5.3GHz power amp settings */
+#define SSB_SROM8_5G_PA_1		0x0E
+#define SSB_SROM8_5G_PA_2		0x10
+#define SSB_SROM8_5GL_PA_0		0x12	/* 5.2GHz power amp settings */
+#define SSB_SROM8_5GL_PA_1		0x14
+#define SSB_SROM8_5GL_PA_2		0x16
+#define SSB_SROM8_5GH_PA_0		0x18	/* 5.8GHz power amp settings */
+#define SSB_SROM8_5GH_PA_1		0x1A
+#define SSB_SROM8_5GH_PA_2		0x1C
+
+/* TODO: Make it deprecated */
 #define SSB_SPROM8_MAXP_BG		0x00C0  /* Max Power 2GHz in path 1 */
 #define  SSB_SPROM8_MAXP_BG_MASK	0x00FF  /* Mask for Max Power 2GHz */
 #define  SSB_SPROM8_ITSSI_BG		0xFF00	/* Mask for path 1 itssi_bg */
@@ -451,12 +506,53 @@
 #define SSB_SPROM8_PA1HIB0		0x00D8	/* 5.8GHz power amp settings */
 #define SSB_SPROM8_PA1HIB1		0x00DA
 #define SSB_SPROM8_PA1HIB2		0x00DC
+
 #define SSB_SPROM8_CCK2GPO		0x0140	/* CCK power offset */
 #define SSB_SPROM8_OFDM2GPO		0x0142	/* 2.4GHz OFDM power offset */
 #define SSB_SPROM8_OFDM5GPO		0x0146	/* 5.3GHz OFDM power offset */
 #define SSB_SPROM8_OFDM5GLPO		0x014A	/* 5.2GHz OFDM power offset */
 #define SSB_SPROM8_OFDM5GHPO		0x014E	/* 5.8GHz OFDM power offset */
 
+/* Values for boardflags_lo read from SPROM */
+#define SSB_BFL_BTCOEXIST		0x0001	/* implements Bluetooth coexistance */
+#define SSB_BFL_PACTRL			0x0002	/* GPIO 9 controlling the PA */
+#define SSB_BFL_AIRLINEMODE		0x0004	/* implements GPIO 13 radio disable indication */
+#define SSB_BFL_RSSI			0x0008	/* software calculates nrssi slope. */
+#define SSB_BFL_ENETSPI			0x0010	/* has ephy roboswitch spi */
+#define SSB_BFL_XTAL_NOSLOW		0x0020	/* no slow clock available */
+#define SSB_BFL_CCKHIPWR		0x0040	/* can do high power CCK transmission */
+#define SSB_BFL_ENETADM			0x0080	/* has ADMtek switch */
+#define SSB_BFL_ENETVLAN		0x0100	/* can do vlan */
+#define SSB_BFL_AFTERBURNER		0x0200	/* supports Afterburner mode */
+#define SSB_BFL_NOPCI			0x0400	/* board leaves PCI floating */
+#define SSB_BFL_FEM			0x0800	/* supports the Front End Module */
+#define SSB_BFL_EXTLNA			0x1000	/* has an external LNA */
+#define SSB_BFL_HGPA			0x2000	/* had high gain PA */
+#define SSB_BFL_BTCMOD			0x4000	/* BFL_BTCOEXIST is given in alternate GPIOs */
+#define SSB_BFL_ALTIQ			0x8000	/* alternate I/Q settings */
+
+/* Values for boardflags_hi read from SPROM */
+#define SSB_BFH_NOPA			0x0001	/* has no PA */
+#define SSB_BFH_RSSIINV			0x0002	/* RSSI uses positive slope (not TSSI) */
+#define SSB_BFH_PAREF			0x0004	/* uses the PARef LDO */
+#define SSB_BFH_3TSWITCH		0x0008	/* uses a triple throw switch shared with bluetooth */
+#define SSB_BFH_PHASESHIFT		0x0010	/* can support phase shifter */
+#define SSB_BFH_BUCKBOOST		0x0020	/* has buck/booster */
+#define SSB_BFH_FEM_BT			0x0040	/* has FEM and switch to share antenna with bluetooth */
+
+/* Values for boardflags2_lo read from SPROM */
+#define SSB_BFL2_RXBB_INT_REG_DIS	0x0001	/* external RX BB regulator present */
+#define SSB_BFL2_APLL_WAR		0x0002	/* alternative A-band PLL settings implemented */
+#define SSB_BFL2_TXPWRCTRL_EN 		0x0004	/* permits enabling TX Power Control */
+#define SSB_BFL2_2X4_DIV		0x0008	/* 2x4 diversity switch */
+#define SSB_BFL2_5G_PWRGAIN		0x0010	/* supports 5G band power gain */
+#define SSB_BFL2_PCIEWAR_OVR		0x0020	/* overrides ASPM and Clkreq settings */
+#define SSB_BFL2_CAESERS_BRD		0x0040	/* is Caesers board (unused) */
+#define SSB_BFL2_BTC3WIRE		0x0080	/* used 3-wire bluetooth coexist */
+#define SSB_BFL2_SKWRKFEM_BRD		0x0100	/* 4321mcm93 uses Skyworks FEM */
+#define SSB_BFL2_SPUR_WAR		0x0200	/* has a workaround for clock-harmonic spurs */
+#define SSB_BFL2_GPLL_WAR		0x0400	/* altenative G-band PLL settings implemented */
+
 /* Values for SSB_SPROM1_BINF_CCODE */
 enum {
 	SSB_SPROM1CCODE_WORLD = 0,
--- a/drivers/ssb/driver_chipcommon.c
+++ b/drivers/ssb/driver_chipcommon.c
@@ -3,7 +3,7 @@
  * Broadcom ChipCommon core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -46,40 +46,66 @@ void ssb_chipco_set_clockmode(struct ssb
 	if (!ccdev)
 		return;
 	bus = ccdev->bus;
+
+	/* We support SLOW only on 6..9 */
+	if (ccdev->id.revision >= 10 && mode == SSB_CLKMODE_SLOW)
+		mode = SSB_CLKMODE_DYNAMIC;
+
+	if (cc->capabilities & SSB_CHIPCO_CAP_PMU)
+		return; /* PMU controls clockmode, separated function needed */
+	SSB_WARN_ON(ccdev->id.revision >= 20);
+
 	/* chipcommon cores prior to rev6 don't support dynamic clock control */
 	if (ccdev->id.revision < 6)
 		return;
-	/* chipcommon cores rev10 are a whole new ball game */
+
+	/* ChipCommon cores rev10+ need testing */
 	if (ccdev->id.revision >= 10)
 		return;
+
 	if (!(cc->capabilities & SSB_CHIPCO_CAP_PCTL))
 		return;
 
 	switch (mode) {
-	case SSB_CLKMODE_SLOW:
+	case SSB_CLKMODE_SLOW: /* For revs 6..9 only */
 		tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
 		tmp |= SSB_CHIPCO_SLOWCLKCTL_FSLOW;
 		chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
 		break;
 	case SSB_CLKMODE_FAST:
-		ssb_pci_xtal(bus, SSB_GPIO_XTAL, 1); /* Force crystal on */
-		tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
-		tmp |= SSB_CHIPCO_SLOWCLKCTL_IPLL;
-		chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
+		if (ccdev->id.revision < 10) {
+			ssb_pci_xtal(bus, SSB_GPIO_XTAL, 1); /* Force crystal on */
+			tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
+			tmp |= SSB_CHIPCO_SLOWCLKCTL_IPLL;
+			chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
+		} else {
+			chipco_write32(cc, SSB_CHIPCO_SYSCLKCTL,
+				(chipco_read32(cc, SSB_CHIPCO_SYSCLKCTL) |
+				 SSB_CHIPCO_SYSCLKCTL_FORCEHT));
+			/* udelay(150); TODO: not available in early init */
+		}
 		break;
 	case SSB_CLKMODE_DYNAMIC:
-		tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_IPLL;
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
-		if ((tmp & SSB_CHIPCO_SLOWCLKCTL_SRC) != SSB_CHIPCO_SLOWCLKCTL_SRC_XTAL)
-			tmp |= SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
-		chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
-
-		/* for dynamic control, we have to release our xtal_pu "force on" */
-		if (tmp & SSB_CHIPCO_SLOWCLKCTL_ENXTAL)
-			ssb_pci_xtal(bus, SSB_GPIO_XTAL, 0);
+		if (ccdev->id.revision < 10) {
+			tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_IPLL;
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
+			if ((tmp & SSB_CHIPCO_SLOWCLKCTL_SRC) !=
+			    SSB_CHIPCO_SLOWCLKCTL_SRC_XTAL)
+				tmp |= SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
+			chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
+
+			/* For dynamic control, we have to release our xtal_pu
+			 * "force on" */
+			if (tmp & SSB_CHIPCO_SLOWCLKCTL_ENXTAL)
+				ssb_pci_xtal(bus, SSB_GPIO_XTAL, 0);
+		} else {
+			chipco_write32(cc, SSB_CHIPCO_SYSCLKCTL,
+				(chipco_read32(cc, SSB_CHIPCO_SYSCLKCTL) &
+				 ~SSB_CHIPCO_SYSCLKCTL_FORCEHT));
+		}
 		break;
 	default:
 		SSB_WARN_ON(1);
@@ -260,6 +286,12 @@ void ssb_chipcommon_init(struct ssb_chip
 	if (cc->dev->id.revision >= 11)
 		cc->status = chipco_read32(cc, SSB_CHIPCO_CHIPSTAT);
 	ssb_dprintk(KERN_INFO PFX "chipcommon status is 0x%x\n", cc->status);
+
+	if (cc->dev->id.revision >= 20) {
+		chipco_write32(cc, SSB_CHIPCO_GPIOPULLUP, 0);
+		chipco_write32(cc, SSB_CHIPCO_GPIOPULLDOWN, 0);
+	}
+
 	ssb_pmu_init(cc);
 	chipco_powercontrol_init(cc);
 	ssb_chipco_set_clockmode(cc, SSB_CLKMODE_FAST);
--- a/drivers/ssb/driver_chipcommon_pmu.c
+++ b/drivers/ssb/driver_chipcommon_pmu.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Broadcom ChipCommon Power Management Unit driver
  *
- * Copyright 2009, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2009, Michael Buesch <m@bues.ch>
  * Copyright 2007, Broadcom Corporation
  *
  * Licensed under the GNU/GPL. See COPYING for details.
@@ -12,6 +12,9 @@
 #include <linux/ssb/ssb_regs.h>
 #include <linux/ssb/ssb_driver_chipcommon.h>
 #include <linux/delay.h>
+#ifdef CONFIG_BCM47XX
+#include <asm/mach-bcm47xx/nvram.h>
+#endif
 
 #include "ssb_private.h"
 
@@ -91,10 +94,6 @@ static void ssb_pmu0_pllinit_r0(struct s
 	u32 pmuctl, tmp, pllctl;
 	unsigned int i;
 
-	if ((bus->chip_id == 0x5354) && !crystalfreq) {
-		/* The 5354 crystal freq is 25MHz */
-		crystalfreq = 25000;
-	}
 	if (crystalfreq)
 		e = pmu0_plltab_find_entry(crystalfreq);
 	if (!e)
@@ -320,7 +319,11 @@ static void ssb_pmu_pll_init(struct ssb_
 	u32 crystalfreq = 0; /* in kHz. 0 = keep default freq. */
 
 	if (bus->bustype == SSB_BUSTYPE_SSB) {
-		/* TODO: The user may override the crystal frequency. */
+#ifdef CONFIG_BCM47XX
+		char buf[20];
+		if (nvram_getenv("xtalfreq", buf, sizeof(buf)) >= 0)
+			crystalfreq = simple_strtoul(buf, NULL, 0);
+#endif
 	}
 
 	switch (bus->chip_id) {
@@ -329,7 +332,11 @@ static void ssb_pmu_pll_init(struct ssb_
 		ssb_pmu1_pllinit_r0(cc, crystalfreq);
 		break;
 	case 0x4328:
+		ssb_pmu0_pllinit_r0(cc, crystalfreq);
+		break;
 	case 0x5354:
+		if (crystalfreq == 0)
+			crystalfreq = 25000;
 		ssb_pmu0_pllinit_r0(cc, crystalfreq);
 		break;
 	case 0x4322:
@@ -417,12 +424,14 @@ static void ssb_pmu_resources_init(struc
 	u32 min_msk = 0, max_msk = 0;
 	unsigned int i;
 	const struct pmu_res_updown_tab_entry *updown_tab = NULL;
-	unsigned int updown_tab_size;
+	unsigned int updown_tab_size = 0;
 	const struct pmu_res_depend_tab_entry *depend_tab = NULL;
-	unsigned int depend_tab_size;
+	unsigned int depend_tab_size = 0;
 
 	switch (bus->chip_id) {
 	case 0x4312:
+		 min_msk = 0xCBB;
+		 break;
 	case 0x4322:
 		/* We keep the default settings:
 		 * min_msk = 0xCBB
@@ -604,3 +613,34 @@ void ssb_pmu_set_ldo_paref(struct ssb_ch
 
 EXPORT_SYMBOL(ssb_pmu_set_ldo_voltage);
 EXPORT_SYMBOL(ssb_pmu_set_ldo_paref);
+
+u32 ssb_pmu_get_cpu_clock(struct ssb_chipcommon *cc)
+{
+	struct ssb_bus *bus = cc->dev->bus;
+
+	switch (bus->chip_id) {
+	case 0x5354:
+		/* 5354 chip uses a non programmable PLL of frequency 240MHz */
+		return 240000000;
+	default:
+		ssb_printk(KERN_ERR PFX
+			   "ERROR: PMU cpu clock unknown for device %04X\n",
+			   bus->chip_id);
+		return 0;
+	}
+}
+
+u32 ssb_pmu_get_controlclock(struct ssb_chipcommon *cc)
+{
+	struct ssb_bus *bus = cc->dev->bus;
+
+	switch (bus->chip_id) {
+	case 0x5354:
+		return 120000000;
+	default:
+		ssb_printk(KERN_ERR PFX
+			   "ERROR: PMU controlclock unknown for device %04X\n",
+			   bus->chip_id);
+		return 0;
+	}
+}
--- a/drivers/ssb/driver_gige.c
+++ b/drivers/ssb/driver_gige.c
@@ -3,7 +3,7 @@
  * Broadcom Gigabit Ethernet core driver
  *
  * Copyright 2008, Broadcom Corporation
- * Copyright 2008, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2008, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -106,8 +106,9 @@ void gige_pcicfg_write32(struct ssb_gige
 	gige_write32(dev, SSB_GIGE_PCICFG + offset, value);
 }
 
-static int ssb_gige_pci_read_config(struct pci_bus *bus, unsigned int devfn,
-				    int reg, int size, u32 *val)
+static int __devinit ssb_gige_pci_read_config(struct pci_bus *bus,
+					      unsigned int devfn, int reg,
+					      int size, u32 *val)
 {
 	struct ssb_gige *dev = container_of(bus->ops, struct ssb_gige, pci_ops);
 	unsigned long flags;
@@ -136,8 +137,9 @@ static int ssb_gige_pci_read_config(stru
 	return PCIBIOS_SUCCESSFUL;
 }
 
-static int ssb_gige_pci_write_config(struct pci_bus *bus, unsigned int devfn,
-				     int reg, int size, u32 val)
+static int __devinit ssb_gige_pci_write_config(struct pci_bus *bus,
+					       unsigned int devfn, int reg,
+					       int size, u32 val)
 {
 	struct ssb_gige *dev = container_of(bus->ops, struct ssb_gige, pci_ops);
 	unsigned long flags;
@@ -166,7 +168,8 @@ static int ssb_gige_pci_write_config(str
 	return PCIBIOS_SUCCESSFUL;
 }
 
-static int ssb_gige_probe(struct ssb_device *sdev, const struct ssb_device_id *id)
+static int __devinit ssb_gige_probe(struct ssb_device *sdev,
+				    const struct ssb_device_id *id)
 {
 	struct ssb_gige *dev;
 	u32 base, tmslow, tmshigh;
--- a/drivers/ssb/driver_pcicore.c
+++ b/drivers/ssb/driver_pcicore.c
@@ -3,7 +3,7 @@
  * Broadcom PCI-core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -15,6 +15,11 @@
 
 #include "ssb_private.h"
 
+static u32 ssb_pcie_read(struct ssb_pcicore *pc, u32 address);
+static void ssb_pcie_write(struct ssb_pcicore *pc, u32 address, u32 data);
+static u16 ssb_pcie_mdio_read(struct ssb_pcicore *pc, u8 device, u8 address);
+static void ssb_pcie_mdio_write(struct ssb_pcicore *pc, u8 device,
+				u8 address, u16 data);
 
 static inline
 u32 pcicore_read32(struct ssb_pcicore *pc, u16 offset)
@@ -69,7 +74,7 @@ static u32 get_cfgspace_addr(struct ssb_
 	u32 tmp;
 
 	/* We do only have one cardbus device behind the bridge. */
-	if (pc->cardbusmode && (dev >= 1))
+	if (pc->cardbusmode && (dev > 1))
 		goto out;
 
 	if (bus == 0) {
@@ -309,7 +314,7 @@ int ssb_pcicore_pcibios_map_irq(const st
 	return ssb_mips_irq(extpci_core->dev) + 2;
 }
 
-static void ssb_pcicore_init_hostmode(struct ssb_pcicore *pc)
+static void __devinit ssb_pcicore_init_hostmode(struct ssb_pcicore *pc)
 {
 	u32 val;
 
@@ -374,7 +379,7 @@ static void ssb_pcicore_init_hostmode(st
 	register_pci_controller(&ssb_pcicore_controller);
 }
 
-static int pcicore_is_in_hostmode(struct ssb_pcicore *pc)
+static int __devinit pcicore_is_in_hostmode(struct ssb_pcicore *pc)
 {
 	struct ssb_bus *bus = pc->dev->bus;
 	u16 chipid_top;
@@ -403,25 +408,137 @@ static int pcicore_is_in_hostmode(struct
 }
 #endif /* CONFIG_SSB_PCICORE_HOSTMODE */
 
+/**************************************************
+ * Workarounds.
+ **************************************************/
+
+static void __devinit ssb_pcicore_fix_sprom_core_index(struct ssb_pcicore *pc)
+{
+	u16 tmp = pcicore_read16(pc, SSB_PCICORE_SPROM(0));
+	if (((tmp & 0xF000) >> 12) != pc->dev->core_index) {
+		tmp &= ~0xF000;
+		tmp |= (pc->dev->core_index << 12);
+		pcicore_write16(pc, SSB_PCICORE_SPROM(0), tmp);
+	}
+}
+
+static u8 ssb_pcicore_polarity_workaround(struct ssb_pcicore *pc)
+{
+	return (ssb_pcie_read(pc, 0x204) & 0x10) ? 0xC0 : 0x80;
+}
+
+static void ssb_pcicore_serdes_workaround(struct ssb_pcicore *pc)
+{
+	const u8 serdes_pll_device = 0x1D;
+	const u8 serdes_rx_device = 0x1F;
+	u16 tmp;
+
+	ssb_pcie_mdio_write(pc, serdes_rx_device, 1 /* Control */,
+			    ssb_pcicore_polarity_workaround(pc));
+	tmp = ssb_pcie_mdio_read(pc, serdes_pll_device, 1 /* Control */);
+	if (tmp & 0x4000)
+		ssb_pcie_mdio_write(pc, serdes_pll_device, 1, tmp & ~0x4000);
+}
+
+static void ssb_pcicore_pci_setup_workarounds(struct ssb_pcicore *pc)
+{
+	struct ssb_device *pdev = pc->dev;
+	struct ssb_bus *bus = pdev->bus;
+	u32 tmp;
+
+	tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
+	tmp |= SSB_PCICORE_SBTOPCI_PREF;
+	tmp |= SSB_PCICORE_SBTOPCI_BURST;
+	pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
+
+	if (pdev->id.revision < 5) {
+		tmp = ssb_read32(pdev, SSB_IMCFGLO);
+		tmp &= ~SSB_IMCFGLO_SERTO;
+		tmp |= 2;
+		tmp &= ~SSB_IMCFGLO_REQTO;
+		tmp |= 3 << SSB_IMCFGLO_REQTO_SHIFT;
+		ssb_write32(pdev, SSB_IMCFGLO, tmp);
+		ssb_commit_settings(bus);
+	} else if (pdev->id.revision >= 11) {
+		tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
+		tmp |= SSB_PCICORE_SBTOPCI_MRM;
+		pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
+	}
+}
+
+static void ssb_pcicore_pcie_setup_workarounds(struct ssb_pcicore *pc)
+{
+	u32 tmp;
+	u8 rev = pc->dev->id.revision;
+
+	if (rev == 0 || rev == 1) {
+		/* TLP Workaround register. */
+		tmp = ssb_pcie_read(pc, 0x4);
+		tmp |= 0x8;
+		ssb_pcie_write(pc, 0x4, tmp);
+	}
+	if (rev == 1) {
+		/* DLLP Link Control register. */
+		tmp = ssb_pcie_read(pc, 0x100);
+		tmp |= 0x40;
+		ssb_pcie_write(pc, 0x100, tmp);
+	}
+
+	if (rev == 0) {
+		const u8 serdes_rx_device = 0x1F;
+
+		ssb_pcie_mdio_write(pc, serdes_rx_device,
+					2 /* Timer */, 0x8128);
+		ssb_pcie_mdio_write(pc, serdes_rx_device,
+					6 /* CDR */, 0x0100);
+		ssb_pcie_mdio_write(pc, serdes_rx_device,
+					7 /* CDR BW */, 0x1466);
+	} else if (rev == 3 || rev == 4 || rev == 5) {
+		/* TODO: DLLP Power Management Threshold */
+		ssb_pcicore_serdes_workaround(pc);
+		/* TODO: ASPM */
+	} else if (rev == 7) {
+		/* TODO: No PLL down */
+	}
+
+	if (rev >= 6) {
+		/* Miscellaneous Configuration Fixup */
+		tmp = pcicore_read16(pc, SSB_PCICORE_SPROM(5));
+		if (!(tmp & 0x8000))
+			pcicore_write16(pc, SSB_PCICORE_SPROM(5),
+					tmp | 0x8000);
+	}
+}
 
 /**************************************************
  * Generic and Clientmode operation code.
  **************************************************/
 
-static void ssb_pcicore_init_clientmode(struct ssb_pcicore *pc)
+static void __devinit ssb_pcicore_init_clientmode(struct ssb_pcicore *pc)
 {
+	struct ssb_device *pdev = pc->dev;
+	struct ssb_bus *bus = pdev->bus;
+
+	if (bus->bustype == SSB_BUSTYPE_PCI)
+		ssb_pcicore_fix_sprom_core_index(pc);
+
 	/* Disable PCI interrupts. */
-	ssb_write32(pc->dev, SSB_INTVEC, 0);
+	ssb_write32(pdev, SSB_INTVEC, 0);
+
+	/* Additional PCIe always once-executed workarounds */
+	if (pc->dev->id.coreid == SSB_DEV_PCIE) {
+		ssb_pcicore_serdes_workaround(pc);
+		/* TODO: ASPM */
+		/* TODO: Clock Request Update */
+	}
 }
 
-void ssb_pcicore_init(struct ssb_pcicore *pc)
+void __devinit ssb_pcicore_init(struct ssb_pcicore *pc)
 {
 	struct ssb_device *dev = pc->dev;
-	struct ssb_bus *bus;
 
 	if (!dev)
 		return;
-	bus = dev->bus;
 	if (!ssb_device_is_enabled(dev))
 		ssb_device_enable(dev, 0);
 
@@ -446,11 +563,35 @@ static void ssb_pcie_write(struct ssb_pc
 	pcicore_write32(pc, 0x134, data);
 }
 
-static void ssb_pcie_mdio_write(struct ssb_pcicore *pc, u8 device,
-				u8 address, u16 data)
+static void ssb_pcie_mdio_set_phy(struct ssb_pcicore *pc, u8 phy)
+{
+	const u16 mdio_control = 0x128;
+	const u16 mdio_data = 0x12C;
+	u32 v;
+	int i;
+
+	v = (1 << 30); /* Start of Transaction */
+	v |= (1 << 28); /* Write Transaction */
+	v |= (1 << 17); /* Turnaround */
+	v |= (0x1F << 18);
+	v |= (phy << 4);
+	pcicore_write32(pc, mdio_data, v);
+
+	udelay(10);
+	for (i = 0; i < 200; i++) {
+		v = pcicore_read32(pc, mdio_control);
+		if (v & 0x100 /* Trans complete */)
+			break;
+		msleep(1);
+	}
+}
+
+static u16 ssb_pcie_mdio_read(struct ssb_pcicore *pc, u8 device, u8 address)
 {
 	const u16 mdio_control = 0x128;
 	const u16 mdio_data = 0x12C;
+	int max_retries = 10;
+	u16 ret = 0;
 	u32 v;
 	int i;
 
@@ -458,46 +599,68 @@ static void ssb_pcie_mdio_write(struct s
 	v |= 0x2; /* MDIO Clock Divisor */
 	pcicore_write32(pc, mdio_control, v);
 
+	if (pc->dev->id.revision >= 10) {
+		max_retries = 200;
+		ssb_pcie_mdio_set_phy(pc, device);
+	}
+
 	v = (1 << 30); /* Start of Transaction */
-	v |= (1 << 28); /* Write Transaction */
+	v |= (1 << 29); /* Read Transaction */
 	v |= (1 << 17); /* Turnaround */
-	v |= (u32)device << 22;
+	if (pc->dev->id.revision < 10)
+		v |= (u32)device << 22;
 	v |= (u32)address << 18;
-	v |= data;
 	pcicore_write32(pc, mdio_data, v);
 	/* Wait for the device to complete the transaction */
 	udelay(10);
-	for (i = 0; i < 10; i++) {
+	for (i = 0; i < max_retries; i++) {
 		v = pcicore_read32(pc, mdio_control);
-		if (v & 0x100 /* Trans complete */)
+		if (v & 0x100 /* Trans complete */) {
+			udelay(10);
+			ret = pcicore_read32(pc, mdio_data);
 			break;
+		}
 		msleep(1);
 	}
 	pcicore_write32(pc, mdio_control, 0);
+	return ret;
 }
 
-static void ssb_broadcast_value(struct ssb_device *dev,
-				u32 address, u32 data)
+static void ssb_pcie_mdio_write(struct ssb_pcicore *pc, u8 device,
+				u8 address, u16 data)
 {
-	/* This is used for both, PCI and ChipCommon core, so be careful. */
-	BUILD_BUG_ON(SSB_PCICORE_BCAST_ADDR != SSB_CHIPCO_BCAST_ADDR);
-	BUILD_BUG_ON(SSB_PCICORE_BCAST_DATA != SSB_CHIPCO_BCAST_DATA);
+	const u16 mdio_control = 0x128;
+	const u16 mdio_data = 0x12C;
+	int max_retries = 10;
+	u32 v;
+	int i;
 
-	ssb_write32(dev, SSB_PCICORE_BCAST_ADDR, address);
-	ssb_read32(dev, SSB_PCICORE_BCAST_ADDR); /* flush */
-	ssb_write32(dev, SSB_PCICORE_BCAST_DATA, data);
-	ssb_read32(dev, SSB_PCICORE_BCAST_DATA); /* flush */
-}
+	v = 0x80; /* Enable Preamble Sequence */
+	v |= 0x2; /* MDIO Clock Divisor */
+	pcicore_write32(pc, mdio_control, v);
 
-static void ssb_commit_settings(struct ssb_bus *bus)
-{
-	struct ssb_device *dev;
+	if (pc->dev->id.revision >= 10) {
+		max_retries = 200;
+		ssb_pcie_mdio_set_phy(pc, device);
+	}
 
-	dev = bus->chipco.dev ? bus->chipco.dev : bus->pcicore.dev;
-	if (WARN_ON(!dev))
-		return;
-	/* This forces an update of the cached registers. */
-	ssb_broadcast_value(dev, 0xFD8, 0);
+	v = (1 << 30); /* Start of Transaction */
+	v |= (1 << 28); /* Write Transaction */
+	v |= (1 << 17); /* Turnaround */
+	if (pc->dev->id.revision < 10)
+		v |= (u32)device << 22;
+	v |= (u32)address << 18;
+	v |= data;
+	pcicore_write32(pc, mdio_data, v);
+	/* Wait for the device to complete the transaction */
+	udelay(10);
+	for (i = 0; i < max_retries; i++) {
+		v = pcicore_read32(pc, mdio_control);
+		if (v & 0x100 /* Trans complete */)
+			break;
+		msleep(1);
+	}
+	pcicore_write32(pc, mdio_control, 0);
 }
 
 int ssb_pcicore_dev_irqvecs_enable(struct ssb_pcicore *pc,
@@ -550,48 +713,10 @@ int ssb_pcicore_dev_irqvecs_enable(struc
 	if (pc->setup_done)
 		goto out;
 	if (pdev->id.coreid == SSB_DEV_PCI) {
-		tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
-		tmp |= SSB_PCICORE_SBTOPCI_PREF;
-		tmp |= SSB_PCICORE_SBTOPCI_BURST;
-		pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
-
-		if (pdev->id.revision < 5) {
-			tmp = ssb_read32(pdev, SSB_IMCFGLO);
-			tmp &= ~SSB_IMCFGLO_SERTO;
-			tmp |= 2;
-			tmp &= ~SSB_IMCFGLO_REQTO;
-			tmp |= 3 << SSB_IMCFGLO_REQTO_SHIFT;
-			ssb_write32(pdev, SSB_IMCFGLO, tmp);
-			ssb_commit_settings(bus);
-		} else if (pdev->id.revision >= 11) {
-			tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
-			tmp |= SSB_PCICORE_SBTOPCI_MRM;
-			pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
-		}
+		ssb_pcicore_pci_setup_workarounds(pc);
 	} else {
 		WARN_ON(pdev->id.coreid != SSB_DEV_PCIE);
-		//TODO: Better make defines for all these magic PCIE values.
-		if ((pdev->id.revision == 0) || (pdev->id.revision == 1)) {
-			/* TLP Workaround register. */
-			tmp = ssb_pcie_read(pc, 0x4);
-			tmp |= 0x8;
-			ssb_pcie_write(pc, 0x4, tmp);
-		}
-		if (pdev->id.revision == 0) {
-			const u8 serdes_rx_device = 0x1F;
-
-			ssb_pcie_mdio_write(pc, serdes_rx_device,
-					    2 /* Timer */, 0x8128);
-			ssb_pcie_mdio_write(pc, serdes_rx_device,
-					    6 /* CDR */, 0x0100);
-			ssb_pcie_mdio_write(pc, serdes_rx_device,
-					    7 /* CDR BW */, 0x1466);
-		} else if (pdev->id.revision == 1) {
-			/* DLLP Link Control register. */
-			tmp = ssb_pcie_read(pc, 0x100);
-			tmp |= 0x40;
-			ssb_pcie_write(pc, 0x100, tmp);
-		}
+		ssb_pcicore_pcie_setup_workarounds(pc);
 	}
 	pc->setup_done = 1;
 out:
--- a/drivers/ssb/pcihost_wrapper.c
+++ b/drivers/ssb/pcihost_wrapper.c
@@ -6,7 +6,7 @@
  * Copyright (c) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (c) 2005 Danny van Dyk <kugelfang@gentoo.org>
  * Copyright (c) 2005 Andreas Jaggi <andreas.jaggi@waterwave.ch>
- * Copyright (c) 2005-2007 Michael Buesch <mbuesch@freenet.de>
+ * Copyright (c) 2005-2007 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -53,8 +53,8 @@ static int ssb_pcihost_resume(struct pci
 # define ssb_pcihost_resume	NULL
 #endif /* CONFIG_PM */
 
-static int ssb_pcihost_probe(struct pci_dev *dev,
-			     const struct pci_device_id *id)
+static int __devinit ssb_pcihost_probe(struct pci_dev *dev,
+				       const struct pci_device_id *id)
 {
 	struct ssb_bus *ssb;
 	int err = -ENOMEM;
@@ -110,7 +110,7 @@ static void ssb_pcihost_remove(struct pc
 	pci_set_drvdata(dev, NULL);
 }
 
-int ssb_pcihost_register(struct pci_driver *driver)
+int __devinit ssb_pcihost_register(struct pci_driver *driver)
 {
 	driver->probe = ssb_pcihost_probe;
 	driver->remove = ssb_pcihost_remove;
--- a/drivers/ssb/scan.c
+++ b/drivers/ssb/scan.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Bus scanning
  *
- * Copyright (C) 2005-2007 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2007 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -258,7 +258,10 @@ static int we_support_multiple_80211_cor
 #ifdef CONFIG_SSB_PCIHOST
 	if (bus->bustype == SSB_BUSTYPE_PCI) {
 		if (bus->host_pci->vendor == PCI_VENDOR_ID_BROADCOM &&
-		    bus->host_pci->device == 0x4324)
+		    ((bus->host_pci->device == 0x4313) ||
+		     (bus->host_pci->device == 0x431A) ||
+		     (bus->host_pci->device == 0x4321) ||
+		     (bus->host_pci->device == 0x4324)))
 			return 1;
 	}
 #endif /* CONFIG_SSB_PCIHOST */
@@ -307,8 +310,7 @@ int ssb_bus_scan(struct ssb_bus *bus,
 	} else {
 		if (bus->bustype == SSB_BUSTYPE_PCI) {
 			bus->chip_id = pcidev_to_chipid(bus->host_pci);
-			pci_read_config_word(bus->host_pci, PCI_REVISION_ID,
-					     &bus->chip_rev);
+			bus->chip_rev = bus->host_pci->revision;
 			bus->chip_package = 0;
 		} else {
 			bus->chip_id = 0x4710;
@@ -316,6 +318,9 @@ int ssb_bus_scan(struct ssb_bus *bus,
 			bus->chip_package = 0;
 		}
 	}
+	ssb_printk(KERN_INFO PFX "Found chip with id 0x%04X, rev 0x%02X and "
+		   "package 0x%02X\n", bus->chip_id, bus->chip_rev,
+		   bus->chip_package);
 	if (!bus->nr_devices)
 		bus->nr_devices = chipid_to_nrcores(bus->chip_id);
 	if (bus->nr_devices > ARRAY_SIZE(bus->devices)) {
--- a/drivers/ssb/sprom.c
+++ b/drivers/ssb/sprom.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Common SPROM support routines
  *
- * Copyright (C) 2005-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2008 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -17,7 +17,7 @@
 #include <linux/slab.h>
 
 
-static const struct ssb_sprom *fallback_sprom;
+static int(*get_fallback_sprom)(struct ssb_bus *dev, struct ssb_sprom *out);
 
 
 static int sprom2hex(const u16 *sprom, char *buf, size_t buf_len,
@@ -145,36 +145,43 @@ out:
 }
 
 /**
- * ssb_arch_set_fallback_sprom - Set a fallback SPROM for use if no SPROM is found.
+ * ssb_arch_register_fallback_sprom - Registers a method providing a
+ * fallback SPROM if no SPROM is found.
  *
- * @sprom: The SPROM data structure to register.
+ * @sprom_callback: The callback function.
  *
- * With this function the architecture implementation may register a fallback
- * SPROM data structure. The fallback is only used for PCI based SSB devices,
- * where no valid SPROM can be found in the shadow registers.
+ * With this function the architecture implementation may register a
+ * callback handler which fills the SPROM data structure. The fallback is
+ * only used for PCI based SSB devices, where no valid SPROM can be found
+ * in the shadow registers.
+ *
+ * This function is useful for weird architectures that have a half-assed
+ * SSB device hardwired to their PCI bus.
+ *
+ * Note that it does only work with PCI attached SSB devices. PCMCIA
+ * devices currently don't use this fallback.
+ * Architectures must provide the SPROM for native SSB devices anyway, so
+ * the fallback also isn't used for native devices.
  *
- * This function is useful for weird architectures that have a half-assed SSB device
- * hardwired to their PCI bus.
- *
- * Note that it does only work with PCI attached SSB devices. PCMCIA devices currently
- * don't use this fallback.
- * Architectures must provide the SPROM for native SSB devices anyway,
- * so the fallback also isn't used for native devices.
- *
- * This function is available for architecture code, only. So it is not exported.
+ * This function is available for architecture code, only. So it is not
+ * exported.
  */
-int ssb_arch_set_fallback_sprom(const struct ssb_sprom *sprom)
+int ssb_arch_register_fallback_sprom(int (*sprom_callback)(struct ssb_bus *bus,
+				     struct ssb_sprom *out))
 {
-	if (fallback_sprom)
+	if (get_fallback_sprom)
 		return -EEXIST;
-	fallback_sprom = sprom;
+	get_fallback_sprom = sprom_callback;
 
 	return 0;
 }
 
-const struct ssb_sprom *ssb_get_fallback_sprom(void)
+int ssb_fill_sprom_with_fallback(struct ssb_bus *bus, struct ssb_sprom *out)
 {
-	return fallback_sprom;
+	if (!get_fallback_sprom)
+		return -ENOENT;
+
+	return get_fallback_sprom(bus, out);
 }
 
 /* http://bcm-v4.sipsolutions.net/802.11/IsSpromAvailable */
@@ -185,7 +192,7 @@ bool ssb_is_sprom_available(struct ssb_b
 	/* this routine differs from specs as we do not access SPROM directly
 	   on PCMCIA */
 	if (bus->bustype == SSB_BUSTYPE_PCI &&
-	    bus->chipco.dev &&	/* can be unavailible! */
+	    bus->chipco.dev &&	/* can be unavailable! */
 	    bus->chipco.dev->id.revision >= 31)
 		return bus->chipco.capabilities & SSB_CHIPCO_CAP_SPROM;
 
--- a/drivers/ssb/ssb_private.h
+++ b/drivers/ssb/ssb_private.h
@@ -171,7 +171,8 @@ ssize_t ssb_attr_sprom_store(struct ssb_
 			     const char *buf, size_t count,
 			     int (*sprom_check_crc)(const u16 *sprom, size_t size),
 			     int (*sprom_write)(struct ssb_bus *bus, const u16 *sprom));
-extern const struct ssb_sprom *ssb_get_fallback_sprom(void);
+extern int ssb_fill_sprom_with_fallback(struct ssb_bus *bus,
+					struct ssb_sprom *out);
 
 
 /* core.c */
@@ -206,4 +207,8 @@ static inline void b43_pci_ssb_bridge_ex
 }
 #endif /* CONFIG_SSB_B43_PCI_BRIDGE */
 
+/* driver_chipcommon_pmu.c */
+extern u32 ssb_pmu_get_cpu_clock(struct ssb_chipcommon *cc);
+extern u32 ssb_pmu_get_controlclock(struct ssb_chipcommon *cc);
+
 #endif /* LINUX_SSB_PRIVATE_H_ */
--- a/include/linux/ssb/ssb.h
+++ b/include/linux/ssb/ssb.h
@@ -16,6 +16,12 @@ struct pcmcia_device;
 struct ssb_bus;
 struct ssb_driver;
 
+struct ssb_sprom_core_pwr_info {
+	u8 itssi_2g, itssi_5g;
+	u8 maxpwr_2g, maxpwr_5gl, maxpwr_5g, maxpwr_5gh;
+	u16 pa_2g[4], pa_5gl[4], pa_5g[4], pa_5gh[4];
+};
+
 struct ssb_sprom {
 	u8 revision;
 	u8 il0mac[6];		/* MAC address for 802.11b/g */
@@ -25,8 +31,13 @@ struct ssb_sprom {
 	u8 et1phyaddr;		/* MII address for enet1 */
 	u8 et0mdcport;		/* MDIO for enet0 */
 	u8 et1mdcport;		/* MDIO for enet1 */
-	u8 board_rev;		/* Board revision number from SPROM. */
+	u16 board_rev;		/* Board revision number from SPROM. */
+	u16 board_num;		/* Board number from SPROM. */
+	u16 board_type;		/* Board type from SPROM. */
 	u8 country_code;	/* Country Code */
+	char alpha2[2];		/* Country Code as two chars like EU or US */
+	u8 leddc_on_time;	/* LED Powersave Duty Cycle On Count */
+	u8 leddc_off_time;	/* LED Powersave Duty Cycle Off Count */
 	u8 ant_available_a;	/* 2GHz antenna available bits (up to 4) */
 	u8 ant_available_bg;	/* 5GHz antenna available bits (up to 4) */
 	u16 pa0b0;
@@ -45,10 +56,10 @@ struct ssb_sprom {
 	u8 gpio1;		/* GPIO pin 1 */
 	u8 gpio2;		/* GPIO pin 2 */
 	u8 gpio3;		/* GPIO pin 3 */
-	u16 maxpwr_bg;		/* 2.4GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_al;		/* 5.2GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_a;		/* 5.3GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_ah;		/* 5.8GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_bg;		/* 2.4GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_al;		/* 5.2GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_a;		/* 5.3GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_ah;		/* 5.8GHz Amplifier Max Power (in dBm Q5.2) */
 	u8 itssi_a;		/* Idle TSSI Target for A-PHY */
 	u8 itssi_bg;		/* Idle TSSI Target for B/G-PHY */
 	u8 tri2g;		/* 2.4GHz TX isolation */
@@ -59,8 +70,8 @@ struct ssb_sprom {
 	u8 txpid5gl[4];		/* 4.9 - 5.1GHz TX power index */
 	u8 txpid5g[4];		/* 5.1 - 5.5GHz TX power index */
 	u8 txpid5gh[4];		/* 5.5 - ...GHz TX power index */
-	u8 rxpo2g;		/* 2GHz RX power offset */
-	u8 rxpo5g;		/* 5GHz RX power offset */
+	s8 rxpo2g;		/* 2GHz RX power offset */
+	s8 rxpo5g;		/* 5GHz RX power offset */
 	u8 rssisav2g;		/* 2GHz RSSI params */
 	u8 rssismc2g;
 	u8 rssismf2g;
@@ -80,26 +91,104 @@ struct ssb_sprom {
 	u16 boardflags2_hi;	/* Board flags (bits 48-63) */
 	/* TODO store board flags in a single u64 */
 
+	struct ssb_sprom_core_pwr_info core_pwr_info[4];
+
 	/* Antenna gain values for up to 4 antennas
 	 * on each band. Values in dBm/4 (Q5.2). Negative gain means the
 	 * loss in the connectors is bigger than the gain. */
 	struct {
-		struct {
-			s8 a0, a1, a2, a3;
-		} ghz24;	/* 2.4GHz band */
-		struct {
-			s8 a0, a1, a2, a3;
-		} ghz5;		/* 5GHz band */
+		s8 a0, a1, a2, a3;
 	} antenna_gain;
 
-	/* TODO - add any parameters needed from rev 2, 3, 4, 5 or 8 SPROMs */
+	struct {
+		struct {
+			u8 tssipos, extpa_gain, pdet_range, tr_iso, antswlut;
+		} ghz2;
+		struct {
+			u8 tssipos, extpa_gain, pdet_range, tr_iso, antswlut;
+		} ghz5;
+	} fem;
+
+	u16 mcs2gpo[8];
+	u16 mcs5gpo[8];
+	u16 mcs5glpo[8];
+	u16 mcs5ghpo[8];
+	u8 opo;
+
+	u8 rxgainerr2ga[3];
+	u8 rxgainerr5gla[3];
+	u8 rxgainerr5gma[3];
+	u8 rxgainerr5gha[3];
+	u8 rxgainerr5gua[3];
+
+	u8 noiselvl2ga[3];
+	u8 noiselvl5gla[3];
+	u8 noiselvl5gma[3];
+	u8 noiselvl5gha[3];
+	u8 noiselvl5gua[3];
+
+	u8 regrev;
+	u8 txchain;
+	u8 rxchain;
+	u8 antswitch;
+	u16 cddpo;
+	u16 stbcpo;
+	u16 bw40po;
+	u16 bwduppo;
+
+	u8 tempthresh;
+	u8 tempoffset;
+	u16 rawtempsense;
+	u8 measpower;
+	u8 tempsense_slope;
+	u8 tempcorrx;
+	u8 tempsense_option;
+	u8 freqoffset_corr;
+	u8 iqcal_swp_dis;
+	u8 hw_iqcal_en;
+	u8 elna2g;
+	u8 elna5g;
+	u8 phycal_tempdelta;
+	u8 temps_period;
+	u8 temps_hysteresis;
+	u8 measpower1;
+	u8 measpower2;
+	u8 pcieingress_war;
+
+	/* power per rate from sromrev 9 */
+	u16 cckbw202gpo;
+	u16 cckbw20ul2gpo;
+	u32 legofdmbw202gpo;
+	u32 legofdmbw20ul2gpo;
+	u32 legofdmbw205glpo;
+	u32 legofdmbw20ul5glpo;
+	u32 legofdmbw205gmpo;
+	u32 legofdmbw20ul5gmpo;
+	u32 legofdmbw205ghpo;
+	u32 legofdmbw20ul5ghpo;
+	u32 mcsbw202gpo;
+	u32 mcsbw20ul2gpo;
+	u32 mcsbw402gpo;
+	u32 mcsbw205glpo;
+	u32 mcsbw20ul5glpo;
+	u32 mcsbw405glpo;
+	u32 mcsbw205gmpo;
+	u32 mcsbw20ul5gmpo;
+	u32 mcsbw405gmpo;
+	u32 mcsbw205ghpo;
+	u32 mcsbw20ul5ghpo;
+	u32 mcsbw405ghpo;
+	u16 mcs32po;
+	u16 legofdm40duppo;
+	u8 sar2g;
+	u8 sar5g;
 };
 
 /* Information about the PCB the circuitry is soldered on. */
 struct ssb_boardinfo {
 	u16 vendor;
 	u16 type;
-	u16 rev;
+	u8  rev;
 };
 
 
@@ -229,10 +318,9 @@ struct ssb_driver {
 #define drv_to_ssb_drv(_drv) container_of(_drv, struct ssb_driver, drv)
 
 extern int __ssb_driver_register(struct ssb_driver *drv, struct module *owner);
-static inline int ssb_driver_register(struct ssb_driver *drv)
-{
-	return __ssb_driver_register(drv, THIS_MODULE);
-}
+#define ssb_driver_register(drv) \
+	__ssb_driver_register(drv, THIS_MODULE)
+
 extern void ssb_driver_unregister(struct ssb_driver *drv);
 
 
@@ -308,7 +396,7 @@ struct ssb_bus {
 
 	/* ID information about the Chip. */
 	u16 chip_id;
-	u16 chip_rev;
+	u8 chip_rev;
 	u16 sprom_offset;
 	u16 sprom_size;		/* number of words in sprom */
 	u8 chip_package;
@@ -404,7 +492,9 @@ extern bool ssb_is_sprom_available(struc
 
 /* Set a fallback SPROM.
  * See kdoc at the function definition for complete documentation. */
-extern int ssb_arch_set_fallback_sprom(const struct ssb_sprom *sprom);
+extern int ssb_arch_register_fallback_sprom(
+		int (*sprom_callback)(struct ssb_bus *bus,
+		struct ssb_sprom *out));
 
 /* Suspend a SSB bus.
  * Call this from the parent bus suspend routine. */
@@ -518,6 +608,7 @@ extern int ssb_bus_may_powerdown(struct
  * Otherwise static always-on powercontrol will be used. */
 extern int ssb_bus_powerup(struct ssb_bus *bus, bool dynamic_pctl);
 
+extern void ssb_commit_settings(struct ssb_bus *bus);
 
 /* Various helper functions */
 extern u32 ssb_admatch_base(u32 adm);
--- a/include/linux/ssb/ssb_driver_chipcommon.h
+++ b/include/linux/ssb/ssb_driver_chipcommon.h
@@ -8,7 +8,7 @@
  * gpio interface, extbus, and support for serial and parallel flashes.
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GPL version 2. See COPYING for details.
  */
@@ -123,6 +123,8 @@
 #define SSB_CHIPCO_FLASHDATA		0x0048
 #define SSB_CHIPCO_BCAST_ADDR		0x0050
 #define SSB_CHIPCO_BCAST_DATA		0x0054
+#define SSB_CHIPCO_GPIOPULLUP		0x0058		/* Rev >= 20 only */
+#define SSB_CHIPCO_GPIOPULLDOWN		0x005C		/* Rev >= 20 only */
 #define SSB_CHIPCO_GPIOIN		0x0060
 #define SSB_CHIPCO_GPIOOUT		0x0064
 #define SSB_CHIPCO_GPIOOUTEN		0x0068
@@ -131,6 +133,9 @@
 #define SSB_CHIPCO_GPIOIRQ		0x0074
 #define SSB_CHIPCO_WATCHDOG		0x0080
 #define SSB_CHIPCO_GPIOTIMER		0x0088		/* LED powersave (corerev >= 16) */
+#define  SSB_CHIPCO_GPIOTIMER_OFFTIME	0x0000FFFF
+#define  SSB_CHIPCO_GPIOTIMER_OFFTIME_SHIFT	0
+#define  SSB_CHIPCO_GPIOTIMER_ONTIME	0xFFFF0000
 #define  SSB_CHIPCO_GPIOTIMER_ONTIME_SHIFT	16
 #define SSB_CHIPCO_GPIOTOUTM		0x008C		/* LED powersave (corerev >= 16) */
 #define SSB_CHIPCO_CLOCK_N		0x0090
@@ -189,8 +194,10 @@
 #define  SSB_CHIPCO_CLKCTLST_HAVEALPREQ	0x00000008 /* ALP available request */
 #define  SSB_CHIPCO_CLKCTLST_HAVEHTREQ	0x00000010 /* HT available request */
 #define  SSB_CHIPCO_CLKCTLST_HWCROFF	0x00000020 /* Force HW clock request off */
-#define  SSB_CHIPCO_CLKCTLST_HAVEHT	0x00010000 /* HT available */
-#define  SSB_CHIPCO_CLKCTLST_HAVEALP	0x00020000 /* APL available */
+#define  SSB_CHIPCO_CLKCTLST_HAVEALP	0x00010000 /* ALP available */
+#define  SSB_CHIPCO_CLKCTLST_HAVEHT	0x00020000 /* HT available */
+#define  SSB_CHIPCO_CLKCTLST_4328A0_HAVEHT	0x00010000 /* 4328a0 has reversed bits */
+#define  SSB_CHIPCO_CLKCTLST_4328A0_HAVEALP	0x00020000 /* 4328a0 has reversed bits */
 #define SSB_CHIPCO_HW_WORKAROUND	0x01E4 /* Hardware workaround (rev >= 20) */
 #define SSB_CHIPCO_UART0_DATA		0x0300
 #define SSB_CHIPCO_UART0_IMR		0x0304
--- a/drivers/ssb/b43_pci_bridge.c
+++ b/drivers/ssb/b43_pci_bridge.c
@@ -5,12 +5,13 @@
  * because of its small size we include it in the SSB core
  * instead of creating a standalone module.
  *
- * Copyright 2007  Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007  Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
 #include <linux/pci.h>
+#include <linux/module.h>
 #include <linux/ssb/ssb.h>
 
 #include "ssb_private.h"
--- a/drivers/ssb/driver_extif.c
+++ b/drivers/ssb/driver_extif.c
@@ -3,7 +3,7 @@
  * Broadcom EXTIF core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  * Copyright 2006, 2007, Felix Fietkau <nbd@openwrt.org>
  * Copyright 2007, Aurelien Jarno <aurelien@aurel32.net>
  *
--- a/drivers/ssb/driver_mipscore.c
+++ b/drivers/ssb/driver_mipscore.c
@@ -3,7 +3,7 @@
  * Broadcom MIPS core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -208,6 +208,9 @@ u32 ssb_cpu_clock(struct ssb_mipscore *m
 	struct ssb_bus *bus = mcore->dev->bus;
 	u32 pll_type, n, m, rate = 0;
 
+	if (bus->chipco.capabilities & SSB_CHIPCO_CAP_PMU)
+		return ssb_pmu_get_cpu_clock(&bus->chipco);
+
 	if (bus->extif.dev) {
 		ssb_extif_get_clockcontrol(&bus->extif, &pll_type, &n, &m);
 	} else if (bus->chipco.dev) {
--- a/drivers/ssb/embedded.c
+++ b/drivers/ssb/embedded.c
@@ -3,7 +3,7 @@
  * Embedded systems support code
  *
  * Copyright 2005-2008, Broadcom Corporation
- * Copyright 2006-2008, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006-2008, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
--- a/drivers/ssb/pcmcia.c
+++ b/drivers/ssb/pcmcia.c
@@ -3,7 +3,7 @@
  * PCMCIA-Hostbus related functions
  *
  * Copyright 2006 Johannes Berg <johannes@sipsolutions.net>
- * Copyright 2007-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007-2008 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -676,14 +676,10 @@ static int ssb_pcmcia_do_get_invariants(
 	case SSB_PCMCIA_CIS_ANTGAIN:
 		GOTO_ERROR_ON(tuple->TupleDataLen != 2,
 			"antg tpl size");
-		sprom->antenna_gain.ghz24.a0 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz24.a1 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz24.a2 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz24.a3 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a0 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a1 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a2 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a3 = tuple->TupleData[1];
+		sprom->antenna_gain.a0 = tuple->TupleData[1];
+		sprom->antenna_gain.a1 = tuple->TupleData[1];
+		sprom->antenna_gain.a2 = tuple->TupleData[1];
+		sprom->antenna_gain.a3 = tuple->TupleData[1];
 		break;
 	case SSB_PCMCIA_CIS_BFLAGS:
 		GOTO_ERROR_ON((tuple->TupleDataLen != 3) &&
--- a/drivers/ssb/sdio.c
+++ b/drivers/ssb/sdio.c
@@ -6,7 +6,7 @@
  *
  * Based on drivers/ssb/pcmcia.c
  * Copyright 2006 Johannes Berg <johannes@sipsolutions.net>
- * Copyright 2007-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007-2008 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  *
@@ -551,14 +551,10 @@ int ssb_sdio_get_invariants(struct ssb_b
 			case SSB_SDIO_CIS_ANTGAIN:
 				GOTO_ERROR_ON(tuple->size != 2,
 					      "antg tpl size");
-				sprom->antenna_gain.ghz24.a0 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a1 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a2 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a3 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a0 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a1 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a2 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a3 = tuple->data[1];
+				sprom->antenna_gain.a0 = tuple->data[1];
+				sprom->antenna_gain.a1 = tuple->data[1];
+				sprom->antenna_gain.a2 = tuple->data[1];
+				sprom->antenna_gain.a3 = tuple->data[1];
 				break;
 			case SSB_SDIO_CIS_BFLAGS:
 				GOTO_ERROR_ON((tuple->size != 3) &&
--- a/include/linux/ssb/ssb_driver_gige.h
+++ b/include/linux/ssb/ssb_driver_gige.h
@@ -2,6 +2,7 @@
 #define LINUX_SSB_DRIVER_GIGE_H_
 
 #include <linux/ssb/ssb.h>
+#include <linux/bug.h>
 #include <linux/pci.h>
 #include <linux/spinlock.h>
 
