#!/bin/sh
#
# Copyright (C) 2012 OpenWrt.org
#

uboot_environment_configuration() {
	local dev=$1
	local offset=$2
	local envsize=$3
	local secsize=$4
	local numsec=$5
	echo "$dev $offset $envsize $secsize $numsec" > /etc/fw_env.config
}

[ -e /etc/config/fw_env.config ] && exit 0

. /lib/lantiq.sh

board=$(lantiq_board_name)

case "$board" in
GIGASX76X)
	uboot_environment_configuration "/dev/mtd1" "0x0" "0x10000" "0x10000" "1"
	;;

*)
	# custom foo goes here
	true
	;;
esac

exit 0
