From 4f4bb58cba3a6c44e9f9f113609287d9d50be9c4 Mon Sep 17 00:00:00 2001
From: Joseph Kortje <jpktech@rogers.com>
Date: Wed, 28 Oct 2009 21:11:28 -0400
Subject: [PATCH] [ARM] Gumstix Verdex Pro arch support

add an option for Verdex Pro when ARCH_GUMSTIX is selected, and
factor earlier Gumstix support into a seperate option

Signed-off-by: Bobby Powers <bobbypowers@gmail.com>
---
 arch/arm/mach-pxa/Kconfig                   |   29 +-
 arch/arm/mach-pxa/Makefile                  |    3 +-
 arch/arm/mach-pxa/gumstix-verdex.c          |  749 +++++++++++++++++++++++++++
 arch/arm/mach-pxa/include/mach/mfp-pxa27x.h |    1 +
 4 files changed, 772 insertions(+), 10 deletions(-)
 create mode 100644 arch/arm/mach-pxa/gumstix-verdex.c

--- a/arch/arm/mach-pxa/Kconfig
+++ b/arch/arm/mach-pxa/Kconfig
@@ -116,23 +116,34 @@ config MACH_CAPC7117
 	select PXA3xx
 
 config ARCH_GUMSTIX
-	bool "Gumstix XScale 255 boards"
-	select PXA25x
+	bool "Gumstix boards"
 	help
-	  Say Y here if you intend to run this kernel on
-	  Basix, Connex, ws-200ax, ws-400ax systems
+        Say Y here if you intend to run this kernel on a
+	  gumstix computer.
 
-choice
-	prompt "Gumstix Carrier/Expansion Board"
 	depends on ARCH_GUMSTIX
 
-config GUMSTIX_AM200EPD
+config MACH_GUMSTIX_F
+	bool "Gumstix Basix/Connex ..."
+	depends on ARCH_GUMSTIX
+	select PXA25x
+
+ choice
+	prompt "Gumstix Carrier/Expansion Board"
+	depends on MACH_GUMSTIX_F
+
+ config GUMSTIX_AM200EPD
 	bool "Enable AM200EPD board support"
 
-config GUMSTIX_AM300EPD
+ config GUMSTIX_AM300EPD
 	bool "Enable AM300EPD board support"
 
-endchoice
+ endchoice
+
+config MACH_GUMSTIX_VERDEX
+	bool "Gumstix VERDEX ..."
+	depends on ARCH_GUMSTIX
+	select PXA27x
 
 config MACH_INTELMOTE2
 	bool "Intel Mote 2 Platform"
--- a/arch/arm/mach-pxa/Makefile
+++ b/arch/arm/mach-pxa/Makefile
@@ -49,7 +49,8 @@ endif
 obj-$(CONFIG_MACH_EM_X270)	+= em-x270.o
 obj-$(CONFIG_MACH_CM_X300)      += cm-x300.o
 obj-$(CONFIG_MACH_CAPC7117)     += capc7117.o mxm8x10.o
-obj-$(CONFIG_ARCH_GUMSTIX)	+= gumstix.o
+obj-$(CONFIG_MACH_GUMSTIX_F)	+= gumstix.o
+obj-$(CONFIG_MACH_GUMSTIX_VERDEX)	+= gumstix-verdex.o
 obj-$(CONFIG_GUMSTIX_AM200EPD)	+= am200epd.o
 obj-$(CONFIG_GUMSTIX_AM300EPD)	+= am300epd.o
 obj-$(CONFIG_MACH_INTELMOTE2)	+= stargate2.o
--- /dev/null
+++ b/arch/arm/mach-pxa/gumstix-verdex.c
@@ -0,0 +1,747 @@
+/*
+ *  linux/arch/arm/mach-pxa/gumstix-verdex.c
+ *
+ *  Support for the Gumstix verdex motherboard.
+ *
+ *  Original Author:  Craig Hughes
+ *  Created:          Feb 14, 2008
+ *  Copyright:        Craig Hughes
+ *
+ *  This program is free software; you can redistribute it and/or modify
+ *  it under the terms of the GNU General Public License version 2 as
+ *  published by the Free Software Foundation.
+ *
+ *  Implemented based on lubbock.c by Nicolas Pitre and code from Craig
+ *  Hughes
+ */
+
+#include <linux/module.h>
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/interrupt.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/i2c/tsc2007.h>
+
+#include <asm/setup.h>
+#include <asm/memory.h>
+#include <asm/mach-types.h>
+#include <asm/irq.h>
+#include <asm/sizes.h>
+#include <asm/io.h>
+
+#include <asm/mach/arch.h>
+#include <asm/mach/map.h>
+#include <asm/mach/irq.h>
+#include <asm/mach/flash.h>
+
+#include <mach/mmc.h>
+#include <mach/udc.h>
+#include <mach/pxafb.h>
+#include <mach/ohci.h>
+#include <plat/i2c.h>
+#include <mach/pxa27x.h>
+#include <mach/pxa27x-udc.h>
+#include <mach/gpio.h>
+
+#include <mach/gumstix.h>
+
+#include "generic.h"
+
+#include <linux/delay.h>
+
+#if defined(CONFIG_SMSC911X) || defined(CONFIG_SMSC911X_MODULE)
+
+#include <linux/smsc911x.h>
+
+static struct resource verdex_smsc911x_resources[] = {
+	[0] = {
+		.name	= "smsc911x-memory",
+		.start  = PXA_CS1_PHYS,
+		.end    = PXA_CS1_PHYS + 0x000fffff,
+		.flags  = IORESOURCE_MEM,
+	},
+	[1] = {
+		.start  = IRQ_GPIO(GPIO_GUMSTIX_ETH0),
+		.end    = IRQ_GPIO(GPIO_GUMSTIX_ETH0),
+		.flags	= IORESOURCE_IRQ | IORESOURCE_IRQ_LOWEDGE,
+	},
+};
+
+static struct smsc911x_platform_config verdex_smsc911x_config = {
+	.irq_polarity	= SMSC911X_IRQ_POLARITY_ACTIVE_LOW,
+	.irq_type	= SMSC911X_IRQ_TYPE_PUSH_PULL,
+	.flags		= SMSC911X_USE_16BIT | SMSC911X_SAVE_MAC_ADDRESS,
+	.phy_interface	= PHY_INTERFACE_MODE_MII,
+};
+
+static struct platform_device verdex_smsc911x_device = {
+	.name		= "smsc911x",
+	.id		= -1,
+	.num_resources	= ARRAY_SIZE(verdex_smsc911x_resources),
+	.resource	= verdex_smsc911x_resources,
+	.dev		= {
+		.platform_data = &verdex_smsc911x_config,
+	},
+};
+
+static void __init verdex_init_smsc911x(void)
+{
+
+        printk(KERN_INFO "Initializing Gumstix verdex smsc911x\n");
+
+	if (gpio_request(GPIO_GUMSTIX_ETH0_RST, "SMSC911x_ETH0_RST") != 0) {
+		printk(KERN_ERR "could not obtain gpio for SMSC911x_ETH0_RST\n");
+		goto err_request_gpio_eth0_rst;
+	}
+
+	if (gpio_request(GPIO_GUMSTIX_ETH0, "SMSC911x_ETH0_IRQ") != 0) {
+		printk(KERN_ERR "could not obtain gpio for SMSC911x_ETH0_IRQ\n");
+		goto err_request_gpio_eth0_irq;
+	}
+
+	if (gpio_direction_output(GPIO_GUMSTIX_ETH0_RST, 0) != 0) {
+		printk(KERN_ERR "could not set SMSC911x_ETH0_RST pin to output\n");
+		goto err_dir;
+	}
+
+	gpio_set_value(GPIO_GUMSTIX_ETH0_RST, 0);
+
+	msleep(500); // Hold RESET for at least 200ms
+
+	gpio_set_value(GPIO_GUMSTIX_ETH0_RST, 1);
+
+	msleep(50);
+
+	if (gpio_direction_input(GPIO_GUMSTIX_ETH0) != 0) {
+		printk(KERN_ERR "could not set SMSC911x_ETH0_IRQ pin to input\n");
+		goto err_dir;
+	}
+
+	gpio_export(GPIO_GUMSTIX_ETH0, 0);
+	platform_device_register(&verdex_smsc911x_device);
+	return;
+
+err_dir:
+	gpio_free(GPIO_GUMSTIX_ETH0_RST);
+
+err_request_gpio_eth0_irq:
+	gpio_free(GPIO_GUMSTIX_ETH0);
+
+err_request_gpio_eth0_rst:
+	return;
+}
+
+#else
+static void __init verdex_init_smsc911x(void) { return; }
+#endif
+
+static unsigned long verdex_pin_config[] = {
+    /* MMC */
+    GPIO32_MMC_CLK,
+    GPIO112_MMC_CMD,
+    GPIO92_MMC_DAT_0,
+    GPIO109_MMC_DAT_1,
+    GPIO110_MMC_DAT_2,
+    GPIO111_MMC_DAT_3,
+
+    /* BTUART */
+    GPIO42_BTUART_RXD,
+    GPIO43_BTUART_TXD,
+    GPIO44_BTUART_CTS,
+    GPIO45_BTUART_RTS,
+
+    /* STUART */
+    GPIO46_STUART_RXD,
+    GPIO47_STUART_TXD,
+
+    /* FFUART */
+    GPIO34_FFUART_RXD,
+    GPIO39_FFUART_TXD,
+
+    /* SSP 2 */
+    GPIO19_SSP2_SCLK,
+    GPIO14_SSP2_SFRM,
+    GPIO13_SSP2_TXD,
+    GPIO11_SSP2_RXD,
+
+    /* SDRAM and local bus */
+    GPIO49_nPWE,
+    GPIO15_nCS_1,
+
+    /* I2C */
+    GPIO117_I2C_SCL,
+    GPIO118_I2C_SDA,
+
+    /* PWM 0 */
+    GPIO16_PWM0_OUT,
+
+    /* BRIGHTNESS */
+    GPIO17_PWM1_OUT,
+
+    /* LCD */
+    GPIO58_LCD_LDD_0,
+    GPIO59_LCD_LDD_1,
+    GPIO60_LCD_LDD_2,
+    GPIO61_LCD_LDD_3,
+    GPIO62_LCD_LDD_4,
+    GPIO63_LCD_LDD_5,
+    GPIO64_LCD_LDD_6,
+    GPIO65_LCD_LDD_7,
+    GPIO66_LCD_LDD_8,
+    GPIO67_LCD_LDD_9,
+    GPIO68_LCD_LDD_10,
+    GPIO69_LCD_LDD_11,
+    GPIO70_LCD_LDD_12,
+    GPIO71_LCD_LDD_13,
+    GPIO72_LCD_LDD_14,
+    GPIO73_LCD_LDD_15,
+    GPIO74_LCD_FCLK,
+    GPIO75_LCD_LCLK,
+    GPIO76_LCD_PCLK,
+#ifdef CONFIG_FB_PXA_SHARP_LQ043_PSP
+    /* DISP must be always high while screen is on */
+    /* Done below in verdex_init */
+#else
+    GPIO77_LCD_BIAS,
+#endif
+
+};
+
+#if defined(CONFIG_PCMCIA_PXA2XX) || defined(CONFIG_PCMCIA_PXA2XX_MODULE)
+
+static unsigned long gpio_ntschg_0[] = {
+	GPIO104_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_nCD_0_MD);
+};
+
+static unsigned long gpio_ntschg_1[] = {
+	GPIO18_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_nSTSCHG_1_MD);
+	GPIO36_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_nCD_1_MD);
+	GPIO27_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_PRDY_nBSY_1_MD);
+};
+
+static unsigned long gpio_prdy_nbsy_old[] = {
+	GPIO111_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_nSTSCHG_0_MD);
+	GPIO109_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_PRDY_nBSY_0_OLD_MD);
+};
+
+static unsigned long gpio_prdy_nbsy[] = {
+	GPIO96_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_PRDY_nBSY_0_MD);
+};
+
+static unsigned long gpio_nhw_init[] = {
+	GPIO48_nPOE,			// pxa_gpio_mode(GPIO_GUMSTIX_nPOE_MD);
+	GPIO102_nPCE_1,			// pxa_gpio_mode(GPIO_GUMSTIX_nPCE_1_MD);
+	GPIO105_nPCE_2,			// pxa_gpio_mode(GPIO_GUMSTIX_nPCE_2_MD);
+	GPIO104_GPIO,			// pxa_gpio_mode(GPIO_GUMSTIX_nCD_0_MD);
+
+	GPIO49_nPWE,			// pxa_gpio_mode(GPIO_GUMSTIX_nPWE_MD);
+	GPIO50_nPIOR,			// pxa_gpio_mode(GPIO_GUMSTIX_nPIOR_MD);
+	GPIO51_nPIOW,			// pxa_gpio_mode(GPIO_GUMSTIX_nPIOW_MD);
+	GPIO79_PSKTSEL,			// pxa_gpio_mode(GPIO_GUMSTIX_pSKTSEL_MD);
+	GPIO55_nPREG,			// pxa_gpio_mode(GPIO_GUMSTIX_nPREG_MD);
+	GPIO56_nPWAIT,			// pxa_gpio_mode(GPIO_GUMSTIX_nPWAIT_MD);
+	GPIO57_nIOIS16,			// pxa_gpio_mode(GPIO_GUMSTIX_nIOIS16_MD);
+};
+
+static	int net_cf_vx_mode = 0;
+static	int pcmcia_cf_nr = 2; 
+
+inline void __init gumstix_pcmcia_cpld_clk(void)
+{
+	GPCR(GPIO_GUMSTIX_nPOE) = GPIO_bit(GPIO_GUMSTIX_nPOE);
+	GPSR(GPIO_GUMSTIX_nPOE) = GPIO_bit(GPIO_GUMSTIX_nPOE);
+}
+
+inline unsigned char __init gumstix_pcmcia_cpld_read_bits(int bits)
+{
+	unsigned char result = 0;
+	unsigned int shift = 0;
+	while(bits--)
+	{
+		result |= !!(GPLR(GPIO_GUMSTIX_nCD_0) & GPIO_bit(GPIO_GUMSTIX_nCD_0)) << shift;
+		shift ++;
+		gumstix_pcmcia_cpld_clk();
+	}
+	printk("CPLD responded with: %02x\n",result);
+	return result;
+}
+
+/* We use the CPLD on the CF-CF card to read a value from a shift register.  If we can read that
+ * magic sequence, then we have 2 CF cards; otherwise we assume just one
+ * The CPLD will send the value of the shift register on GPIO11 (the CD line for slot 0)
+ * when RESET is held in reset.  We use GPIO48 (nPOE) as a clock signal,
+ * GPIO52/53 (card enable for both cards) to control read/write to the shift register
+ */
+static void __init gumstix_count_cards(void)
+{
+
+	if ((gpio_request(GPIO_GUMSTIX_nPOE, "GPIO_GUMSTIX_nPOE") == 0) &&
+	    (gpio_direction_output(GPIO_GUMSTIX_nPOE, 1) == 0))
+		gpio_export(GPIO_GUMSTIX_nPOE, 0);
+	else
+		printk(KERN_ERR "could not obtain gpio for GPIO_GUMSTIX_nPOE\n");
+	
+	if ((gpio_request(GPIO_GUMSTIX_nPCE_1, "GPIO_GUMSTIX_nPCE_1") == 0) &&
+	    (gpio_direction_output(GPIO_GUMSTIX_nPCE_1, 1) == 0))
+		gpio_export(GPIO_GUMSTIX_nPCE_1, 0);
+	else
+		printk(KERN_ERR "could not obtain gpio for GPIO_GUMSTIX_nPCE_1\n");
+
+	if ((gpio_request(GPIO_GUMSTIX_nPCE_2, "GPIO_GUMSTIX_nPCE_2") == 0) &&
+	    (gpio_direction_output(GPIO_GUMSTIX_nPCE_2, 1) == 0))
+		gpio_export(GPIO_GUMSTIX_nPCE_2, 0);
+	else
+		printk(KERN_ERR "could not obtain gpio for GPIO_GUMSTIX_nPCE_2\n");
+
+	if ((gpio_request(GPIO_GUMSTIX_nCD_0, "GPIO_GUMSTIX_nCD_0") == 0) &&
+	    (gpio_direction_input(GPIO_GUMSTIX_nCD_0) == 0))
+		gpio_export(GPIO_GUMSTIX_nCD_0, 0);
+	else
+		printk(KERN_ERR "could not obtain gpio for GPIO_GUMSTIX_nCD_0\n");
+
+	if (net_cf_vx_mode) {
+		if ((gpio_request(GPIO_GUMSTIX_CF_OLD_RESET, "GPIO_GUMSTIX_CF_OLD_RESET") == 0) &&
+	    	    (gpio_direction_output(GPIO_GUMSTIX_CF_OLD_RESET, 1) == 0)) {
+			gpio_export(GPIO_GUMSTIX_CF_OLD_RESET, 0);
+		} else {
+			printk(KERN_ERR "could not obtain gpio for GPIO_GUMSTIX_CF_OLD_RESET\n");
+		}
+	} else {
+		if ((gpio_request(GPIO_GUMSTIX_CF_RESET, "GPIO_GUMSTIX_CF_RESET") == 0) &&
+	    	    (gpio_direction_output(GPIO_GUMSTIX_CF_RESET, 1) == 0)) {
+			gpio_export(GPIO_GUMSTIX_CF_RESET, 0);
+		} else {
+			printk(KERN_ERR "could not obtain gpio for GPIO_GUMSTIX_CF_RESET\n");
+		}
+	}
+
+	// Setup the shift register
+	GPSR(GPIO_GUMSTIX_nPCE_1) = GPIO_bit(GPIO_GUMSTIX_nPCE_1);
+	GPCR(GPIO_GUMSTIX_nPCE_2) = GPIO_bit(GPIO_GUMSTIX_nPCE_2);
+
+	// Tick the clock to program the shift register
+	gumstix_pcmcia_cpld_clk();
+
+	// Now set shift register into read mode
+	GPCR(GPIO_GUMSTIX_nPCE_1) = GPIO_bit(GPIO_GUMSTIX_nPCE_1);
+	GPSR(GPIO_GUMSTIX_nPCE_2) = GPIO_bit(GPIO_GUMSTIX_nPCE_2);
+
+	// We can read the bits now -- 0xC2 means "Dual compact flash"
+	if(gumstix_pcmcia_cpld_read_bits(8) != 0xC2)
+	{
+		// We do not have 2 CF slots
+		pcmcia_cf_nr = 1;
+	}
+
+	udelay(50);
+
+	if (net_cf_vx_mode) {
+		gpio_set_value(GPIO_GUMSTIX_CF_OLD_RESET, 0);
+		gpio_free(GPIO_GUMSTIX_CF_OLD_RESET);
+	} else {
+		gpio_set_value(GPIO_GUMSTIX_CF_RESET, 0);
+		gpio_free(GPIO_GUMSTIX_CF_RESET);
+	}
+
+	printk(KERN_INFO "found %d CF slots\n", pcmcia_cf_nr);
+
+	gpio_free(GPIO_GUMSTIX_nPCE_2);
+	gpio_free(GPIO_GUMSTIX_nPCE_1);
+	gpio_free(GPIO_GUMSTIX_nPOE);
+	return;
+}
+
+#define	SMC_IO_EXTENT	16
+#define	BANK_SELECT	14
+
+static void __init verdex_pcmcia_pin_config(void)
+{
+	struct resource *res;
+	void *network_controller_memory;
+	struct platform_device *pdev = &verdex_smsc911x_device;
+
+        printk(KERN_INFO "Initializing Gumstix verdex pcmcia\n");
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (res == NULL) {
+		printk(KERN_ERR "no memory resource defined\n");
+		goto err_done;
+	}
+
+	res = request_mem_region(res->start, SMC_IO_EXTENT, "smc91x probe");
+	if (res == NULL) {
+		printk(KERN_ERR "failed to request memory resource\n");
+		goto err_done;
+	}
+
+	// We check for the possibility of SMSC91c111 (reg base offset 0x300 from CS1 base)
+	network_controller_memory = ioremap(res->start + 0x300, SMC_IO_EXTENT);
+	if (network_controller_memory == NULL) {
+		printk(KERN_ERR "failed to ioremap() registers\n");
+		goto err_free_mem;
+	}
+
+	// Look for the special 91c111 value in the bank select register
+	if((0xff00 & readw(network_controller_memory+BANK_SELECT)) == 0x3300) {
+		printk(KERN_INFO "Detected netCF-vx board: pcmcia using older GPIO configuration\n");
+		net_cf_vx_mode = 1;
+	} else {
+		printk(KERN_INFO "Not netCF-vx board: pcmcia using newer GPIO configuration\n");
+		net_cf_vx_mode = 0;
+	}
+
+	iounmap(network_controller_memory);
+err_free_mem:
+	release_mem_region(res->start, SMC_IO_EXTENT);
+err_done:
+
+	gumstix_count_cards();	// this can update pcmcia_cf_nr
+
+	// If pcmcia_cf_nr is 1 then we do not have 2 CF slots
+	// Note: logic sequence was altered from previous kernel revs
+	// so that this works as intended now.
+	if (pcmcia_cf_nr != 0)
+	{
+		pxa2xx_mfp_config(ARRAY_AND_SIZE(gpio_ntschg_0));
+
+		if(net_cf_vx_mode)
+			pxa2xx_mfp_config(gpio_prdy_nbsy_old, 1);
+		else
+			pxa2xx_mfp_config(gpio_prdy_nbsy, 1);
+
+	} else {
+		// Note: this reconfigures pin GPIO18 to be GPIO-IN so make
+		// sure that this only gets done for the old dual slot board
+		// since that pin is an active AF1 out-mode signal (RDY) on
+		// newer boards and changing the pin mode on the newer boards
+		// would result in memory corruption for the NIC (and hang during
+		// PHY test). 
+		pxa2xx_mfp_config(ARRAY_AND_SIZE(gpio_ntschg_1));
+	}
+
+	pxa2xx_mfp_config(ARRAY_AND_SIZE(gpio_nhw_init));
+	return;
+}
+
+int __init gumstix_get_cf_cards(void)
+{
+	return pcmcia_cf_nr;
+}
+EXPORT_SYMBOL(gumstix_get_cf_cards);
+
+#ifdef CONFIG_MACH_GUMSTIX_VERDEX
+int __init gumstix_check_if_netCF_vx(void)
+{
+	return net_cf_vx_mode;
+}
+EXPORT_SYMBOL(gumstix_check_if_netCF_vx);
+#endif
+
+#endif
+
+#if defined(CONFIG_FB_PXA_SHARP_LQ043_PSP) || defined(CONFIG_FB_PXA_SAMSUNG_LTE430WQ_F0C)
+static void gumstix_lcd_backlight(int on_or_off)
+{
+	int err;
+	err = gpio_request(17, "LCD BACKLIGHT");
+	if (err) {
+		//pr_warning("Gumstix Verdex: Failed to request LCD Backlight gpio\n");
+		return;
+	}
+
+	if(on_or_off) {
+		gpio_direction_input(17);
+	} else {
+		GPCR(17) = GPIO_bit(17);
+		gpio_direction_output(17, 0);
+		GPCR(17) = GPIO_bit(17);
+	}
+
+	return;	
+}
+#endif
+
+#ifdef CONFIG_FB_PXA_ALPS_CDOLLAR
+static struct pxafb_mode_info gumstix_fb_mode = {
+	.pixclock	= 300000,
+	.xres		= 240,
+	.yres		= 320,
+	.bpp		= 16,
+	.hsync_len	= 2,
+	.left_margin	= 1,
+	.right_margin	= 1,
+	.vsync_len	= 3,
+	.upper_margin	= 0,
+	.lower_margin	= 0,
+	.sync		= FB_SYNC_HOR_HIGH_ACT | FB_SYNC_VERT_HIGH_ACT,
+};
+
+static struct pxafb_mach_info gumstix_fb_info = {
+	.modes		= &gumstix_fb_mode,
+	.num_modes	= 1,
+	.lccr0		= LCCR0_Pas | LCCR0_Sngl | LCCR0_Color,
+	.lccr3		= LCCR3_PixFlEdg,
+};
+#elif defined(CONFIG_FB_PXA_SHARP_LQ043_PSP)
+static struct pxafb_mode_info gumstix_fb_mode = {
+	.pixclock	= 110000,
+	.xres		= 480,
+	.yres		= 272,
+	.bpp		= 16,
+	.hsync_len	= 41,
+	.left_margin	= 2,
+	.right_margin	= 2,
+	.vsync_len	= 10,
+	.upper_margin	= 2,
+	.lower_margin	= 2,
+	.sync		= 0, // Hsync and Vsync both active low
+};
+
+static struct pxafb_mach_info gumstix_fb_info = {
+	.modes			= &gumstix_fb_mode,
+	.num_modes		= 1,
+	.lccr0			= LCCR0_Act | LCCR0_Sngl | LCCR0_Color,
+	.lccr3			= LCCR3_OutEnH | LCCR3_PixFlEdg | (0 << 30),
+	.pxafb_backlight_power	= &gumstix_lcd_backlight,
+};
+#elif defined(CONFIG_FB_PXA_SAMSUNG_LTE430WQ_F0C)
+static struct pxafb_mode_info gumstix_fb_mode = {
+	.pixclock	= 108696, // 9.2MHz typical DOTCLK from datasheet
+	.xres		= 480,
+	.hsync_len	= 41, // HLW from datasheet: 41 typ
+	.left_margin	= 4, // HBP - HLW from datasheet: 45 - 41 = 4
+	.right_margin	= 8, // HFP from datasheet: 8 typ
+	.yres		= 272,
+	.vsync_len	= 10, // VLW from datasheet: 10 typ
+	.upper_margin	= 2, // VBP - VLW from datasheet: 12 - 10 = 2
+	.lower_margin	= 4, // VFP from datasheet: 4 typ
+	.bpp		= 16,
+	.sync		= 0, // Hsync and Vsync both active low
+};
+
+static struct pxafb_mach_info gumstix_fb_info = {
+	.modes			= &gumstix_fb_mode,
+	.num_modes		= 1,
+	.lccr0			= LCCR0_Act | LCCR0_Sngl | LCCR0_Color,
+	.lccr3			= LCCR3_OutEnH | LCCR3_PixFlEdg | (0 << 30),
+	.pxafb_backlight_power	= &gumstix_lcd_backlight,
+};
+#endif
+
+static struct platform_device verdex_audio_device = {
+    .name       = "pxa2xx-ac97",
+    .id         = -1,
+};
+
+static struct platform_device *devices[] __initdata = {
+    &verdex_audio_device,
+};
+
+/* PXA27x OHCI controller setup */
+#if defined(CONFIG_USB_OHCI_HCD) || defined(CONFIG_USB_OHCI_HCD_MODULE)
+static int ohci_verdex_init(struct device *dev)
+{
+	// Turn on port 2 in host mode
+	UP2OCR = UP2OCR_HXS | UP2OCR_HXOE | UP2OCR_DPPDE | UP2OCR_DMPDE;
+
+	/* See drivers/usb/host/ohci-pxa27x.c for further details but
+           ENABLE_PORT_ALL flag is equivalent to using this old sequence:
+ 	UHCHR = (UHCHR) &
+		~(UHCHR_SSEP1 | UHCHR_SSEP2 | UHCHR_SSEP3 | UHCHR_SSE);
+	*/
+	return 0;
+}
+
+static struct pxaohci_platform_data verdex_ohci_platform_data = {
+	.port_mode	= PMM_PERPORT_MODE,
+	.flags		= ENABLE_PORT_ALL,
+	.init		= ohci_verdex_init,
+};
+
+static void __init verdex_ohci_init(void)
+{
+	pxa_set_ohci_info(&verdex_ohci_platform_data);
+}
+#else
+static void __init verdex_ohci_init(void) {
+    printk(KERN_INFO "Gumstix verdex host usb ohci is disabled\n");
+}
+#endif
+
+
+#if defined(CONFIG_MMC_PXA) || defined(CONFIG_MMC_PXA_MODULE)
+static struct pxamci_platform_data verdex_mci_platform_data;
+
+static int verdex_mci_init(struct device *dev, irq_handler_t detect_int,
+                void *data)
+{
+    /* GPIO setup for MMC on the 120-pin connector is done in verdex_init.
+     * There is no card detect on a uSD connector so no interrupt to register.
+     * There is no WP detect GPIO line either.
+     */
+
+    return 0;
+}
+
+static struct pxamci_platform_data verdex_mci_platform_data = {
+    .ocr_mask   = MMC_VDD_32_33|MMC_VDD_33_34,
+    .init       = verdex_mci_init,
+};
+
+static void __init verdex_mmc_init(void)
+{
+    pxa_set_mci_info(&verdex_mci_platform_data);
+}
+#else
+static void __init verdex_mmc_init(void)
+{
+    printk(KERN_INFO "Gumstix verdex mmc disabled\n");
+}
+#endif
+
+#if defined(CONFIG_USB_GADGET_PXA2XX) || defined(CONFIG_USB_GADGET_PXA2XX_MODULE)
+static struct pxa2xx_udc_mach_info verdex_udc_info __initdata = {
+    .gpio_vbus      = GPIO35,
+    .gpio_pullup    = GPIO41,
+};
+
+static void __init verdex_udc_init(void)
+{
+    pxa_set_udc_info(&verdex_udc_info);
+}
+#else
+static void __init verdex_udc_init(void)
+{
+    printk(KERN_INFO "Gumstix verdex udc is disabled\n");
+}
+#endif
+
+#if defined(CONFIG_I2C) || defined(CONFIG_I2C_MODULE)
+
+#if defined(CONFIG_TOUCHSCREEN_TSC2003) || defined(CONFIG_TOUCHSCREEN_TSC2003_MODULE)
+
+#define VERDEX_GPIO_PENDOWN	16
+
+static int tsc2003_init_platform_hw(void)
+{
+	return 0;
+}
+
+static void tsc2003_exit_platform_hw(void)
+{
+	return;
+}
+
+static void tsc2003_clear_penirq(void)
+{
+	return;
+}
+
+static int tsc2003_get_pendown_state(void)
+{
+	return !gpio_get_value(VERDEX_GPIO_PENDOWN);
+}
+
+static struct tsc2007_platform_data tsc2003_config = {
+	.model = 2003,
+	.x_plate_ohms = 100,
+	.get_pendown_state	= tsc2003_get_pendown_state,
+	.clear_penirq		= tsc2003_clear_penirq,
+	.init_platform_hw	= tsc2003_init_platform_hw,
+	.exit_platform_hw	= tsc2003_exit_platform_hw,
+};
+#endif
+
+static struct i2c_board_info __initdata verdex_i2c_board_info[] = {
+#if defined(CONFIG_RTC_DRV_DS1307) || defined(CONFIG_RTC_DRV_DS1307_MODULE)
+
+	{
+		I2C_BOARD_INFO("rtc-ds1307", 0x68),
+	},
+#endif
+#if defined(CONFIG_TOUCHSCREEN_TSC2003) || defined(CONFIG_TOUCHSCREEN_TSC2003_MODULE)
+	{
+		I2C_BOARD_INFO("tsc2003", 0x48),
+		.platform_data	= &tsc2003_config,
+		.irq		= IRQ_GPIO(VERDEX_GPIO_PENDOWN),
+	},
+#endif
+};
+
+static struct i2c_pxa_platform_data verdex_i2c_pwr_info = {
+	.fast_mode = 1,
+};
+
+static struct i2c_pxa_platform_data verdex_i2c_info = {
+	.fast_mode = 1,
+};
+
+static void __init verdex_i2c_init(void)
+{
+        printk(KERN_INFO "Initializing Gumstix verdex i2c\n");
+
+#if defined(CONFIG_TOUCHSCREEN_TSC2003) || defined(CONFIG_TOUCHSCREEN_TSC2003_MODULE)
+	if ((gpio_request(VERDEX_GPIO_PENDOWN, "TSC2003_PENDOWN") == 0) &&
+	    (gpio_direction_input(VERDEX_GPIO_PENDOWN) == 0)) {
+		gpio_export(VERDEX_GPIO_PENDOWN, 0);
+	} else {
+		printk(KERN_ERR "could not obtain gpio for TSC2003_PENDOWN\n");
+		return;
+	}
+#endif
+
+	i2c_register_board_info(0, verdex_i2c_board_info,
+				ARRAY_SIZE(verdex_i2c_board_info));
+	pxa_set_i2c_info(&verdex_i2c_info);
+	pxa27x_set_i2c_power_info(&verdex_i2c_pwr_info);
+}
+#else
+static inline void verdex_i2c_init(void) {}
+#endif
+
+#if defined(CONFIG_PCMCIA_PXA2XX) || defined(CONFIG_PCMCIA_PXA2XX_MODULE)
+static void __init verdex_pcmcia_init(void)
+{
+	verdex_pcmcia_pin_config();
+}
+#else
+static void __init verdex_pcmcia_init(void) {
+	printk(KERN_INFO "Gumstix verdex pcmcia is disabled\n");
+}
+#endif
+
+
+static void __init verdex_init(void)
+{
+    pxa2xx_mfp_config(ARRAY_AND_SIZE(verdex_pin_config));
+
+#ifdef CONFIG_FB_PXA_SHARP_LQ043_PSP
+    /* DISP must be always high while screen is on */
+	gpio_direction_output(GPIO77, 0);
+	GPSR(GPIO77) = GPIO_bit(GPIO77);
+#endif 
+    verdex_udc_init();
+    verdex_mmc_init();
+    verdex_ohci_init();
+    verdex_i2c_init();
+    verdex_init_smsc911x();
+    verdex_pcmcia_init();
+ 
+#if defined(CONFIG_FB_PXA_ALPS_CDOLLAR) || defined(CONFIG_FB_PXA_SHARP_LQ043_PSP) || defined(CONFIG_FB_PXA_SAMSUNG_LTE430WQ_F0C)
+        printk(KERN_INFO "Initializing Gumstix verdex FB info\n");
+	set_pxa_fb_info(&gumstix_fb_info);
+#endif
+    printk(KERN_INFO "Initializing Gumstix platform_add_devices\n");
+    (void) platform_add_devices(devices, ARRAY_SIZE(devices));
+}
+
+MACHINE_START(GUMSTIX, "Gumstix verdex")
+    .boot_params    = 0xa0000100, /* match u-boot bi_boot_params */
+    .map_io         = pxa_map_io,
+    .init_irq       = pxa27x_init_irq,
+    .timer          = &pxa_timer,
+    .init_machine   = verdex_init,
+MACHINE_END
+
--- a/arch/arm/mach-pxa/include/mach/mfp-pxa27x.h
+++ b/arch/arm/mach-pxa/include/mach/mfp-pxa27x.h
@@ -109,6 +109,7 @@
 #define GPIO54_nPCE_2		MFP_CFG_OUT(GPIO54, AF2, DRIVE_HIGH)
 #define GPIO78_nPCE_2		MFP_CFG_OUT(GPIO78, AF1, DRIVE_HIGH)
 #define GPIO87_nPCE_2		MFP_CFG_IN(GPIO87, AF1)
+#define GPIO105_nPCE_2		MFP_CFG_OUT(GPIO105, AF1, DRIVE_HIGH)
 #define GPIO55_nPREG		MFP_CFG_OUT(GPIO55, AF2, DRIVE_HIGH)
 #define GPIO50_nPIOR		MFP_CFG_OUT(GPIO50, AF2, DRIVE_HIGH)
 #define GPIO51_nPIOW		MFP_CFG_OUT(GPIO51, AF2, DRIVE_HIGH)
