--- a/arch/mips/include/asm/mach-bcm63xx/bcm963xx_tag.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm963xx_tag.h
@@ -85,8 +85,10 @@ struct bcm_tag {
 	__u32 rootfs_crc;
 	/* 224-227: CRC32 of kernel partition */
 	__u32 kernel_crc;
-	/* 228-235: Unused at present */
-	char reserved1[8];
+	/* 228-231: Image sequence number */
+	char image_sequence[4];
+	/* 222-235: Openwrt: real rootfs length */
+	__u32 real_rootfs_length;
 	/* 236-239: CRC32 of header excluding last 20 bytes */
 	__u32 header_crc;
 	/* 240-255: Unused at present */
--- a/drivers/mtd/bcm63xxpart.c
+++ b/drivers/mtd/bcm63xxpart.c
@@ -77,7 +77,7 @@ static int bcm63xx_parse_cfe_partitions(
 	int ret;
 	size_t retlen;
 	unsigned int rootfsaddr, kerneladdr, spareaddr;
-	unsigned int rootfslen, kernellen, sparelen, totallen;
+	unsigned int rootfslen, kernellen, sparelen;
 	unsigned int cfelen, nvramlen;
 	int namelen = 0;
 	int i;
@@ -111,14 +111,15 @@ static int bcm63xx_parse_cfe_partitions(
 
 		sscanf(buf->kernel_address, "%u", &kerneladdr);
 		sscanf(buf->kernel_length, "%u", &kernellen);
-		sscanf(buf->total_length, "%u", &totallen);
+		rootfslen = buf->real_rootfs_length;
 
 		pr_info("CFE boot tag found with version %s and board type %s\n",
 			tagversion, boardid);
 
 		kerneladdr = kerneladdr - BCM63XX_EXTENDED_SIZE;
 		rootfsaddr = kerneladdr + kernellen;
-		spareaddr = roundup(totallen, master->erasesize) + cfelen;
+		rootfslen = roundup(rootfslen, master->erasesize);
+		spareaddr = rootfsaddr + rootfslen;
 		sparelen = master->size - spareaddr - nvramlen;
 		rootfslen = spareaddr - rootfsaddr;
 	} else {
