--- a/lib/ipfix_FOKUS_IEs.txt
+++ b/lib/ipfix_FOKUS_IEs.txt
@@ -86,3 +86,41 @@
 435, IPFIX_FT_ORmodulation, 1, IPFIX_CODING_UINT, "ORmodulation", "CREST factor"
 436, IPFIX_FT_ORprofileRecord, 65535, IPFIX_CODING_STRING, "ORprofileRecord", "profile record has variable length, First 8 bits in data describe the length (in bytes) of the field"
 
+500, IPFIX_FT_WPROBE_NOISE_N, 4, IPFIX_CODING_UINT, "global_noise_n", "wprobe global noice floor - Number of samples"
+501, IPFIX_FT_WPROBE_NOISE_S, 8, IPFIX_CODING_UINT, "global_noise_s", "wprobe global noice floor - Sum of samples"
+502, IPFIX_FT_WPROBE_NOISE_SS, 8, IPFIX_CODING_UINT, "global_noise_ss", "wprobe global noice floor - Sum of squared samples"
+503, IPFIX_FT_WPROBE_PHY_BUSY_N, 4, IPFIX_CODING_UINT, "global_phy_busy_n", "wprobe global airtime total - Number of samples"
+504, IPFIX_FT_WPROBE_PHY_BUSY_S, 8, IPFIX_CODING_UINT, "global_phy_busy_s", "wprobe global airtime total - Sum of samples"
+505, IPFIX_FT_WPROBE_PHY_BUSY_SS, 8, IPFIX_CODING_UINT, "global_phy_busy_ss", "wprobe global airtime total - Sum of squared samples"
+506, IPFIX_FT_WPROBE_PHY_RX_N, 4, IPFIX_CODING_UINT, "global_phy_rx_n", "wprobe global airtime total from rx-frame - Number of samples"
+507, IPFIX_FT_WPROBE_PHY_RX_S, 8, IPFIX_CODING_UINT, "global_phy_rx_s", "wprobe global airtime total from rx-frame - Sum of samples"
+508, IPFIX_FT_WPROBE_PHY_RX_SS, 8, IPFIX_CODING_UINT, "global_phy_rx_ss", "wprobe global airtime total from rx-frame - Sum of squared samples"
+509, IPFIX_FT_WPROBE_PHY_TX_N, 4, IPFIX_CODING_UINT, "global_phy_tx_n", "wprobe global airtime total from tx-frame - Number of samples"
+510, IPFIX_FT_WPROBE_PHY_TX_S, 8, IPFIX_CODING_UINT, "global_phy_tx_s", "wprobe global airtime total from tx-frame - Sum of samples"
+511, IPFIX_FT_WPROBE_PHY_TX_SS, 8, IPFIX_CODING_UINT, "global_phy_tx_ss", "wprobe global airtime total from tx-frame - Sum of squared samples"
+512, IPFIX_FT_WPROBE_RSSI_N, 4, IPFIX_CODING_UINT, "link_rssi_n", "wprobe link received signal strength indication - Number of samples"
+513, IPFIX_FT_WPROBE_RSSI_S, 8, IPFIX_CODING_UINT, "link_rssi_s", "wprobe link received signal strength indication - Sum of samples"
+514, IPFIX_FT_WPROBE_RSSI_SS, 8, IPFIX_CODING_UINT, "link_rssi_ss", "wprobe link received signal strength indication - Sum of squared samples"
+515, IPFIX_FT_WPROBE_SIGNAL_N, 4, IPFIX_CODING_UINT, "link_signal_n", "wprobe link signal strength in dB - Number of samples"
+516, IPFIX_FT_WPROBE_SIGNAL_S, 8, IPFIX_CODING_UINT, "link_signal_s", "wprobe link signal strength in dB - Sum of samples"
+517, IPFIX_FT_WPROBE_SIGNAL_SS, 8, IPFIX_CODING_UINT, "link_signal_ss", "wprobe link signal strength in dB - Sum of squared samples"
+518, IPFIX_FT_WPROBE_IEEE_RX_RATE_N, 4, IPFIX_CODING_UINT, "link_ieee_rx_rate_n", "wprobe link IEEE 802.11 RX data rate - Number of samples"
+519, IPFIX_FT_WPROBE_IEEE_RX_RATE_S, 8, IPFIX_CODING_UINT, "link_ieee_rx_rate_s", "wprobe link IEEE 802.11 RX data rate - Sum of samples"
+520, IPFIX_FT_WPROBE_IEEE_RX_RATE_SS, 8, IPFIX_CODING_UINT, "link_ieee_rx_rate_ss", "wprobe link IEEE 802.11 RX data rate - Sum of squared samples"
+521, IPFIX_FT_WPROBE_IEEE_TX_RATE_N, 4, IPFIX_CODING_UINT, "link_ieee_tx_rate_n", "wprobe link IEEE 802.11 TX data rate - Number of samples"
+522, IPFIX_FT_WPROBE_IEEE_TX_RATE_S, 8, IPFIX_CODING_UINT, "link_ieee_tx_rate_s", "wprobe link IEEE 802.11 TX data rate - Sum of samples"
+523, IPFIX_FT_WPROBE_IEEE_TX_RATE_SS, 8, IPFIX_CODING_UINT, "link_ieee_tx_rate_ss", "wprobe link IEEE 802.11 TX data rate - Sum of squared samples"
+524, IPFIX_FT_WPROBE_RETRANSMIT_200_N, 4, IPFIX_CODING_UINT, "link_retransmit_200_n", "wprobe link total retransmissions per packet - <200 bytes - Number of samples"
+525, IPFIX_FT_WPROBE_RETRANSMIT_200_S, 8, IPFIX_CODING_UINT, "link_retransmit_200_s", "wprobe link total retransmissions per packet - <200 bytes - Sum of samples"
+526, IPFIX_FT_WPROBE_RETRANSMIT_200_SS, 8, IPFIX_CODING_UINT, "link_retransmit_200_ss", "wprobe link total retransmissions per packet - <200 bytes - Sum of squared samples"
+527, IPFIX_FT_WPROBE_RETRANSMIT_400_N, 4, IPFIX_CODING_UINT, "link_retransmit_400_n", "wprobe link total retransmissions per packet - <400 bytes - Number of samples"
+528, IPFIX_FT_WPROBE_RETRANSMIT_400_S, 8, IPFIX_CODING_UINT, "link_retransmit_400_s", "wprobe link total retransmissions per packet - <400 bytes - Sum of samples"
+529, IPFIX_FT_WPROBE_RETRANSMIT_400_SS, 8, IPFIX_CODING_UINT, "link_retransmit_400_ss", "wprobe link total retransmissions per packet - <400 bytes - Sum of squared samples"
+530, IPFIX_FT_WPROBE_RETRANSMIT_800_N, 4, IPFIX_CODING_UINT, "link_retransmit_800_n", "wprobe link total retransmissions per packet - <800 bytes - Number of samples"
+531, IPFIX_FT_WPROBE_RETRANSMIT_800_S, 8, IPFIX_CODING_UINT, "link_retransmit_800_s", "wprobe link total retransmissions per packet - <800 bytes - Sum of samples"
+532, IPFIX_FT_WPROBE_RETRANSMIT_800_SS, 8, IPFIX_CODING_UINT, "link_retransmit_800_ss", "wprobe link total retransmissions per packet - <800 bytes - Sum of squared samples"
+533, IPFIX_FT_WPROBE_RETRANSMIT_1600_N, 4, IPFIX_CODING_UINT, "link_retransmit_1600_n", "wprobe link total retransmissions per packet - >800 bytes - Number of samples"
+534, IPFIX_FT_WPROBE_RETRANSMIT_1600_S, 8, IPFIX_CODING_UINT, "link_retransmit_1600_s", "wprobe link total retransmissions per packet - >800 bytes - Sum of samples"
+535, IPFIX_FT_WPROBE_RETRANSMIT_1600_SS, 8, IPFIX_CODING_UINT, "link_retransmit_1600_ss", "wprobe link total retransmissions per packet - >800 bytes - Sum of squared samples"
+536, IPFIX_FT_WPROBE_FRAMES, 4, IPFIX_CODING_UINT, "global_frames", "wprobe global number of 802.11 frames seen"
+537, IPFIX_FT_WPROBE_PROBEREQ, 4, IPFIX_CODING_UINT, "global_probereq", "wprobe global number of 802.11 probe requests seen"
