--- a/drivers/atm/solos-pci.c
+++ b/drivers/atm/solos-pci.c
@@ -710,8 +710,8 @@ void solos_bh(unsigned long card_arg)
 					       le16_to_cpu(header->vci));
 				if (!vcc) {
 					if (net_ratelimit())
-						dev_warn(&card->dev->dev, "Received packet for unknown VCI.VPI %d.%d on port %d\n",
-							 le16_to_cpu(header->vci), le16_to_cpu(header->vpi),
+						dev_warn(&card->dev->dev, "Received packet for unknown VPI.VCI %d.%d on port %d\n",
+							 le16_to_cpu(header->vpi), le16_to_cpu(header->vci),
 							 port);
 					continue;
 				}
