From fab0cbda27ab2400d6a461bf144007a0d5337527 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Wed, 25 Jan 2012 17:40:05 +0100
Subject: [PATCH 12/63] MIPS: BCM63XX: make board setup code register the spi platform device

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |    3 +++
 1 files changed, 3 insertions(+), 0 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -25,6 +25,7 @@
 #include <bcm63xx_dev_enet.h>
 #include <bcm63xx_dev_dsp.h>
 #include <bcm63xx_dev_pcmcia.h>
+#include <bcm63xx_dev_spi.h>
 #include <board_bcm963xx.h>
 
 #define PFX	"board_bcm963xx: "
@@ -890,6 +891,8 @@ int __init board_register_devices(void)
 	}
 #endif
 
+	bcm63xx_spi_register();
+
 	/* read base address of boot chip select (0) */
 	val = bcm_mpi_readl(MPI_CSBASE_REG(0));
 	val &= MPI_CSBASE_BASE_MASK;
