--- a/arch/mips/include/asm/mach-bcm47xx/gpio.h
+++ b/arch/mips/include/asm/mach-bcm47xx/gpio.h
@@ -151,5 +151,9 @@ static inline int gpio_polarity(unsigned
 	return -EINVAL;
 }
 
+static inline int gpio_set_debounce(unsigned gpio, unsigned debounce)
+{
+	return -ENOSYS;
+}
 
 #endif /* __BCM47XX_GPIO_H */
