--- a/arch/powerpc/boot/dts/mpc8568mds.dts
+++ b/arch/powerpc/boot/dts/mpc8568mds.dts
@@ -301,32 +301,24 @@
 			};
 		};
 
-		duart-sleep-nexus {
-			#address-cells = <1>;
-			#size-cells = <1>;
-			compatible = "simple-bus";
-			sleep = <&pmc 0x00000002>;
-			ranges;
-
-			serial0: serial@4500 {
-				cell-index = <0>;
-				device_type = "serial";
-				compatible = "ns16550";
-				reg = <0x4500 0x100>;
-				clock-frequency = <0>;
-				interrupts = <42 2>;
-				interrupt-parent = <&mpic>;
-			};
+		serial0: serial@4500 {
+			cell-index = <0>;
+			device_type = "serial";
+			compatible = "ns16550";
+			reg = <0x4500 0x100>;
+			clock-frequency = <0>;
+			interrupts = <42 2>;
+			interrupt-parent = <&mpic>;
+		};
 
-			serial1: serial@4600 {
-				cell-index = <1>;
-				device_type = "serial";
-				compatible = "ns16550";
-				reg = <0x4600 0x100>;
-				clock-frequency = <0>;
-				interrupts = <42 2>;
-				interrupt-parent = <&mpic>;
-			};
+		serial1: serial@4600 {
+			cell-index = <1>;
+			device_type = "serial";
+			compatible = "ns16550";
+			reg = <0x4600 0x100>;
+			clock-frequency = <0>;
+			interrupts = <42 2>;
+			interrupt-parent = <&mpic>;
 		};
 
 		global-utilities@e0000 {
@@ -669,4 +661,7 @@
 			gpios = <&bcsr5 3 0>;
 		};
 	};
+	chosen {
+		linux,stdout-path = "/soc8568@e0000000/serial@4500";
+	};
 };
