
. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
netgear,r8000)
	ucidef_set_led_usbport "usb2" "USB 2.0" "bcm53xx:white:usb2" "usb1-port2" "usb2-port2"
	ucidef_set_led_usbport "usb3" "USB 3.0" "bcm53xx:white:usb3" "usb1-port1" "usb2-port1" "usb4-port1"
	;;
esac

board_config_flush

exit 0
