From 74abbfe99f43eb7466d26d9e48fbeb46b8f3d804 Mon Sep 17 00:00:00 2001
From: Serge Semin <Sergey.Semin@baikalelectronics.ru>
Date: Tue, 20 Oct 2020 14:59:37 +0300
Subject: [PATCH] ARM: dts: BCM5301X: Harmonize EHCI/OHCI DT nodes name

In accordance with the Generic EHCI/OHCI bindings the corresponding node
name is suppose to comply with the Generic USB HCD DT schema, which
requires the USB nodes to have the name acceptable by the regexp:
"^usb(@.*)?" . Make sure the "generic-ehci" and "generic-ohci"-compatible
nodes are correctly named.

Signed-off-by: Serge Semin <Sergey.Semin@baikalelectronics.ru>
Acked-by: Florian Fainelli <f.fainelli@gmail.com>
Acked-by: Krzysztof Kozlowski <krzk@kernel.org>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm5301x.dtsi | 4 ++--
 arch/arm/boot/dts/bcm53573.dtsi | 4 ++--
 2 files changed, 4 insertions(+), 4 deletions(-)

--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -265,7 +265,7 @@
 
 			interrupt-parent = <&gic>;
 
-			ehci: ehci@21000 {
+			ehci: usb@21000 {
 				#usb-cells = <0>;
 
 				compatible = "generic-ehci";
@@ -287,7 +287,7 @@
 				};
 			};
 
-			ohci: ohci@22000 {
+			ohci: usb@22000 {
 				#usb-cells = <0>;
 
 				compatible = "generic-ohci";
--- a/arch/arm/boot/dts/bcm53573.dtsi
+++ b/arch/arm/boot/dts/bcm53573.dtsi
@@ -135,7 +135,7 @@
 			#address-cells = <1>;
 			#size-cells = <1>;
 
-			ehci: ehci@4000 {
+			ehci: usb@4000 {
 				compatible = "generic-ehci";
 				reg = <0x4000 0x1000>;
 				interrupt-parent = <&gic>;
@@ -155,7 +155,7 @@
 				};
 			};
 
-			ohci: ohci@d000 {
+			ohci: usb@d000 {
 				#usb-cells = <0>;
 
 				compatible = "generic-ohci";
