#include "qca953x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
		label-mac-device = &eth0;
	};

	keys {
		compatible = "gpio-keys";

		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		right {
			label = "button right";
			linux,code = <BTN_0>;
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
		};

		left {
			label = "button left";
			linux,code = <BTN_1>;
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		};
	};

	leds {
		compatible = "gpio-leds";

		// Colors for non-Lite versions

		led_status: status {
			label = "green:status";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "green:lan";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led_wlan: wlan {
			label = "red:wlan";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	i2c: i2c {
		compatible = "i2c-gpio";

		sda-gpios = <&gpio 17 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio 16 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>;
	};
};

&pcie0 {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			nor_firmware: partition@50000 {
				label = "nor_firmware";
				reg = <0x050000 0xfa0000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};

	nand_flash: flash@1 {
		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			nand_kernel: partition@0 {
				label = "nand_kernel";
				reg = <0x000000 0x400000>;
			};

			nand_ubi: partition@400000 {
				label = "nand_ubi";
				reg = <0x400000 0x7c00000>;
			};
		};
	};
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy4>;

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
