From ffbb1b37a3e1ce1a5c574a6bd4f5aede8bc468ac Mon Sep 17 00:00:00 2001
From: Ilya Lipnitskiy <ilya.lipnitskiy@gmail.com>
Date: Sat, 27 Feb 2021 20:20:07 -0800
Subject: [PATCH] Revert "net: phy: simplify phy_link_change arguments"

This reverts commit a307593a644443db12888f45eed0dafb5869e2cc.

This brings back the do_carrier flags used by the (hacky) next patch,
still required by target/linux/ramips/files/drivers/net/ethernet/ralink/mdio.c
---
 drivers/net/phy/phy.c        | 12 ++++++------
 drivers/net/phy/phy_device.c | 12 +++++++-----
 drivers/net/phy/phylink.c    |  3 ++-
 include/linux/phy.h          |  2 +-
 4 files changed, 16 insertions(+), 13 deletions(-)

--- a/drivers/net/phy/phy.c
+++ b/drivers/net/phy/phy.c
@@ -58,13 +58,13 @@ static const char *phy_state_to_str(enum
 
 static void phy_link_up(struct phy_device *phydev)
 {
-	phydev->phy_link_change(phydev, true);
+	phydev->phy_link_change(phydev, true, true);
 	phy_led_trigger_change_speed(phydev);
 }
 
-static void phy_link_down(struct phy_device *phydev)
+static void phy_link_down(struct phy_device *phydev, bool do_carrier)
 {
-	phydev->phy_link_change(phydev, false);
+	phydev->phy_link_change(phydev, false, do_carrier);
 	phy_led_trigger_change_speed(phydev);
 }
 
@@ -567,7 +567,7 @@ int phy_start_cable_test(struct phy_devi
 		goto out;
 
 	/* Mark the carrier down until the test is complete */
-	phy_link_down(phydev);
+	phy_link_down(phydev, true);
 
 	netif_testing_on(dev);
 	err = phydev->drv->cable_test_start(phydev);
@@ -638,7 +638,7 @@ int phy_start_cable_test_tdr(struct phy_
 		goto out;
 
 	/* Mark the carrier down until the test is complete */
-	phy_link_down(phydev);
+	phy_link_down(phydev, true);
 
 	netif_testing_on(dev);
 	err = phydev->drv->cable_test_tdr_start(phydev, config);
@@ -709,7 +709,7 @@ static int phy_check_link_status(struct
 		phy_link_up(phydev);
 	} else if (!phydev->link && phydev->state != PHY_NOLINK) {
 		phydev->state = PHY_NOLINK;
-		phy_link_down(phydev);
+		phy_link_down(phydev, true);
 	}
 
 	return 0;
@@ -1191,7 +1191,7 @@ void phy_state_machine(struct work_struc
 	case PHY_HALTED:
 		if (phydev->link) {
 			phydev->link = 0;
-			phy_link_down(phydev);
+			phy_link_down(phydev, true);
 		}
 		do_suspend = true;
 		break;
--- a/drivers/net/phy/phy_device.c
+++ b/drivers/net/phy/phy_device.c
@@ -936,14 +936,16 @@ struct phy_device *phy_find_first(struct
 }
 EXPORT_SYMBOL(phy_find_first);
 
-static void phy_link_change(struct phy_device *phydev, bool up)
+static void phy_link_change(struct phy_device *phydev, bool up, bool do_carrier)
 {
 	struct net_device *netdev = phydev->attached_dev;
 
-	if (up)
-		netif_carrier_on(netdev);
-	else
-		netif_carrier_off(netdev);
+	if (do_carrier) {
+		if (up)
+			netif_carrier_on(netdev);
+		else
+			netif_carrier_off(netdev);
+	}
 	phydev->adjust_link(netdev);
 	if (phydev->mii_ts && phydev->mii_ts->link_state)
 		phydev->mii_ts->link_state(phydev->mii_ts, phydev);
--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -907,7 +907,8 @@ void phylink_destroy(struct phylink *pl)
 }
 EXPORT_SYMBOL_GPL(phylink_destroy);
 
-static void phylink_phy_change(struct phy_device *phydev, bool up)
+static void phylink_phy_change(struct phy_device *phydev, bool up,
+			       bool do_carrier)
 {
 	struct phylink *pl = phydev->phylink;
 	bool tx_pause, rx_pause;
--- a/include/linux/phy.h
+++ b/include/linux/phy.h
@@ -642,7 +642,7 @@ struct phy_device {
 	u8 mdix;
 	u8 mdix_ctrl;
 
-	void (*phy_link_change)(struct phy_device *phydev, bool up);
+	void (*phy_link_change)(struct phy_device *, bool up, bool do_carrier);
 	void (*adjust_link)(struct net_device *dev);
 
 #if IS_ENABLED(CONFIG_MACSEC)
