From patchwork Thu Dec 27 14:05:26 2018
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit
X-Patchwork-Submitter: Tom Psyborg <pozega.tomislav@gmail.com>
X-Patchwork-Id: 10743707
X-Patchwork-Delegate: kvalo@adurom.com
From: =?utf-8?q?Tomislav_Po=C5=BEega?= <pozega.tomislav@gmail.com>
To: linux-wireless@vger.kernel.org
Cc: kvalo@codeaurora.org, hauke@hauke-m.de, nbd@nbd.name,
        john@phrozen.org, sgruszka@redhat.com, daniel@makrotopia.org
Subject: [PATCH 2/2] rt2x00: define RF5592 in init_eeprom routine
Date: Thu, 27 Dec 2018 15:05:26 +0100
Message-Id: <1545919526-4074-2-git-send-email-pozega.tomislav@gmail.com>
X-Mailer: git-send-email 1.7.0.4
In-Reply-To: <1545919526-4074-1-git-send-email-pozega.tomislav@gmail.com>
References: <1545919526-4074-1-git-send-email-pozega.tomislav@gmail.com>
MIME-Version: 1.0
Sender: linux-wireless-owner@vger.kernel.org
Precedence: bulk
List-ID: <linux-wireless.vger.kernel.org>
X-Mailing-List: linux-wireless@vger.kernel.org
X-Virus-Scanned: ClamAV using ClamSMTP

This patch fixes following crash on Linksys EA2750 during 5GHz wifi
init:

[    7.955153] rt2800pci 0000:01:00.0: card - bus=0x1, slot = 0x0 irq=4
[    7.962259] rt2800pci 0000:01:00.0: loaded eeprom from mtd device "Factory"
[    7.969435] ieee80211 phy0: rt2x00_set_rt: Info - RT chipset 5592, rev 0222 detected
[    7.977348] ieee80211 phy0: rt2800_init_eeprom: Error - Invalid RF chipset 0x0000 detected
[    7.985793] ieee80211 phy0: rt2x00lib_probe_dev: Error - Failed to allocate device
[    7.993569] CPU 0 Unable to handle kernel paging request at virtual address 00000024, epc == 800c8f54, ra == 80249ff8
[    8.004408] Oops[#1]:

Signed-off-by: Tomislav Požega <pozega.tomislav@gmail.com>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    2 ++
 1 files changed, 2 insertions(+), 0 deletions(-)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -9435,6 +9435,8 @@ static int rt2800_init_eeprom(struct rt2
 		rf = RF3853;
 	else if (rt2x00_rt(rt2x00dev, RT5350))
 		rf = RF5350;
+	else if (rt2x00_rt(rt2x00dev, RT5592))
+		rf = RF5592;
 	else
 		rf = rt2x00_get_field16(eeprom, EEPROM_NIC_CONF0_RF_TYPE);
 
