From 3559c1ea4336636c886002996d50805365d3055c Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Wed, 10 Mar 2021 09:48:13 +0100
Subject: [PATCH] net: broadcom: bcm4908_enet: read MAC from OF
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM4908 devices have MAC address accessible using NVMEM so it's needed
to use OF helper for reading it.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/broadcom/bcm4908_enet.c | 8 +++++++-
 1 file changed, 7 insertions(+), 1 deletion(-)

--- a/drivers/net/ethernet/broadcom/bcm4908_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm4908_enet.c
@@ -9,6 +9,7 @@
 #include <linux/interrupt.h>
 #include <linux/module.h>
 #include <linux/of.h>
+#include <linux/of_net.h>
 #include <linux/platform_device.h>
 #include <linux/slab.h>
 #include <linux/string.h>
@@ -647,7 +648,9 @@ static int bcm4908_enet_probe(struct pla
 		return err;
 
 	SET_NETDEV_DEV(netdev, &pdev->dev);
-	eth_hw_addr_random(netdev);
+	of_get_mac_address(dev->of_node, netdev->dev_addr);
+	if (!is_valid_ether_addr(netdev->dev_addr))
+		eth_hw_addr_random(netdev);
 	netdev->netdev_ops = &bcm4908_enet_netdev_ops;
 	netdev->min_mtu = ETH_ZLEN;
 	netdev->mtu = ETH_DATA_LEN;
