// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6358.dtsi"

/ {
	compatible = "huawei,hg556a-b", "brcm,bcm6358";
	model = "Huawei EchoLife HG556a (version B)";

	aliases {
		led-boot = &led_power_red;
		led-failsafe = &led_power_red;
		led-running = &led_power_red;
		led-upgrade = &led_power_red;

		led-dsl = &led_dsl_red;
		led-usb = &led_hspa_red;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		help {
			label = "help";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_HELP>;
			debounce-interval = <60>;
		};

		wlan {
			label = "wlan";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		restart {
			label = "restart";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_CONFIG>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led@0 {
			label = "red:message";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		led_hspa_red: led@1 {
			label = "red:hspa";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		led_dsl_red: led@2 {
			label = "red:dsl";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		led_power_red: led@3 {
			label = "red:power";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		led@6 {
			label = "all";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led@12 {
			label = "green:lan1";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		led@13 {
			label = "red:lan1";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led@15 {
			label = "green:lan2";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led@22 {
			label = "red:lan2";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		led@23 {
			label = "green:lan3";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		led@26 {
			label = "red:lan3";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};

		led@27 {
			label = "green:lan4";
			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
		};

		led@28 {
			label = "red:lan4";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-fixup {
		compatible = "brcm,ath9k-fixup";
		reg = <0x30000000 0x8000000>;

		pci-dev = <1>;

		nvmem-cells = <&macaddr_cfe_6a0>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;

		ath,eeprom = <&cal_data 0x1e000>;
		ath,endian-check;
		ath,led-pin = <2>;
		ath,led-active-high;
	};
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&pci {
	status = "okay";
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe: partition@0 {
			label = "cfe";
			reg = <0x000000 0x020000>;
			read-only;
		};

		partition@20000 {
			label = "firmware";
			reg = <0x020000 0xec0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		cal_data: partition@ee0000 {
			label = "cal_data";
			reg = <0xee0000 0x100000>;
			read-only;
		};

		partition@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};

&cfe {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_cfe_6a0: macaddr@6a0 {
		reg = <0x6a0 0x6>;
	};
};
