From d59c125296df424b8e7c5c4900e1b8084b6dd3ba Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 30 Mar 2016 03:18:17 +0200
Subject: [PATCH 70/91] net: mediatek: watchdog_timeo was not set

The original commit failed to set watchdog_timeo. This patch sets
watchdog_timeo to HZ.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |    1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/net/ethernet/mediatek/mtk_eth_soc.c b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
index 7f2126b..7e6d2e2 100644
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1645,6 +1645,7 @@ static int mtk_add_mac(struct mtk_eth *eth, struct device_node *np)
 	mac->hw_stats->reg_offset = id * MTK_STAT_OFFSET;
 
 	SET_NETDEV_DEV(eth->netdev[id], eth->dev);
+	eth->netdev[id]->watchdog_timeo = HZ;
 	eth->netdev[id]->netdev_ops = &mtk_netdev_ops;
 	eth->netdev[id]->base_addr = (unsigned long)eth->base;
 	eth->netdev[id]->vlan_features = MTK_HW_FEATURES &
-- 
1.7.10.4

