From 2206de729d8a873898b983f5ff7633a2489aa71c Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sat, 23 Apr 2016 09:06:05 +0200
Subject: [PATCH 83/91] net-next: mediatek: add missing return code check

The code fails to check if the scratch memory was properly allocated. Add
this check and return with an error if the allocation failed.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |    3 +++
 1 file changed, 3 insertions(+)

diff --git a/drivers/net/ethernet/mediatek/mtk_eth_soc.c b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
index 674e8e3..37e9260 100644
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -483,6 +483,9 @@ static int mtk_init_fq_dma(struct mtk_eth *eth)
 
 	eth->scratch_head = kcalloc(cnt, MTK_QDMA_PAGE_SIZE,
 				    GFP_KERNEL);
+	if (unlikely(!eth->scratch_head))
+		return -ENOMEM;
+
 	dma_addr = dma_map_single(eth->dev,
 				  eth->scratch_head, cnt * MTK_QDMA_PAGE_SIZE,
 				  DMA_FROM_DEVICE);
-- 
1.7.10.4

