From 6aa2c847f76f21c830544e8c79f9030a170ef475 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 21 Jan 2016 17:57:49 +0000
Subject: [PATCH 167/170] BCM270X_DT: Add Pi3 support

---
 arch/arm/boot/dts/Makefile            |   1 +
 arch/arm/boot/dts/bcm2710-rpi-3-b.dts | 174 ++++++++++++++++++++++++++++++++++
 arch/arm/boot/dts/bcm2710.dtsi        | 102 ++++++++++++++++++++
 3 files changed, 277 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm2710-rpi-3-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2710.dtsi

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -5,6 +5,7 @@ dtb-$(CONFIG_ARCH_BCM2708) += bcm2708-rp
 dtb-$(CONFIG_ARCH_BCM2708) += bcm2708-rpi-cm.dtb
 dtb-$(CONFIG_ARCH_BCM2835) += bcm2835-rpi-cm.dtb
 dtb-$(CONFIG_ARCH_BCM2709) += bcm2709-rpi-2-b.dtb
+dtb-$(CONFIG_ARCH_BCM2709) += bcm2710-rpi-3-b.dtb
 
 # Raspberry Pi
 ifeq ($(CONFIG_ARCH_BCM2708),y)
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
@@ -0,0 +1,174 @@
+/dts-v1/;
+
+#include "bcm2710.dtsi"
+
+/ {
+	compatible = "brcm,bcm2710","brcm,bcm2709";
+	model = "Raspberry Pi 3 Model B";
+};
+
+&gpio {
+	sdhost_pins: sdhost_pins {
+		brcm,pins = <48 49 50 51 52 53>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_pins: spi0_pins {
+		brcm,pins = <9 10 11>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	spi0_cs_pins: spi0_cs_pins {
+		brcm,pins = <8 7>;
+		brcm,function = <1>; /* output */
+	};
+
+	i2c0_pins: i2c0 {
+		brcm,pins = <0 1>;
+		brcm,function = <4>;
+	};
+
+	i2c1_pins: i2c1 {
+		brcm,pins = <2 3>;
+		brcm,function = <4>;
+	};
+
+	i2s_pins: i2s {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <4>; /* alt0 */
+	};
+
+	sdio_pins: sdio_pins {
+		brcm,pins =     <34 35 36 37 38 39>;
+		brcm,function = <7>; // alt3 = SD1
+		brcm,pull =     <0 2 2 2 2 2>;
+	};
+
+	bt_pins: bt_pins {
+		brcm,pins =     <28 29 30 31 14 15 43>;
+		brcm,function = <6 6 6 6 2 2 4>;
+			// alt2:PCM alt5:UART1 alt0:GPCLK2
+		brcm,pull =     <0 0 0 0 0 2 0>;
+	};
+
+	uart1_pins: uart1_pins {
+		brcm,pins = <32 33>;
+		brcm,function = <7>; /* alt3=UART0 */
+		brcm,pull = <0>;
+	};
+};
+
+&sdhost {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdhost_pins>;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&mmc {
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio_pins>;
+	non-removable;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&fb {
+	status = "okay";
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins &bt_pins>;
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins &spi0_cs_pins>;
+	cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
+
+	spidev@0{
+		compatible = "spidev";
+		reg = <0>;	/* CE0 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+
+	spidev@1{
+		compatible = "spidev";
+		reg = <1>;	/* CE1 */
+		#address-cells = <1>;
+		#size-cells = <0>;
+		spi-max-frequency = <500000>;
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	clock-frequency = <100000>;
+};
+
+&i2c2 {
+	clock-frequency = <100000>;
+};
+
+&i2s {
+	#sound-dai-cells = <0>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2s_pins>;
+};
+
+&random {
+	status = "okay";
+};
+
+&leds {
+	act_led: act {
+		label = "led0";
+		linux,default-trigger = "mmc0";
+		gpios = <&gpio 47 0>;
+	};
+};
+
+/ {
+	chosen {
+		bootargs = "8250.nr_uarts=1";
+	};
+};
+
+/ {
+	__overrides__ {
+		uart0 = <&uart0>,"status";
+		uart0_clkrate = <&clk_uart0>,"clock-frequency:0";
+		i2s = <&i2s>,"status";
+		spi = <&spi0>,"status";
+		i2c0 = <&i2c0>,"status";
+		i2c1 = <&i2c1>,"status";
+		i2c2_iknowwhatimdoing = <&i2c2>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
+		i2c2_baudrate = <&i2c2>,"clock-frequency:0";
+		core_freq = <&clk_core>,"clock-frequency:0";
+
+		act_led_gpio = <&act_led>,"gpios:4";
+		act_led_activelow = <&act_led>,"gpios:8";
+		act_led_trigger = <&act_led>,"linux,default-trigger";
+
+		audio = <&audio>,"status";
+		watchdog = <&watchdog>,"status";
+		random = <&random>,"status";
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2710.dtsi
@@ -0,0 +1,102 @@
+#include "bcm2708_common.dtsi"
+
+/ {
+	compatible = "brcm,bcm2710","brcm,bcm2709";
+	model = "BCM2710";
+
+	chosen {
+		/* No padding required - the boot loader can do that. */
+		bootargs = "";
+	};
+
+	soc {
+		ranges = <0x7e000000 0x3f000000 0x01000000>,
+		         <0x40000000 0x40000000 0x00040000>;
+
+		local_intc: local_intc {
+			compatible = "brcm,bcm2836-l1-intc";
+			reg = <0x40000000 0x100>;
+			interrupt-controller;
+			#interrupt-cells = <1>;
+			interrupt-parent = <&local_intc>;
+		};
+
+		arm-pmu {
+			compatible = "arm,cortex-a7-pmu";
+			interrupt-parent = <&local_intc>;
+			interrupts = <9>;
+		};
+
+		gpiomem {
+			compatible = "brcm,bcm2835-gpiomem";
+			reg = <0x7e200000 0x1000>;
+			status = "okay";
+		};
+
+		timer {
+			compatible = "arm,armv7-timer";
+			clock-frequency = <19200000>;
+			interrupt-parent = <&local_intc>;
+			interrupts = <0>, // PHYS_SECURE_PPI
+				     <1>, // PHYS_NONSECURE_PPI
+				     <3>, // VIRT_PPI
+				     <2>; // HYP_PPI
+			always-on;
+		};
+
+		syscon@40000000 {
+			compatible = "brcm,bcm2836-arm-local", "syscon";
+			reg = <0x40000000 0x100>;
+		};
+	};
+
+	cpus: cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		v7_cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0x000>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0x001>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0x002>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0x003>;
+			clock-frequency = <800000000>;
+		};
+	};
+
+	__overrides__ {
+		arm_freq = <&v7_cpu0>, "clock-frequency:0",
+		       <&v7_cpu1>, "clock-frequency:0",
+		       <&v7_cpu2>, "clock-frequency:0",
+		       <&v7_cpu3>, "clock-frequency:0";
+	};
+};
+
+&watchdog {
+	status = "okay";
+};
+
+&intc {
+        compatible = "brcm,bcm2836-armctrl-ic";
+        interrupt-parent = <&local_intc>;
+        interrupts = <8>;
+};
