From 1a254735cad9db5c8605c972b0f16b3929dc0d6e Mon Sep 17 00:00:00 2001
From: Biao Huang <biao.huang@mediatek.com>
Date: Mon, 28 Dec 2015 15:09:03 +0800
Subject: [PATCH 13/91] dt-bindings: mediatek: Modify pinctrl bindings for
 mt2701

Signed-off-by: Biao Huang <biao.huang@mediatek.com>
Acked-by: Rob Herring <robh@kernel.org>
Reviewed-by: Mathias Brugger <matthias.bgg@gmail.com>
---
 Documentation/devicetree/bindings/pinctrl/pinctrl-mt65xx.txt |    9 +++++----
 1 file changed, 5 insertions(+), 4 deletions(-)

diff --git a/Documentation/devicetree/bindings/pinctrl/pinctrl-mt65xx.txt b/Documentation/devicetree/bindings/pinctrl/pinctrl-mt65xx.txt
index 0480bc3..9ffb0b2 100644
--- a/Documentation/devicetree/bindings/pinctrl/pinctrl-mt65xx.txt
+++ b/Documentation/devicetree/bindings/pinctrl/pinctrl-mt65xx.txt
@@ -4,10 +4,11 @@ The Mediatek's Pin controller is used to control SoC pins.
 
 Required properties:
 - compatible: value should be one of the following.
-    (a) "mediatek,mt8135-pinctrl", compatible with mt8135 pinctrl.
-    (b) "mediatek,mt8173-pinctrl", compatible with mt8173 pinctrl.
-    (c) "mediatek,mt6397-pinctrl", compatible with mt6397 pinctrl.
-    (d) "mediatek,mt8127-pinctrl", compatible with mt8127 pinctrl.
+	"mediatek,mt2701-pinctrl", compatible with mt2701 pinctrl.
+	"mediatek,mt6397-pinctrl", compatible with mt6397 pinctrl.
+	"mediatek,mt8127-pinctrl", compatible with mt8127 pinctrl.
+	"mediatek,mt8135-pinctrl", compatible with mt8135 pinctrl.
+	"mediatek,mt8173-pinctrl", compatible with mt8173 pinctrl.
 - pins-are-numbered: Specify the subnodes are using numbered pinmux to
   specify pins.
 - gpio-controller : Marks the device node as a gpio controller.
-- 
1.7.10.4

