From e9051f5dbc26e78f91cf23ca79ae4c8471119667 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Emilio=20L=C3=B3pez?= <emilio@elopez.com.ar>
Date: Fri, 18 Jul 2014 15:26:08 -0300
Subject: [PATCH] ARM: sun7i: Add mod1 clock nodes
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This commit adds all the mod1 clocks available on A20 to its device
tree. This list was created by looking at the A20 user manual.

Not-signed-off-by: Emilio López <emilio@elopez.com.ar>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 39 +++++++++++++++++++++++++++++++++++++++
 1 file changed, 39 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -447,6 +447,29 @@
 			clock-output-names = "ir1";
 		};
 
+		iis0_clk: clk@01c200b8 {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-a10-mod1-clk";
+			reg = <0x01c200b8 0x4>;
+			clocks = <&pll2 0>, <&pll2 1>, <&pll2 2>, <&pll2 3>;
+			clock-output-names = "iis0";
+		};
+
+		ac97_clk: clk@01c200bc {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-a10-mod1-clk";
+			reg = <0x01c200bc 0x4>;
+			clocks = <&pll2 3>, <&pll2 2>, <&pll2 1>, <&pll2 0>;
+			clock-output-names = "ac97";
+		};
+
+		spdif_clk: clk@01c200c0 {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-a10-mod1-clk";
+			reg = <0x01c200c0 0x4>;
+			clocks = <&pll2 0>, <&pll2 1>, <&pll2 2>, <&pll2 3>;
+			clock-output-names = "spdif";
+		};
 		usb_clk: clk@01c200cc {
 			#clock-cells = <1>;
 		        #reset-cells = <1>;
@@ -464,6 +487,22 @@
 			clock-output-names = "spi3";
 		};
 
+		iis1_clk: clk@01c200d8 {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-a10-mod1-clk";
+			reg = <0x01c200d8 0x4>;
+			clocks = <&pll2 0>, <&pll2 1>, <&pll2 2>, <&pll2 3>;
+			clock-output-names = "iis1";
+		};
+
+		iis2_clk: clk@01c200dc {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-a10-mod1-clk";
+			reg = <0x01c200dc 0x4>;
+			clocks = <&pll2 0>, <&pll2 1>, <&pll2 2>, <&pll2 3>;
+			clock-output-names = "iis2";
+		};
+
 		codec_clk: clk@01c20140 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-a10-codec-clk";
