From b5116083e227fa478e20d5ed945430088aa1a00b Mon Sep 17 00:00:00 2001
From: Jon Mason <jonmason@broadcom.com>
Date: Thu, 15 Oct 2015 15:48:25 -0400
Subject: [PATCH 44/50] clk: cygnus: Convert all macros to all caps

The macros that are being used to initialize the values of the clk
structures should be all caps.  Find and replace all of them with their
relevant counterparts.

Signed-off-by: Jon Mason <jonmason@broadcom.com>
---
 drivers/clk/bcm/clk-cygnus.c | 146 +++++++++++++++++++++----------------------
 1 file changed, 73 insertions(+), 73 deletions(-)

--- a/drivers/clk/bcm/clk-cygnus.c
+++ b/drivers/clk/bcm/clk-cygnus.c
@@ -23,28 +23,28 @@
 #include <dt-bindings/clock/bcm-cygnus.h>
 #include "clk-iproc.h"
 
-#define reg_val(o, s, w) { .offset = o, .shift = s, .width = w, }
+#define REG_VAL(o, s, w) { .offset = o, .shift = s, .width = w, }
 
-#define aon_val(o, pw, ps, is) { .offset = o, .pwr_width = pw, \
+#define AON_VAL(o, pw, ps, is) { .offset = o, .pwr_width = pw, \
 	.pwr_shift = ps, .iso_shift = is }
 
-#define sw_ctrl_val(o, s) { .offset = o, .shift = s, }
+#define SW_CTRL_VAL(o, s) { .offset = o, .shift = s, }
 
-#define asiu_div_val(o, es, hs, hw, ls, lw) \
+#define ASIU_DIV_VAL(o, es, hs, hw, ls, lw) \
 		{ .offset = o, .en_shift = es, .high_shift = hs, \
 		.high_width = hw, .low_shift = ls, .low_width = lw }
 
-#define reset_val(o, rs, prs, kis, kiw, kps, kpw, kas, kaw) { .offset = o, \
+#define RESET_VAL(o, rs, prs, kis, kiw, kps, kpw, kas, kaw) { .offset = o, \
 	.reset_shift = rs, .p_reset_shift = prs, .ki_shift = kis, \
 	.ki_width = kiw, .kp_shift = kps, .kp_width = kpw, .ka_shift = kas, \
 	.ka_width = kaw }
 
-#define vco_ctrl_val(uo, lo) { .u_offset = uo, .l_offset = lo }
+#define VCO_CTRL_VAL(uo, lo) { .u_offset = uo, .l_offset = lo }
 
-#define enable_val(o, es, hs, bs) { .offset = o, .enable_shift = es, \
+#define ENABLE_VAL(o, es, hs, bs) { .offset = o, .enable_shift = es, \
 	.hold_shift = hs, .bypass_shift = bs }
 
-#define asiu_gate_val(o, es) { .offset = o, .en_shift = es }
+#define ASIU_GATE_VAL(o, es) { .offset = o, .en_shift = es }
 
 static void __init cygnus_armpll_init(struct device_node *node)
 {
@@ -55,52 +55,52 @@ CLK_OF_DECLARE(cygnus_armpll, "brcm,cygn
 static const struct iproc_pll_ctrl genpll = {
 	.flags = IPROC_CLK_AON | IPROC_CLK_PLL_HAS_NDIV_FRAC |
 		IPROC_CLK_PLL_NEEDS_SW_CFG,
-	.aon = aon_val(0x0, 2, 1, 0),
-	.reset = reset_val(0x0, 11, 10, 4, 3, 0, 4, 7, 3),
-	.sw_ctrl = sw_ctrl_val(0x10, 31),
-	.ndiv_int = reg_val(0x10, 20, 10),
-	.ndiv_frac = reg_val(0x10, 0, 20),
-	.pdiv = reg_val(0x14, 0, 4),
-	.vco_ctrl = vco_ctrl_val(0x18, 0x1c),
-	.status = reg_val(0x28, 12, 1),
+	.aon = AON_VAL(0x0, 2, 1, 0),
+	.reset = RESET_VAL(0x0, 11, 10, 4, 3, 0, 4, 7, 3),
+	.sw_ctrl = SW_CTRL_VAL(0x10, 31),
+	.ndiv_int = REG_VAL(0x10, 20, 10),
+	.ndiv_frac = REG_VAL(0x10, 0, 20),
+	.pdiv = REG_VAL(0x14, 0, 4),
+	.vco_ctrl = VCO_CTRL_VAL(0x18, 0x1c),
+	.status = REG_VAL(0x28, 12, 1),
 };
 
 static const struct iproc_clk_ctrl genpll_clk[] = {
 	[BCM_CYGNUS_GENPLL_AXI21_CLK] = {
 		.channel = BCM_CYGNUS_GENPLL_AXI21_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x4, 6, 0, 12),
-		.mdiv = reg_val(0x20, 0, 8),
+		.enable = ENABLE_VAL(0x4, 6, 0, 12),
+		.mdiv = REG_VAL(0x20, 0, 8),
 	},
 	[BCM_CYGNUS_GENPLL_250MHZ_CLK] = {
 		.channel = BCM_CYGNUS_GENPLL_250MHZ_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x4, 7, 1, 13),
-		.mdiv = reg_val(0x20, 10, 8),
+		.enable = ENABLE_VAL(0x4, 7, 1, 13),
+		.mdiv = REG_VAL(0x20, 10, 8),
 	},
 	[BCM_CYGNUS_GENPLL_IHOST_SYS_CLK] = {
 		.channel = BCM_CYGNUS_GENPLL_IHOST_SYS_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x4, 8, 2, 14),
-		.mdiv = reg_val(0x20, 20, 8),
+		.enable = ENABLE_VAL(0x4, 8, 2, 14),
+		.mdiv = REG_VAL(0x20, 20, 8),
 	},
 	[BCM_CYGNUS_GENPLL_ENET_SW_CLK] = {
 		.channel = BCM_CYGNUS_GENPLL_ENET_SW_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x4, 9, 3, 15),
-		.mdiv = reg_val(0x24, 0, 8),
+		.enable = ENABLE_VAL(0x4, 9, 3, 15),
+		.mdiv = REG_VAL(0x24, 0, 8),
 	},
 	[BCM_CYGNUS_GENPLL_AUDIO_125_CLK] = {
 		.channel = BCM_CYGNUS_GENPLL_AUDIO_125_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x4, 10, 4, 16),
-		.mdiv = reg_val(0x24, 10, 8),
+		.enable = ENABLE_VAL(0x4, 10, 4, 16),
+		.mdiv = REG_VAL(0x24, 10, 8),
 	},
 	[BCM_CYGNUS_GENPLL_CAN_CLK] = {
 		.channel = BCM_CYGNUS_GENPLL_CAN_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x4, 11, 5, 17),
-		.mdiv = reg_val(0x24, 20, 8),
+		.enable = ENABLE_VAL(0x4, 11, 5, 17),
+		.mdiv = REG_VAL(0x24, 20, 8),
 	},
 };
 
@@ -113,51 +113,51 @@ CLK_OF_DECLARE(cygnus_genpll, "brcm,cygn
 
 static const struct iproc_pll_ctrl lcpll0 = {
 	.flags = IPROC_CLK_AON | IPROC_CLK_PLL_NEEDS_SW_CFG,
-	.aon = aon_val(0x0, 2, 5, 4),
-	.reset = reset_val(0x0, 31, 30, 27, 3, 23, 4, 19, 4),
-	.sw_ctrl = sw_ctrl_val(0x4, 31),
-	.ndiv_int = reg_val(0x4, 16, 10),
-	.pdiv = reg_val(0x4, 26, 4),
-	.vco_ctrl = vco_ctrl_val(0x10, 0x14),
-	.status = reg_val(0x18, 12, 1),
+	.aon = AON_VAL(0x0, 2, 5, 4),
+	.reset = RESET_VAL(0x0, 31, 30, 27, 3, 23, 4, 19, 4),
+	.sw_ctrl = SW_CTRL_VAL(0x4, 31),
+	.ndiv_int = REG_VAL(0x4, 16, 10),
+	.pdiv = REG_VAL(0x4, 26, 4),
+	.vco_ctrl = VCO_CTRL_VAL(0x10, 0x14),
+	.status = REG_VAL(0x18, 12, 1),
 };
 
 static const struct iproc_clk_ctrl lcpll0_clk[] = {
 	[BCM_CYGNUS_LCPLL0_PCIE_PHY_REF_CLK] = {
 		.channel = BCM_CYGNUS_LCPLL0_PCIE_PHY_REF_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x0, 7, 1, 13),
-		.mdiv = reg_val(0x8, 0, 8),
+		.enable = ENABLE_VAL(0x0, 7, 1, 13),
+		.mdiv = REG_VAL(0x8, 0, 8),
 	},
 	[BCM_CYGNUS_LCPLL0_DDR_PHY_CLK] = {
 		.channel = BCM_CYGNUS_LCPLL0_DDR_PHY_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x0, 8, 2, 14),
-		.mdiv = reg_val(0x8, 10, 8),
+		.enable = ENABLE_VAL(0x0, 8, 2, 14),
+		.mdiv = REG_VAL(0x8, 10, 8),
 	},
 	[BCM_CYGNUS_LCPLL0_SDIO_CLK] = {
 		.channel = BCM_CYGNUS_LCPLL0_SDIO_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x0, 9, 3, 15),
-		.mdiv = reg_val(0x8, 20, 8),
+		.enable = ENABLE_VAL(0x0, 9, 3, 15),
+		.mdiv = REG_VAL(0x8, 20, 8),
 	},
 	[BCM_CYGNUS_LCPLL0_USB_PHY_REF_CLK] = {
 		.channel = BCM_CYGNUS_LCPLL0_USB_PHY_REF_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x0, 10, 4, 16),
-		.mdiv = reg_val(0xc, 0, 8),
+		.enable = ENABLE_VAL(0x0, 10, 4, 16),
+		.mdiv = REG_VAL(0xc, 0, 8),
 	},
 	[BCM_CYGNUS_LCPLL0_SMART_CARD_CLK] = {
 		.channel = BCM_CYGNUS_LCPLL0_SMART_CARD_CLK,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x0, 11, 5, 17),
-		.mdiv = reg_val(0xc, 10, 8),
+		.enable = ENABLE_VAL(0x0, 11, 5, 17),
+		.mdiv = REG_VAL(0xc, 10, 8),
 	},
 	[BCM_CYGNUS_LCPLL0_CH5_UNUSED] = {
 		.channel = BCM_CYGNUS_LCPLL0_CH5_UNUSED,
 		.flags = IPROC_CLK_AON,
-		.enable = enable_val(0x0, 12, 6, 18),
-		.mdiv = reg_val(0xc, 20, 8),
+		.enable = ENABLE_VAL(0x0, 12, 6, 18),
+		.mdiv = REG_VAL(0xc, 20, 8),
 	},
 };
 
@@ -189,52 +189,52 @@ static const struct iproc_pll_vco_param
 static const struct iproc_pll_ctrl mipipll = {
 	.flags = IPROC_CLK_PLL_ASIU | IPROC_CLK_PLL_HAS_NDIV_FRAC |
 		 IPROC_CLK_NEEDS_READ_BACK,
-	.aon = aon_val(0x0, 4, 17, 16),
-	.asiu = asiu_gate_val(0x0, 3),
-	.reset = reset_val(0x0, 11, 10, 4, 3, 0, 4, 7, 4),
-	.ndiv_int = reg_val(0x10, 20, 10),
-	.ndiv_frac = reg_val(0x10, 0, 20),
-	.pdiv = reg_val(0x14, 0, 4),
-	.vco_ctrl = vco_ctrl_val(0x18, 0x1c),
-	.status = reg_val(0x28, 12, 1),
+	.aon = AON_VAL(0x0, 4, 17, 16),
+	.asiu = ASIU_GATE_VAL(0x0, 3),
+	.reset = RESET_VAL(0x0, 11, 10, 4, 3, 0, 4, 7, 4),
+	.ndiv_int = REG_VAL(0x10, 20, 10),
+	.ndiv_frac = REG_VAL(0x10, 0, 20),
+	.pdiv = REG_VAL(0x14, 0, 4),
+	.vco_ctrl = VCO_CTRL_VAL(0x18, 0x1c),
+	.status = REG_VAL(0x28, 12, 1),
 };
 
 static const struct iproc_clk_ctrl mipipll_clk[] = {
 	[BCM_CYGNUS_MIPIPLL_CH0_UNUSED] = {
 		.channel = BCM_CYGNUS_MIPIPLL_CH0_UNUSED,
 		.flags = IPROC_CLK_NEEDS_READ_BACK,
-		.enable = enable_val(0x4, 12, 6, 18),
-		.mdiv = reg_val(0x20, 0, 8),
+		.enable = ENABLE_VAL(0x4, 12, 6, 18),
+		.mdiv = REG_VAL(0x20, 0, 8),
 	},
 	[BCM_CYGNUS_MIPIPLL_CH1_LCD] = {
 		.channel = BCM_CYGNUS_MIPIPLL_CH1_LCD,
 		.flags = IPROC_CLK_NEEDS_READ_BACK,
-		.enable = enable_val(0x4, 13, 7, 19),
-		.mdiv = reg_val(0x20, 10, 8),
+		.enable = ENABLE_VAL(0x4, 13, 7, 19),
+		.mdiv = REG_VAL(0x20, 10, 8),
 	},
 	[BCM_CYGNUS_MIPIPLL_CH2_V3D] = {
 		.channel = BCM_CYGNUS_MIPIPLL_CH2_V3D,
 		.flags = IPROC_CLK_NEEDS_READ_BACK,
-		.enable = enable_val(0x4, 14, 8, 20),
-		.mdiv = reg_val(0x20, 20, 8),
+		.enable = ENABLE_VAL(0x4, 14, 8, 20),
+		.mdiv = REG_VAL(0x20, 20, 8),
 	},
 	[BCM_CYGNUS_MIPIPLL_CH3_UNUSED] = {
 		.channel = BCM_CYGNUS_MIPIPLL_CH3_UNUSED,
 		.flags = IPROC_CLK_NEEDS_READ_BACK,
-		.enable = enable_val(0x4, 15, 9, 21),
-		.mdiv = reg_val(0x24, 0, 8),
+		.enable = ENABLE_VAL(0x4, 15, 9, 21),
+		.mdiv = REG_VAL(0x24, 0, 8),
 	},
 	[BCM_CYGNUS_MIPIPLL_CH4_UNUSED] = {
 		.channel = BCM_CYGNUS_MIPIPLL_CH4_UNUSED,
 		.flags = IPROC_CLK_NEEDS_READ_BACK,
-		.enable = enable_val(0x4, 16, 10, 22),
-		.mdiv = reg_val(0x24, 10, 8),
+		.enable = ENABLE_VAL(0x4, 16, 10, 22),
+		.mdiv = REG_VAL(0x24, 10, 8),
 	},
 	[BCM_CYGNUS_MIPIPLL_CH5_UNUSED] = {
 		.channel = BCM_CYGNUS_MIPIPLL_CH5_UNUSED,
 		.flags = IPROC_CLK_NEEDS_READ_BACK,
-		.enable = enable_val(0x4, 17, 11, 23),
-		.mdiv = reg_val(0x24, 20, 8),
+		.enable = ENABLE_VAL(0x4, 17, 11, 23),
+		.mdiv = REG_VAL(0x24, 20, 8),
 	},
 };
 
@@ -247,15 +247,15 @@ static void __init cygnus_mipipll_clk_in
 CLK_OF_DECLARE(cygnus_mipipll, "brcm,cygnus-mipipll", cygnus_mipipll_clk_init);
 
 static const struct iproc_asiu_div asiu_div[] = {
-	[BCM_CYGNUS_ASIU_KEYPAD_CLK] = asiu_div_val(0x0, 31, 16, 10, 0, 10),
-	[BCM_CYGNUS_ASIU_ADC_CLK] = asiu_div_val(0x4, 31, 16, 10, 0, 10),
-	[BCM_CYGNUS_ASIU_PWM_CLK] = asiu_div_val(0x8, 31, 16, 10, 0, 10),
+	[BCM_CYGNUS_ASIU_KEYPAD_CLK] = ASIU_DIV_VAL(0x0, 31, 16, 10, 0, 10),
+	[BCM_CYGNUS_ASIU_ADC_CLK] = ASIU_DIV_VAL(0x4, 31, 16, 10, 0, 10),
+	[BCM_CYGNUS_ASIU_PWM_CLK] = ASIU_DIV_VAL(0x8, 31, 16, 10, 0, 10),
 };
 
 static const struct iproc_asiu_gate asiu_gate[] = {
-	[BCM_CYGNUS_ASIU_KEYPAD_CLK] = asiu_gate_val(0x0, 7),
-	[BCM_CYGNUS_ASIU_ADC_CLK] = asiu_gate_val(0x0, 9),
-	[BCM_CYGNUS_ASIU_PWM_CLK] = asiu_gate_val(IPROC_CLK_INVALID_OFFSET, 0),
+	[BCM_CYGNUS_ASIU_KEYPAD_CLK] = ASIU_GATE_VAL(0x0, 7),
+	[BCM_CYGNUS_ASIU_ADC_CLK] = ASIU_GATE_VAL(0x0, 9),
+	[BCM_CYGNUS_ASIU_PWM_CLK] = ASIU_GATE_VAL(IPROC_CLK_INVALID_OFFSET, 0),
 };
 
 static void __init cygnus_asiu_init(struct device_node *node)
