--- a/arch/arm/boot/dts/bcm5301x-nand-cs0-bch8.dtsi
+++ b/arch/arm/boot/dts/bcm5301x-nand-cs0-bch8.dtsi
@@ -19,6 +19,8 @@
 
 			nand-ecc-strength = <8>;
 			nand-ecc-step-size = <512>;
+
+			linux,part-probe = "ofpart", "bcm47xxpart";
 		};
 	};
 };
