From b6f1b24448de1d294f9668b14bf02391ff6bef5c Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Tue, 22 Mar 2016 04:42:27 +0100
Subject: [PATCH 71/91] net: mediatek: mtk_cal_txd_req() returns bad value

The code used to also support the PDMA engine, which had 2 packet pointers
per descriptor. Because of this we have to divide the result by 2 and round
it up. This is no longer needed as the code only supports QDMA.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/net/ethernet/mediatek/mtk_eth_soc.c b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
index 7e6d2e2..4d8d0a3 100644
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -681,7 +681,7 @@ static inline int mtk_cal_txd_req(struct sk_buff *skb)
 		nfrags += skb_shinfo(skb)->nr_frags;
 	}
 
-	return DIV_ROUND_UP(nfrags, 2);
+	return nfrags;
 }
 
 static int mtk_start_xmit(struct sk_buff *skb, struct net_device *dev)
-- 
1.7.10.4

