From 22ef77b0ba8fa347fe4b8c4c05d0bf0d08f4c141 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Tue, 26 May 2015 18:01:50 +0200
Subject: [PATCH] ARM: dts: sun5i: Add NFC node to Allwinner A13/A10s SoC

Add NAND Flash controller node definition to the A13/a10s SoC.

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun5i.dtsi | 11 +++++++++++
 1 file changed, 11 insertions(+)

--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -365,6 +365,17 @@
 			#dma-cells = <2>;
 		};
 
+		nfc: nand@01c03000 {
+			compatible = "allwinner,sun4i-a10-nand";
+			reg = <0x01c03000 0x1000>;
+			interrupts = <37>;
+			clocks = <&ahb_gates 13>, <&nand_clk>;
+			clock-names = "ahb", "mod";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
 		spi0: spi@01c05000 {
 			compatible = "allwinner,sun4i-a10-spi";
 			reg = <0x01c05000 0x1000>;
