From a430fa942b3ff0e51f472e53110b7f6b16290295 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 30 Mar 2016 23:48:53 +0200
Subject: [PATCH 63/91] cpufreq: mediatek: add driver

Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/cpufreq/Kconfig.arm      |    9 +
 drivers/cpufreq/Makefile         |    1 +
 drivers/cpufreq/mt7623-cpufreq.c |  389 ++++++++++++++++++++++++++++++++++++++
 3 files changed, 399 insertions(+)
 create mode 100644 drivers/cpufreq/mt7623-cpufreq.c

diff --git a/drivers/cpufreq/Kconfig.arm b/drivers/cpufreq/Kconfig.arm
index b1f8a73..baf945e 100644
--- a/drivers/cpufreq/Kconfig.arm
+++ b/drivers/cpufreq/Kconfig.arm
@@ -81,6 +81,15 @@ config ARM_KIRKWOOD_CPUFREQ
 	  This adds the CPUFreq driver for Marvell Kirkwood
 	  SoCs.
 
+config ARM_MT7623_CPUFREQ
+	bool "Mediatek MT7623 CPUFreq support"
+	depends on ARCH_MEDIATEK && REGULATOR
+	depends on ARM || (ARM_CPU_TOPOLOGY && COMPILE_TEST)
+	depends on !CPU_THERMAL || THERMAL=y
+	select PM_OPP
+	help
+	  This adds the CPUFreq driver support for Mediatek MT7623 SoC.
+
 config ARM_MT8173_CPUFREQ
 	bool "Mediatek MT8173 CPUFreq support"
 	depends on ARCH_MEDIATEK && REGULATOR
diff --git a/drivers/cpufreq/Makefile b/drivers/cpufreq/Makefile
index c0af1a1..e198752 100644
--- a/drivers/cpufreq/Makefile
+++ b/drivers/cpufreq/Makefile
@@ -57,6 +57,7 @@ obj-$(CONFIG_ARM_HISI_ACPU_CPUFREQ)	+= hisi-acpu-cpufreq.o
 obj-$(CONFIG_ARM_IMX6Q_CPUFREQ)		+= imx6q-cpufreq.o
 obj-$(CONFIG_ARM_INTEGRATOR)		+= integrator-cpufreq.o
 obj-$(CONFIG_ARM_KIRKWOOD_CPUFREQ)	+= kirkwood-cpufreq.o
+obj-$(CONFIG_ARM_MT7623_CPUFREQ)	+= mt7623-cpufreq.o
 obj-$(CONFIG_ARM_MT8173_CPUFREQ)	+= mt8173-cpufreq.o
 obj-$(CONFIG_ARM_OMAP2PLUS_CPUFREQ)	+= omap-cpufreq.o
 obj-$(CONFIG_ARM_PXA2xx_CPUFREQ)	+= pxa2xx-cpufreq.o
diff --git a/drivers/cpufreq/mt7623-cpufreq.c b/drivers/cpufreq/mt7623-cpufreq.c
new file mode 100644
index 0000000..8d154ce
--- /dev/null
+++ b/drivers/cpufreq/mt7623-cpufreq.c
@@ -0,0 +1,389 @@
+/*
+ * Copyright (c) 2015 Linaro Ltd.
+ * Author: Pi-Cheng Chen <pi-cheng.chen@linaro.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+
+#include <linux/clk.h>
+#include <linux/cpu.h>
+#include <linux/cpu_cooling.h>
+#include <linux/cpufreq.h>
+#include <linux/cpumask.h>
+#include <linux/of.h>
+#include <linux/platform_device.h>
+#include <linux/pm_opp.h>
+#include <linux/regulator/consumer.h>
+#include <linux/slab.h>
+#include <linux/thermal.h>
+
+#define VOLT_TOL		(10000)
+
+/*
+ * When scaling the clock frequency of a CPU clock domain, the clock source
+ * needs to be switched to another stable PLL clock temporarily until
+ * the original PLL becomes stable at target frequency.
+ */
+struct mtk_cpu_dvfs_info {
+	struct device *cpu_dev;
+	struct regulator *proc_reg;
+	struct clk *cpu_clk;
+	struct clk *inter_clk;
+	struct thermal_cooling_device *cdev;
+	int intermediate_voltage;
+};
+
+static int mtk_cpufreq_set_voltage(struct mtk_cpu_dvfs_info *info, int vproc)
+{
+	return regulator_set_voltage(info->proc_reg, vproc,
+				     vproc + VOLT_TOL);
+}
+
+static int mtk_cpufreq_set_target(struct cpufreq_policy *policy,
+				  unsigned int index)
+{
+	struct cpufreq_frequency_table *freq_table = policy->freq_table;
+	struct clk *cpu_clk = policy->clk;
+	struct clk *armpll = clk_get_parent(cpu_clk);
+	struct mtk_cpu_dvfs_info *info = policy->driver_data;
+	struct device *cpu_dev = info->cpu_dev;
+	struct dev_pm_opp *opp;
+	long freq_hz, old_freq_hz;
+	int vproc, old_vproc, inter_vproc, target_vproc, ret;
+
+	inter_vproc = info->intermediate_voltage;
+
+	old_freq_hz = clk_get_rate(cpu_clk);
+	old_vproc = regulator_get_voltage(info->proc_reg);
+
+	freq_hz = freq_table[index].frequency * 1000;
+
+	rcu_read_lock();
+	opp = dev_pm_opp_find_freq_ceil(cpu_dev, &freq_hz);
+	if (IS_ERR(opp)) {
+		rcu_read_unlock();
+		pr_err("cpu%d: failed to find OPP for %ld\n",
+		       policy->cpu, freq_hz);
+		return PTR_ERR(opp);
+	}
+	vproc = dev_pm_opp_get_voltage(opp);
+	rcu_read_unlock();
+
+	/*
+	 * If the new voltage or the intermediate voltage is higher than the
+	 * current voltage, scale up voltage first.
+	 */
+	target_vproc = (inter_vproc > vproc) ? inter_vproc : vproc;
+	if (old_vproc < target_vproc) {
+		ret = mtk_cpufreq_set_voltage(info, target_vproc);
+		if (ret) {
+			pr_err("cpu%d: failed to scale up voltage!\n",
+			       policy->cpu);
+			mtk_cpufreq_set_voltage(info, old_vproc);
+			return ret;
+		}
+	}
+
+	/* Reparent the CPU clock to intermediate clock. */
+	ret = clk_set_parent(cpu_clk, info->inter_clk);
+	if (ret) {
+		pr_err("cpu%d: failed to re-parent cpu clock!\n",
+		       policy->cpu);
+		mtk_cpufreq_set_voltage(info, old_vproc);
+		WARN_ON(1);
+		return ret;
+	}
+
+	/* Set the original PLL to target rate. */
+	ret = clk_set_rate(armpll, freq_hz);
+	if (ret) {
+		pr_err("cpu%d: failed to scale cpu clock rate!\n",
+		       policy->cpu);
+		clk_set_parent(cpu_clk, armpll);
+		mtk_cpufreq_set_voltage(info, old_vproc);
+		return ret;
+	}
+
+	/* Set parent of CPU clock back to the original PLL. */
+	ret = clk_set_parent(cpu_clk, armpll);
+	if (ret) {
+		pr_err("cpu%d: failed to re-parent cpu clock!\n",
+		       policy->cpu);
+		mtk_cpufreq_set_voltage(info, inter_vproc);
+		WARN_ON(1);
+		return ret;
+	}
+
+	/*
+	 * If the new voltage is lower than the intermediate voltage or the
+	 * original voltage, scale down to the new voltage.
+	 */
+	if (vproc < inter_vproc || vproc < old_vproc) {
+		ret = mtk_cpufreq_set_voltage(info, vproc);
+		if (ret) {
+			pr_err("cpu%d: failed to scale down voltage!\n",
+			       policy->cpu);
+			clk_set_parent(cpu_clk, info->inter_clk);
+			clk_set_rate(armpll, old_freq_hz);
+			clk_set_parent(cpu_clk, armpll);
+			return ret;
+		}
+	}
+
+	return 0;
+}
+
+static void mtk_cpufreq_ready(struct cpufreq_policy *policy)
+{
+	struct mtk_cpu_dvfs_info *info = policy->driver_data;
+	struct device_node *np = of_node_get(info->cpu_dev->of_node);
+
+	if (WARN_ON(!np))
+		return;
+
+	if (of_find_property(np, "#cooling-cells", NULL)) {
+		info->cdev = of_cpufreq_cooling_register(np,
+							 policy->related_cpus);
+
+		if (IS_ERR(info->cdev)) {
+			dev_err(info->cpu_dev,
+				"running cpufreq without cooling device: %ld\n",
+				PTR_ERR(info->cdev));
+
+			info->cdev = NULL;
+		}
+	}
+
+	of_node_put(np);
+}
+
+static int mtk_cpu_dvfs_info_init(struct mtk_cpu_dvfs_info *info, int cpu)
+{
+	struct device *cpu_dev;
+	struct regulator *proc_reg = ERR_PTR(-ENODEV);
+	struct clk *cpu_clk = ERR_PTR(-ENODEV);
+	struct clk *inter_clk = ERR_PTR(-ENODEV);
+	struct dev_pm_opp *opp;
+	unsigned long rate;
+	int ret;
+
+	cpu_dev = get_cpu_device(cpu);
+	if (!cpu_dev) {
+		pr_err("failed to get cpu%d device\n", cpu);
+		return -ENODEV;
+	}
+
+	cpu_clk = clk_get(cpu_dev, "cpu");
+	if (IS_ERR(cpu_clk)) {
+		if (PTR_ERR(cpu_clk) == -EPROBE_DEFER)
+			pr_warn("cpu clk for cpu%d not ready, retry.\n", cpu);
+		else
+			pr_err("failed to get cpu clk for cpu%d\n", cpu);
+
+		ret = PTR_ERR(cpu_clk);
+		return ret;
+	}
+
+	inter_clk = clk_get(cpu_dev, "intermediate");
+	if (IS_ERR(inter_clk)) {
+		if (PTR_ERR(inter_clk) == -EPROBE_DEFER)
+			pr_warn("intermediate clk for cpu%d not ready, retry.\n",
+				cpu);
+		else
+			pr_err("failed to get intermediate clk for cpu%d\n",
+			       cpu);
+
+		ret = PTR_ERR(inter_clk);
+		goto out_free_resources;
+	}
+
+	proc_reg = regulator_get_exclusive(cpu_dev, "proc");
+	if (IS_ERR(proc_reg)) {
+		if (PTR_ERR(proc_reg) == -EPROBE_DEFER)
+			pr_warn("proc regulator for cpu%d not ready, retry.\n",
+				cpu);
+		else
+			pr_err("failed to get proc regulator for cpu%d\n",
+			       cpu);
+
+		ret = PTR_ERR(proc_reg);
+		goto out_free_resources;
+	}
+
+	ret = dev_pm_opp_of_add_table(cpu_dev);
+	if (ret) {
+		pr_warn("no OPP table for cpu%d\n", cpu);
+		goto out_free_resources;
+	}
+
+	/* Search a safe voltage for intermediate frequency. */
+	rate = clk_get_rate(inter_clk);
+	rcu_read_lock();
+	opp = dev_pm_opp_find_freq_ceil(cpu_dev, &rate);
+	if (IS_ERR(opp)) {
+		rcu_read_unlock();
+		pr_err("failed to get intermediate opp for cpu%d\n", cpu);
+		ret = PTR_ERR(opp);
+		goto out_free_opp_table;
+	}
+	info->intermediate_voltage = dev_pm_opp_get_voltage(opp);
+	rcu_read_unlock();
+
+	info->cpu_dev = cpu_dev;
+	info->proc_reg = proc_reg;
+	info->cpu_clk = cpu_clk;
+	info->inter_clk = inter_clk;
+
+	return 0;
+
+out_free_opp_table:
+	dev_pm_opp_of_remove_table(cpu_dev);
+
+out_free_resources:
+	if (!IS_ERR(proc_reg))
+		regulator_put(proc_reg);
+	if (!IS_ERR(cpu_clk))
+		clk_put(cpu_clk);
+	if (!IS_ERR(inter_clk))
+		clk_put(inter_clk);
+
+	return ret;
+}
+
+static void mtk_cpu_dvfs_info_release(struct mtk_cpu_dvfs_info *info)
+{
+	if (!IS_ERR(info->proc_reg))
+		regulator_put(info->proc_reg);
+	if (!IS_ERR(info->cpu_clk))
+		clk_put(info->cpu_clk);
+	if (!IS_ERR(info->inter_clk))
+		clk_put(info->inter_clk);
+
+	dev_pm_opp_of_remove_table(info->cpu_dev);
+}
+
+static int mtk_cpufreq_init(struct cpufreq_policy *policy)
+{
+	struct mtk_cpu_dvfs_info *info;
+	struct cpufreq_frequency_table *freq_table;
+	int ret;
+
+	info = kzalloc(sizeof(*info), GFP_KERNEL);
+	if (!info)
+		return -ENOMEM;
+
+	ret = mtk_cpu_dvfs_info_init(info, policy->cpu);
+	if (ret) {
+		pr_err("%s failed to initialize dvfs info for cpu%d\n",
+		       __func__, policy->cpu);
+		goto out_free_dvfs_info;
+	}
+
+	ret = dev_pm_opp_init_cpufreq_table(info->cpu_dev, &freq_table);
+	if (ret) {
+		pr_err("failed to init cpufreq table for cpu%d: %d\n",
+		       policy->cpu, ret);
+		goto out_release_dvfs_info;
+	}
+
+	ret = cpufreq_table_validate_and_show(policy, freq_table);
+	if (ret) {
+		pr_err("%s: invalid frequency table: %d\n", __func__, ret);
+		goto out_free_cpufreq_table;
+	}
+
+	/* CPUs in the same cluster share a clock and power domain. */
+	cpumask_setall(policy->cpus);
+	policy->driver_data = info;
+	policy->clk = info->cpu_clk;
+
+	return 0;
+
+out_free_cpufreq_table:
+	dev_pm_opp_free_cpufreq_table(info->cpu_dev, &freq_table);
+
+out_release_dvfs_info:
+	mtk_cpu_dvfs_info_release(info);
+
+out_free_dvfs_info:
+	kfree(info);
+
+	return ret;
+}
+
+static int mtk_cpufreq_exit(struct cpufreq_policy *policy)
+{
+	struct mtk_cpu_dvfs_info *info = policy->driver_data;
+
+	cpufreq_cooling_unregister(info->cdev);
+	dev_pm_opp_free_cpufreq_table(info->cpu_dev, &policy->freq_table);
+	mtk_cpu_dvfs_info_release(info);
+	kfree(info);
+
+	return 0;
+}
+
+static struct cpufreq_driver mt7623_cpufreq_driver = {
+	.flags = CPUFREQ_STICKY | CPUFREQ_NEED_INITIAL_FREQ_CHECK,
+	.verify = cpufreq_generic_frequency_table_verify,
+	.target_index = mtk_cpufreq_set_target,
+	.get = cpufreq_generic_get,
+	.init = mtk_cpufreq_init,
+	.exit = mtk_cpufreq_exit,
+	.ready = mtk_cpufreq_ready,
+	.name = "mtk-cpufreq",
+	.attr = cpufreq_generic_attr,
+};
+
+static int mt7623_cpufreq_probe(struct platform_device *pdev)
+{
+	int ret;
+
+	ret = cpufreq_register_driver(&mt7623_cpufreq_driver);
+	if (ret)
+		pr_err("failed to register mtk cpufreq driver\n");
+
+	return ret;
+}
+
+static struct platform_driver mt7623_cpufreq_platdrv = {
+	.driver = {
+		.name	= "mt7623-cpufreq",
+	},
+	.probe		= mt7623_cpufreq_probe,
+};
+
+static int mt7623_cpufreq_driver_init(void)
+{
+	struct platform_device *pdev;
+	int err;
+
+	if (!of_machine_is_compatible("mediatek,mt7623"))
+		return -ENODEV;
+
+	err = platform_driver_register(&mt7623_cpufreq_platdrv);
+	if (err)
+		return err;
+
+	/*
+	 * Since there's no place to hold device registration code and no
+	 * device tree based way to match cpufreq driver yet, both the driver
+	 * and the device registration codes are put here to handle defer
+	 * probing.
+	 */
+	pdev = platform_device_register_simple("mt7623-cpufreq", -1, NULL, 0);
+	if (IS_ERR(pdev)) {
+		pr_err("failed to register mtk-cpufreq platform device\n");
+		return PTR_ERR(pdev);
+	}
+
+	return 0;
+}
+device_initcall(mt7623_cpufreq_driver_init);
-- 
1.7.10.4

