From 504dba5b073a9009ae1e3f2fc53ea9c3aa10c38a Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@openwrt.org>
Date: Wed, 13 May 2015 20:56:38 +0200
Subject: [PATCH] ARM: BCM5301X: Add Buffalo WXR-1900DHP clock and USB power
 control
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts | 17 +++++++++++++++++
 1 file changed, 17 insertions(+)

--- a/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
+++ b/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
@@ -24,6 +24,23 @@
 		reg = <0x00000000 0x08000000>;
 	};
 
+	clocks {
+		clk_periph: periph {
+			clock-frequency = <500000000>;
+		};
+	};
+
+	axi@18000000 {
+		usb2@21000 {
+			reg = <0x00021000 0x1000>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			vcc-gpio = <&chipcommon 13 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
