From 842f2d4df49fccc31424f9bc6bcc45d1e1d2fda7 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Mon, 1 Feb 2016 12:37:00 +0100
Subject: [PATCH] ARM: BCM5301X: Fix NAND flash parameters for D-Link DIR-885L
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

It doesn't use 8-bit ECC strength.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts | 6 +++++-
 1 file changed, 5 insertions(+), 1 deletion(-)

--- a/arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts
+++ b/arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts
@@ -10,7 +10,6 @@
 /dts-v1/;
 
 #include "bcm4708.dtsi"
-#include "bcm5301x-nand-cs0-bch8.dtsi"
 
 / {
 	compatible = "dlink,dir-885l", "brcm,bcm47094", "brcm,bcm4708";
@@ -27,6 +26,13 @@
 
 	nand: nand@18028000 {
 		nandcs@0 {
+			compatible = "brcm,nandcs";
+			reg = <0>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			linux,part-probe = "ofpart", "bcm47xxpart";
+
 			partition@0 {
 				label = "firmware";
 				reg = <0x00000000 0x08000000>;
