--- a/drivers/mtd/spi-nor/Kconfig
+++ b/drivers/mtd/spi-nor/Kconfig
@@ -41,4 +41,10 @@ config SPI_NXP_SPIFI
 	  Flash. Enable this option if you have a device with a SPIFI
 	  controller and want to access the Flash as a mtd device.
 
+config MTD_SPI_BCM53XXSPIFLASH
+	tristate "SPI-NOR flashes connected to the Broadcom ARM SoC"
+	depends on MTD_SPI_NOR
+	help
+	  SPI driver for flashes used on Broadcom ARM SoCs.
+
 endif # MTD_SPI_NOR
--- a/drivers/mtd/spi-nor/Makefile
+++ b/drivers/mtd/spi-nor/Makefile
@@ -1,3 +1,4 @@
 obj-$(CONFIG_MTD_SPI_NOR)	+= spi-nor.o
 obj-$(CONFIG_SPI_FSL_QUADSPI)	+= fsl-quadspi.o
+obj-$(CONFIG_MTD_SPI_BCM53XXSPIFLASH)	+= bcm53xxspiflash.o
 obj-$(CONFIG_SPI_NXP_SPIFI)	+= nxp-spifi.o
