From 65f0d87a26f7cec860b89b40eebc48a4eb71acf8 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 11 Apr 2016 06:00:23 +0200
Subject: [PATCH 90/91] net: mediatek: v4.4 backports

---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |   23 ++++++++++++++---------
 1 file changed, 14 insertions(+), 9 deletions(-)

diff --git a/drivers/net/ethernet/mediatek/mtk_eth_soc.c b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
index eee4324a..b466f45 100644
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -207,7 +207,7 @@ static int mtk_phy_connect_node(struct mtk_eth *eth, struct mtk_mac *mac,
 
 	dev_info(eth->dev,
 		 "connected mac %d to PHY at %s [uid=%08x, driver=%s]\n",
-		 mac->id, phydev_name(phydev), phydev->phy_id,
+		 mac->id, dev_name(&phydev->dev), phydev->phy_id,
 		 phydev->drv->name);
 
 	mac->phy_dev = phydev;
@@ -1267,9 +1267,10 @@ static irqreturn_t mtk_handle_irq_rx(int irq, void *_eth)
 		return IRQ_NONE;
 
 	if (status & MTK_RX_DONE_INT) {
-		if (likely(napi_schedule_prep(&eth->rx_napi)))
+		if (likely(napi_schedule_prep(&eth->rx_napi))) {
+			mtk_irq_disable(eth, MTK_RX_DONE_INT);
 			__napi_schedule(&eth->rx_napi);
-		mtk_irq_disable(eth, MTK_RX_DONE_INT);
+		}
 	}
 	mtk_w32(eth, status, MTK_QMTK_INT_STATUS);
 
@@ -1288,9 +1289,10 @@ static irqreturn_t mtk_handle_irq_tx(int irq, void *_eth)
 		return IRQ_NONE;
 
 	if (status & MTK_TX_DONE_INT) {
-		if (likely(napi_schedule_prep(&eth->tx_napi)))
+		if (likely(napi_schedule_prep(&eth->tx_napi))) {
+			mtk_irq_disable(eth, MTK_TX_DONE_INT);
 			__napi_schedule(&eth->tx_napi);
-		mtk_irq_disable(eth, MTK_TX_DONE_INT);
+		}
 	}
 	mtk_w32(eth, status, MTK_QMTK_INT_STATUS);
 
@@ -1382,6 +1384,7 @@ static int mtk_stop(struct net_device *dev)
 	struct mtk_mac *mac = netdev_priv(dev);
 	struct mtk_eth *eth = mac->hw;
 
+	netif_carrier_off(dev);
 	netif_tx_disable(dev);
 	phy_stop(mac->phy_dev);
 
@@ -1581,11 +1584,13 @@ static int mtk_set_settings(struct net_device *dev,
 {
 	struct mtk_mac *mac = netdev_priv(dev);
 
-	if (cmd->phy_address != mac->phy_dev->mdio.addr) {
-		mac->phy_dev = mdiobus_get_phy(mac->hw->mii_bus,
-					       cmd->phy_address);
-		if (!mac->phy_dev)
+	if (cmd->phy_address != mac->phy_dev->addr) {
+		if (mac->hw->mii_bus->phy_map[cmd->phy_address]) {
+			mac->phy_dev =
+				mac->hw->mii_bus->phy_map[cmd->phy_address];
+		} else {
 			return -ENODEV;
+		}
 	}
 
 	return phy_ethtool_sset(mac->phy_dev, cmd);
-- 
1.7.10.4

