From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sat, 2 Jan 2016 11:26:28 +0100
Subject: [PATCH] USB: bcma: use simpler devm_gpiod_get
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 drivers/usb/host/bcma-hcd.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/drivers/usb/host/bcma-hcd.c
+++ b/drivers/usb/host/bcma-hcd.c
@@ -519,8 +519,7 @@ static int bcma_hcd_probe(struct bcma_de
 	usb_dev->core = core;
 
 	if (core->dev.of_node)
-		usb_dev->gpio_desc = devm_get_gpiod_from_child(&core->dev, "vcc",
-							       &core->dev.of_node->fwnode);
+		usb_dev->gpio_desc = devm_gpiod_get(&core->dev, "vcc", 0);
 	if (!IS_ERR_OR_NULL(usb_dev->gpio_desc))
 		gpiod_direction_output(usb_dev->gpio_desc, 1);
 
