--- a/arch/arm/boot/dts/imx23.dtsi
+++ b/arch/arm/boot/dts/imx23.dtsi
@@ -404,8 +404,46 @@
 			};
 
 			power@80044000 {
+				compatible = "fsl,imx23-power", "syscon";
 				reg = <0x80044000 0x2000>;
-				status = "disabled";
+				interrupts = <3>;
+
+				dcdc: regulator@1 {
+					compatible = "fsl,imx23-dcdc";
+					regulator-name = "dcdc";
+					regulator-boot-on;
+					regulator-always-on;
+				};
+
+				reg_vddd: regulator@2 {
+					compatible = "fsl,imx23-vddd";
+					regulator-name = "vddd";
+					regulator-min-microvolt = <1350000>;
+					regulator-max-microvolt = <1550000>;
+					vddd-supply = <&reg_vdda>;
+					regulator-boot-on;
+					regulator-always-on;
+				};
+
+				reg_vdda: regulator@3 {
+					compatible = "fsl,imx23-vdda";
+					regulator-name = "vdda";
+					regulator-min-microvolt = <1725000>;
+					regulator-max-microvolt = <1950000>;
+					vdda-supply = <&reg_vddio>;
+					regulator-boot-on;
+					regulator-always-on;
+				};
+
+				reg_vddio: regulator@4 {
+					compatible = "fsl,imx23-vddio";
+					regulator-name = "vddio";
+					regulator-min-microvolt = <3000000>;
+					regulator-max-microvolt = <3575000>;
+					regulator-microvolt-offset = <80000>;
+					regulator-boot-on;
+					regulator-always-on;
+				};
 			};
 
 			saif1: saif@80046000 {
--- a/arch/arm/boot/dts/imx28.dtsi
+++ b/arch/arm/boot/dts/imx28.dtsi
@@ -1035,8 +1035,46 @@
 			};
 
 			power: power@80044000 {
+				compatible = "fsl,imx28-power", "syscon";
 				reg = <0x80044000 0x2000>;
-				status = "disabled";
+				interrupts = <6>;
+
+				dcdc: regulator@1 {
+					compatible = "fsl,imx28-dcdc";
+					regulator-name = "dcdc";
+					regulator-boot-on;
+					regulator-always-on;
+				};
+
+				reg_vddd: regulator@2 {
+					compatible = "fsl,imx28-vddd";
+					regulator-name = "vddd";
+					regulator-min-microvolt = <1350000>;
+					regulator-max-microvolt = <1550000>;
+					vddd-supply = <&reg_vdda>;
+					regulator-boot-on;
+					regulator-always-on;
+				};
+
+				reg_vdda: regulator@3 {
+					compatible = "fsl,imx28-vdda";
+					regulator-name = "vdda";
+					regulator-min-microvolt = <1725000>;
+					regulator-max-microvolt = <1950000>;
+					vdda-supply = <&reg_vddio>;
+					regulator-boot-on;
+					regulator-always-on;
+				};
+
+				reg_vddio: regulator@4 {
+					compatible = "fsl,imx28-vddio";
+					regulator-name = "vddio";
+					regulator-min-microvolt = <3000000>;
+					regulator-max-microvolt = <3550000>;
+					regulator-microvolt-offset = <80000>;
+					regulator-boot-on;
+					regulator-always-on;
+				};
 			};
 
 			saif1: saif@80046000 {
