From d32795d2be55748552ddacd9b1e47efc61264a98 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 8 Feb 2016 12:53:44 +0000
Subject: [PATCH 146/170] FIXUP: Overlay README - Restore spaces deleted in
 error

---
 arch/arm/boot/dts/overlays/README | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -550,7 +550,7 @@ Info:   Configures a single PWM channel
              Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
           2) The onboard analogue audio output uses both PWM channels.
           3) So be careful mixing audio and PWM.
-          4) Currently the clockmust have been enabled and configured
+          4) Currently the clock must have been enabled and configured
              by other means.
 Load:   dtoverlay=pwm,<param>=<val>
 Params: pin                     Output pin (default 18) - see table
@@ -569,7 +569,7 @@ Info:   Configures both PWM channels
              Pins 12 and 13 might be better choices on an A+, B+ or Pi2.
           2) The onboard analogue audio output uses both PWM channels.
           3) So be careful mixing audio and PWM.
-          4) Currently the clockmust have been enabled and configured
+          4) Currently the clock must have been enabled and configured
              by other means.
 Load:   dtoverlay=pwm-2chan,<param>=<val>
 Params: pin                     Output pin (default 18) - see table
@@ -753,7 +753,7 @@ Params: <None>
 
 Name:   vga666
 Info:   Overlay for the Fen Logic VGA666 board
-        This uses GPIOs 2-21 (sono I2C), and activates the output 2-3 seconds
+        This uses GPIOs 2-21 (so no I2C), and activates the output 2-3 seconds
         after the kernel has started.
 Load:   dtoverlay=vga666
 Params: <None>
