From e16393b2c78cc95ec124a46e8da8cfb2af333f00 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 20 Jan 2016 10:54:18 +0100
Subject: [PATCH 38/91] soc: mediatek: PMIC wrap: remove pwrap_is_mt8135() and
 pwrap_is_mt8173()

With more SoCs being added the list of helper functions like these would
grow. To mitigate this problem we remove the existing helpers and change
the code to test against the pmic type stored inside the pmic specific
datastructure that our context structure points at. There is one usage of
pwrap_is_mt8135() that is ambiguous as the test should not be dependent on
mt8135, but rather on the existence of a bridge. Add a new element to
pmic_wrapper_type to indicate if a bridge is present and use this where
appropriate.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/soc/mediatek/mtk-pmic-wrap.c |   28 ++++++++++++----------------
 1 file changed, 12 insertions(+), 16 deletions(-)

diff --git a/drivers/soc/mediatek/mtk-pmic-wrap.c b/drivers/soc/mediatek/mtk-pmic-wrap.c
index aa54df3..a2bacda 100644
--- a/drivers/soc/mediatek/mtk-pmic-wrap.c
+++ b/drivers/soc/mediatek/mtk-pmic-wrap.c
@@ -374,20 +374,11 @@ struct pmic_wrapper_type {
 	u32 int_en_all;
 	u32 spi_w;
 	u32 wdt_src;
+	int has_bridge:1;
 	int (*init_reg_clock)(struct pmic_wrapper *wrp);
 	int (*init_soc_specific)(struct pmic_wrapper *wrp);
 };
 
-static inline int pwrap_is_mt8135(struct pmic_wrapper *wrp)
-{
-	return wrp->master->type == PWRAP_MT8135;
-}
-
-static inline int pwrap_is_mt8173(struct pmic_wrapper *wrp)
-{
-	return wrp->master->type == PWRAP_MT8173;
-}
-
 static u32 pwrap_readl(struct pmic_wrapper *wrp, enum pwrap_regs reg)
 {
 	return readl(wrp->base + wrp->master->regs[reg]);
@@ -619,11 +610,14 @@ static int pwrap_init_cipher(struct pmic_wrapper *wrp)
 	pwrap_writel(wrp, 0x1, PWRAP_CIPHER_KEY_SEL);
 	pwrap_writel(wrp, 0x2, PWRAP_CIPHER_IV_SEL);
 
-	if (pwrap_is_mt8135(wrp)) {
+	switch (wrp->master->type) {
+	case PWRAP_MT8135:
 		pwrap_writel(wrp, 1, PWRAP_CIPHER_LOAD);
 		pwrap_writel(wrp, 1, PWRAP_CIPHER_START);
-	} else {
+		break;
+	case PWRAP_MT8173:
 		pwrap_writel(wrp, 1, PWRAP_CIPHER_EN);
+		break;
 	}
 
 	/* Config cipher mode @PMIC */
@@ -713,7 +707,7 @@ static int pwrap_init(struct pmic_wrapper *wrp)
 	if (wrp->rstc_bridge)
 		reset_control_reset(wrp->rstc_bridge);
 
-	if (pwrap_is_mt8173(wrp)) {
+	if (wrp->master->type == PWRAP_MT8173) {
 		/* Enable DCM */
 		pwrap_writel(wrp, 3, PWRAP_DCM_EN);
 		pwrap_writel(wrp, 0, PWRAP_DCM_DBC_PRD);
@@ -773,7 +767,7 @@ static int pwrap_init(struct pmic_wrapper *wrp)
 	pwrap_writel(wrp, PWRAP_DEW_CRC_VAL, PWRAP_SIG_ADR);
 	pwrap_writel(wrp, wrp->master->arb_en_all, PWRAP_HIPRIO_ARB_EN);
 
-	if (pwrap_is_mt8135(wrp))
+	if (wrp->master->type == PWRAP_MT8135)
 		pwrap_writel(wrp, 0x7, PWRAP_RRARB_EN);
 
 	pwrap_writel(wrp, 0x1, PWRAP_WACS0_EN);
@@ -793,7 +787,7 @@ static int pwrap_init(struct pmic_wrapper *wrp)
 	pwrap_writel(wrp, 1, PWRAP_INIT_DONE0);
 	pwrap_writel(wrp, 1, PWRAP_INIT_DONE1);
 
-	if (pwrap_is_mt8135(wrp)) {
+	if (wrp->master->has_bridge) {
 		writel(1, wrp->bridge_base + PWRAP_MT8135_BRIDGE_INIT_DONE3);
 		writel(1, wrp->bridge_base + PWRAP_MT8135_BRIDGE_INIT_DONE4);
 	}
@@ -831,6 +825,7 @@ static struct pmic_wrapper_type pwrap_mt8135 = {
 	.int_en_all = ~(BIT(31) | BIT(1)),
 	.spi_w = PWRAP_MAN_CMD_SPI_WRITE,
 	.wdt_src = PWRAP_WDT_SRC_MASK_ALL,
+	.has_bridge = 1,
 	.init_reg_clock = pwrap_mt8135_init_reg_clock,
 	.init_soc_specific = pwrap_mt8135_init_soc_specific,
 };
@@ -842,6 +837,7 @@ static struct pmic_wrapper_type pwrap_mt8173 = {
 	.int_en_all = ~(BIT(31) | BIT(1)),
 	.spi_w = PWRAP_MAN_CMD_SPI_WRITE,
 	.wdt_src = PWRAP_WDT_SRC_MASK_NO_STAUPD,
+	.has_bridge = 0,
 	.init_reg_clock = pwrap_mt8173_init_reg_clock,
 	.init_soc_specific = pwrap_mt8173_init_soc_specific,
 };
@@ -889,7 +885,7 @@ static int pwrap_probe(struct platform_device *pdev)
 		return ret;
 	}
 
-	if (pwrap_is_mt8135(wrp)) {
+	if (wrp->master->has_bridge) {
 		res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
 				"pwrap-bridge");
 		wrp->bridge_base = devm_ioremap_resource(wrp->dev, res);
-- 
1.7.10.4

