--- a/drivers/mtd/nand/nand_base.c
+++ b/drivers/mtd/nand/nand_base.c
@@ -4249,6 +4249,8 @@ static inline bool is_full_id_nand(struc
 static bool find_full_id_nand(struct mtd_info *mtd, struct nand_chip *chip,
 		   struct nand_flash_dev *type, const u8 *id_data, int *busw)
 {
+	int mode;
+
 	if (!strncmp(type->id, id_data, type->id_len)) {
 		mtd->writesize = type->pagesize;
 		mtd->erasesize = type->erasesize;
@@ -4259,8 +4261,9 @@ static bool find_full_id_nand(struct mtd
 		chip->options |= type->options;
 		chip->ecc_strength_ds = NAND_ECC_STRENGTH(type);
 		chip->ecc_step_ds = NAND_ECC_STEP(type);
-		chip->onfi_timing_mode_default =
-					type->onfi_timing_mode_default;
+
+		mode = type->onfi_timing_mode_default;
+		chip->sdr_timings = onfi_async_timing_mode_to_sdr_timings(mode);
 
 		*busw = type->options & NAND_BUSWIDTH_16;
 
--- a/drivers/mtd/nand/sunxi_nand.c
+++ b/drivers/mtd/nand/sunxi_nand.c
@@ -1425,7 +1425,7 @@ static int sunxi_nand_chip_init_timings(
 
 	mode = onfi_get_async_timing_mode(&chip->nand);
 	if (mode == ONFI_TIMING_MODE_UNKNOWN) {
-		mode = chip->nand.onfi_timing_mode_default;
+		timings = chip->nand.sdr_timings;
 	} else {
 		uint8_t feature[ONFI_SUBFEATURE_PARAM_LEN] = {};
 
@@ -1439,9 +1439,10 @@ static int sunxi_nand_chip_init_timings(
 						feature);
 		if (ret)
 			return ret;
+
+		timings = onfi_async_timing_mode_to_sdr_timings(mode);
 	}
 
-	timings = onfi_async_timing_mode_to_sdr_timings(mode);
 	if (IS_ERR(timings))
 		return PTR_ERR(timings);
 
--- a/include/linux/mtd/nand.h
+++ b/include/linux/mtd/nand.h
@@ -612,6 +612,55 @@ struct nand_buffers {
 	uint8_t *databuf;
 };
 
+/*
+ * struct nand_sdr_timings - SDR NAND chip timings
+ *
+ * This struct defines the timing requirements of a SDR NAND chip.
+ * These informations can be found in every NAND datasheets and the timings
+ * meaning are described in the ONFI specifications:
+ * www.onfi.org/~/media/ONFI/specs/onfi_3_1_spec.pdf (chapter 4.15 Timing
+ * Parameters)
+ *
+ * All these timings are expressed in picoseconds.
+ */
+
+struct nand_sdr_timings {
+	u32 tALH_min;
+	u32 tADL_min;
+	u32 tALS_min;
+	u32 tAR_min;
+	u32 tCEA_max;
+	u32 tCEH_min;
+	u32 tCH_min;
+	u32 tCHZ_max;
+	u32 tCLH_min;
+	u32 tCLR_min;
+	u32 tCLS_min;
+	u32 tCOH_min;
+	u32 tCS_min;
+	u32 tDH_min;
+	u32 tDS_min;
+	u32 tFEAT_max;
+	u32 tIR_min;
+	u32 tITC_max;
+	u32 tRC_min;
+	u32 tREA_max;
+	u32 tREH_min;
+	u32 tRHOH_min;
+	u32 tRHW_min;
+	u32 tRHZ_max;
+	u32 tRLOH_min;
+	u32 tRP_min;
+	u32 tRR_min;
+	u64 tRST_max;
+	u32 tWB_max;
+	u32 tWC_min;
+	u32 tWH_min;
+	u32 tWHR_min;
+	u32 tWP_min;
+	u32 tWW_min;
+};
+
 /**
  * struct nand_chip - NAND Private Flash Chip Data
  * @IO_ADDR_R:		[BOARDSPECIFIC] address to read the 8 I/O lines of the
@@ -676,11 +725,7 @@ struct nand_buffers {
  * @ecc_step_ds:	[INTERN] ECC step required by the @ecc_strength_ds,
  *                      also from the datasheet. It is the recommended ECC step
  *			size, if known; if unknown, set to zero.
- * @onfi_timing_mode_default: [INTERN] default ONFI timing mode. This field is
- *			      either deduced from the datasheet if the NAND
- *			      chip is not ONFI compliant or set to 0 if it is
- *			      (an ONFI chip is always configured in mode 0
- *			      after a NAND reset)
+ * @sdr_timings		[INTERN] Pointer to default timings for SDR NAND.
  * @numchips:		[INTERN] number of physical chips
  * @chipsize:		[INTERN] the size of one chip for multichip arrays
  * @pagemask:		[INTERN] page number mask = number of (pages / chip) - 1
@@ -769,7 +814,7 @@ struct nand_chip {
 	uint8_t bits_per_cell;
 	uint16_t ecc_strength_ds;
 	uint16_t ecc_step_ds;
-	int onfi_timing_mode_default;
+	const struct nand_sdr_timings *sdr_timings;
 	int badblockpos;
 	int badblockbits;
 
@@ -1156,55 +1201,6 @@ struct ofnandpart_data {
 int ofnandpart_parse(struct mtd_info *master,
 		     const struct ofnandpart_data *data);
 
-/*
- * struct nand_sdr_timings - SDR NAND chip timings
- *
- * This struct defines the timing requirements of a SDR NAND chip.
- * These informations can be found in every NAND datasheets and the timings
- * meaning are described in the ONFI specifications:
- * www.onfi.org/~/media/ONFI/specs/onfi_3_1_spec.pdf (chapter 4.15 Timing
- * Parameters)
- *
- * All these timings are expressed in picoseconds.
- */
-
-struct nand_sdr_timings {
-	u32 tALH_min;
-	u32 tADL_min;
-	u32 tALS_min;
-	u32 tAR_min;
-	u32 tCEA_max;
-	u32 tCEH_min;
-	u32 tCH_min;
-	u32 tCHZ_max;
-	u32 tCLH_min;
-	u32 tCLR_min;
-	u32 tCLS_min;
-	u32 tCOH_min;
-	u32 tCS_min;
-	u32 tDH_min;
-	u32 tDS_min;
-	u32 tFEAT_max;
-	u32 tIR_min;
-	u32 tITC_max;
-	u32 tRC_min;
-	u32 tREA_max;
-	u32 tREH_min;
-	u32 tRHOH_min;
-	u32 tRHW_min;
-	u32 tRHZ_max;
-	u32 tRLOH_min;
-	u32 tRP_min;
-	u32 tRR_min;
-	u64 tRST_max;
-	u32 tWB_max;
-	u32 tWC_min;
-	u32 tWH_min;
-	u32 tWHR_min;
-	u32 tWP_min;
-	u32 tWW_min;
-};
-
 /* get timing characteristics from ONFI timing mode. */
 const struct nand_sdr_timings *onfi_async_timing_mode_to_sdr_timings(int mode);
 #endif /* __LINUX_MTD_NAND_H */
