From 592d94e0e580341fdcce975a97bebb90e71b38fc Mon Sep 17 00:00:00 2001
From: Arnd Bergmann <arnd@arndb.de>
Date: Mon, 14 Mar 2016 15:07:12 +0100
Subject: [PATCH 69/91] net: mediatek: check device_reset return code

The device_reset() function may fail, so we have to check
its return value, e.g. to make deferred probing work correctly.
gcc warns about it because of the warn_unused_result attribute:

drivers/net/ethernet/mediatek/mtk_eth_soc.c: In function 'mtk_probe':
drivers/net/ethernet/mediatek/mtk_eth_soc.c:1679:2: error: ignoring return value of 'device_reset', declared with attribute warn_unused_result [-Werror=unused-result]

This adds the trivial error check to propagate the return value
to the generic platform device probe code.

Signed-off-by: Arnd Bergmann <arnd@arndb.de>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |    4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

diff --git a/drivers/net/ethernet/mediatek/mtk_eth_soc.c b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
index fcd4ed7..7f2126b 100644
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -1678,7 +1678,9 @@ static int mtk_probe(struct platform_device *pdev)
 	struct mtk_eth *eth;
 	int err;
 
-	device_reset(&pdev->dev);
+	err = device_reset(&pdev->dev);
+	if (err)
+		return err;
 
 	match = of_match_device(of_mtk_match, &pdev->dev);
 	soc = (struct mtk_soc_data *)match->data;
-- 
1.7.10.4

