From 56b33ebf188a59d8307c3b748eccf8cda1062981 Mon Sep 17 00:00:00 2001
From: Dan Carpenter <dan.carpenter@oracle.com>
Date: Tue, 15 Mar 2016 10:18:49 +0300
Subject: [PATCH 65/91] net: mediatek: checking for IS_ERR() instead of NULL

of_phy_connect() returns NULL on error, it never returns error pointers.

Fixes: 656e705243fd ('net-next: mediatek: add support for MT7623 ethernet')
Signed-off-by: Dan Carpenter <dan.carpenter@oracle.com>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |    4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/net/ethernet/mediatek/mtk_eth_soc.c b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
index ba3afa5..9759fe5 100644
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -186,9 +186,9 @@ static int mtk_phy_connect_node(struct mtk_eth *eth, struct mtk_mac *mac,
 
 	phydev = of_phy_connect(eth->netdev[mac->id], phy_node,
 				mtk_phy_link_adjust, 0, phy_mode);
-	if (IS_ERR(phydev)) {
+	if (!phydev) {
 		dev_err(eth->dev, "could not connect to PHY\n");
-		return PTR_ERR(phydev);
+		return -ENODEV;
 	}
 
 	dev_info(eth->dev,
-- 
1.7.10.4

