From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Fri, 18 Dec 2015 07:51:08 +0100
Subject: [PATCH] Revert "bcma: switch GPIO portions to use GPIOLIB_IRQCHIP"
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This reverts commit 74f4e0cc61080f63f28e8d519bdf437957e64217.

On BCM47XX (MIPS) bcma_bus_get_host_dev returns NULL which results in:
[    0.157054] missing gpiochip .dev parent pointer
[    0.157287] bcma: bus0: Error registering GPIO driver: -22

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 drivers/bcma/Kconfig                        |  2 +-
 drivers/bcma/driver_gpio.c                  | 92 +++++++++++++++++++----------
 include/linux/bcma/bcma_driver_chipcommon.h |  1 +
 3 files changed, 64 insertions(+), 31 deletions(-)

--- a/drivers/bcma/Kconfig
+++ b/drivers/bcma/Kconfig
@@ -99,7 +99,7 @@ config BCMA_DRIVER_GMAC_CMN
 config BCMA_DRIVER_GPIO
 	bool "BCMA GPIO driver"
 	depends on BCMA && GPIOLIB
-	select GPIOLIB_IRQCHIP if BCMA_HOST_SOC
+	select IRQ_DOMAIN if BCMA_HOST_SOC
 	help
 	  Driver to provide access to the GPIO pins of the bcma bus.
 
--- a/drivers/bcma/driver_gpio.c
+++ b/drivers/bcma/driver_gpio.c
@@ -8,8 +8,10 @@
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
-#include <linux/gpio/driver.h>
+#include <linux/gpio.h>
+#include <linux/irq.h>
 #include <linux/interrupt.h>
+#include <linux/irqdomain.h>
 #include <linux/export.h>
 #include <linux/bcma/bcma.h>
 
@@ -77,11 +79,19 @@ static void bcma_gpio_free(struct gpio_c
 }
 
 #if IS_BUILTIN(CONFIG_BCM47XX) || IS_BUILTIN(CONFIG_ARCH_BCM_5301X)
+static int bcma_gpio_to_irq(struct gpio_chip *chip, unsigned gpio)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	if (cc->core->bus->hosttype == BCMA_HOSTTYPE_SOC)
+		return irq_find_mapping(cc->irq_domain, gpio);
+	else
+		return -EINVAL;
+}
 
 static void bcma_gpio_irq_unmask(struct irq_data *d)
 {
-	struct gpio_chip *gc = irq_data_get_irq_chip_data(d);
-	struct bcma_drv_cc *cc = bcma_gpio_get_cc(gc);
+	struct bcma_drv_cc *cc = irq_data_get_irq_chip_data(d);
 	int gpio = irqd_to_hwirq(d);
 	u32 val = bcma_chipco_gpio_in(cc, BIT(gpio));
 
@@ -91,8 +101,7 @@ static void bcma_gpio_irq_unmask(struct
 
 static void bcma_gpio_irq_mask(struct irq_data *d)
 {
-	struct gpio_chip *gc = irq_data_get_irq_chip_data(d);
-	struct bcma_drv_cc *cc = bcma_gpio_get_cc(gc);
+	struct bcma_drv_cc *cc = irq_data_get_irq_chip_data(d);
 	int gpio = irqd_to_hwirq(d);
 
 	bcma_chipco_gpio_intmask(cc, BIT(gpio), 0);
@@ -107,7 +116,6 @@ static struct irq_chip bcma_gpio_irq_chi
 static irqreturn_t bcma_gpio_irq_handler(int irq, void *dev_id)
 {
 	struct bcma_drv_cc *cc = dev_id;
-	struct gpio_chip *gc = &cc->gpio;
 	u32 val = bcma_cc_read32(cc, BCMA_CC_GPIOIN);
 	u32 mask = bcma_cc_read32(cc, BCMA_CC_GPIOIRQ);
 	u32 pol = bcma_cc_read32(cc, BCMA_CC_GPIOPOL);
@@ -117,58 +125,81 @@ static irqreturn_t bcma_gpio_irq_handler
 	if (!irqs)
 		return IRQ_NONE;
 
-	for_each_set_bit(gpio, &irqs, gc->ngpio)
-		generic_handle_irq(irq_find_mapping(gc->irqdomain, gpio));
+	for_each_set_bit(gpio, &irqs, cc->gpio.ngpio)
+		generic_handle_irq(bcma_gpio_to_irq(&cc->gpio, gpio));
 	bcma_chipco_gpio_polarity(cc, irqs, val & irqs);
 
 	return IRQ_HANDLED;
 }
 
-static int bcma_gpio_irq_init(struct bcma_drv_cc *cc)
+static int bcma_gpio_irq_domain_init(struct bcma_drv_cc *cc)
 {
 	struct gpio_chip *chip = &cc->gpio;
-	int hwirq, err;
+	int gpio, hwirq, err;
 
 	if (cc->core->bus->hosttype != BCMA_HOSTTYPE_SOC)
 		return 0;
 
+	cc->irq_domain = irq_domain_add_linear(NULL, chip->ngpio,
+					       &irq_domain_simple_ops, cc);
+	if (!cc->irq_domain) {
+		err = -ENODEV;
+		goto err_irq_domain;
+	}
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_create_mapping(cc->irq_domain, gpio);
+
+		irq_set_chip_data(irq, cc);
+		irq_set_chip_and_handler(irq, &bcma_gpio_irq_chip,
+					 handle_simple_irq);
+	}
+
 	hwirq = bcma_core_irq(cc->core, 0);
 	err = request_irq(hwirq, bcma_gpio_irq_handler, IRQF_SHARED, "gpio",
 			  cc);
 	if (err)
-		return err;
+		goto err_req_irq;
 
 	bcma_chipco_gpio_intmask(cc, ~0, 0);
 	bcma_cc_set32(cc, BCMA_CC_IRQMASK, BCMA_CC_IRQ_GPIO);
 
-	err =  gpiochip_irqchip_add(chip,
-				    &bcma_gpio_irq_chip,
-				    0,
-				    handle_simple_irq,
-				    IRQ_TYPE_NONE);
-	if (err) {
-		free_irq(hwirq, cc);
-		return err;
-	}
-
 	return 0;
+
+err_req_irq:
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_find_mapping(cc->irq_domain, gpio);
+
+		irq_dispose_mapping(irq);
+	}
+	irq_domain_remove(cc->irq_domain);
+err_irq_domain:
+	return err;
 }
 
-static void bcma_gpio_irq_exit(struct bcma_drv_cc *cc)
+static void bcma_gpio_irq_domain_exit(struct bcma_drv_cc *cc)
 {
+	struct gpio_chip *chip = &cc->gpio;
+	int gpio;
+
 	if (cc->core->bus->hosttype != BCMA_HOSTTYPE_SOC)
 		return;
 
 	bcma_cc_mask32(cc, BCMA_CC_IRQMASK, ~BCMA_CC_IRQ_GPIO);
 	free_irq(bcma_core_irq(cc->core, 0), cc);
+	for (gpio = 0; gpio < chip->ngpio; gpio++) {
+		int irq = irq_find_mapping(cc->irq_domain, gpio);
+
+		irq_dispose_mapping(irq);
+	}
+	irq_domain_remove(cc->irq_domain);
 }
 #else
-static int bcma_gpio_irq_init(struct bcma_drv_cc *cc)
+static int bcma_gpio_irq_domain_init(struct bcma_drv_cc *cc)
 {
 	return 0;
 }
 
-static void bcma_gpio_irq_exit(struct bcma_drv_cc *cc)
+static void bcma_gpio_irq_domain_exit(struct bcma_drv_cc *cc)
 {
 }
 #endif
@@ -187,8 +218,9 @@ int bcma_gpio_init(struct bcma_drv_cc *c
 	chip->set		= bcma_gpio_set_value;
 	chip->direction_input	= bcma_gpio_direction_input;
 	chip->direction_output	= bcma_gpio_direction_output;
-	chip->owner		= THIS_MODULE;
-	chip->dev		= bcma_bus_get_host_dev(bus);
+#if IS_BUILTIN(CONFIG_BCM47XX) || IS_BUILTIN(CONFIG_ARCH_BCM_5301X)
+	chip->to_irq		= bcma_gpio_to_irq;
+#endif
 #if IS_BUILTIN(CONFIG_OF)
 	if (cc->core->bus->hosttype == BCMA_HOSTTYPE_SOC)
 		chip->of_node	= cc->core->dev.of_node;
@@ -217,13 +249,13 @@ int bcma_gpio_init(struct bcma_drv_cc *c
 	else
 		chip->base		= -1;
 
-	err = gpiochip_add(chip);
+	err = bcma_gpio_irq_domain_init(cc);
 	if (err)
 		return err;
 
-	err = bcma_gpio_irq_init(cc);
+	err = gpiochip_add(chip);
 	if (err) {
-		gpiochip_remove(chip);
+		bcma_gpio_irq_domain_exit(cc);
 		return err;
 	}
 
@@ -232,7 +264,7 @@ int bcma_gpio_init(struct bcma_drv_cc *c
 
 int bcma_gpio_unregister(struct bcma_drv_cc *cc)
 {
-	bcma_gpio_irq_exit(cc);
+	bcma_gpio_irq_domain_exit(cc);
 	gpiochip_remove(&cc->gpio);
 	return 0;
 }
--- a/include/linux/bcma/bcma_driver_chipcommon.h
+++ b/include/linux/bcma/bcma_driver_chipcommon.h
@@ -646,6 +646,7 @@ struct bcma_drv_cc {
 	spinlock_t gpio_lock;
 #ifdef CONFIG_BCMA_DRIVER_GPIO
 	struct gpio_chip gpio;
+	struct irq_domain *irq_domain;
 #endif
 };
 
