From 35eecd10ee57b9d4f31e12598296b235ed2b34ae Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@openwrt.org>
Date: Wed, 13 May 2015 09:10:52 +0200
Subject: [PATCH] ARM: BCM5301X: Add DT for Buffalo WXR-1900DHP
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/Makefile                        |   1 +
 arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts | 127 ++++++++++++++++++++++
 2 files changed, 128 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -63,6 +63,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm47081-asus-rt-n18u.dtb \
 	bcm47081-buffalo-wzr-600dhp2.dtb \
 	bcm47081-buffalo-wzr-900dhp.dtb \
+	bcm4709-buffalo-wxr-1900dhp.dtb \
 	bcm4709-netgear-r8000.dtb
 dtb-$(CONFIG_ARCH_BCM_63XX) += \
 	bcm963138dvt.dtb
--- /dev/null
+++ b/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
@@ -0,0 +1,127 @@
+/*
+ * Broadcom BCM470X / BCM5301X ARM platform code.
+ * DTS for Buffalo WXR-1900DHP
+ *
+ * Copyright (C) 2015 Felix Fietkau <nbd@openwrt.org>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+/dts-v1/;
+
+#include "bcm4708.dtsi"
+
+/ {
+	compatible = "buffalo,wxr-1900dhp", "brcm,bcm4709", "brcm,bcm4708";
+	model = "Buffalo WXR-1900DHP";
+
+	chosen {
+		bootargs = "console=ttyS0,115200";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		usb {
+			label = "bcm53xx:green:usb";
+			gpios = <&chipcommon 4 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		power-amber {
+			label = "bcm53xx:amber:power";
+			gpios = <&chipcommon 5 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		power-white {
+			label = "bcm53xx:white:power";
+			gpios = <&chipcommon 6 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-on";
+		};
+
+		router-amber {
+			label = "bcm53xx:amber:router";
+			gpios = <&chipcommon 7 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		router-white {
+			label = "bcm53xx:white:router";
+			gpios = <&chipcommon 8 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		wan-amber {
+			label = "bcm53xx:amber:wan";
+			gpios = <&chipcommon 9 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		wan-white {
+			label = "bcm53xx:white:wan";
+			gpios = <&chipcommon 10 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		wireless-amber {
+			label = "bcm53xx:amber:wireless";
+			gpios = <&chipcommon 11 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		wireless-white {
+			label = "bcm53xx:white:wireless";
+			gpios = <&chipcommon 12 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		power {
+			label = "Power";
+			linux,code = <KEY_POWER>;
+			gpios = <&chipcommon 1 GPIO_ACTIVE_LOW>;
+		};
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 15 GPIO_ACTIVE_LOW>;
+		};
+
+		aoss {
+			label = "AOSS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&chipcommon 16 GPIO_ACTIVE_LOW>;
+		};
+
+		/* Commit mode set by switch? */
+		mode {
+			label = "Mode";
+			linux,code = <KEY_SETUP>;
+			gpios = <&chipcommon 17 GPIO_ACTIVE_LOW>;
+		};
+
+		/* Switch: AP mode */
+		sw_ap {
+			label = "AP";
+			linux,code = <BTN_0>;
+			gpios = <&chipcommon 18 GPIO_ACTIVE_LOW>;
+		};
+
+		eject {
+			label = "USB eject";
+			linux,code = <KEY_EJECTCD>;
+			gpios = <&chipcommon 20 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
