/dts-v1/;

/include/ "vr9.dtsi"

/ {
	model = "BTHOMEHUBV5A - BT Home Hub 5A";

	chosen {
		bootargs = "console=ttyLTQ0,115200 init=/etc/preinit";

		leds {
			boot = &power_green;
			failsafe = &power_red;
			running = &power_blue;

			internet = &broadband_blue;
			wifi = &wireless_blue;
		};
	};

	memory@0 {
		reg = <0x0 0x8000000>;
	};

	fpi@10000000 {
		localbus@0 {
			nand-parts@0 {
				compatible = "gen_nand", "lantiq,nand-xway";
				lantiq,cs = <1>;
				bank-width = <2>;
				reg = <0x1 0x0 0x2000000>;
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "u-boot";
					reg = <0x0 0x40000>;
					read-only;
				};
				partition@40000 {
					label = "uboot-env";
					reg = <0x40000 0x40000>;
				};
				caldata: partition@80000 {
					label = "caldata";
					reg = <0x80000 0x20000>;
					read-only;
				};
				partition@a0000 {
					label = "kernel";
					reg = <0xa0000 0x200000>;
				};
				partition@2a0000 {
					label = "ubi";
					reg = <0x2a0000 0x7d60000>;
				};
			};
		};

		gpio: pinmux@E100B10 {
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			interrupt-parent = <&icu0>;
			interrupts = <166 135 66 40 41 42 38>;

			state_default: pinmux {
				mdio {
					lantiq,groups = "mdio";
					lantiq,function = "mdio";
				};
				pci_rst {
					lantiq,pins = "io21";
					lantiq,output = <1>;
					lantiq,open-drain;
				};
				pcie_rst {
					lantiq,pins = "io38";
					lantiq,pull = <0>;
					lantiq,output = <1>;
					lantiq,open-drain;
				};
				usb_vbus {
					lantiq,pins = "io33";
					lantiq,pull = <0>;
					lantiq,open-drain = <0>;
					lantiq,output = <1>;
				};
				nand_out {
					lantiq,groups = "nand cle", "nand ale";
					lantiq,function = "ebu";
					lantiq,output = <1>;
					lantiq,open-drain = <0>;
					lantiq,pull = <0>;
				};
				nand_cs1 {
					lantiq,groups = "nand cs1";
					lantiq,function = "ebu";
					lantiq,open-drain = <0>;
					lantiq,pull = <0>;
				};
			};
		};

		ifxhcd@E101000 {
			status = "okay";
			gpios = <&gpio 33 0>;
		};

		pci@E105400 {
			status = "okay";
			lantiq,bus-clock = <33333333>;
			interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
			interrupt-map = <0x7000 0 0 1 &icu0 30 1>;
			gpio-reset = <&gpio 21 0>;
		};
	};

	gphy-xrx200 {
		compatible = "lantiq,phy-xrx200";
		firmware1 = "lantiq/vr9_phy11g_a1x.bin";	/*VR9 1.1*/
		firmware2 = "lantiq/vr9_phy11g_a2x.bin";	/*VR9 1.2*/
		phys = [ 00 01 ];
	};

	ath9k_eep {
		compatible = "ath9k,eeprom";
		ath,eep-flash = <&caldata 0x1000>;
		ath,mac-offset = <0x110c>;
		ath,mac-increment = <2>;
		ath,pci-slot = <0xe>; /* 14 */
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 2 1>;
			linux,code = <0x198>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 25 1>;
			linux,code = <0x211>;
		};

		restart {
			label = "restart";
			gpios = <&gpio 39 1>;
			linux,code = <0x198>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		/* broadband-* is a single RGB led */
		broadband-red {
			label = "bthomehubv5a:red:broadband";
			gpios = <&gpio 0 1>;
		};
		broadband-green {
			label = "bthomehubv5a:green:broadband";
			gpios = <&gpio 3 1>;
		};
		broadband_blue: broadband-blue {
			label = "bthomehubv5a:blue:broadband";
			gpios = <&gpio 8 1>;
		};

		/* wireless-* is a single RGB led */
		wireless-red {
			label = "bthomehubv5a:red:wireless";
			gpios = <&gpio 9 1>;
		};
		wireless-green {
			label = "bthomehubv5a:green:wireless";
			gpios = <&gpio 10 1>;
		};
		wireless_blue: wireless-blue {
			label = "bthomehubv5a:blue:wireless";
			gpios = <&gpio 11 1>;
		};

		/* power-* is a single RGB led */
		power_red: power-red {
			label = "bthomehubv5a:red:power";
			gpios = <&gpio 12 1>;
		};
		power_green: power-green {
			label = "bthomehubv5a:green:power";
			gpios = <&gpio 14 1>;
			default-state = "keep";
		};
		power_blue: power-blue {
			label = "bthomehubv5a:blue:power";
			gpios = <&gpio 15 1>;
		};

		dimmed {
			label = "dimmed";
			gpios = <&gpio 19 0>;
		};
	};
};

&eth0 {
	lan: interface@0 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;
		mtd-mac-address = <&caldata 0x110c>;
		lantiq,switch;

		ethernet@0 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <0>;
			phy-mode = "rgmii";
			phy-handle = <&phy0>;
		};
		ethernet@1 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <1>;
			phy-mode = "rgmii";
			phy-handle = <&phy1>;
		};
		ethernet@2 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <2>;
			phy-mode = "gmii";
			phy-handle = <&phy11>;
		};
		ethernet@4 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <4>;
			phy-mode = "gmii";
			phy-handle = <&phy13>;
		};
	};

	wan: interface@1 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <1>;
		mtd-mac-address = <&caldata 0x110c>;
		mtd-mac-address-increment = <4>;
		lantiq,wan;

		ethernet@5 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <5>;
			phy-mode = "rgmii";
			phy-handle = <&phy5>;
		};
	};

	mdio@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";

		phy0: ethernet-phy@0 {
			reg = <0x0>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy1: ethernet-phy@1 {
			reg = <0x1>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy5: ethernet-phy@5 {
			reg = <0x5>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy11: ethernet-phy@11 {
			reg = <0x11>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy13: ethernet-phy@13 {
			reg = <0x13>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
	};
};
