#!/bin/sh
#
# Copyright (C) 2012-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/mcs814x.sh

board_config_update

board=$(mcs814x_board_name)

case "$board" in
dlan-usb-extender)
	ucidef_set_led_usbdev "usb" "USB" "dlan-usb-extender:green:usb" "2-1"
	;;
rbt-832)
	ucidef_set_led_usbdev "usb1" "USB1" "rbt-832:red:usb0" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "rbt-832:red:usb1" "1-2"
	ucidef_set_led_usbdev "usb3" "USB3" "rbt-832:red:usb2" "1-3"
	ucidef_set_led_usbdev "usb4" "USB4" "rbt-832:red:usb3" "1-4"
	ucidef_set_led_netdev "eth" "eth" "rbt-832:red:ethernet" "eth0"
	;;
esac

board_config_flush

exit 0
