From 61e17c2f864698033f4661e1fc7ba63d4d982491 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 7 Dec 2015 17:21:55 +0100
Subject: [PATCH 40/53] nand: add mtk-nand hack/hook

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/mtd/nand/mtk_nand.c         |   34 ++++++++++++++++++++++++++++++----
 drivers/mtd/nand/nand_base.c        |    9 ++++++++-
 drivers/mtd/nand/nand_device_list.h |    2 ++
 include/linux/mtd/nand.h            |    4 ++++
 4 files changed, 44 insertions(+), 5 deletions(-)

--- a/drivers/mtd/nand/mtk_nand.c
+++ b/drivers/mtd/nand/mtk_nand.c
@@ -110,6 +110,10 @@ int part_num = NUM_PARTITIONS;
 int manu_id;
 int dev_id;
 
+/* this constant was taken from linux/nand/nand.h v 3.14
+ * in later versions it seems it was removed in order to save a bit of space
+ */
+#define NAND_MAX_OOBSIZE 774
 static u8 local_oob_buf[NAND_MAX_OOBSIZE];
 
 static u8 nand_badblock_offset = 0;
@@ -348,7 +352,7 @@ mtk_nand_check_bch_error(struct mtd_info
 		if (0xF == u4ErrNum) {
 			mtd->ecc_stats.failed++;
 			bRet = false;
-			//printk(KERN_ERR"UnCorrectable at PageAddr=%d\n", u4PageAddr);
+			printk(KERN_ERR"mtk_nand: UnCorrectable at PageAddr=%d\n", u4PageAddr);
 		} else {
 			for (i = 0; i < ((u4ErrNum + 1) >> 1); ++i) {
 				au4ErrBitLoc[i] = DRV_Reg32(ECC_DECEL0_REG32 + i);
@@ -1422,7 +1426,7 @@ mtk_nand_erase_hw(struct mtd_info *mtd,
 {
 	struct nand_chip *chip = (struct nand_chip *)mtd->priv;
 
-	chip->erase_cmd(mtd, page);
+	chip->erase(mtd, page);
 
 	return chip->waitfunc(mtd, chip);
 }
@@ -2094,8 +2098,8 @@ mtk_nand_probe(struct platform_device *p
 	nand_chip->write_page = mtk_nand_write_page;
 	nand_chip->ecc.write_oob = mtk_nand_write_oob;
 	nand_chip->block_markbad = mtk_nand_block_markbad;   // need to add nand_get_device()/nand_release_device().
-	//	nand_chip->erase = mtk_nand_erase;	
-	//    nand_chip->read_page = mtk_nand_read_page;
+	nand_chip->erase_mtk = mtk_nand_erase;	
+	nand_chip->read_page = mtk_nand_read_page;
 	nand_chip->ecc.read_oob = mtk_nand_read_oob;
 	nand_chip->block_bad = mtk_nand_block_bad;
 
@@ -2175,6 +2179,21 @@ mtk_nand_probe(struct platform_device *p
 	nand_chip->pagemask = (nand_chip->chipsize >> nand_chip->page_shift) - 1;
 	nand_chip->phys_erase_shift = ffs(mtd->erasesize) - 1;
 	nand_chip->chip_shift = ffs(nand_chip->chipsize) - 1;//0x1C;//ffs(nand_chip->chipsize) - 1;
+
+	/* allocate buffers or call select_chip here or a bit earlier*/
+	{
+		struct nand_buffers *nbuf = kzalloc(sizeof(*nbuf) + mtd->writesize + mtd->oobsize * 3, GFP_KERNEL);
+		if (!nbuf) {
+			return -ENOMEM;
+		}
+		nbuf->ecccalc = (uint8_t *)(nbuf + 1);
+		nbuf->ecccode = nbuf->ecccalc + mtd->oobsize;
+		nbuf->databuf = nbuf->ecccode + mtd->oobsize;
+
+		nand_chip->buffers = nbuf;
+		nand_chip->options |= NAND_OWN_BUFFERS;
+	}
+
 	nand_chip->oob_poi = nand_chip->buffers->databuf + mtd->writesize;
 	nand_chip->badblockpos = 0;
 
@@ -2251,6 +2270,9 @@ out:
 	MSG(INIT, "[NFI] mtk_nand_probe fail, err = %d!\n", err);
 	nand_release(mtd);
 	platform_set_drvdata(pdev, NULL);
+	if ( NULL != nand_chip->buffers) {
+		kfree(nand_chip->buffers);
+	}
 	kfree(host);
 	nand_disable_clock();
 	return err;
@@ -2261,8 +2283,12 @@ mtk_nand_remove(struct platform_device *
 {
 	struct mtk_nand_host *host = platform_get_drvdata(pdev);
 	struct mtd_info *mtd = &host->mtd;
+	struct nand_chip *nand_chip = &host->nand_chip;
 
 	nand_release(mtd);
+	if ( NULL != nand_chip->buffers) {
+		kfree(nand_chip->buffers);
+	}
 	kfree(host);
 	nand_disable_clock();
 
--- a/drivers/mtd/nand/nand_base.c
+++ b/drivers/mtd/nand/nand_base.c
@@ -1727,6 +1727,9 @@ static int nand_do_read_ops(struct mtd_i
 						 __func__, buf);
 
 read_retry:
+#ifdef CONFIG_MTK_MTD_NAND
+			ret = chip->read_page(mtd, chip, bufpoi, page);
+#else
 			chip->cmdfunc(mtd, NAND_CMD_READ0, 0x00, page);
 
 			/*
@@ -1745,6 +1748,7 @@ read_retry:
 			else
 				ret = chip->ecc.read_page(mtd, chip, bufpoi,
 							  oob_required, page);
+#endif /* CONFIG_MTK_MTD_NAND */
 			if (ret < 0) {
 				if (use_bufpoi)
 					/* Invalidate page cache */
@@ -2932,8 +2936,11 @@ int nand_erase_nand(struct mtd_info *mtd
 		if (page <= chip->pagebuf && chip->pagebuf <
 		    (page + pages_per_block))
 			chip->pagebuf = -1;
-
+#ifdef CONFIG_MTK_MTD_NAND
+		status = chip->erase_mtk(mtd, page & chip->pagemask);
+#else
 		status = chip->erase(mtd, page & chip->pagemask);
+#endif /* CONFIG_MTK_MTD_NAND */
 
 		/*
 		 * See if operation failed and additional status checks are
--- a/drivers/mtd/nand/nand_device_list.h
+++ b/drivers/mtd/nand/nand_device_list.h
@@ -43,6 +43,8 @@ static const flashdev_info gen_FlashTabl
 	{0xADBC, 0x905554, 5, 16, 512, 128, 2048, 64, 0x10801011, "H9DA4GH4JJAMC", 0},
     {0x01F1, 0x801D01, 4, 8, 128, 128, 2048, 64, 0x30C77fff, "S34ML01G100TF", 0},
     {0x92F1, 0x8095FF, 4, 8, 128, 128, 2048, 64, 0x30C77fff, "F59L1G81A", 0},
+	{0xC8DA, 0x909544, 5, 8, 256, 128, 2048, 64, 0x30C77fff, "F59L2G81A", 0},
+	{0xC8DC, 0x909554, 5, 8, 512, 128, 2048, 64, 0x30C77fff, "F59L4G81A", 0},
 	{0xECD3, 0x519558, 5, 8, 1024, 128, 2048, 64, 0x44333, "K9K8G8000", 0},
     {0xC2F1, 0x801DC2, 4, 8, 128, 128, 2048, 64, 0x30C77fff, "MX30LF1G08AA", 0},
     {0x98D3, 0x902676, 5, 8, 1024, 256, 4096, 224, 0x00C25332, "TC58NVG3S0F", 0},
--- a/include/linux/mtd/nand.h
+++ b/include/linux/mtd/nand.h
@@ -665,6 +665,10 @@ struct nand_chip {
 	int (*write_page)(struct mtd_info *mtd, struct nand_chip *chip,
 			uint32_t offset, int data_len, const uint8_t *buf,
 			int oob_required, int page, int cached, int raw);
+#ifdef CONFIG_MTK_MTD_NAND
+	int (*read_page)(struct mtd_info *mtd, struct nand_chip *chip, u8 *buf, int page);
+	int (*erase_mtk)(struct mtd_info *mtd, int page);
+#endif /* CONFIG_MTK_MTD_NAND */
 	int (*onfi_set_features)(struct mtd_info *mtd, struct nand_chip *chip,
 			int feature_addr, uint8_t *subfeature_para);
 	int (*onfi_get_features)(struct mtd_info *mtd, struct nand_chip *chip,
