From 0afae16fffe2cf547fad21279c120bedf19e9b8e Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Wed, 6 Jan 2016 21:55:10 +0100
Subject: [PATCH 24/91] dt-bindings: add MediaTek PCIe binding documentation

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 .../devicetree/bindings/pci/mediatek-pcie.txt      |  140 ++++++++++++++++++++
 1 file changed, 140 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/pci/mediatek-pcie.txt

diff --git a/Documentation/devicetree/bindings/pci/mediatek-pcie.txt b/Documentation/devicetree/bindings/pci/mediatek-pcie.txt
new file mode 100644
index 0000000..8fea3ed
--- /dev/null
+++ b/Documentation/devicetree/bindings/pci/mediatek-pcie.txt
@@ -0,0 +1,140 @@
+Mediatek PCIe controller
+
+Required properties:
+- compatible: Should be one of:
+	- "mediatek,mt2701-pcie"
+	- "mediatek,mt7623-pcie"
+- device_type: Must be "pci"
+- reg: A list of physical base address and length for each set of controller
+  registers. A list of register ranges to use. Must contain an
+    entry for each entry in the reg-names property.
+- reg-names: Must include the following entries:
+  "pcie": PCIe registers
+  "pcie phy0": PCIe PHY0 registers
+  "pcie phy1": PCIe PHY0 registers
+  "pcie phy2": PCIe PHY0 registers
+- interrupts: A list of interrupt outputs of the controller. Must contain an
+  entry for each entry in the interrupt-names property.
+- interrupt-names: Must include the following entries:
+  "pcie0": The interrupt that is asserted for port0
+  "pcie1": The interrupt that is asserted for port1
+  "pcie2": The interrupt that is asserted for port2
+- bus-range: Range of bus numbers associated with this controller
+- #address-cells: Address representation for root ports (must be 3)
+- #size-cells: Size representation for root ports (must be 2)
+- ranges: Describes the translation of addresses for root ports and standard
+  PCI regions. The entries must be 6 cells each.
+  Please refer to the standard PCI bus binding document for a more detailed
+  explanation.
+- #interrupt-cells: Size representation for interrupts (must be 1)
+- clocks: Must contain an entry for each entry in clock-names.
+  See ../clocks/clock-bindings.txt for details.
+- clock-names: Must include the following entries:
+  - pcie0
+  - pcie1
+  - pcie2
+- resets: Must contain an entry for each entry in reset-names.
+  See ../reset/reset.txt for details.
+- reset-names: Must include the following entries:
+  - pcie0
+  - pcie1
+  - pcie2
+- mediatek,hifsys: Must contain a phandle to the HIFSYS syscon range.
+Root ports are defined as subnodes of the PCIe controller node.
+
+Required properties:
+- device_type: Must be "pci"
+- assigned-addresses: Address and size of the port configuration registers
+- reg: PCI bus address of the root port
+- #address-cells: Must be 3
+- #size-cells: Must be 2
+- ranges: Sub-ranges distributed from the PCIe controller node. An empty
+  property is sufficient.
+
+Example:
+
+SoC DTSI:
+
+	hifsys: clock-controller@1a000000 {
+		compatible = "mediatek,mt7623-hifsys",
+			     "mediatek,mt2701-hifsys",
+			     "syscon";
+		reg = <0 0x1a000000 0 0x1000>;
+		#clock-cells = <1>;
+		#reset-cells = <1>;
+	};
+
+	pcie-controller@1a140000 {
+		compatible = "mediatek,mt7623-pcie";
+		device_type = "pci";
+		reg = <0 0x1a140000 0 0x8000>, /* PCI-Express registers */
+		      <0 0x1a149000 0 0x1000>, /* PCI-Express PHY0 */
+		      <0 0x1a14a000 0 0x1000>, /* PCI-Express PHY1 */
+		      <0 0x1a244000 0 0x1000>; /* PCI-Express PHY2 */
+		reg-names = "pcie", "pcie phy0", "pcie phy1", "pcie phy2";
+		interrupts = <GIC_SPI 193 IRQ_TYPE_LEVEL_LOW>,
+			     <GIC_SPI 194 IRQ_TYPE_LEVEL_LOW>,
+			     <GIC_SPI 195 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-names = "pcie0", "pcie1", "pcie2";
+		clocks = <&topckgen CLK_TOP_ETHIF_SEL>;
+		clock-names = "pcie";
+		power-domains = <&scpsys MT2701_POWER_DOMAIN_HIF>;
+		resets = <&hifsys MT2701_HIFSYS_PCIE0_RST>,
+			 <&hifsys MT2701_HIFSYS_PCIE1_RST>,
+			 <&hifsys MT2701_HIFSYS_PCIE2_RST>;
+		reset-names = "pcie0", "pice1", "pcie2";
+
+		bus-range = <0x00 0xff>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+                mediatek,hifsys = <&hifsys>;
+
+		ranges = <0x81000000 0 0x1a160000 0 0x1a160000 0 0x00010000 /* io space */
+			  0x83000000 0 0x60000000 0 0x60000000 0 0x10000000>; /* pci memory */
+
+		status = "disabled";
+
+		pcie@1,0 {
+			device_type = "pci";
+			reg = <0x0800 0 0 0 0>;
+
+			#address-cells = <3>;
+			#size-cells = <2>;
+			ranges;
+
+			status = "disabled";
+		};
+
+		pcie@2,0{
+			device_type = "pci";
+			reg = <0x1000 0 0 0 0>;
+
+			#address-cells = <3>;
+			#size-cells = <2>;
+			ranges;
+
+			status = "disabled";
+		};
+
+		pcie@3,0{
+			device_type = "pci";
+			reg = <0x1800 0 0 0 0>;
+
+			#address-cells = <3>;
+			#size-cells = <2>;
+			ranges;
+
+			status = "disabled";
+		};
+	};
+
+Board DTS:
+
+	pcie-controller {
+		status = "okay";
+
+		pci@1,0 {
+			status = "okay";
+		};
+	};
-- 
1.7.10.4

