From 7f9781f9875f2aa638d5afdaa9709fa1ef9bda8d Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 18 Feb 2016 15:28:14 +0000
Subject: [PATCH 156/170] BCM270X_DT: at86rf233 overlay - drop to 3MHz

The consensus is that 6MHz is too fast, but that 3MHz is OK.

See: https://github.com/raspberrypi/linux/issues/1294
     https://github.com/raspberrypi/linux/issues/1151
---
 arch/arm/boot/dts/overlays/README                | 2 +-
 arch/arm/boot/dts/overlays/at86rf233-overlay.dts | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -188,7 +188,7 @@ Load:   dtoverlay=at86rf233,<param>=<val
 Params: interrupt               GPIO used for INT (default 23)
         reset                   GPIO used for Reset (default 24)
         sleep                   GPIO used for Sleep (default 25)
-        speed                   SPI bus speed in Hz (default 6000000)
+        speed                   SPI bus speed in Hz (default 3000000)
         trim                    Fine tuning of the internal capacitance
                                 arrays (0=+0pF, 15=+4.5pF, default 15)
 
--- a/arch/arm/boot/dts/overlays/at86rf233-overlay.dts
+++ b/arch/arm/boot/dts/overlays/at86rf233-overlay.dts
@@ -25,7 +25,7 @@
 				interrupts = <23 4>; /* active high */
 				reset-gpio = <&gpio 24 1>;
 				sleep-gpio = <&gpio 25 1>;
-				spi-max-frequency = <6000000>;
+				spi-max-frequency = <3000000>;
 				xtal-trim = /bits/ 8 <0xf>;
 			};
 		};
