From 00f9956384e3cf011e0d5ffd211847bf9336ec78 Mon Sep 17 00:00:00 2001
From: Michal Suchanek <hramrach@gmail.com>
Date: Tue, 26 May 2015 17:01:33 +0200
Subject: [PATCH] ARM: dts: sun4i: Add NAND controller pin definitions

Define the NAND controller pin configs.

Signed-off-by: Michal Suchanek <hramrach@gmail.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun4i-a10.dtsi | 80 ++++++++++++++++++++++++++++++++++++++++
 1 file changed, 80 insertions(+)

--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -774,6 +774,86 @@
 				allwinner,drive = <SUN4I_PINCTRL_10_MA>;
 				allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
 			};
+
+			nand_pins_a: nand_base0@0 {
+				allwinner,pins = "PC0", "PC1", "PC2",
+						"PC5", "PC8", "PC9", "PC10",
+						"PC11", "PC12", "PC13", "PC14",
+						"PC15", "PC16";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs0_pins_a: nand_cs@0 {
+				allwinner,pins = "PC4";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs1_pins_a: nand_cs@1 {
+				allwinner,pins = "PC3";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs2_pins_a: nand_cs@2 {
+				allwinner,pins = "PC17";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs3_pins_a: nand_cs@3 {
+				allwinner,pins = "PC18";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs4_pins_a: nand_cs@4 {
+				allwinner,pins = "PC19";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs5_pins_a: nand_cs@5 {
+				allwinner,pins = "PC20";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs6_pins_a: nand_cs@6 {
+				allwinner,pins = "PC21";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_cs7_pins_a: nand_cs@7 {
+				allwinner,pins = "PC22";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_rb0_pins_a: nand_rb@0 {
+				allwinner,pins = "PC6";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			nand_rb1_pins_a: nand_rb@1 {
+				allwinner,pins = "PC7";
+				allwinner,function = "nand0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
 		};
 
 		timer@01c20c00 {
