From 9789f1fd1fd1d0551132778414faf8e2254408c1 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Fri, 30 Oct 2015 15:44:01 +0100
Subject: [PATCH] ARM: BCM5301X: Add missing Netgear R8000 LEDs
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add a bunch of LEDs missing for the Netgear R8000: wireless, wps, 5Ghz radio
and USB LEDs.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm4709-netgear-r8000.dts | 30 +++++++++++++++++++++++++++++
 1 file changed, 30 insertions(+)

--- a/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
+++ b/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
@@ -50,6 +50,36 @@
 			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
 			linux,default-trigger = "default-off";
 		};
+
+		wireless {
+			label = "bcm53xx:white:wireless";
+			gpios = <&chipcommon 14 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		wps {
+			label = "bcm53xx:white:wps";
+			gpios = <&chipcommon 15 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		5ghz-2 {
+			label = "bcm53xx:white:5ghz-2";
+			gpios = <&chipcommon 16 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+
+		usb3 {
+			label = "bcm53xx:white:usb3";
+			gpios = <&chipcommon 17 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+
+		usb2 {
+			label = "bcm53xx:white:usb2";
+			gpios = <&chipcommon 18 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
 	};
 
 	gpio-keys {
